# Congestion check: Balancing congestion by handover TCH/H -> TCH/F
# One BTS, TCH/H are congested and should move to TCH/F.

network
 handover2 min-free-slots tch/f 0
 handover2 min-free-slots tch/h 6

create-bts trx-count 1 timeslots c+s4 TCH/F TCH/F TCH/F TCH/H  TCH/H TCH/H PDCH
set-ts-use trx 0 0 states        *    -     -     -     TCH/H- -     -     *
meas-rep lchan 0 0 4 0 rxlev 30 rxqual 0 ta 0
expect-no-chan
congestion-check
expect-as from lchan 0 0 4 0 to lchan 0 0 1 0
expect-ts-use trx 0 0 states * TCH/F - - - - - *
