# Congestion check: Balancing congestion by handover TCH/F -> TCH/H
# Two BTS, one MS in the first congested BTS must handover to
# less-congested TCH/H of second BTS, in order to balance congestion

create-n-bts 2
network
 handover2 min-free-slots tch/f 4
 handover2 min-free-slots tch/h 4
set-ts-use trx 0 0 states * TCH/F TCH/F - - TCH/H- - -
meas-rep lchan 0 0 1 0 rxlev 30 rxqual 0 ta 0 neighbors 30
expect-no-chan
congestion-check
expect-ho from lchan 0 0 1 0 to lchan 1 0 1 0
expect-ts-use trx 0 0 states * -     TCH/F - - TCH/H- - -
expect-ts-use trx 1 0 states * TCH/F -     - - -      - -

