# Congestion check: Balancing congestion by handover TCH/F -> TCH/H
# One BTS, and TCH/F are considered congested, TCH/H are not.

create-n-bts 1
network
 bts 0
  handover2 min-free-slots tch/f 3
  handover2 min-free-slots tch/h 0
set-ts-use trx 0 0 states * TCH/F TCH/F - - TCH/H- - -
meas-rep lchan 0 0 1 0 rxlev 30 rxqual 0 ta 0 neighbors 30
expect-no-chan
congestion-check
expect-as from lchan 0 0 1 0 to lchan 0 0 5 1
expect-ts-use trx 0 0 states * - TCH/F - - TCH/HH - -

