# Do not oscillate handover when the BTS applies BS power reduction

create-bts trx-count 1 timeslots c+s4 TCH/F TCH/F TCH/F TCH/F TCH/F TCH/F PDCH
create-bts trx-count 1 timeslots c+s4 TCH/F TCH/F TCH/F TCH/F TCH/F TCH/F PDCH

set-ts-use trx 0 0 states        *    TCH/F -     -     -     -     -     *

meas-rep repeat 10 bspower 20 lchan 0 0 1 0 rxlev 20 rxqual 0 ta 0 neighbors 30
# there should be no handover, because the bspower reduction of 20 with an rxlev of 20 (= 40) is stronger than the
# neighbor at 30.
expect-no-chan
