# TCH/H has good RxLev and RxQual, AFS bias should not move it to TCH/F

network
 handover2 power budget hysteresis 3
 handover2 min rxlev -90
 handover2 min rxqual 5
 handover2 afs-bias rxlev 1

create-bts trx-count 1 timeslots c+s4 TCH/F TCH/F TCH/F TCH/H  TCH/H TCH/H PDCH
set-ts-use trx 0 0 states        *    -     -     -     TCH/H- -     -     *
meas-rep lchan 0 0 4 0 rxlev 50 rxqual 1 ta 0
# The TCH/H should stay where it is, because its levels are fine.
expect-no-chan
