===test_acc_mgr_no_ramp===
(bts=0) ACC: New ACC allowed subset 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
BTS allocation OK in test_acc_mgr_no_ramp()
do_allowed_len_adm_loop(1)
(bts=0) ACC: update ACC allowed active subset 0x3ff -> 0x3fe (active_len=9, ramp_len=10, adm_len=9, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x01, allowed: 1 2 3 4 5 6 7 8 9
(bts=0) ACC: update ACC allowed active subset 0x3fe -> 0x3fc (active_len=8, ramp_len=10, adm_len=8, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x03, allowed: 2 3 4 5 6 7 8 9
(bts=0) ACC: update ACC allowed active subset 0x3fc -> 0x3f8 (active_len=7, ramp_len=10, adm_len=7, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x07, allowed: 3 4 5 6 7 8 9
(bts=0) ACC: update ACC allowed active subset 0x3f8 -> 0x3f0 (active_len=6, ramp_len=10, adm_len=6, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x0f, allowed: 4 5 6 7 8 9
(bts=0) ACC: update ACC allowed active subset 0x3f0 -> 0x3e0 (active_len=5, ramp_len=10, adm_len=5, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x1f, allowed: 5 6 7 8 9
(bts=0) ACC: update ACC allowed active subset 0x3e0 -> 0x3c0 (active_len=4, ramp_len=10, adm_len=4, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x3f, allowed: 6 7 8 9
(bts=0) ACC: update ACC allowed active subset 0x3c0 -> 0x380 (active_len=3, ramp_len=10, adm_len=3, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x7f, allowed: 7 8 9
(bts=0) ACC: update ACC allowed active subset 0x380 -> 0x300 (active_len=2, ramp_len=10, adm_len=2, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0xff, allowed: 8 9
(bts=0) ACC: update ACC allowed active subset 0x300 -> 0x200 (active_len=1, ramp_len=10, adm_len=1, perm_len=10, rotation=on)
pcu_info_update(): t2=0x01 t3=0xff, allowed: 9
(bts=0) ACC: update ACC allowed active subset 0x200 -> 0x000 (active_len=0, ramp_len=10, adm_len=0, perm_len=10, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x001 (active_len=1, ramp_len=10, adm_len=1, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfe, allowed: 0
(bts=0) ACC: update ACC allowed active subset 0x001 -> 0x003 (active_len=2, ramp_len=10, adm_len=2, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfc, allowed: 0 1
(bts=0) ACC: update ACC allowed active subset 0x003 -> 0x007 (active_len=3, ramp_len=10, adm_len=3, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf8, allowed: 0 1 2
(bts=0) ACC: update ACC allowed active subset 0x007 -> 0x00f (active_len=4, ramp_len=10, adm_len=4, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf0, allowed: 0 1 2 3
(bts=0) ACC: update ACC allowed active subset 0x00f -> 0x01f (active_len=5, ramp_len=10, adm_len=5, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe0, allowed: 0 1 2 3 4
(bts=0) ACC: update ACC allowed active subset 0x01f -> 0x03f (active_len=6, ramp_len=10, adm_len=6, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xc0, allowed: 0 1 2 3 4 5
(bts=0) ACC: update ACC allowed active subset 0x03f -> 0x07f (active_len=7, ramp_len=10, adm_len=7, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x80, allowed: 0 1 2 3 4 5 6
(bts=0) ACC: update ACC allowed active subset 0x07f -> 0x0ff (active_len=8, ramp_len=10, adm_len=8, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x00, allowed: 0 1 2 3 4 5 6 7
(bts=0) ACC: update ACC allowed active subset 0x0ff -> 0x1ff (active_len=9, ramp_len=10, adm_len=9, perm_len=10, rotation=on)
pcu_info_update(): t2=0x02 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8
(bts=0) ACC: update ACC allowed active subset 0x1ff -> 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
pcu_info_update(): t2=0x00 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8 9
do_allowed_len_adm_loop(4)
(bts=0) ACC: update ACC allowed active subset 0x3ff -> 0x3f0 (active_len=6, ramp_len=10, adm_len=6, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x0f, allowed: 4 5 6 7 8 9
(bts=0) ACC: update ACC allowed active subset 0x3f0 -> 0x300 (active_len=2, ramp_len=10, adm_len=2, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0xff, allowed: 8 9
(bts=0) ACC: update ACC allowed active subset 0x300 -> 0x000 (active_len=0, ramp_len=10, adm_len=0, perm_len=10, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x00f (active_len=4, ramp_len=10, adm_len=4, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf0, allowed: 0 1 2 3
(bts=0) ACC: update ACC allowed active subset 0x00f -> 0x0ff (active_len=8, ramp_len=10, adm_len=8, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x00, allowed: 0 1 2 3 4 5 6 7
(bts=0) ACC: update ACC allowed active subset 0x0ff -> 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
pcu_info_update(): t2=0x00 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8 9
*** Barring some ACCs ***
(bts=0) ACC: New ACC allowed subset 0x15a (active_len=5, ramp_len=10, adm_len=10, perm_len=5, rotation=off)
pcu_info_update(): t2=0x02 t3=0xa5, allowed: 1 3 4 6 8
do_allowed_len_adm_loop(1)
(bts=0) ACC: update ACC allowed active subset 0x15a -> 0x15a (active_len=5, ramp_len=10, adm_len=9, perm_len=5, rotation=off)
(bts=0) ACC: update ACC allowed active subset 0x15a -> 0x15a (active_len=5, ramp_len=10, adm_len=8, perm_len=5, rotation=off)
(bts=0) ACC: update ACC allowed active subset 0x15a -> 0x15a (active_len=5, ramp_len=10, adm_len=7, perm_len=5, rotation=off)
(bts=0) ACC: update ACC allowed active subset 0x15a -> 0x15a (active_len=5, ramp_len=10, adm_len=6, perm_len=5, rotation=off)
(bts=0) ACC: update ACC allowed active subset 0x15a -> 0x158 (active_len=4, ramp_len=10, adm_len=4, perm_len=5, rotation=on)
pcu_info_update(): t2=0x02 t3=0xa7, allowed: 3 4 6 8
(bts=0) ACC: update ACC allowed active subset 0x158 -> 0x150 (active_len=3, ramp_len=10, adm_len=3, perm_len=5, rotation=on)
pcu_info_update(): t2=0x02 t3=0xaf, allowed: 4 6 8
(bts=0) ACC: update ACC allowed active subset 0x150 -> 0x140 (active_len=2, ramp_len=10, adm_len=2, perm_len=5, rotation=on)
pcu_info_update(): t2=0x02 t3=0xbf, allowed: 6 8
(bts=0) ACC: update ACC allowed active subset 0x140 -> 0x100 (active_len=1, ramp_len=10, adm_len=1, perm_len=5, rotation=on)
pcu_info_update(): t2=0x02 t3=0xff, allowed: 8
(bts=0) ACC: update ACC allowed active subset 0x100 -> 0x000 (active_len=0, ramp_len=10, adm_len=0, perm_len=5, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x002 (active_len=1, ramp_len=10, adm_len=1, perm_len=5, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfd, allowed: 1
(bts=0) ACC: update ACC allowed active subset 0x002 -> 0x00a (active_len=2, ramp_len=10, adm_len=2, perm_len=5, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf5, allowed: 1 3
(bts=0) ACC: update ACC allowed active subset 0x00a -> 0x01a (active_len=3, ramp_len=10, adm_len=3, perm_len=5, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe5, allowed: 1 3 4
(bts=0) ACC: update ACC allowed active subset 0x01a -> 0x05a (active_len=4, ramp_len=10, adm_len=4, perm_len=5, rotation=on)
pcu_info_update(): t2=0x03 t3=0xa5, allowed: 1 3 4 6
(bts=0) ACC: update ACC allowed active subset 0x05a -> 0x15a (active_len=5, ramp_len=10, adm_len=5, perm_len=5, rotation=off)
pcu_info_update(): t2=0x02 t3=0xa5, allowed: 1 3 4 6 8
(bts=0) ACC: update ACC allowed active subset 0x15a -> 0x15a (active_len=5, ramp_len=10, adm_len=6, perm_len=5, rotation=off)
(bts=0) ACC: update ACC allowed active subset 0x15a -> 0x15a (active_len=5, ramp_len=10, adm_len=7, perm_len=5, rotation=off)
(bts=0) ACC: update ACC allowed active subset 0x15a -> 0x15a (active_len=5, ramp_len=10, adm_len=8, perm_len=5, rotation=off)
(bts=0) ACC: update ACC allowed active subset 0x15a -> 0x15a (active_len=5, ramp_len=10, adm_len=9, perm_len=5, rotation=off)
(bts=0) ACC: update ACC allowed active subset 0x15a -> 0x15a (active_len=5, ramp_len=10, adm_len=10, perm_len=5, rotation=off)
do_allowed_len_adm_loop(4)
(bts=0) ACC: update ACC allowed active subset 0x15a -> 0x15a (active_len=5, ramp_len=10, adm_len=6, perm_len=5, rotation=off)
(bts=0) ACC: update ACC allowed active subset 0x15a -> 0x140 (active_len=2, ramp_len=10, adm_len=2, perm_len=5, rotation=on)
pcu_info_update(): t2=0x02 t3=0xbf, allowed: 6 8
(bts=0) ACC: update ACC allowed active subset 0x140 -> 0x000 (active_len=0, ramp_len=10, adm_len=0, perm_len=5, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x05a (active_len=4, ramp_len=10, adm_len=4, perm_len=5, rotation=on)
pcu_info_update(): t2=0x03 t3=0xa5, allowed: 1 3 4 6
(bts=0) ACC: update ACC allowed active subset 0x05a -> 0x15a (active_len=5, ramp_len=10, adm_len=8, perm_len=5, rotation=off)
pcu_info_update(): t2=0x02 t3=0xa5, allowed: 1 3 4 6 8
(bts=0) ACC: update ACC allowed active subset 0x15a -> 0x15a (active_len=5, ramp_len=10, adm_len=10, perm_len=5, rotation=off)
*** Barring ALL ACCs ***
(bts=0) ACC: New ACC allowed subset 0x000 (active_len=0, ramp_len=10, adm_len=10, perm_len=0, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
*** Barring zero ACCs ***
(bts=0) ACC: New ACC allowed subset 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
pcu_info_update(): t2=0x00 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8 9
BTS deallocated OK in test_acc_mgr_no_ramp()
===test_acc_mgr_manual_ramp===
(bts=0) ACC: New ACC allowed subset 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
BTS allocation OK in test_acc_mgr_manual_ramp()
do_allowed_len_ramp_loop(1)
(bts=0) ACC: update ACC allowed active subset 0x3ff -> 0x3fe (active_len=9, ramp_len=9, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x01, allowed: 1 2 3 4 5 6 7 8 9
(bts=0) ACC: update ACC allowed active subset 0x3fe -> 0x3fc (active_len=8, ramp_len=8, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x03, allowed: 2 3 4 5 6 7 8 9
(bts=0) ACC: update ACC allowed active subset 0x3fc -> 0x3f8 (active_len=7, ramp_len=7, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x07, allowed: 3 4 5 6 7 8 9
(bts=0) ACC: update ACC allowed active subset 0x3f8 -> 0x3f0 (active_len=6, ramp_len=6, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x0f, allowed: 4 5 6 7 8 9
(bts=0) ACC: update ACC allowed active subset 0x3f0 -> 0x3e0 (active_len=5, ramp_len=5, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x1f, allowed: 5 6 7 8 9
(bts=0) ACC: update ACC allowed active subset 0x3e0 -> 0x3c0 (active_len=4, ramp_len=4, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x3f, allowed: 6 7 8 9
(bts=0) ACC: update ACC allowed active subset 0x3c0 -> 0x380 (active_len=3, ramp_len=3, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x7f, allowed: 7 8 9
(bts=0) ACC: update ACC allowed active subset 0x380 -> 0x300 (active_len=2, ramp_len=2, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0xff, allowed: 8 9
(bts=0) ACC: update ACC allowed active subset 0x300 -> 0x200 (active_len=1, ramp_len=1, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x01 t3=0xff, allowed: 9
(bts=0) ACC: update ACC allowed active subset 0x200 -> 0x000 (active_len=0, ramp_len=0, adm_len=10, perm_len=10, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x001 (active_len=1, ramp_len=1, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfe, allowed: 0
(bts=0) ACC: update ACC allowed active subset 0x001 -> 0x003 (active_len=2, ramp_len=2, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfc, allowed: 0 1
(bts=0) ACC: update ACC allowed active subset 0x003 -> 0x007 (active_len=3, ramp_len=3, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf8, allowed: 0 1 2
(bts=0) ACC: update ACC allowed active subset 0x007 -> 0x00f (active_len=4, ramp_len=4, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf0, allowed: 0 1 2 3
(bts=0) ACC: update ACC allowed active subset 0x00f -> 0x01f (active_len=5, ramp_len=5, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe0, allowed: 0 1 2 3 4
(bts=0) ACC: update ACC allowed active subset 0x01f -> 0x03f (active_len=6, ramp_len=6, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xc0, allowed: 0 1 2 3 4 5
(bts=0) ACC: update ACC allowed active subset 0x03f -> 0x07f (active_len=7, ramp_len=7, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x80, allowed: 0 1 2 3 4 5 6
(bts=0) ACC: update ACC allowed active subset 0x07f -> 0x0ff (active_len=8, ramp_len=8, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x00, allowed: 0 1 2 3 4 5 6 7
(bts=0) ACC: update ACC allowed active subset 0x0ff -> 0x1ff (active_len=9, ramp_len=9, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x02 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8
(bts=0) ACC: update ACC allowed active subset 0x1ff -> 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
pcu_info_update(): t2=0x00 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8 9
do_allowed_len_ramp_loop(4)
(bts=0) ACC: update ACC allowed active subset 0x3ff -> 0x3f0 (active_len=6, ramp_len=6, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x0f, allowed: 4 5 6 7 8 9
(bts=0) ACC: update ACC allowed active subset 0x3f0 -> 0x300 (active_len=2, ramp_len=2, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0xff, allowed: 8 9
(bts=0) ACC: update ACC allowed active subset 0x300 -> 0x000 (active_len=0, ramp_len=0, adm_len=10, perm_len=10, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x00f (active_len=4, ramp_len=4, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf0, allowed: 0 1 2 3
(bts=0) ACC: update ACC allowed active subset 0x00f -> 0x0ff (active_len=8, ramp_len=8, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x00, allowed: 0 1 2 3 4 5 6 7
(bts=0) ACC: update ACC allowed active subset 0x0ff -> 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
pcu_info_update(): t2=0x00 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8 9
*** Barring some ACCs ***
(bts=0) ACC: New ACC allowed subset 0x24c (active_len=4, ramp_len=10, adm_len=10, perm_len=4, rotation=off)
pcu_info_update(): t2=0x01 t3=0xb3, allowed: 2 3 6 9
do_allowed_len_ramp_loop(1)
(bts=0) ACC: update ACC allowed active subset 0x24c -> 0x24c (active_len=4, ramp_len=9, adm_len=10, perm_len=4, rotation=off)
(bts=0) ACC: update ACC allowed active subset 0x24c -> 0x24c (active_len=4, ramp_len=8, adm_len=10, perm_len=4, rotation=off)
(bts=0) ACC: update ACC allowed active subset 0x24c -> 0x24c (active_len=4, ramp_len=7, adm_len=10, perm_len=4, rotation=off)
(bts=0) ACC: update ACC allowed active subset 0x24c -> 0x24c (active_len=4, ramp_len=6, adm_len=10, perm_len=4, rotation=off)
(bts=0) ACC: update ACC allowed active subset 0x24c -> 0x24c (active_len=4, ramp_len=5, adm_len=10, perm_len=4, rotation=off)
(bts=0) ACC: update ACC allowed active subset 0x24c -> 0x248 (active_len=3, ramp_len=3, adm_len=10, perm_len=4, rotation=on)
pcu_info_update(): t2=0x01 t3=0xb7, allowed: 3 6 9
(bts=0) ACC: update ACC allowed active subset 0x248 -> 0x240 (active_len=2, ramp_len=2, adm_len=10, perm_len=4, rotation=on)
pcu_info_update(): t2=0x01 t3=0xbf, allowed: 6 9
(bts=0) ACC: update ACC allowed active subset 0x240 -> 0x200 (active_len=1, ramp_len=1, adm_len=10, perm_len=4, rotation=on)
pcu_info_update(): t2=0x01 t3=0xff, allowed: 9
(bts=0) ACC: update ACC allowed active subset 0x200 -> 0x000 (active_len=0, ramp_len=0, adm_len=10, perm_len=4, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x004 (active_len=1, ramp_len=1, adm_len=10, perm_len=4, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfb, allowed: 2
(bts=0) ACC: update ACC allowed active subset 0x004 -> 0x00c (active_len=2, ramp_len=2, adm_len=10, perm_len=4, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf3, allowed: 2 3
(bts=0) ACC: update ACC allowed active subset 0x00c -> 0x04c (active_len=3, ramp_len=3, adm_len=10, perm_len=4, rotation=on)
pcu_info_update(): t2=0x03 t3=0xb3, allowed: 2 3 6
(bts=0) ACC: update ACC allowed active subset 0x04c -> 0x24c (active_len=4, ramp_len=4, adm_len=10, perm_len=4, rotation=off)
pcu_info_update(): t2=0x01 t3=0xb3, allowed: 2 3 6 9
(bts=0) ACC: update ACC allowed active subset 0x24c -> 0x24c (active_len=4, ramp_len=5, adm_len=10, perm_len=4, rotation=off)
(bts=0) ACC: update ACC allowed active subset 0x24c -> 0x24c (active_len=4, ramp_len=6, adm_len=10, perm_len=4, rotation=off)
(bts=0) ACC: update ACC allowed active subset 0x24c -> 0x24c (active_len=4, ramp_len=7, adm_len=10, perm_len=4, rotation=off)
(bts=0) ACC: update ACC allowed active subset 0x24c -> 0x24c (active_len=4, ramp_len=8, adm_len=10, perm_len=4, rotation=off)
(bts=0) ACC: update ACC allowed active subset 0x24c -> 0x24c (active_len=4, ramp_len=9, adm_len=10, perm_len=4, rotation=off)
(bts=0) ACC: update ACC allowed active subset 0x24c -> 0x24c (active_len=4, ramp_len=10, adm_len=10, perm_len=4, rotation=off)
do_allowed_len_ramp_loop(4)
(bts=0) ACC: update ACC allowed active subset 0x24c -> 0x24c (active_len=4, ramp_len=6, adm_len=10, perm_len=4, rotation=off)
(bts=0) ACC: update ACC allowed active subset 0x24c -> 0x240 (active_len=2, ramp_len=2, adm_len=10, perm_len=4, rotation=on)
pcu_info_update(): t2=0x01 t3=0xbf, allowed: 6 9
(bts=0) ACC: update ACC allowed active subset 0x240 -> 0x000 (active_len=0, ramp_len=0, adm_len=10, perm_len=4, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x24c (active_len=4, ramp_len=4, adm_len=10, perm_len=4, rotation=off)
pcu_info_update(): t2=0x01 t3=0xb3, allowed: 2 3 6 9
(bts=0) ACC: update ACC allowed active subset 0x24c -> 0x24c (active_len=4, ramp_len=8, adm_len=10, perm_len=4, rotation=off)
(bts=0) ACC: update ACC allowed active subset 0x24c -> 0x24c (active_len=4, ramp_len=10, adm_len=10, perm_len=4, rotation=off)
*** Barring ALL ACCs ***
(bts=0) ACC: New ACC allowed subset 0x000 (active_len=0, ramp_len=10, adm_len=10, perm_len=0, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
do_allowed_len_ramp_loop(1)
(bts=0) ACC: New ACC allowed subset 0x000 (active_len=0, ramp_len=9, adm_len=10, perm_len=0, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x000 (active_len=0, ramp_len=8, adm_len=10, perm_len=0, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x000 (active_len=0, ramp_len=7, adm_len=10, perm_len=0, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x000 (active_len=0, ramp_len=6, adm_len=10, perm_len=0, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x000 (active_len=0, ramp_len=5, adm_len=10, perm_len=0, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x000 (active_len=0, ramp_len=4, adm_len=10, perm_len=0, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x000 (active_len=0, ramp_len=3, adm_len=10, perm_len=0, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x000 (active_len=0, ramp_len=2, adm_len=10, perm_len=0, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x000 (active_len=0, ramp_len=1, adm_len=10, perm_len=0, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x000 (active_len=0, ramp_len=1, adm_len=10, perm_len=0, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x000 (active_len=0, ramp_len=2, adm_len=10, perm_len=0, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x000 (active_len=0, ramp_len=3, adm_len=10, perm_len=0, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x000 (active_len=0, ramp_len=4, adm_len=10, perm_len=0, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x000 (active_len=0, ramp_len=5, adm_len=10, perm_len=0, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x000 (active_len=0, ramp_len=6, adm_len=10, perm_len=0, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x000 (active_len=0, ramp_len=7, adm_len=10, perm_len=0, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x000 (active_len=0, ramp_len=8, adm_len=10, perm_len=0, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x000 (active_len=0, ramp_len=9, adm_len=10, perm_len=0, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x000 (active_len=0, ramp_len=10, adm_len=10, perm_len=0, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
do_allowed_len_ramp_loop(4)
(bts=0) ACC: New ACC allowed subset 0x000 (active_len=0, ramp_len=6, adm_len=10, perm_len=0, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x000 (active_len=0, ramp_len=2, adm_len=10, perm_len=0, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x000 (active_len=0, ramp_len=4, adm_len=10, perm_len=0, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x000 (active_len=0, ramp_len=8, adm_len=10, perm_len=0, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x000 (active_len=0, ramp_len=10, adm_len=10, perm_len=0, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
*** Barring zero ACCs ***
(bts=0) ACC: New ACC allowed subset 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
pcu_info_update(): t2=0x00 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8 9
do_allowed_len_ramp_loop(1)
(bts=0) ACC: update ACC allowed active subset 0x3ff -> 0x3fe (active_len=9, ramp_len=9, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x01, allowed: 1 2 3 4 5 6 7 8 9
(bts=0) ACC: update ACC allowed active subset 0x3fe -> 0x3fc (active_len=8, ramp_len=8, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x03, allowed: 2 3 4 5 6 7 8 9
(bts=0) ACC: update ACC allowed active subset 0x3fc -> 0x3f8 (active_len=7, ramp_len=7, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x07, allowed: 3 4 5 6 7 8 9
(bts=0) ACC: update ACC allowed active subset 0x3f8 -> 0x3f0 (active_len=6, ramp_len=6, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x0f, allowed: 4 5 6 7 8 9
(bts=0) ACC: update ACC allowed active subset 0x3f0 -> 0x3e0 (active_len=5, ramp_len=5, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x1f, allowed: 5 6 7 8 9
(bts=0) ACC: update ACC allowed active subset 0x3e0 -> 0x3c0 (active_len=4, ramp_len=4, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x3f, allowed: 6 7 8 9
(bts=0) ACC: update ACC allowed active subset 0x3c0 -> 0x380 (active_len=3, ramp_len=3, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x7f, allowed: 7 8 9
(bts=0) ACC: update ACC allowed active subset 0x380 -> 0x300 (active_len=2, ramp_len=2, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0xff, allowed: 8 9
(bts=0) ACC: update ACC allowed active subset 0x300 -> 0x200 (active_len=1, ramp_len=1, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x01 t3=0xff, allowed: 9
(bts=0) ACC: update ACC allowed active subset 0x200 -> 0x000 (active_len=0, ramp_len=0, adm_len=10, perm_len=10, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x001 (active_len=1, ramp_len=1, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfe, allowed: 0
(bts=0) ACC: update ACC allowed active subset 0x001 -> 0x003 (active_len=2, ramp_len=2, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfc, allowed: 0 1
(bts=0) ACC: update ACC allowed active subset 0x003 -> 0x007 (active_len=3, ramp_len=3, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf8, allowed: 0 1 2
(bts=0) ACC: update ACC allowed active subset 0x007 -> 0x00f (active_len=4, ramp_len=4, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf0, allowed: 0 1 2 3
(bts=0) ACC: update ACC allowed active subset 0x00f -> 0x01f (active_len=5, ramp_len=5, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe0, allowed: 0 1 2 3 4
(bts=0) ACC: update ACC allowed active subset 0x01f -> 0x03f (active_len=6, ramp_len=6, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xc0, allowed: 0 1 2 3 4 5
(bts=0) ACC: update ACC allowed active subset 0x03f -> 0x07f (active_len=7, ramp_len=7, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x80, allowed: 0 1 2 3 4 5 6
(bts=0) ACC: update ACC allowed active subset 0x07f -> 0x0ff (active_len=8, ramp_len=8, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x00, allowed: 0 1 2 3 4 5 6 7
(bts=0) ACC: update ACC allowed active subset 0x0ff -> 0x1ff (active_len=9, ramp_len=9, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x02 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8
(bts=0) ACC: update ACC allowed active subset 0x1ff -> 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
pcu_info_update(): t2=0x00 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8 9
do_allowed_len_ramp_loop(4)
(bts=0) ACC: update ACC allowed active subset 0x3ff -> 0x3f0 (active_len=6, ramp_len=6, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x0f, allowed: 4 5 6 7 8 9
(bts=0) ACC: update ACC allowed active subset 0x3f0 -> 0x300 (active_len=2, ramp_len=2, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0xff, allowed: 8 9
(bts=0) ACC: update ACC allowed active subset 0x300 -> 0x000 (active_len=0, ramp_len=0, adm_len=10, perm_len=10, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x00f (active_len=4, ramp_len=4, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf0, allowed: 0 1 2 3
(bts=0) ACC: update ACC allowed active subset 0x00f -> 0x0ff (active_len=8, ramp_len=8, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x00, allowed: 0 1 2 3 4 5 6 7
(bts=0) ACC: update ACC allowed active subset 0x0ff -> 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
pcu_info_update(): t2=0x00 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8 9
*** Barring some ACCs + adm len 4 ***
(bts=0) ACC: update ACC allowed active subset 0x3ff -> 0x3c0 (active_len=4, ramp_len=10, adm_len=4, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x3f, allowed: 6 7 8 9
(bts=0) ACC: New ACC allowed subset 0x24c (active_len=4, ramp_len=10, adm_len=4, perm_len=4, rotation=off)
pcu_info_update(): t2=0x01 t3=0xb3, allowed: 2 3 6 9
do_allowed_len_ramp_loop(1)
(bts=0) ACC: update ACC allowed active subset 0x24c -> 0x248 (active_len=3, ramp_len=3, adm_len=4, perm_len=4, rotation=on)
pcu_info_update(): t2=0x01 t3=0xb7, allowed: 3 6 9
(bts=0) ACC: update ACC allowed active subset 0x248 -> 0x240 (active_len=2, ramp_len=2, adm_len=4, perm_len=4, rotation=on)
pcu_info_update(): t2=0x01 t3=0xbf, allowed: 6 9
(bts=0) ACC: update ACC allowed active subset 0x240 -> 0x200 (active_len=1, ramp_len=1, adm_len=4, perm_len=4, rotation=on)
pcu_info_update(): t2=0x01 t3=0xff, allowed: 9
(bts=0) ACC: update ACC allowed active subset 0x200 -> 0x000 (active_len=0, ramp_len=0, adm_len=4, perm_len=4, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x004 (active_len=1, ramp_len=1, adm_len=4, perm_len=4, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfb, allowed: 2
(bts=0) ACC: update ACC allowed active subset 0x004 -> 0x00c (active_len=2, ramp_len=2, adm_len=4, perm_len=4, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf3, allowed: 2 3
(bts=0) ACC: update ACC allowed active subset 0x00c -> 0x04c (active_len=3, ramp_len=3, adm_len=4, perm_len=4, rotation=on)
pcu_info_update(): t2=0x03 t3=0xb3, allowed: 2 3 6
(bts=0) ACC: update ACC allowed active subset 0x04c -> 0x24c (active_len=4, ramp_len=4, adm_len=4, perm_len=4, rotation=off)
pcu_info_update(): t2=0x01 t3=0xb3, allowed: 2 3 6 9
do_allowed_len_ramp_loop(4)
(bts=0) ACC: update ACC allowed active subset 0x24c -> 0x240 (active_len=2, ramp_len=2, adm_len=4, perm_len=4, rotation=on)
pcu_info_update(): t2=0x01 t3=0xbf, allowed: 6 9
(bts=0) ACC: update ACC allowed active subset 0x240 -> 0x000 (active_len=0, ramp_len=0, adm_len=4, perm_len=4, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x24c (active_len=4, ramp_len=4, adm_len=4, perm_len=4, rotation=off)
pcu_info_update(): t2=0x01 t3=0xb3, allowed: 2 3 6 9
BTS deallocated OK in test_acc_mgr_manual_ramp()
===test_acc_mgr_rotate(true, 1)===
(bts=0) ACC: New ACC allowed subset 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
BTS allocation OK in test_acc_mgr_rotate()
*** Barring one ACC ***
(bts=0) ACC: New ACC allowed subset 0x1ff (active_len=9, ramp_len=10, adm_len=10, perm_len=9, rotation=off)
pcu_info_update(): t2=0x02 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8
(bts=0) ACC: update ACC allowed active subset 0x1ff -> 0x100 (active_len=1, ramp_len=10, adm_len=1, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xff, allowed: 8
sys={2.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x100 -> 0x001 (active_len=1, ramp_len=10, adm_len=1, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfe, allowed: 0
sys={4.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x001 -> 0x002 (active_len=1, ramp_len=10, adm_len=1, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfd, allowed: 1
sys={6.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x002 -> 0x004 (active_len=1, ramp_len=10, adm_len=1, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfb, allowed: 2
sys={8.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x004 -> 0x008 (active_len=1, ramp_len=10, adm_len=1, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf7, allowed: 3
sys={10.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x008 -> 0x010 (active_len=1, ramp_len=10, adm_len=1, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xef, allowed: 4
sys={12.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x010 -> 0x020 (active_len=1, ramp_len=10, adm_len=1, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xdf, allowed: 5
sys={14.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x020 -> 0x040 (active_len=1, ramp_len=10, adm_len=1, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xbf, allowed: 6
sys={16.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x040 -> 0x080 (active_len=1, ramp_len=10, adm_len=1, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x7f, allowed: 7
sys={18.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x080 -> 0x100 (active_len=1, ramp_len=10, adm_len=1, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xff, allowed: 8
sys={20.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x100 -> 0x001 (active_len=1, ramp_len=10, adm_len=1, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfe, allowed: 0
sys={22.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x001 -> 0x002 (active_len=1, ramp_len=10, adm_len=1, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfd, allowed: 1
sys={24.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x002 -> 0x004 (active_len=1, ramp_len=10, adm_len=1, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfb, allowed: 2
sys={26.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x004 -> 0x008 (active_len=1, ramp_len=10, adm_len=1, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf7, allowed: 3
sys={28.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x008 -> 0x010 (active_len=1, ramp_len=10, adm_len=1, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xef, allowed: 4
sys={30.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x010 -> 0x020 (active_len=1, ramp_len=10, adm_len=1, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xdf, allowed: 5
sys={32.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x020 -> 0x040 (active_len=1, ramp_len=10, adm_len=1, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xbf, allowed: 6
sys={34.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x040 -> 0x080 (active_len=1, ramp_len=10, adm_len=1, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x7f, allowed: 7
sys={36.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x080 -> 0x100 (active_len=1, ramp_len=10, adm_len=1, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xff, allowed: 8
sys={38.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x100 -> 0x001 (active_len=1, ramp_len=10, adm_len=1, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfe, allowed: 0
sys={40.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x001 -> 0x002 (active_len=1, ramp_len=10, adm_len=1, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfd, allowed: 1
BTS deallocated OK in test_acc_mgr_rotate()
===test_acc_mgr_rotate(false, 1)===
(bts=0) ACC: New ACC allowed subset 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
BTS allocation OK in test_acc_mgr_rotate()
(bts=0) ACC: update ACC allowed active subset 0x3ff -> 0x200 (active_len=1, ramp_len=10, adm_len=1, perm_len=10, rotation=on)
pcu_info_update(): t2=0x01 t3=0xff, allowed: 9
sys={2.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x200 -> 0x001 (active_len=1, ramp_len=10, adm_len=1, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfe, allowed: 0
sys={4.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x001 -> 0x002 (active_len=1, ramp_len=10, adm_len=1, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfd, allowed: 1
sys={6.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x002 -> 0x004 (active_len=1, ramp_len=10, adm_len=1, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfb, allowed: 2
sys={8.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x004 -> 0x008 (active_len=1, ramp_len=10, adm_len=1, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf7, allowed: 3
sys={10.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x008 -> 0x010 (active_len=1, ramp_len=10, adm_len=1, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xef, allowed: 4
sys={12.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x010 -> 0x020 (active_len=1, ramp_len=10, adm_len=1, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xdf, allowed: 5
sys={14.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x020 -> 0x040 (active_len=1, ramp_len=10, adm_len=1, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xbf, allowed: 6
sys={16.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x040 -> 0x080 (active_len=1, ramp_len=10, adm_len=1, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x7f, allowed: 7
sys={18.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x080 -> 0x100 (active_len=1, ramp_len=10, adm_len=1, perm_len=10, rotation=on)
pcu_info_update(): t2=0x02 t3=0xff, allowed: 8
sys={20.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x100 -> 0x200 (active_len=1, ramp_len=10, adm_len=1, perm_len=10, rotation=on)
pcu_info_update(): t2=0x01 t3=0xff, allowed: 9
sys={22.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x200 -> 0x001 (active_len=1, ramp_len=10, adm_len=1, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfe, allowed: 0
sys={24.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x001 -> 0x002 (active_len=1, ramp_len=10, adm_len=1, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfd, allowed: 1
sys={26.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x002 -> 0x004 (active_len=1, ramp_len=10, adm_len=1, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfb, allowed: 2
sys={28.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x004 -> 0x008 (active_len=1, ramp_len=10, adm_len=1, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf7, allowed: 3
sys={30.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x008 -> 0x010 (active_len=1, ramp_len=10, adm_len=1, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xef, allowed: 4
sys={32.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x010 -> 0x020 (active_len=1, ramp_len=10, adm_len=1, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xdf, allowed: 5
sys={34.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x020 -> 0x040 (active_len=1, ramp_len=10, adm_len=1, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xbf, allowed: 6
sys={36.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x040 -> 0x080 (active_len=1, ramp_len=10, adm_len=1, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x7f, allowed: 7
sys={38.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x080 -> 0x100 (active_len=1, ramp_len=10, adm_len=1, perm_len=10, rotation=on)
pcu_info_update(): t2=0x02 t3=0xff, allowed: 8
sys={40.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x100 -> 0x200 (active_len=1, ramp_len=10, adm_len=1, perm_len=10, rotation=on)
pcu_info_update(): t2=0x01 t3=0xff, allowed: 9
BTS deallocated OK in test_acc_mgr_rotate()
===test_acc_mgr_rotate(true, 2)===
(bts=0) ACC: New ACC allowed subset 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
BTS allocation OK in test_acc_mgr_rotate()
*** Barring one ACC ***
(bts=0) ACC: New ACC allowed subset 0x1ff (active_len=9, ramp_len=10, adm_len=10, perm_len=9, rotation=off)
pcu_info_update(): t2=0x02 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8
(bts=0) ACC: update ACC allowed active subset 0x1ff -> 0x180 (active_len=2, ramp_len=10, adm_len=2, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x7f, allowed: 7 8
sys={2.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x180 -> 0x101 (active_len=2, ramp_len=10, adm_len=2, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xfe, allowed: 0 8
sys={4.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x101 -> 0x003 (active_len=2, ramp_len=10, adm_len=2, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfc, allowed: 0 1
sys={6.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x003 -> 0x006 (active_len=2, ramp_len=10, adm_len=2, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf9, allowed: 1 2
sys={8.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x006 -> 0x00c (active_len=2, ramp_len=10, adm_len=2, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf3, allowed: 2 3
sys={10.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x00c -> 0x018 (active_len=2, ramp_len=10, adm_len=2, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe7, allowed: 3 4
sys={12.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x018 -> 0x030 (active_len=2, ramp_len=10, adm_len=2, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xcf, allowed: 4 5
sys={14.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x030 -> 0x060 (active_len=2, ramp_len=10, adm_len=2, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x9f, allowed: 5 6
sys={16.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x060 -> 0x0c0 (active_len=2, ramp_len=10, adm_len=2, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x3f, allowed: 6 7
sys={18.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0c0 -> 0x180 (active_len=2, ramp_len=10, adm_len=2, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x7f, allowed: 7 8
sys={20.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x180 -> 0x101 (active_len=2, ramp_len=10, adm_len=2, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xfe, allowed: 0 8
sys={22.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x101 -> 0x003 (active_len=2, ramp_len=10, adm_len=2, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfc, allowed: 0 1
sys={24.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x003 -> 0x006 (active_len=2, ramp_len=10, adm_len=2, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf9, allowed: 1 2
sys={26.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x006 -> 0x00c (active_len=2, ramp_len=10, adm_len=2, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf3, allowed: 2 3
sys={28.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x00c -> 0x018 (active_len=2, ramp_len=10, adm_len=2, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe7, allowed: 3 4
sys={30.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x018 -> 0x030 (active_len=2, ramp_len=10, adm_len=2, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xcf, allowed: 4 5
sys={32.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x030 -> 0x060 (active_len=2, ramp_len=10, adm_len=2, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x9f, allowed: 5 6
sys={34.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x060 -> 0x0c0 (active_len=2, ramp_len=10, adm_len=2, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x3f, allowed: 6 7
sys={36.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0c0 -> 0x180 (active_len=2, ramp_len=10, adm_len=2, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x7f, allowed: 7 8
sys={38.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x180 -> 0x101 (active_len=2, ramp_len=10, adm_len=2, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xfe, allowed: 0 8
sys={40.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x101 -> 0x003 (active_len=2, ramp_len=10, adm_len=2, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfc, allowed: 0 1
BTS deallocated OK in test_acc_mgr_rotate()
===test_acc_mgr_rotate(false, 2)===
(bts=0) ACC: New ACC allowed subset 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
BTS allocation OK in test_acc_mgr_rotate()
(bts=0) ACC: update ACC allowed active subset 0x3ff -> 0x300 (active_len=2, ramp_len=10, adm_len=2, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0xff, allowed: 8 9
sys={2.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x300 -> 0x201 (active_len=2, ramp_len=10, adm_len=2, perm_len=10, rotation=on)
pcu_info_update(): t2=0x01 t3=0xfe, allowed: 0 9
sys={4.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x201 -> 0x003 (active_len=2, ramp_len=10, adm_len=2, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfc, allowed: 0 1
sys={6.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x003 -> 0x006 (active_len=2, ramp_len=10, adm_len=2, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf9, allowed: 1 2
sys={8.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x006 -> 0x00c (active_len=2, ramp_len=10, adm_len=2, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf3, allowed: 2 3
sys={10.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x00c -> 0x018 (active_len=2, ramp_len=10, adm_len=2, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe7, allowed: 3 4
sys={12.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x018 -> 0x030 (active_len=2, ramp_len=10, adm_len=2, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xcf, allowed: 4 5
sys={14.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x030 -> 0x060 (active_len=2, ramp_len=10, adm_len=2, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x9f, allowed: 5 6
sys={16.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x060 -> 0x0c0 (active_len=2, ramp_len=10, adm_len=2, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x3f, allowed: 6 7
sys={18.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0c0 -> 0x180 (active_len=2, ramp_len=10, adm_len=2, perm_len=10, rotation=on)
pcu_info_update(): t2=0x02 t3=0x7f, allowed: 7 8
sys={20.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x180 -> 0x300 (active_len=2, ramp_len=10, adm_len=2, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0xff, allowed: 8 9
sys={22.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x300 -> 0x201 (active_len=2, ramp_len=10, adm_len=2, perm_len=10, rotation=on)
pcu_info_update(): t2=0x01 t3=0xfe, allowed: 0 9
sys={24.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x201 -> 0x003 (active_len=2, ramp_len=10, adm_len=2, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfc, allowed: 0 1
sys={26.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x003 -> 0x006 (active_len=2, ramp_len=10, adm_len=2, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf9, allowed: 1 2
sys={28.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x006 -> 0x00c (active_len=2, ramp_len=10, adm_len=2, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf3, allowed: 2 3
sys={30.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x00c -> 0x018 (active_len=2, ramp_len=10, adm_len=2, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe7, allowed: 3 4
sys={32.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x018 -> 0x030 (active_len=2, ramp_len=10, adm_len=2, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xcf, allowed: 4 5
sys={34.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x030 -> 0x060 (active_len=2, ramp_len=10, adm_len=2, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x9f, allowed: 5 6
sys={36.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x060 -> 0x0c0 (active_len=2, ramp_len=10, adm_len=2, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x3f, allowed: 6 7
sys={38.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0c0 -> 0x180 (active_len=2, ramp_len=10, adm_len=2, perm_len=10, rotation=on)
pcu_info_update(): t2=0x02 t3=0x7f, allowed: 7 8
sys={40.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x180 -> 0x300 (active_len=2, ramp_len=10, adm_len=2, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0xff, allowed: 8 9
BTS deallocated OK in test_acc_mgr_rotate()
===test_acc_mgr_rotate(true, 3)===
(bts=0) ACC: New ACC allowed subset 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
BTS allocation OK in test_acc_mgr_rotate()
*** Barring one ACC ***
(bts=0) ACC: New ACC allowed subset 0x1ff (active_len=9, ramp_len=10, adm_len=10, perm_len=9, rotation=off)
pcu_info_update(): t2=0x02 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8
(bts=0) ACC: update ACC allowed active subset 0x1ff -> 0x1c0 (active_len=3, ramp_len=10, adm_len=3, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x3f, allowed: 6 7 8
sys={2.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1c0 -> 0x181 (active_len=3, ramp_len=10, adm_len=3, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x7e, allowed: 0 7 8
sys={4.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x181 -> 0x103 (active_len=3, ramp_len=10, adm_len=3, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xfc, allowed: 0 1 8
sys={6.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x103 -> 0x007 (active_len=3, ramp_len=10, adm_len=3, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf8, allowed: 0 1 2
sys={8.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x007 -> 0x00e (active_len=3, ramp_len=10, adm_len=3, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf1, allowed: 1 2 3
sys={10.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x00e -> 0x01c (active_len=3, ramp_len=10, adm_len=3, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe3, allowed: 2 3 4
sys={12.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x01c -> 0x038 (active_len=3, ramp_len=10, adm_len=3, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xc7, allowed: 3 4 5
sys={14.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x038 -> 0x070 (active_len=3, ramp_len=10, adm_len=3, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x8f, allowed: 4 5 6
sys={16.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x070 -> 0x0e0 (active_len=3, ramp_len=10, adm_len=3, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x1f, allowed: 5 6 7
sys={18.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0e0 -> 0x1c0 (active_len=3, ramp_len=10, adm_len=3, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x3f, allowed: 6 7 8
sys={20.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1c0 -> 0x181 (active_len=3, ramp_len=10, adm_len=3, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x7e, allowed: 0 7 8
sys={22.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x181 -> 0x103 (active_len=3, ramp_len=10, adm_len=3, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xfc, allowed: 0 1 8
sys={24.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x103 -> 0x007 (active_len=3, ramp_len=10, adm_len=3, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf8, allowed: 0 1 2
sys={26.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x007 -> 0x00e (active_len=3, ramp_len=10, adm_len=3, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf1, allowed: 1 2 3
sys={28.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x00e -> 0x01c (active_len=3, ramp_len=10, adm_len=3, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe3, allowed: 2 3 4
sys={30.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x01c -> 0x038 (active_len=3, ramp_len=10, adm_len=3, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xc7, allowed: 3 4 5
sys={32.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x038 -> 0x070 (active_len=3, ramp_len=10, adm_len=3, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x8f, allowed: 4 5 6
sys={34.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x070 -> 0x0e0 (active_len=3, ramp_len=10, adm_len=3, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x1f, allowed: 5 6 7
sys={36.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0e0 -> 0x1c0 (active_len=3, ramp_len=10, adm_len=3, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x3f, allowed: 6 7 8
sys={38.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1c0 -> 0x181 (active_len=3, ramp_len=10, adm_len=3, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x7e, allowed: 0 7 8
sys={40.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x181 -> 0x103 (active_len=3, ramp_len=10, adm_len=3, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xfc, allowed: 0 1 8
BTS deallocated OK in test_acc_mgr_rotate()
===test_acc_mgr_rotate(false, 3)===
(bts=0) ACC: New ACC allowed subset 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
BTS allocation OK in test_acc_mgr_rotate()
(bts=0) ACC: update ACC allowed active subset 0x3ff -> 0x380 (active_len=3, ramp_len=10, adm_len=3, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x7f, allowed: 7 8 9
sys={2.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x380 -> 0x301 (active_len=3, ramp_len=10, adm_len=3, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0xfe, allowed: 0 8 9
sys={4.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x301 -> 0x203 (active_len=3, ramp_len=10, adm_len=3, perm_len=10, rotation=on)
pcu_info_update(): t2=0x01 t3=0xfc, allowed: 0 1 9
sys={6.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x203 -> 0x007 (active_len=3, ramp_len=10, adm_len=3, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf8, allowed: 0 1 2
sys={8.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x007 -> 0x00e (active_len=3, ramp_len=10, adm_len=3, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf1, allowed: 1 2 3
sys={10.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x00e -> 0x01c (active_len=3, ramp_len=10, adm_len=3, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe3, allowed: 2 3 4
sys={12.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x01c -> 0x038 (active_len=3, ramp_len=10, adm_len=3, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xc7, allowed: 3 4 5
sys={14.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x038 -> 0x070 (active_len=3, ramp_len=10, adm_len=3, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x8f, allowed: 4 5 6
sys={16.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x070 -> 0x0e0 (active_len=3, ramp_len=10, adm_len=3, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x1f, allowed: 5 6 7
sys={18.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0e0 -> 0x1c0 (active_len=3, ramp_len=10, adm_len=3, perm_len=10, rotation=on)
pcu_info_update(): t2=0x02 t3=0x3f, allowed: 6 7 8
sys={20.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1c0 -> 0x380 (active_len=3, ramp_len=10, adm_len=3, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x7f, allowed: 7 8 9
sys={22.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x380 -> 0x301 (active_len=3, ramp_len=10, adm_len=3, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0xfe, allowed: 0 8 9
sys={24.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x301 -> 0x203 (active_len=3, ramp_len=10, adm_len=3, perm_len=10, rotation=on)
pcu_info_update(): t2=0x01 t3=0xfc, allowed: 0 1 9
sys={26.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x203 -> 0x007 (active_len=3, ramp_len=10, adm_len=3, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf8, allowed: 0 1 2
sys={28.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x007 -> 0x00e (active_len=3, ramp_len=10, adm_len=3, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf1, allowed: 1 2 3
sys={30.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x00e -> 0x01c (active_len=3, ramp_len=10, adm_len=3, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe3, allowed: 2 3 4
sys={32.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x01c -> 0x038 (active_len=3, ramp_len=10, adm_len=3, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xc7, allowed: 3 4 5
sys={34.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x038 -> 0x070 (active_len=3, ramp_len=10, adm_len=3, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x8f, allowed: 4 5 6
sys={36.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x070 -> 0x0e0 (active_len=3, ramp_len=10, adm_len=3, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x1f, allowed: 5 6 7
sys={38.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0e0 -> 0x1c0 (active_len=3, ramp_len=10, adm_len=3, perm_len=10, rotation=on)
pcu_info_update(): t2=0x02 t3=0x3f, allowed: 6 7 8
sys={40.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1c0 -> 0x380 (active_len=3, ramp_len=10, adm_len=3, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x7f, allowed: 7 8 9
BTS deallocated OK in test_acc_mgr_rotate()
===test_acc_mgr_rotate(true, 4)===
(bts=0) ACC: New ACC allowed subset 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
BTS allocation OK in test_acc_mgr_rotate()
*** Barring one ACC ***
(bts=0) ACC: New ACC allowed subset 0x1ff (active_len=9, ramp_len=10, adm_len=10, perm_len=9, rotation=off)
pcu_info_update(): t2=0x02 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8
(bts=0) ACC: update ACC allowed active subset 0x1ff -> 0x1e0 (active_len=4, ramp_len=10, adm_len=4, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x1f, allowed: 5 6 7 8
sys={2.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1e0 -> 0x1c1 (active_len=4, ramp_len=10, adm_len=4, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x3e, allowed: 0 6 7 8
sys={4.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1c1 -> 0x183 (active_len=4, ramp_len=10, adm_len=4, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x7c, allowed: 0 1 7 8
sys={6.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x183 -> 0x107 (active_len=4, ramp_len=10, adm_len=4, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xf8, allowed: 0 1 2 8
sys={8.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x107 -> 0x00f (active_len=4, ramp_len=10, adm_len=4, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf0, allowed: 0 1 2 3
sys={10.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x00f -> 0x01e (active_len=4, ramp_len=10, adm_len=4, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe1, allowed: 1 2 3 4
sys={12.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x01e -> 0x03c (active_len=4, ramp_len=10, adm_len=4, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xc3, allowed: 2 3 4 5
sys={14.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x03c -> 0x078 (active_len=4, ramp_len=10, adm_len=4, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x87, allowed: 3 4 5 6
sys={16.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x078 -> 0x0f0 (active_len=4, ramp_len=10, adm_len=4, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x0f, allowed: 4 5 6 7
sys={18.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0f0 -> 0x1e0 (active_len=4, ramp_len=10, adm_len=4, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x1f, allowed: 5 6 7 8
sys={20.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1e0 -> 0x1c1 (active_len=4, ramp_len=10, adm_len=4, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x3e, allowed: 0 6 7 8
sys={22.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1c1 -> 0x183 (active_len=4, ramp_len=10, adm_len=4, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x7c, allowed: 0 1 7 8
sys={24.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x183 -> 0x107 (active_len=4, ramp_len=10, adm_len=4, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xf8, allowed: 0 1 2 8
sys={26.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x107 -> 0x00f (active_len=4, ramp_len=10, adm_len=4, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf0, allowed: 0 1 2 3
sys={28.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x00f -> 0x01e (active_len=4, ramp_len=10, adm_len=4, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe1, allowed: 1 2 3 4
sys={30.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x01e -> 0x03c (active_len=4, ramp_len=10, adm_len=4, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xc3, allowed: 2 3 4 5
sys={32.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x03c -> 0x078 (active_len=4, ramp_len=10, adm_len=4, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x87, allowed: 3 4 5 6
sys={34.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x078 -> 0x0f0 (active_len=4, ramp_len=10, adm_len=4, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x0f, allowed: 4 5 6 7
sys={36.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0f0 -> 0x1e0 (active_len=4, ramp_len=10, adm_len=4, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x1f, allowed: 5 6 7 8
sys={38.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1e0 -> 0x1c1 (active_len=4, ramp_len=10, adm_len=4, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x3e, allowed: 0 6 7 8
sys={40.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1c1 -> 0x183 (active_len=4, ramp_len=10, adm_len=4, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x7c, allowed: 0 1 7 8
BTS deallocated OK in test_acc_mgr_rotate()
===test_acc_mgr_rotate(false, 4)===
(bts=0) ACC: New ACC allowed subset 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
BTS allocation OK in test_acc_mgr_rotate()
(bts=0) ACC: update ACC allowed active subset 0x3ff -> 0x3c0 (active_len=4, ramp_len=10, adm_len=4, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x3f, allowed: 6 7 8 9
sys={2.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3c0 -> 0x381 (active_len=4, ramp_len=10, adm_len=4, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x7e, allowed: 0 7 8 9
sys={4.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x381 -> 0x303 (active_len=4, ramp_len=10, adm_len=4, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0xfc, allowed: 0 1 8 9
sys={6.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x303 -> 0x207 (active_len=4, ramp_len=10, adm_len=4, perm_len=10, rotation=on)
pcu_info_update(): t2=0x01 t3=0xf8, allowed: 0 1 2 9
sys={8.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x207 -> 0x00f (active_len=4, ramp_len=10, adm_len=4, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf0, allowed: 0 1 2 3
sys={10.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x00f -> 0x01e (active_len=4, ramp_len=10, adm_len=4, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe1, allowed: 1 2 3 4
sys={12.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x01e -> 0x03c (active_len=4, ramp_len=10, adm_len=4, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xc3, allowed: 2 3 4 5
sys={14.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x03c -> 0x078 (active_len=4, ramp_len=10, adm_len=4, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x87, allowed: 3 4 5 6
sys={16.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x078 -> 0x0f0 (active_len=4, ramp_len=10, adm_len=4, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x0f, allowed: 4 5 6 7
sys={18.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0f0 -> 0x1e0 (active_len=4, ramp_len=10, adm_len=4, perm_len=10, rotation=on)
pcu_info_update(): t2=0x02 t3=0x1f, allowed: 5 6 7 8
sys={20.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1e0 -> 0x3c0 (active_len=4, ramp_len=10, adm_len=4, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x3f, allowed: 6 7 8 9
sys={22.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3c0 -> 0x381 (active_len=4, ramp_len=10, adm_len=4, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x7e, allowed: 0 7 8 9
sys={24.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x381 -> 0x303 (active_len=4, ramp_len=10, adm_len=4, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0xfc, allowed: 0 1 8 9
sys={26.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x303 -> 0x207 (active_len=4, ramp_len=10, adm_len=4, perm_len=10, rotation=on)
pcu_info_update(): t2=0x01 t3=0xf8, allowed: 0 1 2 9
sys={28.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x207 -> 0x00f (active_len=4, ramp_len=10, adm_len=4, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf0, allowed: 0 1 2 3
sys={30.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x00f -> 0x01e (active_len=4, ramp_len=10, adm_len=4, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe1, allowed: 1 2 3 4
sys={32.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x01e -> 0x03c (active_len=4, ramp_len=10, adm_len=4, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xc3, allowed: 2 3 4 5
sys={34.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x03c -> 0x078 (active_len=4, ramp_len=10, adm_len=4, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x87, allowed: 3 4 5 6
sys={36.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x078 -> 0x0f0 (active_len=4, ramp_len=10, adm_len=4, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x0f, allowed: 4 5 6 7
sys={38.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0f0 -> 0x1e0 (active_len=4, ramp_len=10, adm_len=4, perm_len=10, rotation=on)
pcu_info_update(): t2=0x02 t3=0x1f, allowed: 5 6 7 8
sys={40.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1e0 -> 0x3c0 (active_len=4, ramp_len=10, adm_len=4, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x3f, allowed: 6 7 8 9
BTS deallocated OK in test_acc_mgr_rotate()
===test_acc_mgr_rotate(true, 5)===
(bts=0) ACC: New ACC allowed subset 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
BTS allocation OK in test_acc_mgr_rotate()
*** Barring one ACC ***
(bts=0) ACC: New ACC allowed subset 0x1ff (active_len=9, ramp_len=10, adm_len=10, perm_len=9, rotation=off)
pcu_info_update(): t2=0x02 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8
(bts=0) ACC: update ACC allowed active subset 0x1ff -> 0x1f0 (active_len=5, ramp_len=10, adm_len=5, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x0f, allowed: 4 5 6 7 8
sys={2.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1f0 -> 0x1e1 (active_len=5, ramp_len=10, adm_len=5, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x1e, allowed: 0 5 6 7 8
sys={4.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1e1 -> 0x1c3 (active_len=5, ramp_len=10, adm_len=5, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x3c, allowed: 0 1 6 7 8
sys={6.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1c3 -> 0x187 (active_len=5, ramp_len=10, adm_len=5, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x78, allowed: 0 1 2 7 8
sys={8.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x187 -> 0x10f (active_len=5, ramp_len=10, adm_len=5, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xf0, allowed: 0 1 2 3 8
sys={10.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x10f -> 0x01f (active_len=5, ramp_len=10, adm_len=5, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe0, allowed: 0 1 2 3 4
sys={12.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x01f -> 0x03e (active_len=5, ramp_len=10, adm_len=5, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xc1, allowed: 1 2 3 4 5
sys={14.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x03e -> 0x07c (active_len=5, ramp_len=10, adm_len=5, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x83, allowed: 2 3 4 5 6
sys={16.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x07c -> 0x0f8 (active_len=5, ramp_len=10, adm_len=5, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x07, allowed: 3 4 5 6 7
sys={18.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0f8 -> 0x1f0 (active_len=5, ramp_len=10, adm_len=5, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x0f, allowed: 4 5 6 7 8
sys={20.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1f0 -> 0x1e1 (active_len=5, ramp_len=10, adm_len=5, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x1e, allowed: 0 5 6 7 8
sys={22.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1e1 -> 0x1c3 (active_len=5, ramp_len=10, adm_len=5, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x3c, allowed: 0 1 6 7 8
sys={24.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1c3 -> 0x187 (active_len=5, ramp_len=10, adm_len=5, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x78, allowed: 0 1 2 7 8
sys={26.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x187 -> 0x10f (active_len=5, ramp_len=10, adm_len=5, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xf0, allowed: 0 1 2 3 8
sys={28.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x10f -> 0x01f (active_len=5, ramp_len=10, adm_len=5, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe0, allowed: 0 1 2 3 4
sys={30.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x01f -> 0x03e (active_len=5, ramp_len=10, adm_len=5, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xc1, allowed: 1 2 3 4 5
sys={32.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x03e -> 0x07c (active_len=5, ramp_len=10, adm_len=5, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x83, allowed: 2 3 4 5 6
sys={34.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x07c -> 0x0f8 (active_len=5, ramp_len=10, adm_len=5, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x07, allowed: 3 4 5 6 7
sys={36.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0f8 -> 0x1f0 (active_len=5, ramp_len=10, adm_len=5, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x0f, allowed: 4 5 6 7 8
sys={38.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1f0 -> 0x1e1 (active_len=5, ramp_len=10, adm_len=5, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x1e, allowed: 0 5 6 7 8
sys={40.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1e1 -> 0x1c3 (active_len=5, ramp_len=10, adm_len=5, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x3c, allowed: 0 1 6 7 8
BTS deallocated OK in test_acc_mgr_rotate()
===test_acc_mgr_rotate(false, 5)===
(bts=0) ACC: New ACC allowed subset 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
BTS allocation OK in test_acc_mgr_rotate()
(bts=0) ACC: update ACC allowed active subset 0x3ff -> 0x3e0 (active_len=5, ramp_len=10, adm_len=5, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x1f, allowed: 5 6 7 8 9
sys={2.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3e0 -> 0x3c1 (active_len=5, ramp_len=10, adm_len=5, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x3e, allowed: 0 6 7 8 9
sys={4.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3c1 -> 0x383 (active_len=5, ramp_len=10, adm_len=5, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x7c, allowed: 0 1 7 8 9
sys={6.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x383 -> 0x307 (active_len=5, ramp_len=10, adm_len=5, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0xf8, allowed: 0 1 2 8 9
sys={8.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x307 -> 0x20f (active_len=5, ramp_len=10, adm_len=5, perm_len=10, rotation=on)
pcu_info_update(): t2=0x01 t3=0xf0, allowed: 0 1 2 3 9
sys={10.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x20f -> 0x01f (active_len=5, ramp_len=10, adm_len=5, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe0, allowed: 0 1 2 3 4
sys={12.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x01f -> 0x03e (active_len=5, ramp_len=10, adm_len=5, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xc1, allowed: 1 2 3 4 5
sys={14.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x03e -> 0x07c (active_len=5, ramp_len=10, adm_len=5, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x83, allowed: 2 3 4 5 6
sys={16.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x07c -> 0x0f8 (active_len=5, ramp_len=10, adm_len=5, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x07, allowed: 3 4 5 6 7
sys={18.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0f8 -> 0x1f0 (active_len=5, ramp_len=10, adm_len=5, perm_len=10, rotation=on)
pcu_info_update(): t2=0x02 t3=0x0f, allowed: 4 5 6 7 8
sys={20.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1f0 -> 0x3e0 (active_len=5, ramp_len=10, adm_len=5, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x1f, allowed: 5 6 7 8 9
sys={22.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3e0 -> 0x3c1 (active_len=5, ramp_len=10, adm_len=5, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x3e, allowed: 0 6 7 8 9
sys={24.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3c1 -> 0x383 (active_len=5, ramp_len=10, adm_len=5, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x7c, allowed: 0 1 7 8 9
sys={26.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x383 -> 0x307 (active_len=5, ramp_len=10, adm_len=5, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0xf8, allowed: 0 1 2 8 9
sys={28.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x307 -> 0x20f (active_len=5, ramp_len=10, adm_len=5, perm_len=10, rotation=on)
pcu_info_update(): t2=0x01 t3=0xf0, allowed: 0 1 2 3 9
sys={30.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x20f -> 0x01f (active_len=5, ramp_len=10, adm_len=5, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe0, allowed: 0 1 2 3 4
sys={32.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x01f -> 0x03e (active_len=5, ramp_len=10, adm_len=5, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xc1, allowed: 1 2 3 4 5
sys={34.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x03e -> 0x07c (active_len=5, ramp_len=10, adm_len=5, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x83, allowed: 2 3 4 5 6
sys={36.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x07c -> 0x0f8 (active_len=5, ramp_len=10, adm_len=5, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x07, allowed: 3 4 5 6 7
sys={38.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0f8 -> 0x1f0 (active_len=5, ramp_len=10, adm_len=5, perm_len=10, rotation=on)
pcu_info_update(): t2=0x02 t3=0x0f, allowed: 4 5 6 7 8
sys={40.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1f0 -> 0x3e0 (active_len=5, ramp_len=10, adm_len=5, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x1f, allowed: 5 6 7 8 9
BTS deallocated OK in test_acc_mgr_rotate()
===test_acc_mgr_rotate(true, 6)===
(bts=0) ACC: New ACC allowed subset 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
BTS allocation OK in test_acc_mgr_rotate()
*** Barring one ACC ***
(bts=0) ACC: New ACC allowed subset 0x1ff (active_len=9, ramp_len=10, adm_len=10, perm_len=9, rotation=off)
pcu_info_update(): t2=0x02 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8
(bts=0) ACC: update ACC allowed active subset 0x1ff -> 0x1f8 (active_len=6, ramp_len=10, adm_len=6, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x07, allowed: 3 4 5 6 7 8
sys={2.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1f8 -> 0x1f1 (active_len=6, ramp_len=10, adm_len=6, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x0e, allowed: 0 4 5 6 7 8
sys={4.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1f1 -> 0x1e3 (active_len=6, ramp_len=10, adm_len=6, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x1c, allowed: 0 1 5 6 7 8
sys={6.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1e3 -> 0x1c7 (active_len=6, ramp_len=10, adm_len=6, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x38, allowed: 0 1 2 6 7 8
sys={8.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1c7 -> 0x18f (active_len=6, ramp_len=10, adm_len=6, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x70, allowed: 0 1 2 3 7 8
sys={10.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x18f -> 0x11f (active_len=6, ramp_len=10, adm_len=6, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xe0, allowed: 0 1 2 3 4 8
sys={12.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x11f -> 0x03f (active_len=6, ramp_len=10, adm_len=6, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xc0, allowed: 0 1 2 3 4 5
sys={14.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x03f -> 0x07e (active_len=6, ramp_len=10, adm_len=6, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x81, allowed: 1 2 3 4 5 6
sys={16.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x07e -> 0x0fc (active_len=6, ramp_len=10, adm_len=6, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x03, allowed: 2 3 4 5 6 7
sys={18.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0fc -> 0x1f8 (active_len=6, ramp_len=10, adm_len=6, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x07, allowed: 3 4 5 6 7 8
sys={20.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1f8 -> 0x1f1 (active_len=6, ramp_len=10, adm_len=6, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x0e, allowed: 0 4 5 6 7 8
sys={22.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1f1 -> 0x1e3 (active_len=6, ramp_len=10, adm_len=6, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x1c, allowed: 0 1 5 6 7 8
sys={24.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1e3 -> 0x1c7 (active_len=6, ramp_len=10, adm_len=6, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x38, allowed: 0 1 2 6 7 8
sys={26.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1c7 -> 0x18f (active_len=6, ramp_len=10, adm_len=6, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x70, allowed: 0 1 2 3 7 8
sys={28.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x18f -> 0x11f (active_len=6, ramp_len=10, adm_len=6, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xe0, allowed: 0 1 2 3 4 8
sys={30.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x11f -> 0x03f (active_len=6, ramp_len=10, adm_len=6, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xc0, allowed: 0 1 2 3 4 5
sys={32.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x03f -> 0x07e (active_len=6, ramp_len=10, adm_len=6, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x81, allowed: 1 2 3 4 5 6
sys={34.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x07e -> 0x0fc (active_len=6, ramp_len=10, adm_len=6, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x03, allowed: 2 3 4 5 6 7
sys={36.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0fc -> 0x1f8 (active_len=6, ramp_len=10, adm_len=6, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x07, allowed: 3 4 5 6 7 8
sys={38.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1f8 -> 0x1f1 (active_len=6, ramp_len=10, adm_len=6, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x0e, allowed: 0 4 5 6 7 8
sys={40.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1f1 -> 0x1e3 (active_len=6, ramp_len=10, adm_len=6, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x1c, allowed: 0 1 5 6 7 8
BTS deallocated OK in test_acc_mgr_rotate()
===test_acc_mgr_rotate(false, 6)===
(bts=0) ACC: New ACC allowed subset 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
BTS allocation OK in test_acc_mgr_rotate()
(bts=0) ACC: update ACC allowed active subset 0x3ff -> 0x3f0 (active_len=6, ramp_len=10, adm_len=6, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x0f, allowed: 4 5 6 7 8 9
sys={2.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3f0 -> 0x3e1 (active_len=6, ramp_len=10, adm_len=6, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x1e, allowed: 0 5 6 7 8 9
sys={4.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3e1 -> 0x3c3 (active_len=6, ramp_len=10, adm_len=6, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x3c, allowed: 0 1 6 7 8 9
sys={6.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3c3 -> 0x387 (active_len=6, ramp_len=10, adm_len=6, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x78, allowed: 0 1 2 7 8 9
sys={8.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x387 -> 0x30f (active_len=6, ramp_len=10, adm_len=6, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0xf0, allowed: 0 1 2 3 8 9
sys={10.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x30f -> 0x21f (active_len=6, ramp_len=10, adm_len=6, perm_len=10, rotation=on)
pcu_info_update(): t2=0x01 t3=0xe0, allowed: 0 1 2 3 4 9
sys={12.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x21f -> 0x03f (active_len=6, ramp_len=10, adm_len=6, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xc0, allowed: 0 1 2 3 4 5
sys={14.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x03f -> 0x07e (active_len=6, ramp_len=10, adm_len=6, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x81, allowed: 1 2 3 4 5 6
sys={16.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x07e -> 0x0fc (active_len=6, ramp_len=10, adm_len=6, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x03, allowed: 2 3 4 5 6 7
sys={18.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0fc -> 0x1f8 (active_len=6, ramp_len=10, adm_len=6, perm_len=10, rotation=on)
pcu_info_update(): t2=0x02 t3=0x07, allowed: 3 4 5 6 7 8
sys={20.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1f8 -> 0x3f0 (active_len=6, ramp_len=10, adm_len=6, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x0f, allowed: 4 5 6 7 8 9
sys={22.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3f0 -> 0x3e1 (active_len=6, ramp_len=10, adm_len=6, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x1e, allowed: 0 5 6 7 8 9
sys={24.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3e1 -> 0x3c3 (active_len=6, ramp_len=10, adm_len=6, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x3c, allowed: 0 1 6 7 8 9
sys={26.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3c3 -> 0x387 (active_len=6, ramp_len=10, adm_len=6, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x78, allowed: 0 1 2 7 8 9
sys={28.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x387 -> 0x30f (active_len=6, ramp_len=10, adm_len=6, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0xf0, allowed: 0 1 2 3 8 9
sys={30.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x30f -> 0x21f (active_len=6, ramp_len=10, adm_len=6, perm_len=10, rotation=on)
pcu_info_update(): t2=0x01 t3=0xe0, allowed: 0 1 2 3 4 9
sys={32.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x21f -> 0x03f (active_len=6, ramp_len=10, adm_len=6, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xc0, allowed: 0 1 2 3 4 5
sys={34.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x03f -> 0x07e (active_len=6, ramp_len=10, adm_len=6, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x81, allowed: 1 2 3 4 5 6
sys={36.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x07e -> 0x0fc (active_len=6, ramp_len=10, adm_len=6, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x03, allowed: 2 3 4 5 6 7
sys={38.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0fc -> 0x1f8 (active_len=6, ramp_len=10, adm_len=6, perm_len=10, rotation=on)
pcu_info_update(): t2=0x02 t3=0x07, allowed: 3 4 5 6 7 8
sys={40.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1f8 -> 0x3f0 (active_len=6, ramp_len=10, adm_len=6, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x0f, allowed: 4 5 6 7 8 9
BTS deallocated OK in test_acc_mgr_rotate()
===test_acc_mgr_rotate(true, 7)===
(bts=0) ACC: New ACC allowed subset 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
BTS allocation OK in test_acc_mgr_rotate()
*** Barring one ACC ***
(bts=0) ACC: New ACC allowed subset 0x1ff (active_len=9, ramp_len=10, adm_len=10, perm_len=9, rotation=off)
pcu_info_update(): t2=0x02 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8
(bts=0) ACC: update ACC allowed active subset 0x1ff -> 0x1fc (active_len=7, ramp_len=10, adm_len=7, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x03, allowed: 2 3 4 5 6 7 8
sys={2.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1fc -> 0x1f9 (active_len=7, ramp_len=10, adm_len=7, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x06, allowed: 0 3 4 5 6 7 8
sys={4.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1f9 -> 0x1f3 (active_len=7, ramp_len=10, adm_len=7, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x0c, allowed: 0 1 4 5 6 7 8
sys={6.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1f3 -> 0x1e7 (active_len=7, ramp_len=10, adm_len=7, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x18, allowed: 0 1 2 5 6 7 8
sys={8.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1e7 -> 0x1cf (active_len=7, ramp_len=10, adm_len=7, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x30, allowed: 0 1 2 3 6 7 8
sys={10.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1cf -> 0x19f (active_len=7, ramp_len=10, adm_len=7, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x60, allowed: 0 1 2 3 4 7 8
sys={12.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x19f -> 0x13f (active_len=7, ramp_len=10, adm_len=7, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xc0, allowed: 0 1 2 3 4 5 8
sys={14.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x13f -> 0x07f (active_len=7, ramp_len=10, adm_len=7, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x80, allowed: 0 1 2 3 4 5 6
sys={16.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x07f -> 0x0fe (active_len=7, ramp_len=10, adm_len=7, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x01, allowed: 1 2 3 4 5 6 7
sys={18.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0fe -> 0x1fc (active_len=7, ramp_len=10, adm_len=7, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x03, allowed: 2 3 4 5 6 7 8
sys={20.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1fc -> 0x1f9 (active_len=7, ramp_len=10, adm_len=7, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x06, allowed: 0 3 4 5 6 7 8
sys={22.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1f9 -> 0x1f3 (active_len=7, ramp_len=10, adm_len=7, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x0c, allowed: 0 1 4 5 6 7 8
sys={24.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1f3 -> 0x1e7 (active_len=7, ramp_len=10, adm_len=7, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x18, allowed: 0 1 2 5 6 7 8
sys={26.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1e7 -> 0x1cf (active_len=7, ramp_len=10, adm_len=7, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x30, allowed: 0 1 2 3 6 7 8
sys={28.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1cf -> 0x19f (active_len=7, ramp_len=10, adm_len=7, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x60, allowed: 0 1 2 3 4 7 8
sys={30.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x19f -> 0x13f (active_len=7, ramp_len=10, adm_len=7, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xc0, allowed: 0 1 2 3 4 5 8
sys={32.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x13f -> 0x07f (active_len=7, ramp_len=10, adm_len=7, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x80, allowed: 0 1 2 3 4 5 6
sys={34.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x07f -> 0x0fe (active_len=7, ramp_len=10, adm_len=7, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x01, allowed: 1 2 3 4 5 6 7
sys={36.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0fe -> 0x1fc (active_len=7, ramp_len=10, adm_len=7, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x03, allowed: 2 3 4 5 6 7 8
sys={38.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1fc -> 0x1f9 (active_len=7, ramp_len=10, adm_len=7, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x06, allowed: 0 3 4 5 6 7 8
sys={40.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1f9 -> 0x1f3 (active_len=7, ramp_len=10, adm_len=7, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x0c, allowed: 0 1 4 5 6 7 8
BTS deallocated OK in test_acc_mgr_rotate()
===test_acc_mgr_rotate(false, 7)===
(bts=0) ACC: New ACC allowed subset 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
BTS allocation OK in test_acc_mgr_rotate()
(bts=0) ACC: update ACC allowed active subset 0x3ff -> 0x3f8 (active_len=7, ramp_len=10, adm_len=7, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x07, allowed: 3 4 5 6 7 8 9
sys={2.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3f8 -> 0x3f1 (active_len=7, ramp_len=10, adm_len=7, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x0e, allowed: 0 4 5 6 7 8 9
sys={4.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3f1 -> 0x3e3 (active_len=7, ramp_len=10, adm_len=7, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x1c, allowed: 0 1 5 6 7 8 9
sys={6.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3e3 -> 0x3c7 (active_len=7, ramp_len=10, adm_len=7, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x38, allowed: 0 1 2 6 7 8 9
sys={8.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3c7 -> 0x38f (active_len=7, ramp_len=10, adm_len=7, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x70, allowed: 0 1 2 3 7 8 9
sys={10.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x38f -> 0x31f (active_len=7, ramp_len=10, adm_len=7, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0xe0, allowed: 0 1 2 3 4 8 9
sys={12.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x31f -> 0x23f (active_len=7, ramp_len=10, adm_len=7, perm_len=10, rotation=on)
pcu_info_update(): t2=0x01 t3=0xc0, allowed: 0 1 2 3 4 5 9
sys={14.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x23f -> 0x07f (active_len=7, ramp_len=10, adm_len=7, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x80, allowed: 0 1 2 3 4 5 6
sys={16.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x07f -> 0x0fe (active_len=7, ramp_len=10, adm_len=7, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x01, allowed: 1 2 3 4 5 6 7
sys={18.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0fe -> 0x1fc (active_len=7, ramp_len=10, adm_len=7, perm_len=10, rotation=on)
pcu_info_update(): t2=0x02 t3=0x03, allowed: 2 3 4 5 6 7 8
sys={20.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1fc -> 0x3f8 (active_len=7, ramp_len=10, adm_len=7, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x07, allowed: 3 4 5 6 7 8 9
sys={22.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3f8 -> 0x3f1 (active_len=7, ramp_len=10, adm_len=7, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x0e, allowed: 0 4 5 6 7 8 9
sys={24.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3f1 -> 0x3e3 (active_len=7, ramp_len=10, adm_len=7, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x1c, allowed: 0 1 5 6 7 8 9
sys={26.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3e3 -> 0x3c7 (active_len=7, ramp_len=10, adm_len=7, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x38, allowed: 0 1 2 6 7 8 9
sys={28.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3c7 -> 0x38f (active_len=7, ramp_len=10, adm_len=7, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x70, allowed: 0 1 2 3 7 8 9
sys={30.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x38f -> 0x31f (active_len=7, ramp_len=10, adm_len=7, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0xe0, allowed: 0 1 2 3 4 8 9
sys={32.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x31f -> 0x23f (active_len=7, ramp_len=10, adm_len=7, perm_len=10, rotation=on)
pcu_info_update(): t2=0x01 t3=0xc0, allowed: 0 1 2 3 4 5 9
sys={34.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x23f -> 0x07f (active_len=7, ramp_len=10, adm_len=7, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x80, allowed: 0 1 2 3 4 5 6
sys={36.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x07f -> 0x0fe (active_len=7, ramp_len=10, adm_len=7, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x01, allowed: 1 2 3 4 5 6 7
sys={38.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0fe -> 0x1fc (active_len=7, ramp_len=10, adm_len=7, perm_len=10, rotation=on)
pcu_info_update(): t2=0x02 t3=0x03, allowed: 2 3 4 5 6 7 8
sys={40.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1fc -> 0x3f8 (active_len=7, ramp_len=10, adm_len=7, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x07, allowed: 3 4 5 6 7 8 9
BTS deallocated OK in test_acc_mgr_rotate()
===test_acc_mgr_rotate(true, 8)===
(bts=0) ACC: New ACC allowed subset 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
BTS allocation OK in test_acc_mgr_rotate()
*** Barring one ACC ***
(bts=0) ACC: New ACC allowed subset 0x1ff (active_len=9, ramp_len=10, adm_len=10, perm_len=9, rotation=off)
pcu_info_update(): t2=0x02 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8
(bts=0) ACC: update ACC allowed active subset 0x1ff -> 0x1fe (active_len=8, ramp_len=10, adm_len=8, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x01, allowed: 1 2 3 4 5 6 7 8
sys={2.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1fe -> 0x1fd (active_len=8, ramp_len=10, adm_len=8, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x02, allowed: 0 2 3 4 5 6 7 8
sys={4.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1fd -> 0x1fb (active_len=8, ramp_len=10, adm_len=8, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x04, allowed: 0 1 3 4 5 6 7 8
sys={6.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1fb -> 0x1f7 (active_len=8, ramp_len=10, adm_len=8, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x08, allowed: 0 1 2 4 5 6 7 8
sys={8.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1f7 -> 0x1ef (active_len=8, ramp_len=10, adm_len=8, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x10, allowed: 0 1 2 3 5 6 7 8
sys={10.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1ef -> 0x1df (active_len=8, ramp_len=10, adm_len=8, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x20, allowed: 0 1 2 3 4 6 7 8
sys={12.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1df -> 0x1bf (active_len=8, ramp_len=10, adm_len=8, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x40, allowed: 0 1 2 3 4 5 7 8
sys={14.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1bf -> 0x17f (active_len=8, ramp_len=10, adm_len=8, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x80, allowed: 0 1 2 3 4 5 6 8
sys={16.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x17f -> 0x0ff (active_len=8, ramp_len=10, adm_len=8, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x00, allowed: 0 1 2 3 4 5 6 7
sys={18.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0ff -> 0x1fe (active_len=8, ramp_len=10, adm_len=8, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x01, allowed: 1 2 3 4 5 6 7 8
sys={20.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1fe -> 0x1fd (active_len=8, ramp_len=10, adm_len=8, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x02, allowed: 0 2 3 4 5 6 7 8
sys={22.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1fd -> 0x1fb (active_len=8, ramp_len=10, adm_len=8, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x04, allowed: 0 1 3 4 5 6 7 8
sys={24.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1fb -> 0x1f7 (active_len=8, ramp_len=10, adm_len=8, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x08, allowed: 0 1 2 4 5 6 7 8
sys={26.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1f7 -> 0x1ef (active_len=8, ramp_len=10, adm_len=8, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x10, allowed: 0 1 2 3 5 6 7 8
sys={28.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1ef -> 0x1df (active_len=8, ramp_len=10, adm_len=8, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x20, allowed: 0 1 2 3 4 6 7 8
sys={30.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1df -> 0x1bf (active_len=8, ramp_len=10, adm_len=8, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x40, allowed: 0 1 2 3 4 5 7 8
sys={32.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1bf -> 0x17f (active_len=8, ramp_len=10, adm_len=8, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x80, allowed: 0 1 2 3 4 5 6 8
sys={34.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x17f -> 0x0ff (active_len=8, ramp_len=10, adm_len=8, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x00, allowed: 0 1 2 3 4 5 6 7
sys={36.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0ff -> 0x1fe (active_len=8, ramp_len=10, adm_len=8, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x01, allowed: 1 2 3 4 5 6 7 8
sys={38.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1fe -> 0x1fd (active_len=8, ramp_len=10, adm_len=8, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x02, allowed: 0 2 3 4 5 6 7 8
sys={40.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1fd -> 0x1fb (active_len=8, ramp_len=10, adm_len=8, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x04, allowed: 0 1 3 4 5 6 7 8
BTS deallocated OK in test_acc_mgr_rotate()
===test_acc_mgr_rotate(false, 8)===
(bts=0) ACC: New ACC allowed subset 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
BTS allocation OK in test_acc_mgr_rotate()
(bts=0) ACC: update ACC allowed active subset 0x3ff -> 0x3fc (active_len=8, ramp_len=10, adm_len=8, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x03, allowed: 2 3 4 5 6 7 8 9
sys={2.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3fc -> 0x3f9 (active_len=8, ramp_len=10, adm_len=8, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x06, allowed: 0 3 4 5 6 7 8 9
sys={4.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3f9 -> 0x3f3 (active_len=8, ramp_len=10, adm_len=8, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x0c, allowed: 0 1 4 5 6 7 8 9
sys={6.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3f3 -> 0x3e7 (active_len=8, ramp_len=10, adm_len=8, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x18, allowed: 0 1 2 5 6 7 8 9
sys={8.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3e7 -> 0x3cf (active_len=8, ramp_len=10, adm_len=8, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x30, allowed: 0 1 2 3 6 7 8 9
sys={10.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3cf -> 0x39f (active_len=8, ramp_len=10, adm_len=8, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x60, allowed: 0 1 2 3 4 7 8 9
sys={12.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x39f -> 0x33f (active_len=8, ramp_len=10, adm_len=8, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0xc0, allowed: 0 1 2 3 4 5 8 9
sys={14.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x33f -> 0x27f (active_len=8, ramp_len=10, adm_len=8, perm_len=10, rotation=on)
pcu_info_update(): t2=0x01 t3=0x80, allowed: 0 1 2 3 4 5 6 9
sys={16.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x27f -> 0x0ff (active_len=8, ramp_len=10, adm_len=8, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x00, allowed: 0 1 2 3 4 5 6 7
sys={18.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0ff -> 0x1fe (active_len=8, ramp_len=10, adm_len=8, perm_len=10, rotation=on)
pcu_info_update(): t2=0x02 t3=0x01, allowed: 1 2 3 4 5 6 7 8
sys={20.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1fe -> 0x3fc (active_len=8, ramp_len=10, adm_len=8, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x03, allowed: 2 3 4 5 6 7 8 9
sys={22.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3fc -> 0x3f9 (active_len=8, ramp_len=10, adm_len=8, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x06, allowed: 0 3 4 5 6 7 8 9
sys={24.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3f9 -> 0x3f3 (active_len=8, ramp_len=10, adm_len=8, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x0c, allowed: 0 1 4 5 6 7 8 9
sys={26.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3f3 -> 0x3e7 (active_len=8, ramp_len=10, adm_len=8, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x18, allowed: 0 1 2 5 6 7 8 9
sys={28.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3e7 -> 0x3cf (active_len=8, ramp_len=10, adm_len=8, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x30, allowed: 0 1 2 3 6 7 8 9
sys={30.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3cf -> 0x39f (active_len=8, ramp_len=10, adm_len=8, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x60, allowed: 0 1 2 3 4 7 8 9
sys={32.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x39f -> 0x33f (active_len=8, ramp_len=10, adm_len=8, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0xc0, allowed: 0 1 2 3 4 5 8 9
sys={34.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x33f -> 0x27f (active_len=8, ramp_len=10, adm_len=8, perm_len=10, rotation=on)
pcu_info_update(): t2=0x01 t3=0x80, allowed: 0 1 2 3 4 5 6 9
sys={36.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x27f -> 0x0ff (active_len=8, ramp_len=10, adm_len=8, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x00, allowed: 0 1 2 3 4 5 6 7
sys={38.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0ff -> 0x1fe (active_len=8, ramp_len=10, adm_len=8, perm_len=10, rotation=on)
pcu_info_update(): t2=0x02 t3=0x01, allowed: 1 2 3 4 5 6 7 8
sys={40.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1fe -> 0x3fc (active_len=8, ramp_len=10, adm_len=8, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x03, allowed: 2 3 4 5 6 7 8 9
BTS deallocated OK in test_acc_mgr_rotate()
===test_acc_mgr_rotate(false, 9)===
(bts=0) ACC: New ACC allowed subset 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
BTS allocation OK in test_acc_mgr_rotate()
(bts=0) ACC: update ACC allowed active subset 0x3ff -> 0x3fe (active_len=9, ramp_len=10, adm_len=9, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x01, allowed: 1 2 3 4 5 6 7 8 9
sys={2.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3fe -> 0x3fd (active_len=9, ramp_len=10, adm_len=9, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x02, allowed: 0 2 3 4 5 6 7 8 9
sys={4.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3fd -> 0x3fb (active_len=9, ramp_len=10, adm_len=9, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x04, allowed: 0 1 3 4 5 6 7 8 9
sys={6.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3fb -> 0x3f7 (active_len=9, ramp_len=10, adm_len=9, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x08, allowed: 0 1 2 4 5 6 7 8 9
sys={8.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3f7 -> 0x3ef (active_len=9, ramp_len=10, adm_len=9, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x10, allowed: 0 1 2 3 5 6 7 8 9
sys={10.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3ef -> 0x3df (active_len=9, ramp_len=10, adm_len=9, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x20, allowed: 0 1 2 3 4 6 7 8 9
sys={12.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3df -> 0x3bf (active_len=9, ramp_len=10, adm_len=9, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x40, allowed: 0 1 2 3 4 5 7 8 9
sys={14.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3bf -> 0x37f (active_len=9, ramp_len=10, adm_len=9, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x80, allowed: 0 1 2 3 4 5 6 8 9
sys={16.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x37f -> 0x2ff (active_len=9, ramp_len=10, adm_len=9, perm_len=10, rotation=on)
pcu_info_update(): t2=0x01 t3=0x00, allowed: 0 1 2 3 4 5 6 7 9
sys={18.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x2ff -> 0x1ff (active_len=9, ramp_len=10, adm_len=9, perm_len=10, rotation=on)
pcu_info_update(): t2=0x02 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8
sys={20.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1ff -> 0x3fe (active_len=9, ramp_len=10, adm_len=9, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x01, allowed: 1 2 3 4 5 6 7 8 9
sys={22.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3fe -> 0x3fd (active_len=9, ramp_len=10, adm_len=9, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x02, allowed: 0 2 3 4 5 6 7 8 9
sys={24.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3fd -> 0x3fb (active_len=9, ramp_len=10, adm_len=9, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x04, allowed: 0 1 3 4 5 6 7 8 9
sys={26.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3fb -> 0x3f7 (active_len=9, ramp_len=10, adm_len=9, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x08, allowed: 0 1 2 4 5 6 7 8 9
sys={28.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3f7 -> 0x3ef (active_len=9, ramp_len=10, adm_len=9, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x10, allowed: 0 1 2 3 5 6 7 8 9
sys={30.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3ef -> 0x3df (active_len=9, ramp_len=10, adm_len=9, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x20, allowed: 0 1 2 3 4 6 7 8 9
sys={32.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3df -> 0x3bf (active_len=9, ramp_len=10, adm_len=9, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x40, allowed: 0 1 2 3 4 5 7 8 9
sys={34.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x3bf -> 0x37f (active_len=9, ramp_len=10, adm_len=9, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x80, allowed: 0 1 2 3 4 5 6 8 9
sys={36.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x37f -> 0x2ff (active_len=9, ramp_len=10, adm_len=9, perm_len=10, rotation=on)
pcu_info_update(): t2=0x01 t3=0x00, allowed: 0 1 2 3 4 5 6 7 9
sys={38.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x2ff -> 0x1ff (active_len=9, ramp_len=10, adm_len=9, perm_len=10, rotation=on)
pcu_info_update(): t2=0x02 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8
sys={40.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1ff -> 0x3fe (active_len=9, ramp_len=10, adm_len=9, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x01, allowed: 1 2 3 4 5 6 7 8 9
BTS deallocated OK in test_acc_mgr_rotate()
===test_acc_ramp===
(bts=0) ACC: New ACC allowed subset 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
BTS allocation OK in test_acc_ramp()
(bts=0) ACC: update ACC allowed active subset 0x3ff -> 0x000 (active_len=0, ramp_len=0, adm_len=10, perm_len=10, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x001 (active_len=1, ramp_len=1, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfe, allowed: 0
sys={50.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x001 -> 0x003 (active_len=2, ramp_len=2, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfc, allowed: 0 1
sys={100.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x003 -> 0x007 (active_len=3, ramp_len=3, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf8, allowed: 0 1 2
sys={150.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x007 -> 0x00f (active_len=4, ramp_len=4, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf0, allowed: 0 1 2 3
sys={200.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x00f -> 0x01f (active_len=5, ramp_len=5, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe0, allowed: 0 1 2 3 4
sys={250.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x01f -> 0x03f (active_len=6, ramp_len=6, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xc0, allowed: 0 1 2 3 4 5
sys={300.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x03f -> 0x07f (active_len=7, ramp_len=7, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x80, allowed: 0 1 2 3 4 5 6
sys={350.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x07f -> 0x0ff (active_len=8, ramp_len=8, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x00, allowed: 0 1 2 3 4 5 6 7
sys={400.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x0ff -> 0x1ff (active_len=9, ramp_len=9, adm_len=10, perm_len=10, rotation=on)
pcu_info_update(): t2=0x02 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8
sys={450.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x1ff -> 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
pcu_info_update(): t2=0x00 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8 9
BTS deallocated OK in test_acc_ramp()
===test_acc_ramp2===
(bts=0) ACC: New ACC allowed subset 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
BTS allocation OK in test_acc_ramp2()
(bts=0) ACC: update ACC allowed active subset 0x3ff -> 0x3f8 (active_len=7, ramp_len=10, adm_len=7, perm_len=10, rotation=on)
pcu_info_update(): t2=0x00 t3=0x07, allowed: 3 4 5 6 7 8 9
(bts=0) ACC: update ACC allowed active subset 0x3f8 -> 0x000 (active_len=0, ramp_len=0, adm_len=7, perm_len=10, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x007 (active_len=3, ramp_len=3, adm_len=7, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf8, allowed: 0 1 2
sys={5.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x007 -> 0x03f (active_len=6, ramp_len=6, adm_len=7, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0xc0, allowed: 0 1 2 3 4 5
sys={10.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x03f -> 0x07f (active_len=7, ramp_len=7, adm_len=7, perm_len=10, rotation=on)
pcu_info_update(): t2=0x03 t3=0x80, allowed: 0 1 2 3 4 5 6
sys={15.000000}: select()
BTS deallocated OK in test_acc_ramp2()
===test_acc_ramp3===
(bts=0) ACC: New ACC allowed subset 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
BTS allocation OK in test_acc_ramp3()
*** Barring some ACCs ***
(bts=0) ACC: New ACC allowed subset 0x15a (active_len=5, ramp_len=10, adm_len=10, perm_len=5, rotation=off)
pcu_info_update(): t2=0x02 t3=0xa5, allowed: 1 3 4 6 8
(bts=0) ACC: update ACC allowed active subset 0x15a -> 0x000 (active_len=0, ramp_len=0, adm_len=10, perm_len=5, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x002 (active_len=1, ramp_len=1, adm_len=10, perm_len=5, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfd, allowed: 1
sys={5.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x002 -> 0x00a (active_len=2, ramp_len=2, adm_len=10, perm_len=5, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf5, allowed: 1 3
sys={10.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x00a -> 0x01a (active_len=3, ramp_len=3, adm_len=10, perm_len=5, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe5, allowed: 1 3 4
sys={15.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x01a -> 0x05a (active_len=4, ramp_len=4, adm_len=10, perm_len=5, rotation=on)
pcu_info_update(): t2=0x03 t3=0xa5, allowed: 1 3 4 6
sys={20.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x05a -> 0x15a (active_len=5, ramp_len=5, adm_len=10, perm_len=5, rotation=off)
pcu_info_update(): t2=0x02 t3=0xa5, allowed: 1 3 4 6 8
sys={25.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x15a -> 0x15a (active_len=5, ramp_len=6, adm_len=10, perm_len=5, rotation=off)
sys={30.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x15a -> 0x15a (active_len=5, ramp_len=7, adm_len=10, perm_len=5, rotation=off)
sys={35.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x15a -> 0x15a (active_len=5, ramp_len=8, adm_len=10, perm_len=5, rotation=off)
sys={40.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x15a -> 0x15a (active_len=5, ramp_len=9, adm_len=10, perm_len=5, rotation=off)
sys={45.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x15a -> 0x15a (active_len=5, ramp_len=10, adm_len=10, perm_len=5, rotation=off)
BTS deallocated OK in test_acc_ramp3()
===test_acc_ramp_up_rotate(0, 100, 100)===
(bts=0) ACC: New ACC allowed subset 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
BTS allocation OK in test_acc_ramp_up_rotate()
*** Barring one ACC ***
(bts=0) ACC: New ACC allowed subset 0x1ff (active_len=9, ramp_len=10, adm_len=10, perm_len=9, rotation=off)
pcu_info_update(): t2=0x02 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8
(bts=0) ACC: update ACC allowed active subset 0x1ff -> 0x000 (active_len=0, ramp_len=0, adm_len=10, perm_len=9, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x001 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfe, allowed: 0
sys={100.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x001 -> 0x002 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfd, allowed: 1
sys={200.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x002 -> 0x004 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfb, allowed: 2
sys={250.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x004 -> 0x00c (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf3, allowed: 2 3
sys={350.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x00c -> 0x018 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe7, allowed: 3 4
sys={450.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x018 -> 0x030 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xcf, allowed: 4 5
sys={500.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x030 -> 0x070 (active_len=3, ramp_len=3, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x8f, allowed: 4 5 6
sys={600.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x070 -> 0x0e0 (active_len=3, ramp_len=3, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x1f, allowed: 5 6 7
sys={700.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0e0 -> 0x1c0 (active_len=3, ramp_len=3, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x3f, allowed: 6 7 8
sys={750.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x1c0 -> 0x1c1 (active_len=4, ramp_len=4, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x3e, allowed: 0 6 7 8
sys={850.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1c1 -> 0x183 (active_len=4, ramp_len=4, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x7c, allowed: 0 1 7 8
sys={950.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x183 -> 0x107 (active_len=4, ramp_len=4, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xf8, allowed: 0 1 2 8
sys={1000.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x107 -> 0x10f (active_len=5, ramp_len=5, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xf0, allowed: 0 1 2 3 8
sys={1100.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x10f -> 0x01f (active_len=5, ramp_len=5, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe0, allowed: 0 1 2 3 4
sys={1200.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x01f -> 0x03e (active_len=5, ramp_len=5, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xc1, allowed: 1 2 3 4 5
sys={1250.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x03e -> 0x07e (active_len=6, ramp_len=6, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x81, allowed: 1 2 3 4 5 6
sys={1350.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x07e -> 0x0fc (active_len=6, ramp_len=6, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x03, allowed: 2 3 4 5 6 7
sys={1450.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0fc -> 0x1f8 (active_len=6, ramp_len=6, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x07, allowed: 3 4 5 6 7 8
sys={1500.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x1f8 -> 0x1f9 (active_len=7, ramp_len=7, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x06, allowed: 0 3 4 5 6 7 8
sys={1600.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1f9 -> 0x1f3 (active_len=7, ramp_len=7, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x0c, allowed: 0 1 4 5 6 7 8
sys={1700.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1f3 -> 0x1e7 (active_len=7, ramp_len=7, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x18, allowed: 0 1 2 5 6 7 8
sys={1750.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x1e7 -> 0x1ef (active_len=8, ramp_len=8, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x10, allowed: 0 1 2 3 5 6 7 8
sys={1850.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1ef -> 0x1df (active_len=8, ramp_len=8, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x20, allowed: 0 1 2 3 4 6 7 8
sys={1950.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1df -> 0x1bf (active_len=8, ramp_len=8, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x40, allowed: 0 1 2 3 4 5 7 8
sys={2000.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x1bf -> 0x1ff (active_len=9, ramp_len=9, adm_len=10, perm_len=9, rotation=off)
pcu_info_update(): t2=0x02 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8
sys={2250.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x1ff -> 0x1ff (active_len=9, ramp_len=10, adm_len=10, perm_len=9, rotation=off)
sys={2500.000000}: select()
sys={2750.000000}: select()
sys={3000.000000}: select()
sys={3250.000000}: select()
BTS deallocated OK in test_acc_ramp_up_rotate()
===test_acc_ramp_up_rotate(0, 20, 50)===
(bts=0) ACC: New ACC allowed subset 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
BTS allocation OK in test_acc_ramp_up_rotate()
*** Barring one ACC ***
(bts=0) ACC: New ACC allowed subset 0x1ff (active_len=9, ramp_len=10, adm_len=10, perm_len=9, rotation=off)
pcu_info_update(): t2=0x02 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8
(bts=0) ACC: update ACC allowed active subset 0x1ff -> 0x000 (active_len=0, ramp_len=0, adm_len=10, perm_len=9, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x001 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfe, allowed: 0
sys={100.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x001 -> 0x002 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfd, allowed: 1
sys={200.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x002 -> 0x004 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfb, allowed: 2
sys={250.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x004 -> 0x00c (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf3, allowed: 2 3
sys={350.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x00c -> 0x018 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe7, allowed: 3 4
sys={450.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x018 -> 0x030 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xcf, allowed: 4 5
sys={500.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x030 -> 0x070 (active_len=3, ramp_len=3, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x8f, allowed: 4 5 6
sys={600.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x070 -> 0x0e0 (active_len=3, ramp_len=3, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x1f, allowed: 5 6 7
sys={700.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0e0 -> 0x1c0 (active_len=3, ramp_len=3, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x3f, allowed: 6 7 8
sys={750.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x1c0 -> 0x1c1 (active_len=4, ramp_len=4, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x3e, allowed: 0 6 7 8
sys={850.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1c1 -> 0x183 (active_len=4, ramp_len=4, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x7c, allowed: 0 1 7 8
sys={950.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x183 -> 0x107 (active_len=4, ramp_len=4, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xf8, allowed: 0 1 2 8
sys={1000.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x107 -> 0x10f (active_len=5, ramp_len=5, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xf0, allowed: 0 1 2 3 8
sys={1100.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x10f -> 0x01f (active_len=5, ramp_len=5, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe0, allowed: 0 1 2 3 4
sys={1200.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x01f -> 0x03e (active_len=5, ramp_len=5, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xc1, allowed: 1 2 3 4 5
sys={1250.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x03e -> 0x07e (active_len=6, ramp_len=6, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x81, allowed: 1 2 3 4 5 6
sys={1350.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x07e -> 0x0fc (active_len=6, ramp_len=6, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x03, allowed: 2 3 4 5 6 7
sys={1450.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0fc -> 0x1f8 (active_len=6, ramp_len=6, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x07, allowed: 3 4 5 6 7 8
sys={1500.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x1f8 -> 0x1f9 (active_len=7, ramp_len=7, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x06, allowed: 0 3 4 5 6 7 8
sys={1600.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1f9 -> 0x1f3 (active_len=7, ramp_len=7, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x0c, allowed: 0 1 4 5 6 7 8
sys={1700.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1f3 -> 0x1e7 (active_len=7, ramp_len=7, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x18, allowed: 0 1 2 5 6 7 8
sys={1750.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x1e7 -> 0x1ef (active_len=8, ramp_len=8, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x10, allowed: 0 1 2 3 5 6 7 8
sys={1850.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1ef -> 0x1df (active_len=8, ramp_len=8, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x20, allowed: 0 1 2 3 4 6 7 8
sys={1950.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1df -> 0x1bf (active_len=8, ramp_len=8, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x40, allowed: 0 1 2 3 4 5 7 8
sys={2000.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x1bf -> 0x1ff (active_len=9, ramp_len=9, adm_len=10, perm_len=9, rotation=off)
pcu_info_update(): t2=0x02 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8
sys={2250.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x1ff -> 0x1ff (active_len=9, ramp_len=10, adm_len=10, perm_len=9, rotation=off)
sys={2500.000000}: select()
sys={2750.000000}: select()
sys={3000.000000}: select()
sys={3250.000000}: select()
BTS deallocated OK in test_acc_ramp_up_rotate()
===test_acc_ramp_up_rotate(70, 80, 90)===
(bts=0) ACC: New ACC allowed subset 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
BTS allocation OK in test_acc_ramp_up_rotate()
*** Barring one ACC ***
(bts=0) ACC: New ACC allowed subset 0x1ff (active_len=9, ramp_len=10, adm_len=10, perm_len=9, rotation=off)
pcu_info_update(): t2=0x02 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8
(bts=0) ACC: update ACC allowed active subset 0x1ff -> 0x000 (active_len=0, ramp_len=0, adm_len=10, perm_len=9, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x001 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfe, allowed: 0
sys={100.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x001 -> 0x002 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfd, allowed: 1
sys={200.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x002 -> 0x004 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfb, allowed: 2
sys={250.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x004 -> 0x00c (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf3, allowed: 2 3
sys={350.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x00c -> 0x018 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe7, allowed: 3 4
sys={450.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x018 -> 0x030 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xcf, allowed: 4 5
sys={500.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x030 -> 0x070 (active_len=3, ramp_len=3, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x8f, allowed: 4 5 6
sys={600.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x070 -> 0x0e0 (active_len=3, ramp_len=3, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x1f, allowed: 5 6 7
sys={700.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0e0 -> 0x1c0 (active_len=3, ramp_len=3, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x3f, allowed: 6 7 8
sys={750.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x1c0 -> 0x1c1 (active_len=4, ramp_len=4, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x3e, allowed: 0 6 7 8
sys={850.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1c1 -> 0x183 (active_len=4, ramp_len=4, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x7c, allowed: 0 1 7 8
sys={950.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x183 -> 0x107 (active_len=4, ramp_len=4, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xf8, allowed: 0 1 2 8
sys={1000.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x107 -> 0x10f (active_len=5, ramp_len=5, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xf0, allowed: 0 1 2 3 8
sys={1100.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x10f -> 0x01f (active_len=5, ramp_len=5, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe0, allowed: 0 1 2 3 4
sys={1200.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x01f -> 0x03e (active_len=5, ramp_len=5, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xc1, allowed: 1 2 3 4 5
sys={1250.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x03e -> 0x07e (active_len=6, ramp_len=6, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x81, allowed: 1 2 3 4 5 6
sys={1350.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x07e -> 0x0fc (active_len=6, ramp_len=6, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x03, allowed: 2 3 4 5 6 7
sys={1450.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x0fc -> 0x1f8 (active_len=6, ramp_len=6, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x07, allowed: 3 4 5 6 7 8
sys={1500.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x1f8 -> 0x1f9 (active_len=7, ramp_len=7, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x06, allowed: 0 3 4 5 6 7 8
sys={1600.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1f9 -> 0x1f3 (active_len=7, ramp_len=7, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x0c, allowed: 0 1 4 5 6 7 8
sys={1700.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1f3 -> 0x1e7 (active_len=7, ramp_len=7, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x18, allowed: 0 1 2 5 6 7 8
sys={1750.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x1e7 -> 0x1ef (active_len=8, ramp_len=8, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x10, allowed: 0 1 2 3 5 6 7 8
sys={1850.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1ef -> 0x1df (active_len=8, ramp_len=8, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x20, allowed: 0 1 2 3 4 6 7 8
sys={1950.000000}: select()
(bts=0) ACC: rotate ACC allowed active subset 0x1df -> 0x1bf (active_len=8, ramp_len=8, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x40, allowed: 0 1 2 3 4 5 7 8
sys={2000.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x1bf -> 0x1ff (active_len=9, ramp_len=9, adm_len=10, perm_len=9, rotation=off)
pcu_info_update(): t2=0x02 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8
sys={2250.000000}: select()
(bts=0) ACC: update ACC allowed active subset 0x1ff -> 0x1ff (active_len=9, ramp_len=10, adm_len=10, perm_len=9, rotation=off)
sys={2500.000000}: select()
sys={2750.000000}: select()
sys={3000.000000}: select()
sys={3250.000000}: select()
BTS deallocated OK in test_acc_ramp_up_rotate()
===test_acc_ramp_updown_rotate(80, 90, 0, 100, 15)===
(bts=0) ACC: New ACC allowed subset 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
BTS allocation OK in test_acc_ramp_updown_rotate()
*** Barring one ACC ***
(bts=0) ACC: New ACC allowed subset 0x1ff (active_len=9, ramp_len=10, adm_len=10, perm_len=9, rotation=off)
pcu_info_update(): t2=0x02 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8
(bts=0) ACC: update ACC allowed active subset 0x1ff -> 0x000 (active_len=0, ramp_len=0, adm_len=10, perm_len=9, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x001 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfe, allowed: 0
sys={100.000000}: select(0): chan_load_avg=0
(bts=0) ACC: rotate ACC allowed active subset 0x001 -> 0x002 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfd, allowed: 1
sys={200.000000}: select(1): chan_load_avg=15
(bts=0) ACC: rotate ACC allowed active subset 0x002 -> 0x004 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfb, allowed: 2
sys={250.000000}: select(2): chan_load_avg=30
(bts=0) ACC: update ACC allowed active subset 0x004 -> 0x00c (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf3, allowed: 2 3
sys={350.000000}: select(3): chan_load_avg=45
(bts=0) ACC: rotate ACC allowed active subset 0x00c -> 0x018 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe7, allowed: 3 4
sys={450.000000}: select(4): chan_load_avg=60
(bts=0) ACC: rotate ACC allowed active subset 0x018 -> 0x030 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xcf, allowed: 4 5
sys={500.000000}: select(5): chan_load_avg=75
(bts=0) ACC: update ACC allowed active subset 0x030 -> 0x070 (active_len=3, ramp_len=3, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x8f, allowed: 4 5 6
sys={600.000000}: select(6): chan_load_avg=90
(bts=0) ACC: rotate ACC allowed active subset 0x070 -> 0x0e0 (active_len=3, ramp_len=3, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x1f, allowed: 5 6 7
sys={700.000000}: select(7): chan_load_avg=100
(bts=0) ACC: rotate ACC allowed active subset 0x0e0 -> 0x1c0 (active_len=3, ramp_len=3, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x3f, allowed: 6 7 8
sys={750.000000}: select(8): chan_load_avg=85
sys={850.000000}: select(9): chan_load_avg=70
(bts=0) ACC: rotate ACC allowed active subset 0x1c0 -> 0x181 (active_len=3, ramp_len=3, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x7e, allowed: 0 7 8
sys={950.000000}: select(10): chan_load_avg=55
(bts=0) ACC: rotate ACC allowed active subset 0x181 -> 0x103 (active_len=3, ramp_len=3, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xfc, allowed: 0 1 8
sys={1000.000000}: select(11): chan_load_avg=40
(bts=0) ACC: update ACC allowed active subset 0x103 -> 0x107 (active_len=4, ramp_len=4, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xf8, allowed: 0 1 2 8
sys={1100.000000}: select(12): chan_load_avg=25
(bts=0) ACC: rotate ACC allowed active subset 0x107 -> 0x00f (active_len=4, ramp_len=4, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf0, allowed: 0 1 2 3
sys={1200.000000}: select(13): chan_load_avg=10
(bts=0) ACC: rotate ACC allowed active subset 0x00f -> 0x01e (active_len=4, ramp_len=4, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe1, allowed: 1 2 3 4
sys={1250.000000}: select(14): chan_load_avg=0
(bts=0) ACC: update ACC allowed active subset 0x01e -> 0x03e (active_len=5, ramp_len=5, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xc1, allowed: 1 2 3 4 5
sys={1350.000000}: select(15): chan_load_avg=15
(bts=0) ACC: rotate ACC allowed active subset 0x03e -> 0x07c (active_len=5, ramp_len=5, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x83, allowed: 2 3 4 5 6
sys={1450.000000}: select(16): chan_load_avg=30
(bts=0) ACC: rotate ACC allowed active subset 0x07c -> 0x0f8 (active_len=5, ramp_len=5, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x07, allowed: 3 4 5 6 7
sys={1500.000000}: select(17): chan_load_avg=45
(bts=0) ACC: update ACC allowed active subset 0x0f8 -> 0x1f8 (active_len=6, ramp_len=6, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x07, allowed: 3 4 5 6 7 8
sys={1600.000000}: select(18): chan_load_avg=60
(bts=0) ACC: rotate ACC allowed active subset 0x1f8 -> 0x1f1 (active_len=6, ramp_len=6, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x0e, allowed: 0 4 5 6 7 8
sys={1700.000000}: select(19): chan_load_avg=75
(bts=0) ACC: rotate ACC allowed active subset 0x1f1 -> 0x1e3 (active_len=6, ramp_len=6, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x1c, allowed: 0 1 5 6 7 8
sys={1750.000000}: select(20): chan_load_avg=90
sys={1850.000000}: select(21): chan_load_avg=100
(bts=0) ACC: rotate ACC allowed active subset 0x1e3 -> 0x1c7 (active_len=6, ramp_len=6, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x38, allowed: 0 1 2 6 7 8
sys={1950.000000}: select(22): chan_load_avg=85
(bts=0) ACC: rotate ACC allowed active subset 0x1c7 -> 0x18f (active_len=6, ramp_len=6, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x70, allowed: 0 1 2 3 7 8
sys={2000.000000}: select(23): chan_load_avg=70
(bts=0) ACC: update ACC allowed active subset 0x18f -> 0x19f (active_len=7, ramp_len=7, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x60, allowed: 0 1 2 3 4 7 8
sys={2100.000000}: select(24): chan_load_avg=55
(bts=0) ACC: rotate ACC allowed active subset 0x19f -> 0x13f (active_len=7, ramp_len=7, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xc0, allowed: 0 1 2 3 4 5 8
sys={2200.000000}: select(25): chan_load_avg=40
(bts=0) ACC: rotate ACC allowed active subset 0x13f -> 0x07f (active_len=7, ramp_len=7, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x80, allowed: 0 1 2 3 4 5 6
sys={2250.000000}: select(26): chan_load_avg=25
(bts=0) ACC: update ACC allowed active subset 0x07f -> 0x0ff (active_len=8, ramp_len=8, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x00, allowed: 0 1 2 3 4 5 6 7
sys={2350.000000}: select(27): chan_load_avg=10
(bts=0) ACC: rotate ACC allowed active subset 0x0ff -> 0x1fe (active_len=8, ramp_len=8, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x01, allowed: 1 2 3 4 5 6 7 8
sys={2450.000000}: select(28): chan_load_avg=0
(bts=0) ACC: rotate ACC allowed active subset 0x1fe -> 0x1fd (active_len=8, ramp_len=8, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x02, allowed: 0 2 3 4 5 6 7 8
sys={2500.000000}: select(29): chan_load_avg=15
(bts=0) ACC: update ACC allowed active subset 0x1fd -> 0x1ff (active_len=9, ramp_len=9, adm_len=10, perm_len=9, rotation=off)
pcu_info_update(): t2=0x02 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8
sys={2750.000000}: select(30): chan_load_avg=30
(bts=0) ACC: update ACC allowed active subset 0x1ff -> 0x1ff (active_len=9, ramp_len=10, adm_len=10, perm_len=9, rotation=off)
sys={3000.000000}: select(31): chan_load_avg=45
sys={3250.000000}: select(32): chan_load_avg=60
sys={3500.000000}: select(33): chan_load_avg=75
sys={3750.000000}: select(34): chan_load_avg=90
sys={4000.000000}: select(35): chan_load_avg=100
sys={4250.000000}: select(36): chan_load_avg=85
sys={4500.000000}: select(37): chan_load_avg=70
(bts=0) ACC: update ACC allowed active subset 0x1ff -> 0x1ff (active_len=9, ramp_len=10, adm_len=10, perm_len=9, rotation=off)
sys={4750.000000}: select(38): chan_load_avg=55
sys={5000.000000}: select(39): chan_load_avg=40
sys={5250.000000}: select(40): chan_load_avg=25
sys={5500.000000}: select(41): chan_load_avg=10
sys={5750.000000}: select(42): chan_load_avg=0
sys={6000.000000}: select(43): chan_load_avg=15
sys={6250.000000}: select(44): chan_load_avg=30
sys={6500.000000}: select(45): chan_load_avg=45
sys={6750.000000}: select(46): chan_load_avg=60
sys={7000.000000}: select(47): chan_load_avg=75
sys={7250.000000}: select(48): chan_load_avg=90
sys={7500.000000}: select(49): chan_load_avg=100
BTS deallocated OK in test_acc_ramp_updown_rotate()
===test_acc_ramp_updown_rotate(30, 50, 10, 100, 15)===
(bts=0) ACC: New ACC allowed subset 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
BTS allocation OK in test_acc_ramp_updown_rotate()
*** Barring one ACC ***
(bts=0) ACC: New ACC allowed subset 0x1ff (active_len=9, ramp_len=10, adm_len=10, perm_len=9, rotation=off)
pcu_info_update(): t2=0x02 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8
(bts=0) ACC: update ACC allowed active subset 0x1ff -> 0x000 (active_len=0, ramp_len=0, adm_len=10, perm_len=9, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x001 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfe, allowed: 0
sys={100.000000}: select(0): chan_load_avg=10
(bts=0) ACC: rotate ACC allowed active subset 0x001 -> 0x002 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfd, allowed: 1
sys={200.000000}: select(1): chan_load_avg=25
(bts=0) ACC: rotate ACC allowed active subset 0x002 -> 0x004 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfb, allowed: 2
sys={250.000000}: select(2): chan_load_avg=40
sys={350.000000}: select(3): chan_load_avg=55
(bts=0) ACC: rotate ACC allowed active subset 0x004 -> 0x008 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf7, allowed: 3
sys={450.000000}: select(4): chan_load_avg=70
(bts=0) ACC: rotate ACC allowed active subset 0x008 -> 0x010 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xef, allowed: 4
sys={500.000000}: select(5): chan_load_avg=85
sys={600.000000}: select(6): chan_load_avg=100
(bts=0) ACC: rotate ACC allowed active subset 0x010 -> 0x020 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xdf, allowed: 5
sys={700.000000}: select(7): chan_load_avg=85
(bts=0) ACC: rotate ACC allowed active subset 0x020 -> 0x040 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xbf, allowed: 6
sys={750.000000}: select(8): chan_load_avg=70
sys={850.000000}: select(9): chan_load_avg=55
(bts=0) ACC: rotate ACC allowed active subset 0x040 -> 0x080 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x7f, allowed: 7
sys={950.000000}: select(10): chan_load_avg=40
(bts=0) ACC: rotate ACC allowed active subset 0x080 -> 0x100 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xff, allowed: 8
sys={1000.000000}: select(11): chan_load_avg=25
(bts=0) ACC: update ACC allowed active subset 0x100 -> 0x101 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xfe, allowed: 0 8
sys={1100.000000}: select(12): chan_load_avg=10
(bts=0) ACC: rotate ACC allowed active subset 0x101 -> 0x003 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfc, allowed: 0 1
sys={1200.000000}: select(13): chan_load_avg=25
(bts=0) ACC: rotate ACC allowed active subset 0x003 -> 0x006 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf9, allowed: 1 2
sys={1250.000000}: select(14): chan_load_avg=40
sys={1350.000000}: select(15): chan_load_avg=55
(bts=0) ACC: rotate ACC allowed active subset 0x006 -> 0x00c (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf3, allowed: 2 3
sys={1450.000000}: select(16): chan_load_avg=70
(bts=0) ACC: rotate ACC allowed active subset 0x00c -> 0x018 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe7, allowed: 3 4
sys={1500.000000}: select(17): chan_load_avg=85
(bts=0) ACC: update ACC allowed active subset 0x018 -> 0x010 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xef, allowed: 4
sys={1600.000000}: select(18): chan_load_avg=100
(bts=0) ACC: rotate ACC allowed active subset 0x010 -> 0x020 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xdf, allowed: 5
sys={1700.000000}: select(19): chan_load_avg=85
(bts=0) ACC: rotate ACC allowed active subset 0x020 -> 0x040 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xbf, allowed: 6
sys={1750.000000}: select(20): chan_load_avg=70
sys={1850.000000}: select(21): chan_load_avg=55
(bts=0) ACC: rotate ACC allowed active subset 0x040 -> 0x080 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x7f, allowed: 7
sys={1950.000000}: select(22): chan_load_avg=40
(bts=0) ACC: rotate ACC allowed active subset 0x080 -> 0x100 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xff, allowed: 8
sys={2000.000000}: select(23): chan_load_avg=25
(bts=0) ACC: update ACC allowed active subset 0x100 -> 0x101 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xfe, allowed: 0 8
sys={2100.000000}: select(24): chan_load_avg=10
(bts=0) ACC: rotate ACC allowed active subset 0x101 -> 0x003 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfc, allowed: 0 1
sys={2200.000000}: select(25): chan_load_avg=25
(bts=0) ACC: rotate ACC allowed active subset 0x003 -> 0x006 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf9, allowed: 1 2
sys={2250.000000}: select(26): chan_load_avg=40
sys={2350.000000}: select(27): chan_load_avg=55
(bts=0) ACC: rotate ACC allowed active subset 0x006 -> 0x00c (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf3, allowed: 2 3
sys={2450.000000}: select(28): chan_load_avg=70
(bts=0) ACC: rotate ACC allowed active subset 0x00c -> 0x018 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe7, allowed: 3 4
sys={2500.000000}: select(29): chan_load_avg=85
(bts=0) ACC: update ACC allowed active subset 0x018 -> 0x010 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xef, allowed: 4
sys={2600.000000}: select(30): chan_load_avg=100
(bts=0) ACC: rotate ACC allowed active subset 0x010 -> 0x020 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xdf, allowed: 5
sys={2700.000000}: select(31): chan_load_avg=85
(bts=0) ACC: rotate ACC allowed active subset 0x020 -> 0x040 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xbf, allowed: 6
sys={2750.000000}: select(32): chan_load_avg=70
sys={2850.000000}: select(33): chan_load_avg=55
(bts=0) ACC: rotate ACC allowed active subset 0x040 -> 0x080 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x7f, allowed: 7
sys={2950.000000}: select(34): chan_load_avg=40
(bts=0) ACC: rotate ACC allowed active subset 0x080 -> 0x100 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xff, allowed: 8
sys={3000.000000}: select(35): chan_load_avg=25
(bts=0) ACC: update ACC allowed active subset 0x100 -> 0x101 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xfe, allowed: 0 8
sys={3100.000000}: select(36): chan_load_avg=10
(bts=0) ACC: rotate ACC allowed active subset 0x101 -> 0x003 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfc, allowed: 0 1
sys={3200.000000}: select(37): chan_load_avg=25
(bts=0) ACC: rotate ACC allowed active subset 0x003 -> 0x006 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf9, allowed: 1 2
sys={3250.000000}: select(38): chan_load_avg=40
sys={3350.000000}: select(39): chan_load_avg=55
(bts=0) ACC: rotate ACC allowed active subset 0x006 -> 0x00c (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf3, allowed: 2 3
sys={3450.000000}: select(40): chan_load_avg=70
(bts=0) ACC: rotate ACC allowed active subset 0x00c -> 0x018 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe7, allowed: 3 4
sys={3500.000000}: select(41): chan_load_avg=85
(bts=0) ACC: update ACC allowed active subset 0x018 -> 0x010 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xef, allowed: 4
sys={3600.000000}: select(42): chan_load_avg=100
(bts=0) ACC: rotate ACC allowed active subset 0x010 -> 0x020 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xdf, allowed: 5
sys={3700.000000}: select(43): chan_load_avg=85
(bts=0) ACC: rotate ACC allowed active subset 0x020 -> 0x040 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xbf, allowed: 6
sys={3750.000000}: select(44): chan_load_avg=70
sys={3850.000000}: select(45): chan_load_avg=55
(bts=0) ACC: rotate ACC allowed active subset 0x040 -> 0x080 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x7f, allowed: 7
sys={3950.000000}: select(46): chan_load_avg=40
(bts=0) ACC: rotate ACC allowed active subset 0x080 -> 0x100 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xff, allowed: 8
sys={4000.000000}: select(47): chan_load_avg=25
(bts=0) ACC: update ACC allowed active subset 0x100 -> 0x101 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xfe, allowed: 0 8
sys={4100.000000}: select(48): chan_load_avg=10
(bts=0) ACC: rotate ACC allowed active subset 0x101 -> 0x003 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfc, allowed: 0 1
sys={4200.000000}: select(49): chan_load_avg=25
(bts=0) ACC: rotate ACC allowed active subset 0x003 -> 0x006 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf9, allowed: 1 2
BTS deallocated OK in test_acc_ramp_updown_rotate()
===test_acc_ramp_updown_rotate(50, 49, 0, 100, 10)===
(bts=0) ACC: New ACC allowed subset 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
BTS allocation OK in test_acc_ramp_updown_rotate()
*** Barring one ACC ***
(bts=0) ACC: New ACC allowed subset 0x1ff (active_len=9, ramp_len=10, adm_len=10, perm_len=9, rotation=off)
pcu_info_update(): t2=0x02 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8
(bts=0) ACC: update ACC allowed active subset 0x1ff -> 0x000 (active_len=0, ramp_len=0, adm_len=10, perm_len=9, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
(bts=0) ACC: New ACC allowed subset 0x001 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfe, allowed: 0
sys={100.000000}: select(0): chan_load_avg=0
(bts=0) ACC: rotate ACC allowed active subset 0x001 -> 0x002 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfd, allowed: 1
sys={200.000000}: select(1): chan_load_avg=10
(bts=0) ACC: rotate ACC allowed active subset 0x002 -> 0x004 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfb, allowed: 2
sys={250.000000}: select(2): chan_load_avg=20
(bts=0) ACC: update ACC allowed active subset 0x004 -> 0x00c (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf3, allowed: 2 3
sys={350.000000}: select(3): chan_load_avg=30
(bts=0) ACC: rotate ACC allowed active subset 0x00c -> 0x018 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe7, allowed: 3 4
sys={450.000000}: select(4): chan_load_avg=40
(bts=0) ACC: rotate ACC allowed active subset 0x018 -> 0x030 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xcf, allowed: 4 5
sys={500.000000}: select(5): chan_load_avg=50
(bts=0) ACC: update ACC allowed active subset 0x030 -> 0x020 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xdf, allowed: 5
sys={600.000000}: select(6): chan_load_avg=60
(bts=0) ACC: rotate ACC allowed active subset 0x020 -> 0x040 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xbf, allowed: 6
sys={700.000000}: select(7): chan_load_avg=70
(bts=0) ACC: rotate ACC allowed active subset 0x040 -> 0x080 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x7f, allowed: 7
sys={750.000000}: select(8): chan_load_avg=80
sys={850.000000}: select(9): chan_load_avg=90
(bts=0) ACC: rotate ACC allowed active subset 0x080 -> 0x100 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xff, allowed: 8
sys={950.000000}: select(10): chan_load_avg=100
(bts=0) ACC: rotate ACC allowed active subset 0x100 -> 0x001 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfe, allowed: 0
sys={1000.000000}: select(11): chan_load_avg=90
sys={1100.000000}: select(12): chan_load_avg=80
(bts=0) ACC: rotate ACC allowed active subset 0x001 -> 0x002 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfd, allowed: 1
sys={1200.000000}: select(13): chan_load_avg=70
(bts=0) ACC: rotate ACC allowed active subset 0x002 -> 0x004 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfb, allowed: 2
sys={1250.000000}: select(14): chan_load_avg=60
sys={1350.000000}: select(15): chan_load_avg=50
(bts=0) ACC: rotate ACC allowed active subset 0x004 -> 0x008 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf7, allowed: 3
sys={1450.000000}: select(16): chan_load_avg=40
(bts=0) ACC: rotate ACC allowed active subset 0x008 -> 0x010 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xef, allowed: 4
sys={1500.000000}: select(17): chan_load_avg=30
(bts=0) ACC: update ACC allowed active subset 0x010 -> 0x030 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xcf, allowed: 4 5
sys={1600.000000}: select(18): chan_load_avg=20
(bts=0) ACC: rotate ACC allowed active subset 0x030 -> 0x060 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x9f, allowed: 5 6
sys={1700.000000}: select(19): chan_load_avg=10
(bts=0) ACC: rotate ACC allowed active subset 0x060 -> 0x0c0 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x3f, allowed: 6 7
sys={1750.000000}: select(20): chan_load_avg=0
(bts=0) ACC: update ACC allowed active subset 0x0c0 -> 0x1c0 (active_len=3, ramp_len=3, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x3f, allowed: 6 7 8
sys={1850.000000}: select(21): chan_load_avg=10
(bts=0) ACC: rotate ACC allowed active subset 0x1c0 -> 0x181 (active_len=3, ramp_len=3, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x7e, allowed: 0 7 8
sys={1950.000000}: select(22): chan_load_avg=20
(bts=0) ACC: rotate ACC allowed active subset 0x181 -> 0x103 (active_len=3, ramp_len=3, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xfc, allowed: 0 1 8
sys={2000.000000}: select(23): chan_load_avg=30
(bts=0) ACC: update ACC allowed active subset 0x103 -> 0x107 (active_len=4, ramp_len=4, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xf8, allowed: 0 1 2 8
sys={2100.000000}: select(24): chan_load_avg=40
(bts=0) ACC: rotate ACC allowed active subset 0x107 -> 0x00f (active_len=4, ramp_len=4, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf0, allowed: 0 1 2 3
sys={2200.000000}: select(25): chan_load_avg=50
(bts=0) ACC: rotate ACC allowed active subset 0x00f -> 0x01e (active_len=4, ramp_len=4, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe1, allowed: 1 2 3 4
sys={2250.000000}: select(26): chan_load_avg=60
(bts=0) ACC: update ACC allowed active subset 0x01e -> 0x01c (active_len=3, ramp_len=3, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe3, allowed: 2 3 4
sys={2350.000000}: select(27): chan_load_avg=70
(bts=0) ACC: rotate ACC allowed active subset 0x01c -> 0x038 (active_len=3, ramp_len=3, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xc7, allowed: 3 4 5
sys={2450.000000}: select(28): chan_load_avg=80
(bts=0) ACC: rotate ACC allowed active subset 0x038 -> 0x070 (active_len=3, ramp_len=3, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x8f, allowed: 4 5 6
sys={2500.000000}: select(29): chan_load_avg=90
(bts=0) ACC: update ACC allowed active subset 0x070 -> 0x060 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x9f, allowed: 5 6
sys={2600.000000}: select(30): chan_load_avg=100
(bts=0) ACC: rotate ACC allowed active subset 0x060 -> 0x0c0 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x3f, allowed: 6 7
sys={2700.000000}: select(31): chan_load_avg=90
(bts=0) ACC: rotate ACC allowed active subset 0x0c0 -> 0x180 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x7f, allowed: 7 8
sys={2750.000000}: select(32): chan_load_avg=80
(bts=0) ACC: update ACC allowed active subset 0x180 -> 0x100 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xff, allowed: 8
sys={2850.000000}: select(33): chan_load_avg=70
(bts=0) ACC: rotate ACC allowed active subset 0x100 -> 0x001 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfe, allowed: 0
sys={2950.000000}: select(34): chan_load_avg=60
(bts=0) ACC: rotate ACC allowed active subset 0x001 -> 0x002 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfd, allowed: 1
sys={3000.000000}: select(35): chan_load_avg=50
sys={3100.000000}: select(36): chan_load_avg=40
(bts=0) ACC: rotate ACC allowed active subset 0x002 -> 0x004 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xfb, allowed: 2
sys={3200.000000}: select(37): chan_load_avg=30
(bts=0) ACC: rotate ACC allowed active subset 0x004 -> 0x008 (active_len=1, ramp_len=1, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf7, allowed: 3
sys={3250.000000}: select(38): chan_load_avg=20
(bts=0) ACC: update ACC allowed active subset 0x008 -> 0x018 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe7, allowed: 3 4
sys={3350.000000}: select(39): chan_load_avg=10
(bts=0) ACC: rotate ACC allowed active subset 0x018 -> 0x030 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xcf, allowed: 4 5
sys={3450.000000}: select(40): chan_load_avg=0
(bts=0) ACC: rotate ACC allowed active subset 0x030 -> 0x060 (active_len=2, ramp_len=2, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x9f, allowed: 5 6
sys={3500.000000}: select(41): chan_load_avg=10
(bts=0) ACC: update ACC allowed active subset 0x060 -> 0x0e0 (active_len=3, ramp_len=3, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0x1f, allowed: 5 6 7
sys={3600.000000}: select(42): chan_load_avg=20
(bts=0) ACC: rotate ACC allowed active subset 0x0e0 -> 0x1c0 (active_len=3, ramp_len=3, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x3f, allowed: 6 7 8
sys={3700.000000}: select(43): chan_load_avg=30
(bts=0) ACC: rotate ACC allowed active subset 0x1c0 -> 0x181 (active_len=3, ramp_len=3, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x7e, allowed: 0 7 8
sys={3750.000000}: select(44): chan_load_avg=40
(bts=0) ACC: update ACC allowed active subset 0x181 -> 0x183 (active_len=4, ramp_len=4, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0x7c, allowed: 0 1 7 8
sys={3850.000000}: select(45): chan_load_avg=50
(bts=0) ACC: rotate ACC allowed active subset 0x183 -> 0x107 (active_len=4, ramp_len=4, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x02 t3=0xf8, allowed: 0 1 2 8
sys={3950.000000}: select(46): chan_load_avg=60
(bts=0) ACC: rotate ACC allowed active subset 0x107 -> 0x00f (active_len=4, ramp_len=4, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf0, allowed: 0 1 2 3
sys={4000.000000}: select(47): chan_load_avg=70
(bts=0) ACC: update ACC allowed active subset 0x00f -> 0x00e (active_len=3, ramp_len=3, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xf1, allowed: 1 2 3
sys={4100.000000}: select(48): chan_load_avg=80
(bts=0) ACC: rotate ACC allowed active subset 0x00e -> 0x01c (active_len=3, ramp_len=3, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xe3, allowed: 2 3 4
sys={4200.000000}: select(49): chan_load_avg=90
(bts=0) ACC: rotate ACC allowed active subset 0x01c -> 0x038 (active_len=3, ramp_len=3, adm_len=10, perm_len=9, rotation=on)
pcu_info_update(): t2=0x03 t3=0xc7, allowed: 3 4 5
BTS deallocated OK in test_acc_ramp_updown_rotate()
===test_acc_ramp_updown_rotate(30, 80, 30, 80, 5)===
(bts=0) ACC: New ACC allowed subset 0x3ff (active_len=10, ramp_len=10, adm_len=10, perm_len=10, rotation=off)
BTS allocation OK in test_acc_ramp_updown_rotate()
*** Barring one ACC ***
(bts=0) ACC: New ACC allowed subset 0x1ff (active_len=9, ramp_len=10, adm_len=10, perm_len=9, rotation=off)
pcu_info_update(): t2=0x02 t3=0x00, allowed: 0 1 2 3 4 5 6 7 8
(bts=0) ACC: update ACC allowed active subset 0x1ff -> 0x000 (active_len=0, ramp_len=0, adm_len=10, perm_len=9, rotation=off)
pcu_info_update(): t2=0x03 t3=0xff, allowed:
sys={250.000000}: select(0): chan_load_avg=30
sys={500.000000}: select(1): chan_load_avg=35
sys={750.000000}: select(2): chan_load_avg=40
sys={1000.000000}: select(3): chan_load_avg=45
sys={1250.000000}: select(4): chan_load_avg=50
sys={1500.000000}: select(5): chan_load_avg=55
sys={1750.000000}: select(6): chan_load_avg=60
sys={2000.000000}: select(7): chan_load_avg=65
sys={2250.000000}: select(8): chan_load_avg=70
sys={2500.000000}: select(9): chan_load_avg=75
sys={2750.000000}: select(10): chan_load_avg=80
sys={3000.000000}: select(11): chan_load_avg=75
sys={3250.000000}: select(12): chan_load_avg=70
sys={3500.000000}: select(13): chan_load_avg=65
sys={3750.000000}: select(14): chan_load_avg=60
sys={4000.000000}: select(15): chan_load_avg=55
sys={4250.000000}: select(16): chan_load_avg=50
sys={4500.000000}: select(17): chan_load_avg=45
sys={4750.000000}: select(18): chan_load_avg=40
sys={5000.000000}: select(19): chan_load_avg=35
sys={5250.000000}: select(20): chan_load_avg=30
sys={5500.000000}: select(21): chan_load_avg=35
sys={5750.000000}: select(22): chan_load_avg=40
sys={6000.000000}: select(23): chan_load_avg=45
sys={6250.000000}: select(24): chan_load_avg=50
sys={6500.000000}: select(25): chan_load_avg=55
sys={6750.000000}: select(26): chan_load_avg=60
sys={7000.000000}: select(27): chan_load_avg=65
sys={7250.000000}: select(28): chan_load_avg=70
sys={7500.000000}: select(29): chan_load_avg=75
sys={7750.000000}: select(30): chan_load_avg=80
sys={8000.000000}: select(31): chan_load_avg=75
sys={8250.000000}: select(32): chan_load_avg=70
sys={8500.000000}: select(33): chan_load_avg=65
sys={8750.000000}: select(34): chan_load_avg=60
sys={9000.000000}: select(35): chan_load_avg=55
sys={9250.000000}: select(36): chan_load_avg=50
sys={9500.000000}: select(37): chan_load_avg=45
sys={9750.000000}: select(38): chan_load_avg=40
sys={10000.000000}: select(39): chan_load_avg=35
sys={10250.000000}: select(40): chan_load_avg=30
sys={10500.000000}: select(41): chan_load_avg=35
sys={10750.000000}: select(42): chan_load_avg=40
sys={11000.000000}: select(43): chan_load_avg=45
sys={11250.000000}: select(44): chan_load_avg=50
sys={11500.000000}: select(45): chan_load_avg=55
sys={11750.000000}: select(46): chan_load_avg=60
sys={12000.000000}: select(47): chan_load_avg=65
sys={12250.000000}: select(48): chan_load_avg=70
sys={12500.000000}: select(49): chan_load_avg=75
BTS deallocated OK in test_acc_ramp_updown_rotate()
