# Congestion check: Solving congestion by handover TCH/F -> TCH/H
# Two BTS, one MS in the first congested BTS must handover to
# non-congested TCH/H of second BTS, in order to solve congestion

create-n-bts 2
network
 bts 0
  handover2 min-free-slots tch/f 4
  handover2 min-free-slots tch/h 4
 bts 1
  handover2 min-free-slots tch/f 4
set-ts-use trx 0 0 states * TCH/F - - - - - -
meas-rep lchan 0 0 1 0 rxlev 30 rxqual 0 ta 0 neighbors 30
expect-no-chan
congestion-check
expect-ho from lchan 0 0 1 0 to lchan 1 0 5 0
expect-ts-use trx 0 0 states * - - - - -      - -
expect-ts-use trx 1 0 states * - - - - TCH/H- - -

