# No handover to congested cell
# The better neighbor cell is congested, so no handover is performed.
# After the congestion is over, handover will be performed.

create-n-bts 2
set-ts-use trx 0 0 states * TCH/F - - - - - -
network
 bts 1
  handover2 min-free-slots tch/f 4
  handover2 min-free-slots tch/h 4
meas-rep lchan 0 0 1 0 rxlev 20 rxqual 0 ta 0 neighbors 30
expect-no-chan
network
 bts 1
  handover2 min-free-slots tch/f 3
  handover2 min-free-slots tch/h 3
meas-rep lchan 0 0 1 0 rxlev 20 rxqual 0 ta 0 neighbors 30
expect-ho from lchan 0 0 1 0 to lchan 1 0 1 0
expect-ts-use trx 0 0 states * - - - - - - -
expect-ts-use trx 1 0 states * TCH/F - - - - - -

