# No handover to a cell with no slots available
# If no slot is available, no handover is performed

create-n-bts 2
set-ts-use trx 0 0 states * TCH/F - - - - - -
set-ts-use trx 1 0 states * TCH/F TCH/F TCH/F TCH/F TCH/HH TCH/HH -
meas-rep lchan 0 0 1 0 rxlev 0 rxqual 0 ta 0 neighbors 30
expect-no-chan

