# Congestion check: Balancing over congested cells
# Two cells are congested, but the second cell is less congested.
# Handover is performed to solve the congestion.

create-n-bts 2
network
 handover2 min-free-slots tch/f 4
codec tch/f FR
set-ts-use trx 0 0 states * TCH/F TCH/F TCH/F - - - -
set-ts-use trx 1 0 states * TCH/F - - - - - -
meas-rep lchan * * * * rxlev 30 rxqual 0 ta 0 neighbors 20
meas-rep lchan 0 0 2 0 rxlev 30 rxqual 0 ta 0 neighbors 21
expect-no-chan
congestion-check
expect-ho from lchan 0 0 2 0 to lchan 1 0 2 0
expect-ts-use trx 0 0 states * TCH/F -     TCH/F - - - -
expect-ts-use trx 1 0 states * TCH/F TCH/F -     - - - -

