# Handover to balance congestion
# The current and the better cell are congested, so no handover is
# performed. This is because handover would congest the neighbor cell
# more. After congestion rises in the current cell, the handover is
# performed to balance congestion

create-n-bts 2
create-ms bts 0 TCH/F AMR
expect-ts-use trx 0 0 states * TCH/F - - - - - -
network
 handover2 min-free-slots tch/f 4
 handover2 min-free-slots tch/h 4
meas-rep lchan 0 0 1 0 rxlev 20 rxqual 0 ta 0 neighbors 30
expect-no-chan
set-ts-use trx 0 0 states * TCH/F TCH/F - - - - -
meas-rep lchan 0 0 1 0 rxlev 20 rxqual 0 ta 0 neighbors 30
expect-ho from lchan 0 0 1 0 to lchan 1 0 1 0
expect-ts-use trx 0 0 states * - TCH/F - - - - -
expect-ts-use trx 1 0 states * TCH/F - - - - - -

