=== Transcoding Good Cases ===
== Transcoding test ==
converting l16 -> l16
encoded:
    80 0b 00 01 00 00 00 a0 11 22 33 44 00 00 40 13 
    5a 9e 40 13 00 00 bf ed a5 62 bf ed 00 00 40 13 
    5a 9e 40 13 00 00 bf ed a5 62 bf ed 00 00 40 13 
    5a 9e 40 13 00 00 bf ed a5 62 bf ed 00 00 40 13 
    5a 9e 40 13 00 00 bf ed a5 62 bf ed 00 00 40 13 
    5a 9e 40 13 00 00 bf ed a5 62 bf ed 00 00 40 13 
    5a 9e 40 13 00 00 bf ed a5 62 bf ed 00 00 40 13 
    5a 9e 40 13 00 00 bf ed a5 62 bf ed 00 00 40 13 
    5a 9e 40 13 00 00 bf ed a5 62 bf ed 00 00 40 13 
    5a 9e 40 13 00 00 bf ed a5 62 bf ed 00 00 40 13 
    5a 9e 40 13 00 00 bf ed a5 62 bf ed 00 00 40 13 
    5a 9e 40 13 00 00 bf ed a5 62 bf ed 00 00 40 13 
    5a 9e 40 13 00 00 bf ed a5 62 bf ed 00 00 40 13 
    5a 9e 40 13 00 00 bf ed a5 62 bf ed 00 00 40 13 
    5a 9e 40 13 00 00 bf ed a5 62 bf ed 00 00 40 13 
    5a 9e 40 13 00 00 bf ed a5 62 bf ed 00 00 40 13 
    5a 9e 40 13 00 00 bf ed a5 62 bf ed 00 00 40 13 
    5a 9e 40 13 00 00 bf ed a5 62 bf ed 00 00 40 13 
    5a 9e 40 13 00 00 bf ed a5 62 bf ed 00 00 40 13 
    5a 9e 40 13 00 00 bf ed a5 62 bf ed 00 00 40 13 
    5a 9e 40 13 00 00 bf ed a5 62 bf ed 
counted: 0
== Transcoding test ==
converting l16 -> gsm
encoded:
    80 0b 00 01 00 00 00 a0 11 22 33 44 d4 7c e3 e9 
    62 50 39 f0 f8 b4 68 ea 6c 0e 81 1b 56 2a d5 bc 
    69 9c d1 f0 66 7a ec 49 7a 33 3d 0a de 
counted: 12
== Transcoding test ==
converting l16 -> pcma
encoded:
    80 0b 00 01 00 00 00 a0 11 22 33 44 d5 a5 a3 a5 
    d5 25 23 25 d5 a5 a3 a5 d5 25 23 25 d5 a5 a3 a5 
    d5 25 23 25 d5 a5 a3 a5 d5 25 23 25 d5 a5 a3 a5 
    d5 25 23 25 d5 a5 a3 a5 d5 25 23 25 d5 a5 a3 a5 
    d5 25 23 25 d5 a5 a3 a5 d5 25 23 25 d5 a5 a3 a5 
    d5 25 23 25 d5 a5 a3 a5 d5 25 23 25 d5 a5 a3 a5 
    d5 25 23 25 d5 a5 a3 a5 d5 25 23 25 d5 a5 a3 a5 
    d5 25 23 25 d5 a5 a3 a5 d5 25 23 25 d5 a5 a3 a5 
    d5 25 23 25 d5 a5 a3 a5 d5 25 23 25 d5 a5 a3 a5 
    d5 25 23 25 d5 a5 a3 a5 d5 25 23 25 d5 a5 a3 a5 
    d5 25 23 25 d5 a5 a3 a5 d5 25 23 25 
counted: 12
== Transcoding test ==
converting gsm -> l16
encoded:
    80 03 00 01 00 00 00 a0 11 22 33 44 00 00 54 00 
    59 f0 34 20 c4 c8 b9 f8 e2 18 f1 e8 f2 28 f0 e0 
    46 08 4f 80 2c a0 a9 c8 80 00 c0 58 3f 80 63 c0 
    24 b8 fa b8 f6 88 0b a0 c8 70 a8 b0 c8 c0 3b a8 
    66 a0 2e 38 d1 f8 98 98 aa 18 e8 30 26 a0 37 40 
    37 e8 17 00 ee 50 b7 80 b1 88 de 28 18 40 45 b0 
    4f 48 21 d8 df 78 ae 68 ab 98 d6 b8 18 18 48 90 
    4e 70 27 40 e8 10 b5 b0 ac 80 d4 60 14 50 48 48 
    50 10 2a 00 ec 08 ba 00 af 58 d1 c0 10 60 45 c8 
    54 10 30 78 f1 a8 bb 18 ad 48 ce 30 0a e8 3f 30 
    4f 10 32 18 f6 18 bf 20 ac 30 cd 80 0b d0 43 d8 
    55 e0 34 a0 f5 78 bc 98 ad 98 cd c8 0a 80 40 58 
    51 c0 35 40 f9 60 c1 68 ac c8 cb 38 08 00 40 98 
    51 e0 34 d8 fa 28 c2 f0 ae 40 c7 70 02 d0 3c a8 
    54 78 38 a0 fc 68 c2 08 ad 50 c7 78 01 60 39 c0 
    51 38 3a e8 00 e8 c6 38 ab d8 c4 00 fe 08 39 18 
    50 30 39 50 01 d8 ca 70 b1 80 c4 c8 fc 58 36 40 
    51 d8 3b 08 02 80 c8 58 b0 60 c5 a8 fb d0 33 e8 
    4e 80 3c e0 06 10 cb 90 ae 48 c2 60 f9 58 34 08 
    4d a0 3a a8 06 48 cf 80 b4 60 c3 e8 f7 90 30 18 
    4d a0 3b 98 07 90 cf 18 b4 68 c4 88 
counted: 12
== Transcoding test ==
converting gsm -> gsm
encoded:
    80 03 00 01 00 00 00 a0 11 22 33 44 d4 7c e3 e9 
    62 50 39 f0 f8 b4 68 ea 6c 0e 81 1b 56 2a d5 bc 
    69 9c d1 f0 66 7a ec 49 7a 33 3d 0a de 
counted: 0
== Transcoding test ==
converting gsm -> pcma
encoded:
    80 03 00 01 00 00 00 a0 11 22 33 44 d5 a0 a3 bf 
    38 24 08 19 1e 1b a4 a6 b3 20 2a 3a ba ad b7 60 
    17 92 3e 20 3e b8 ac b2 32 2c 20 02 b6 be be 82 
    04 27 26 35 8d a4 a6 b5 35 21 20 31 8d a7 a6 b6 
    02 27 21 30 81 a7 a1 b0 06 24 21 32 85 a4 a0 bd 
    19 24 21 3d 90 ba a6 bc 16 25 21 3c 92 a5 a0 bf 
    10 25 21 3c 90 a5 a1 bf 6f 3a 21 3f 95 a5 a1 bf 
    62 3b 21 39 f3 bb a0 b9 79 3b 21 39 c3 b9 a1 b8 
    db 39 20 3b 4a b9 a1 b9 c8 3f 26 38 78 be a1 b8 
    f1 3e 26 38 65 bc a6 bb ed 3f 21 3b 6f bf a6 b8 
    ec 3d 27 3b 15 bd a6 b8 eb 3d 27 38 
counted: 12
== Transcoding test ==
converting pcma -> l16
encoded:
    80 08 00 01 00 00 00 a0 11 22 33 44 00 08 42 00 
    5a 00 42 00 00 08 be 00 a6 00 be 00 00 08 42 00 
    5a 00 42 00 00 08 be 00 a6 00 be 00 00 08 42 00 
    5a 00 42 00 00 08 be 00 a6 00 be 00 00 08 42 00 
    5a 00 42 00 00 08 be 00 a6 00 be 00 00 08 42 00 
    5a 00 42 00 00 08 be 00 a6 00 be 00 00 08 42 00 
    5a 00 42 00 00 08 be 00 a6 00 be 00 00 08 42 00 
    5a 00 42 00 00 08 be 00 a6 00 be 00 00 08 42 00 
    5a 00 42 00 00 08 be 00 a6 00 be 00 00 08 42 00 
    5a 00 42 00 00 08 be 00 a6 00 be 00 00 08 42 00 
    5a 00 42 00 00 08 be 00 a6 00 be 00 00 08 42 00 
    5a 00 42 00 00 08 be 00 a6 00 be 00 00 08 42 00 
    5a 00 42 00 00 08 be 00 a6 00 be 00 00 08 42 00 
    5a 00 42 00 00 08 be 00 a6 00 be 00 00 08 42 00 
    5a 00 42 00 00 08 be 00 a6 00 be 00 00 08 42 00 
    5a 00 42 00 00 08 be 00 a6 00 be 00 00 08 42 00 
    5a 00 42 00 00 08 be 00 a6 00 be 00 00 08 42 00 
    5a 00 42 00 00 08 be 00 a6 00 be 00 00 08 42 00 
    5a 00 42 00 00 08 be 00 a6 00 be 00 00 08 42 00 
    5a 00 42 00 00 08 be 00 a6 00 be 00 00 08 42 00 
    5a 00 42 00 00 08 be 00 a6 00 be 00 
counted: 12
== Transcoding test ==
converting pcma -> gsm
encoded:
    80 08 00 01 00 00 00 a0 11 22 33 44 d4 b9 f4 5d 
    d9 50 5a e1 a0 cd 76 ea 52 0e 87 53 ad d4 ea a2 
    0a 63 ca e9 60 79 e2 2a 25 d2 c0 f3 39 
counted: 12
== Transcoding test ==
converting pcma -> pcma
encoded:
    80 08 00 01 00 00 00 a0 11 22 33 44 d5 a5 a3 a5 
    d5 25 23 25 d5 a5 a3 a5 d5 25 23 25 d5 a5 a3 a5 
    d5 25 23 25 d5 a5 a3 a5 d5 25 23 25 d5 a5 a3 a5 
    d5 25 23 25 d5 a5 a3 a5 d5 25 23 25 d5 a5 a3 a5 
    d5 25 23 25 d5 a5 a3 a5 d5 25 23 25 d5 a5 a3 a5 
    d5 25 23 25 d5 a5 a3 a5 d5 25 23 25 d5 a5 a3 a5 
    d5 25 23 25 d5 a5 a3 a5 d5 25 23 25 d5 a5 a3 a5 
    d5 25 23 25 d5 a5 a3 a5 d5 25 23 25 d5 a5 a3 a5 
    d5 25 23 25 d5 a5 a3 a5 d5 25 23 25 d5 a5 a3 a5 
    d5 25 23 25 d5 a5 a3 a5 d5 25 23 25 d5 a5 a3 a5 
    d5 25 23 25 d5 a5 a3 a5 d5 25 23 25 
counted: 0
=== Transcoding Bad Cases ===
Invalid size:
== Transcoding test ==
converting gsm -> pcma
Nothing encoded due: No message of desired type
Invalid data:
== Transcoding test ==
converting gsm -> pcma
Nothing encoded due: No message of desired type
Invalid payload type:
== Transcoding test ==
converting gsm -> pcma
encoded:
    80 08 00 01 00 00 00 a0 11 22 33 44 d5 a0 a3 bf 
    38 24 08 19 1e 1b a4 a6 b3 20 2a 3a ba ad b7 60 
    17 92 3e 20 3e b8 ac b2 32 2c 20 02 b6 be be 82 
    04 27 26 35 8d a4 a6 b5 35 21 20 31 8d a7 a6 b6 
    02 27 21 30 81 a7 a1 b0 06 24 21 32 85 a4 a0 bd 
    19 24 21 3d 90 ba a6 bc 16 25 21 3c 92 a5 a0 bf 
    10 25 21 3c 90 a5 a1 bf 6f 3a 21 3f 95 a5 a1 bf 
    62 3b 21 39 f3 bb a0 b9 79 3b 21 39 c3 b9 a1 b8 
    db 39 20 3b 4a b9 a1 b9 c8 3f 26 38 78 be a1 b8 
    f1 3e 26 38 65 bc a6 bb ed 3f 21 3b 6f bf a6 b8 
    ec 3d 27 3b 15 bd a6 b8 eb 3d 27 38 
counted: 12
=== Repacking ===
== Transcoding test ==
converting pcma -> l16
generating 160 pcma input samples
got 2 l16 output frames (320 octets) count=12
generating 160 pcma input samples
got 2 l16 output frames (320 octets) count=12
generating 160 pcma input samples
got 2 l16 output frames (320 octets) count=12
generating 160 pcma input samples
got 2 l16 output frames (320 octets) count=12
generating 160 pcma input samples
got 2 l16 output frames (320 octets) count=12
generating 160 pcma input samples
got 2 l16 output frames (320 octets) count=12
generating 160 pcma input samples
got 2 l16 output frames (320 octets) count=12
generating 160 pcma input samples
got 2 l16 output frames (320 octets) count=12
generating 160 pcma input samples
got 2 l16 output frames (320 octets) count=12
generating 160 pcma input samples
got 2 l16 output frames (320 octets) count=12
generating 160 pcma input samples
got 2 l16 output frames (320 octets) count=12
generating 160 pcma input samples
got 2 l16 output frames (320 octets) count=12
generating 160 pcma input samples
got 2 l16 output frames (320 octets) count=12
generating 160 pcma input samples
got 2 l16 output frames (320 octets) count=12
generating 160 pcma input samples
got 2 l16 output frames (320 octets) count=12
generating 160 pcma input samples
got 2 l16 output frames (320 octets) count=12
== Transcoding test ==
converting pcma -> pcma
generating 160 pcma input samples
got 2 pcma output frames (160 octets) count=12
generating 160 pcma input samples
got 2 pcma output frames (160 octets) count=12
generating 160 pcma input samples
got 2 pcma output frames (160 octets) count=12
generating 160 pcma input samples
got 2 pcma output frames (160 octets) count=12
generating 160 pcma input samples
got 2 pcma output frames (160 octets) count=12
generating 160 pcma input samples
got 2 pcma output frames (160 octets) count=12
generating 160 pcma input samples
got 2 pcma output frames (160 octets) count=12
generating 160 pcma input samples
got 2 pcma output frames (160 octets) count=12
generating 160 pcma input samples
got 2 pcma output frames (160 octets) count=12
generating 160 pcma input samples
got 2 pcma output frames (160 octets) count=12
generating 160 pcma input samples
got 2 pcma output frames (160 octets) count=12
generating 160 pcma input samples
got 2 pcma output frames (160 octets) count=12
generating 160 pcma input samples
got 2 pcma output frames (160 octets) count=12
generating 160 pcma input samples
got 2 pcma output frames (160 octets) count=12
generating 160 pcma input samples
got 2 pcma output frames (160 octets) count=12
generating 160 pcma input samples
got 2 pcma output frames (160 octets) count=12
== Transcoding test ==
converting pcma -> l16
generating 160 pcma input samples
got 1 l16 output frames (160 octets) count=12
got 1 l16 output frames (160 octets) count=12
generating 160 pcma input samples
got 1 l16 output frames (160 octets) count=12
got 1 l16 output frames (160 octets) count=12
generating 160 pcma input samples
got 1 l16 output frames (160 octets) count=12
got 1 l16 output frames (160 octets) count=12
generating 160 pcma input samples
got 1 l16 output frames (160 octets) count=12
got 1 l16 output frames (160 octets) count=12
generating 160 pcma input samples
got 1 l16 output frames (160 octets) count=12
got 1 l16 output frames (160 octets) count=12
generating 160 pcma input samples
got 1 l16 output frames (160 octets) count=12
got 1 l16 output frames (160 octets) count=12
generating 160 pcma input samples
got 1 l16 output frames (160 octets) count=12
got 1 l16 output frames (160 octets) count=12
generating 160 pcma input samples
got 1 l16 output frames (160 octets) count=12
got 1 l16 output frames (160 octets) count=12
generating 160 pcma input samples
got 1 l16 output frames (160 octets) count=12
got 1 l16 output frames (160 octets) count=12
generating 160 pcma input samples
got 1 l16 output frames (160 octets) count=12
got 1 l16 output frames (160 octets) count=12
generating 160 pcma input samples
got 1 l16 output frames (160 octets) count=12
got 1 l16 output frames (160 octets) count=12
generating 160 pcma input samples
got 1 l16 output frames (160 octets) count=12
got 1 l16 output frames (160 octets) count=12
generating 160 pcma input samples
got 1 l16 output frames (160 octets) count=12
got 1 l16 output frames (160 octets) count=12
generating 160 pcma input samples
got 1 l16 output frames (160 octets) count=12
got 1 l16 output frames (160 octets) count=12
generating 160 pcma input samples
got 1 l16 output frames (160 octets) count=12
got 1 l16 output frames (160 octets) count=12
generating 160 pcma input samples
got 1 l16 output frames (160 octets) count=12
got 1 l16 output frames (160 octets) count=12
== Transcoding test ==
converting pcma -> pcma
generating 160 pcma input samples
got 1 pcma output frames (80 octets) count=12
got 1 pcma output frames (80 octets) count=12
generating 160 pcma input samples
got 1 pcma output frames (80 octets) count=12
got 1 pcma output frames (80 octets) count=12
generating 160 pcma input samples
got 1 pcma output frames (80 octets) count=12
got 1 pcma output frames (80 octets) count=12
generating 160 pcma input samples
got 1 pcma output frames (80 octets) count=12
got 1 pcma output frames (80 octets) count=12
generating 160 pcma input samples
got 1 pcma output frames (80 octets) count=12
got 1 pcma output frames (80 octets) count=12
generating 160 pcma input samples
got 1 pcma output frames (80 octets) count=12
got 1 pcma output frames (80 octets) count=12
generating 160 pcma input samples
got 1 pcma output frames (80 octets) count=12
got 1 pcma output frames (80 octets) count=12
generating 160 pcma input samples
got 1 pcma output frames (80 octets) count=12
got 1 pcma output frames (80 octets) count=12
generating 160 pcma input samples
got 1 pcma output frames (80 octets) count=12
got 1 pcma output frames (80 octets) count=12
generating 160 pcma input samples
got 1 pcma output frames (80 octets) count=12
got 1 pcma output frames (80 octets) count=12
generating 160 pcma input samples
got 1 pcma output frames (80 octets) count=12
got 1 pcma output frames (80 octets) count=12
generating 160 pcma input samples
got 1 pcma output frames (80 octets) count=12
got 1 pcma output frames (80 octets) count=12
generating 160 pcma input samples
got 1 pcma output frames (80 octets) count=12
got 1 pcma output frames (80 octets) count=12
generating 160 pcma input samples
got 1 pcma output frames (80 octets) count=12
got 1 pcma output frames (80 octets) count=12
generating 160 pcma input samples
got 1 pcma output frames (80 octets) count=12
got 1 pcma output frames (80 octets) count=12
generating 160 pcma input samples
got 1 pcma output frames (80 octets) count=12
got 1 pcma output frames (80 octets) count=12
== Transcoding test ==
converting pcma -> l16
generating 160 pcma input samples
generating 160 pcma input samples
got 4 l16 output frames (640 octets) count=12
generating 160 pcma input samples
generating 160 pcma input samples
got 4 l16 output frames (640 octets) count=12
generating 160 pcma input samples
generating 160 pcma input samples
got 4 l16 output frames (640 octets) count=12
generating 160 pcma input samples
generating 160 pcma input samples
got 4 l16 output frames (640 octets) count=12
generating 160 pcma input samples
generating 160 pcma input samples
got 4 l16 output frames (640 octets) count=12
generating 160 pcma input samples
generating 160 pcma input samples
got 4 l16 output frames (640 octets) count=12
generating 160 pcma input samples
generating 160 pcma input samples
got 4 l16 output frames (640 octets) count=12
generating 160 pcma input samples
generating 160 pcma input samples
got 4 l16 output frames (640 octets) count=12
== Transcoding test ==
converting pcma -> pcma
generating 160 pcma input samples
generating 160 pcma input samples
got 4 pcma output frames (320 octets) count=12
generating 160 pcma input samples
generating 160 pcma input samples
got 4 pcma output frames (320 octets) count=12
generating 160 pcma input samples
generating 160 pcma input samples
got 4 pcma output frames (320 octets) count=12
generating 160 pcma input samples
generating 160 pcma input samples
got 4 pcma output frames (320 octets) count=12
generating 160 pcma input samples
generating 160 pcma input samples
got 4 pcma output frames (320 octets) count=12
generating 160 pcma input samples
generating 160 pcma input samples
got 4 pcma output frames (320 octets) count=12
generating 160 pcma input samples
generating 160 pcma input samples
got 4 pcma output frames (320 octets) count=12
generating 160 pcma input samples
generating 160 pcma input samples
got 4 pcma output frames (320 octets) count=12
== Transcoding test ==
converting pcma -> l16
generating 160 pcma input samples
generating 160 pcma input samples
got 3 l16 output frames (480 octets) count=12
generating 160 pcma input samples
generating 160 pcma input samples
got 3 l16 output frames (480 octets) count=12
generating 160 pcma input samples
generating 160 pcma input samples
got 3 l16 output frames (480 octets) count=12
generating 160 pcma input samples
generating 160 pcma input samples
got 3 l16 output frames (480 octets) count=12
generating 160 pcma input samples
generating 160 pcma input samples
got 3 l16 output frames (480 octets) count=12
generating 160 pcma input samples
generating 160 pcma input samples
got 3 l16 output frames (480 octets) count=12
generating 160 pcma input samples
generating 160 pcma input samples
got 3 l16 output frames (480 octets) count=12
generating 160 pcma input samples
generating 160 pcma input samples
got 3 l16 output frames (480 octets) count=12
== Transcoding test ==
converting pcma -> pcma
generating 160 pcma input samples
generating 160 pcma input samples
got 3 pcma output frames (240 octets) count=12
generating 160 pcma input samples
generating 160 pcma input samples
got 3 pcma output frames (240 octets) count=12
generating 160 pcma input samples
generating 160 pcma input samples
got 3 pcma output frames (240 octets) count=12
generating 160 pcma input samples
generating 160 pcma input samples
got 3 pcma output frames (240 octets) count=12
generating 160 pcma input samples
generating 160 pcma input samples
got 3 pcma output frames (240 octets) count=12
generating 160 pcma input samples
generating 160 pcma input samples
got 3 pcma output frames (240 octets) count=12
generating 160 pcma input samples
generating 160 pcma input samples
got 3 pcma output frames (240 octets) count=12
generating 160 pcma input samples
generating 160 pcma input samples
got 3 pcma output frames (240 octets) count=12
== Transcoding test ==
converting pcma -> l16
generating 160 pcma input samples
got 1 l16 output frames (160 octets) count=12
generating 160 pcma input samples
got 1 l16 output frames (160 octets) count=12
got 1 l16 output frames (160 octets) count=12
generating 160 pcma input samples
got 1 l16 output frames (160 octets) count=12
got 1 l16 output frames (160 octets) count=12
generating 160 pcma input samples
got 1 l16 output frames (160 octets) count=12
got 1 l16 output frames (160 octets) count=12
generating 160 pcma input samples
got 1 l16 output frames (160 octets) count=12
got 1 l16 output frames (160 octets) count=12
generating 160 pcma input samples
got 1 l16 output frames (160 octets) count=12
got 1 l16 output frames (160 octets) count=12
generating 160 pcma input samples
got 1 l16 output frames (160 octets) count=12
got 1 l16 output frames (160 octets) count=12
generating 160 pcma input samples
got 1 l16 output frames (160 octets) count=12
got 1 l16 output frames (160 octets) count=12
generating 160 pcma input samples
got 1 l16 output frames (160 octets) count=12
got 1 l16 output frames (160 octets) count=12
generating 160 pcma input samples
got 1 l16 output frames (160 octets) count=12
got 1 l16 output frames (160 octets) count=12
generating 160 pcma input samples
got 1 l16 output frames (160 octets) count=12
got 1 l16 output frames (160 octets) count=12
generating 160 pcma input samples
got 1 l16 output frames (160 octets) count=12
got 1 l16 output frames (160 octets) count=12
generating 160 pcma input samples
got 1 l16 output frames (160 octets) count=12
got 1 l16 output frames (160 octets) count=12
generating 160 pcma input samples
got 1 l16 output frames (160 octets) count=12
got 1 l16 output frames (160 octets) count=12
generating 160 pcma input samples
got 1 l16 output frames (160 octets) count=12
got 1 l16 output frames (160 octets) count=12
generating 160 pcma input samples
got 1 l16 output frames (160 octets) count=12
got 1 l16 output frames (160 octets) count=12
== Transcoding test ==
converting pcma -> pcma
generating 160 pcma input samples
got 1 pcma output frames (80 octets) count=12
generating 160 pcma input samples
got 1 pcma output frames (80 octets) count=12
got 1 pcma output frames (80 octets) count=12
generating 160 pcma input samples
got 1 pcma output frames (80 octets) count=12
got 1 pcma output frames (80 octets) count=12
generating 160 pcma input samples
got 1 pcma output frames (80 octets) count=12
got 1 pcma output frames (80 octets) count=12
generating 160 pcma input samples
got 1 pcma output frames (80 octets) count=12
got 1 pcma output frames (80 octets) count=12
generating 160 pcma input samples
got 1 pcma output frames (80 octets) count=12
got 1 pcma output frames (80 octets) count=12
generating 160 pcma input samples
got 1 pcma output frames (80 octets) count=12
got 1 pcma output frames (80 octets) count=12
generating 160 pcma input samples
got 1 pcma output frames (80 octets) count=12
got 1 pcma output frames (80 octets) count=12
generating 160 pcma input samples
got 1 pcma output frames (80 octets) count=12
got 1 pcma output frames (80 octets) count=12
generating 160 pcma input samples
got 1 pcma output frames (80 octets) count=12
got 1 pcma output frames (80 octets) count=12
generating 160 pcma input samples
got 1 pcma output frames (80 octets) count=12
got 1 pcma output frames (80 octets) count=12
generating 160 pcma input samples
got 1 pcma output frames (80 octets) count=12
got 1 pcma output frames (80 octets) count=12
generating 160 pcma input samples
got 1 pcma output frames (80 octets) count=12
got 1 pcma output frames (80 octets) count=12
generating 160 pcma input samples
got 1 pcma output frames (80 octets) count=12
got 1 pcma output frames (80 octets) count=12
generating 160 pcma input samples
got 1 pcma output frames (80 octets) count=12
got 1 pcma output frames (80 octets) count=12
generating 160 pcma input samples
got 1 pcma output frames (80 octets) count=12
got 1 pcma output frames (80 octets) count=12
Testing Initial L16->GSM, PCMA->GSM
