===== test_umts_authen_geran
- Location Update request causes a GSUP Send Auth Info request to HLR
  MSC <--RAN_GERAN_A-- MS: GSM48_MT_MM_LOC_UPD_REQUEST
  new conn
DREF unknown: MSC conn use + 1 == 1
DRLL Dispatching 04.08 message GSM48_MT_MM_LOC_UPD_REQUEST (0x5:0x8)
DREF unknown: MSC conn use + 1 == 2
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_INIT}: Allocated
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_INIT}: Received Event SUBSCR_CONN_E_START
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_INIT}: state_chg to SUBSCR_CONN_S_NEW
DMM LOCATION UPDATING REQUEST: MI(IMSI)=901700000010650 type=NORMAL
DMM LU/new-LAC: 0/0
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_IDLE}: Allocated
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_IDLE}: is child of Subscr_Conn(901700000010650)
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_IDLE}: rev=R99 net=GERAN Auth (no Ciph)
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_IDLE}: Received Event VLR_ULA_E_UPDATE_LA
DREF VLR subscr unknown usage increases to: 1
DVLR set IMSI on subscriber; IMSI=901700000010650 id=901700000010650
DVLR New subscr, IMSI: 901700000010650
DREF VLR subscr IMSI:901700000010650 usage increases to: 2
DREF VLR subscr IMSI:901700000010650 usage decreases to: 1
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_IDLE}: vlr_loc_upd_node1()
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_IDLE}: state_chg to VLR_ULA_S_WAIT_AUTH
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH}: is child of vlr_lu_fsm(901700000010650)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
DVLR GSUP tx: 08010809710000000156f0
GSUP --> HLR: OSMO_GSUP_MSGT_SEND_AUTH_INFO_REQUEST: 08010809710000000156f0
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_NEEDS_AUTH_WAIT_AI
DMM IMSI:901700000010650: bump: conn still being established (SUBSCR_CONN_S_NEW)
DREF IMSI:901700000010650: MSC conn use - 1 == 1
  lu_result_sent == 0
- from HLR, rx _SEND_AUTH_INFO_RESULT; VLR sends Auth Req to MS
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: 0a010809710000000156f00362201039fa2f4e3d523d8619a73b4f65c3e14d21049b36efdf2208059a4f668f6fbe39231027497388b6cb044648f396aa155b95ef2410f64735036e5871319c679f4742a75ea125108704f5ba55f30000d2ee44b22c8ea9192708e229c19e791f2e4103622010c187a53a5e6b9d573cac7c74451fd46d210485aa31302208d3d50a000bf04f6e23101159ec926a50e98c034a6b7d7c9f418d2410df3a03d9ca5335641efc8e36d76cd20b25101843a645b98d00005b2d666af46c45d927087db47cf7f81e4dc703622010efa9c29a9742148d5c9070348716e1bb210469d5f9fb22083df176f0c29f1a3d2310eb50e770ddcc3060101d2f43b6c2b884241076542abce5ff9345b0e8947f4c6e019c2510f9375e6d41e1000096e7fe4ff1c27e392708706f996719ba609c03622010f023d5a3b24726e0631b64b3840f82532104d570c03f2208ec011be8919883d62310c4e58af4ba43f3bcd904e16984f086d724100593f65e752e5cb7f473862bda05aa0a2510541ff1f077270000c5ea00d658bc7e9a27083fd26072eaa2a04d036220102f8f90c780d6a9c0c53da7ac57b6707e2104b072446f220823f39f9f425ad6e6231065af0527fda95b0dc5ae4aa515cdf32f2410537c3b35a3b13b08d08eeb28098f45cc25104bf4e564f75300009bc796706bc6574427080edb0eadbea94ac2
DVLR GSUP rx 511: 0a010809710000000156f00362201039fa2f4e3d523d8619a73b4f65c3e14d21049b36efdf2208059a4f668f6fbe39231027497388b6cb044648f396aa155b95ef2410f64735036e5871319c679f4742a75ea125108704f5ba55f30000d2ee44b22c8ea9192708e229c19e791f2e4103622010c187a53a5e6b9d573cac7c74451fd46d210485aa31302208d3d50a000bf04f6e23101159ec926a50e98c034a6b7d7c9f418d2410df3a03d9ca5335641efc8e36d76cd20b25101843a645b98d00005b2d666af46c45d927087db47cf7f81e4dc703622010efa9c29a9742148d5c9070348716e1bb210469d5f9fb22083df176f0c29f1a3d2310eb50e770ddcc3060101d2f43b6c2b884241076542abce5ff9345b0e8947f4c6e019c2510f9375e6d41e1000096e7fe4ff1c27e392708706f996719ba609c03622010f023d5a3b24726e0631b64b3840f82532104d570c03f2208ec011be8919883d62310c4e58af4ba43f3bcd904e16984f086d724100593f65e752e5cb7f473862bda05aa0a2510541ff1f077270000c5ea00d658bc7e9a27083fd26072eaa2a04d036220102f8f90c780d6a9c0c53da7ac57b6707e2104b072446f220823f39f9f425ad6e6231065af0527fda95b0dc5ae4aa515cdf32f2410537c3b35a3b13b08d08eeb28098f45cc25104bf4e564f75300009bc796706bc6574427080edb0eadbea94ac2
DREF VLR subscr IMSI:901700000010650 usage increases to: 2
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: Received Event VLR_AUTH_E_HLR_SAI_ACK
DVLR SUBSCR(IMSI:901700000010650) Received 5 auth tuples
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=0
- sending UMTS Auth Request for IMSI:901700000010650: tuple use_count=1 key_seq=0 auth_types=0x3 and...
- ...rand=39fa2f4e3d523d8619a73b4f65c3e14d
- ...autn=8704f5ba55f30000d2ee44b22c8ea919
- ...expecting res=e229c19e791f2e41
DREF VLR subscr IMSI:901700000010650 usage decreases to: 1
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: vlr_gsupc_read_cb() returns 0
  auth_request_sent == 1
  lu_result_sent == 0
- MS sends Authen Response, VLR accepts and sends GSUP LU Req to HLR
  MSC <--RAN_GERAN_A-- MS: GSM48_MT_MM_AUTH_RESP
DREF IMSI:901700000010650: MSC conn use + 1 == 2
DRLL Dispatching 04.08 message GSM48_MT_MM_AUTH_RESP (0x5:0x14)
DMM IMSI:901700000010650: MM R99 AUTHENTICATION RESPONSE (res = e229c19e791f2e41)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(IMSI:901700000010650) received res: e2 29 c1 9e 79 1f 2e 41 
DVLR SUBSCR(IMSI:901700000010650) AUTH established UMTS security context
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP}: Authentication terminating with result VLR_AUTH_RES_PASSED
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_AUTHENTICATED}: Removing from parent vlr_lu_fsm(901700000010650)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_AUTHENTICATED}: Freeing instance
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_AUTH}: Received Event VLR_ULA_E_AUTH_RES
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_post_auth()
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_post_ciph()
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_node_4()
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_AUTH}: state_chg to VLR_ULA_S_WAIT_HLR_UPD
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_INIT}: Allocated
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_INIT}: is child of vlr_lu_fsm(901700000010650)
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_INIT}: Received Event UPD_HLR_VLR_E_START
DVLR GSUP tx: 04010809710000000156f0
GSUP --> HLR: OSMO_GSUP_MSGT_UPDATE_LOCATION_REQUEST: 04010809710000000156f0
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_INIT}: state_chg to UPD_HLR_VLR_S_WAIT_FOR_DATA
DMM IMSI:901700000010650: bump: conn still being established (SUBSCR_CONN_S_NEW)
DREF IMSI:901700000010650: MSC conn use - 1 == 1
  gsup_tx_confirmed == 1
  lu_result_sent == 0
- HLR sends _INSERT_DATA_REQUEST, VLR responds with _INSERT_DATA_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: 10010809710000000156f00804032443f2
DVLR GSUP rx 17: 10010809710000000156f00804032443f2
DREF VLR subscr IMSI:901700000010650 usage increases to: 2
DVLR IMSI:901700000010650 has MSISDN:42342
DVLR GSUP tx: 12010809710000000156f0
GSUP --> HLR: OSMO_GSUP_MSGT_INSERT_DATA_RESULT: 12010809710000000156f0
DREF VLR subscr MSISDN:42342 usage decreases to: 1
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: vlr_gsupc_read_cb() returns 0
  lu_result_sent == 0
- HLR also sends GSUP _UPDATE_LOCATION_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: 06010809710000000156f0
DVLR GSUP rx 11: 06010809710000000156f0
DREF VLR subscr MSISDN:42342 usage increases to: 2
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_HLR_LU_RES
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_WAIT_FOR_DATA}: Received Event UPD_HLR_VLR_E_UPD_LOC_ACK
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_WAIT_FOR_DATA}: state_chg to UPD_HLR_VLR_S_DONE
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_DONE}: Removing from parent vlr_lu_fsm(901700000010650)
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_DONE}: Freeing instance
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_DONE}: Deallocated
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_UPD_HLR_COMPL
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_HLR_UPD}: state_chg to VLR_ULA_S_WAIT_LU_COMPL
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_INIT}: Allocated
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_INIT}: is child of vlr_lu_fsm(901700000010650)
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_INIT}: Received Event LU_COMPL_VLR_E_START
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_INIT}: state_chg to LU_COMPL_VLR_S_WAIT_SUB_PRES
DVLR sub_pres_vlr_fsm(901700000010650){SUB_PRES_VLR_S_INIT}: Allocated
DVLR sub_pres_vlr_fsm(901700000010650){SUB_PRES_VLR_S_INIT}: is child of lu_compl_vlr_fsm(901700000010650)
DVLR sub_pres_vlr_fsm(901700000010650){SUB_PRES_VLR_S_INIT}: Received Event SUB_PRES_VLR_E_START
DVLR sub_pres_vlr_fsm(901700000010650){SUB_PRES_VLR_S_INIT}: state_chg to SUB_PRES_VLR_S_DONE
DVLR sub_pres_vlr_fsm(901700000010650){SUB_PRES_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR sub_pres_vlr_fsm(901700000010650){SUB_PRES_VLR_S_DONE}: Removing from parent lu_compl_vlr_fsm(901700000010650)
DVLR sub_pres_vlr_fsm(901700000010650){SUB_PRES_VLR_S_DONE}: Freeing instance
DVLR sub_pres_vlr_fsm(901700000010650){SUB_PRES_VLR_S_DONE}: Deallocated
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_WAIT_SUB_PRES}: Received Event LU_COMPL_VLR_E_SUB_PRES_COMPL
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_WAIT_SUB_PRES}: lu_compl_vlr_new_tmsi()
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_WAIT_SUB_PRES}: state_chg to LU_COMPL_VLR_S_WAIT_TMSI_CNF
- sending LU Accept for MSISDN:42342, with TMSI 0x03020100
DREF VLR subscr MSISDN:42342 usage decreases to: 1
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: vlr_gsupc_read_cb() returns 0
  lu_result_sent == 1
- a LU Accept with a new TMSI was sent, waiting for TMSI Realloc Compl
  llist_count(&net->subscr_conns) == 1
msc_subscr_conn_is_accepted() == false
  requests shall be thwarted
DRLL Dispatching 04.08 message GSM48_MT_CC_SETUP (0x3:0x5)
DRLL subscr MSISDN:42342: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DRLL Dispatching 04.08 message unknown 0x33 (0x5:0x33)
DRLL subscr MSISDN:42342: Message not permitted for initial conn: unknown 0x33
DRLL Dispatching 04.08 message GSM48_MT_RR_SYSINFO_1 (0x6:0x19)
DRLL subscr MSISDN:42342: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DRLL Dispatching 04.08 message GSM48_PDISC_SMS:0x01 (0x9:0x1)
DRLL subscr MSISDN:42342: Message not permitted for initial conn: GSM48_PDISC_SMS:0x01
- even though the TMSI is not acked, we can already find the subscr with it
DREF VLR subscr MSISDN:42342 usage increases to: 2
  vsub != NULL == 1
  strcmp(vsub->imsi, imsi) == 0
  vsub->tmsi_new == 0x03020100
  vsub->tmsi == 0xffffffff
DREF VLR subscr MSISDN:42342 usage decreases to: 1
- MS sends TMSI Realloc Complete
  MSC <--RAN_GERAN_A-- MS: GSM48_MT_MM_TMSI_REALL_COMPL
DREF MSISDN:42342: MSC conn use + 1 == 2
DRLL Dispatching 04.08 message GSM48_MT_MM_TMSI_REALL_COMPL (0x5:0x1b)
DMM TMSI Reallocation Completed. Subscriber: MSISDN:42342
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_NEW_TMSI_ACK
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_WAIT_TMSI_CNF}: Received Event LU_COMPL_VLR_E_NEW_TMSI_ACK
DREF VLR subscr MSISDN:42342 usage increases to: 2
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_WAIT_TMSI_CNF}: state_chg to LU_COMPL_VLR_S_DONE
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_LU_COMPL_SUCCESS
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_DONE}: Removing from parent vlr_lu_fsm(901700000010650)
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_DONE}: Freeing instance
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_DONE}: Deallocated
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_LU_COMPL}: state_chg to VLR_ULA_S_DONE
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_NEW}: Received Event SUBSCR_CONN_E_ACCEPTED
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_NEW}: SUBSCR_CONN_FROM_LU
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_NEW}: state_chg to SUBSCR_CONN_S_ACCEPTED
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: Received Event SUBSCR_CONN_E_BUMP
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: bump: releasing conn
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: state_chg to SUBSCR_CONN_S_RELEASED
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_DONE}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_DONE}: Removing from parent Subscr_Conn(901700000010650)
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_DONE}: fsm_lu_cleanup called with cause OSMO_FSM_TERM_PARENT
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_DONE}: Freeing instance
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_DONE}: Deallocated
DMM msc_subscr_conn_close(vsub=MSISDN:42342, cause=2): no conn fsm, releasing directly without release event.
DREF MSISDN:42342: MSC conn use - 1 == 1
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_RELEASED}: Freeing instance
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_RELEASED}: Deallocated
DREF MSISDN:42342: MSC conn use - 1 == 0
DRLL subscr MSISDN:42342: Freeing subscriber connection
DREF VLR subscr MSISDN:42342 usage decreases to: 1
- LU was successful, and the conn has already been closed
  llist_count(&net->subscr_conns) == 0
---
- after a while, a new conn sends a CM Service Request. VLR responds with Auth Req, 2nd auth vector
  MSC <--RAN_GERAN_A-- MS: GSM48_MT_MM_CM_SERV_REQ
  new conn
DREF unknown: MSC conn use + 1 == 1
DRLL Dispatching 04.08 message GSM48_MT_MM_CM_SERV_REQ (0x5:0x24)
DMM <- CM SERVICE REQUEST serv_type=0x08 MI(IMSI)=901700000010650
DREF unknown: MSC conn use + 1 == 2
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_INIT}: Allocated
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_INIT}: Received Event SUBSCR_CONN_E_START
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_INIT}: state_chg to SUBSCR_CONN_S_NEW
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_INIT}: Allocated
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_INIT}: is child of Subscr_Conn(901700000010650)
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_INIT}: rev=R99 net=GERAN Auth (no Ciph)
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_INIT}: Received Event PR_ARQ_E_START
DREF VLR subscr MSISDN:42342 usage increases to: 2
DREF VLR subscr MSISDN:42342 usage increases to: 3
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_INIT}: proc_arq_vlr_fn_post_imsi()
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_INIT}: state_chg to PR_ARQ_S_WAIT_AUTH
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH}: is child of Process_Access_Request_VLR(901700000010650)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=1
- sending UMTS Auth Request for MSISDN:42342: tuple use_count=1 key_seq=1 auth_types=0x3 and...
- ...rand=c187a53a5e6b9d573cac7c74451fd46d
- ...autn=1843a645b98d00005b2d666af46c45d9
- ...expecting res=7db47cf7f81e4dc7
DREF VLR subscr MSISDN:42342 usage decreases to: 2
DMM MSISDN:42342: bump: conn still being established (SUBSCR_CONN_S_NEW)
DREF MSISDN:42342: MSC conn use - 1 == 1
  cm_service_result_sent == 0
  auth_request_sent == 1
- needs auth, not yet accepted
msc_subscr_conn_is_accepted() == false
  requests shall be thwarted
DRLL Dispatching 04.08 message GSM48_MT_CC_SETUP (0x3:0x5)
DRLL subscr MSISDN:42342: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DRLL Dispatching 04.08 message unknown 0x33 (0x5:0x33)
DRLL subscr MSISDN:42342: Message not permitted for initial conn: unknown 0x33
DRLL Dispatching 04.08 message GSM48_MT_RR_SYSINFO_1 (0x6:0x19)
DRLL subscr MSISDN:42342: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DRLL Dispatching 04.08 message GSM48_PDISC_SMS:0x01 (0x9:0x1)
DRLL subscr MSISDN:42342: Message not permitted for initial conn: GSM48_PDISC_SMS:0x01
- MS sends Authen Response, VLR accepts with a CM Service Accept
  MSC <--RAN_GERAN_A-- MS: GSM48_MT_MM_AUTH_RESP
DREF MSISDN:42342: MSC conn use + 1 == 2
DRLL Dispatching 04.08 message GSM48_MT_MM_AUTH_RESP (0x5:0x14)
DMM MSISDN:42342: MM R99 AUTHENTICATION RESPONSE (res = 7db47cf7f81e4dc7)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(MSISDN:42342) received res: 7d b4 7c f7 f8 1e 4d c7 
DVLR SUBSCR(MSISDN:42342) AUTH established UMTS security context
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP}: Authentication terminating with result VLR_AUTH_RES_PASSED
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_AUTHENTICATED}: Removing from parent Process_Access_Request_VLR(901700000010650)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_AUTHENTICATED}: Freeing instance
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_AUTH}: Received Event PR_ARQ_E_AUTH_RES
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_AUTH}: got VLR_AUTH_RES_PASSED
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_node2()
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_node2_post_ciph()
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_node2_post_vlr()
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_post_pres()
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_post_trace()
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_post_imei()
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_AUTH}: proc_arq_fsm_done(VLR_PR_ARQ_RES_PASSED)
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_AUTH}: state_chg to PR_ARQ_S_DONE
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_DONE}: Process Access Request result: VLR_PR_ARQ_RES_PASSED
- sending CM Service Accept for MSISDN:42342
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_NEW}: Received Event SUBSCR_CONN_E_ACCEPTED
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_NEW}: SUBSCR_CONN_FROM_CM_SERVICE_REQ
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_NEW}: state_chg to SUBSCR_CONN_S_ACCEPTED
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: received_cm_service_request = true
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: Received Event SUBSCR_CONN_E_BUMP
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: bump: still awaiting first request after a CM Service Request
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: Received Event SUBSCR_CONN_E_BUMP
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: bump: still awaiting first request after a CM Service Request
DREF MSISDN:42342: MSC conn use - 1 == 1
  cm_service_result_sent == 1
- a USSD request is serviced
  expecting USSD:
  Your extension is 42342
  MSC <--RAN_GERAN_A-- MS: GSM48_PDISC_NC_SS:0x3b
DREF MSISDN:42342: MSC conn use + 1 == 2
DRLL Dispatching 04.08 message GSM48_PDISC_NC_SS:0x3b (0xb:0x3b)
DMM MSISDN:42342: rx msg GSM48_PDISC_NC_SS:0x3b: received_cm_service_request changes to false
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: Received Event SUBSCR_CONN_E_COMMUNICATING
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: state_chg to SUBSCR_CONN_S_COMMUNICATING
DMM USSD: Own number requested
DMM MSISDN:42342: MSISDN = 42342
DMSC msc_tx 43 bytes to MSISDN:42342 via RAN_GERAN_A
- DTAP --RAN_GERAN_A--> MS: GSM48_PDISC_NC_SS:0x2a: 8b2a1c27a225020100302002013b301b04010f0416d9775d0e2ae3e965f73cfd7683d273104d36a3c91a0d
- DTAP matches expected message
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_COMMUNICATING}: Received Event SUBSCR_CONN_E_BUMP
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_COMMUNICATING}: bump: releasing conn
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_COMMUNICATING}: state_chg to SUBSCR_CONN_S_RELEASED
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_DONE}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_DONE}: Removing from parent Subscr_Conn(901700000010650)
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_DONE}: Freeing instance
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_DONE}: Deallocated
DMM msc_subscr_conn_close(vsub=MSISDN:42342, cause=2): no conn fsm, releasing directly without release event.
DREF MSISDN:42342: MSC conn use - 1 == 1
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_RELEASED}: Freeing instance
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_RELEASED}: Deallocated
DREF MSISDN:42342: MSC conn use - 1 == 0
DRLL subscr MSISDN:42342: Freeing subscriber connection
DREF VLR subscr MSISDN:42342 usage decreases to: 1
- all requests serviced, conn has been released
  llist_count(&net->subscr_conns) == 0
---
- an SMS is sent, MS is paged
DREF VLR subscr MSISDN:42342 usage increases to: 2
  llist_count(&vsub->cs.requests) == 0
DREF VLR subscr MSISDN:42342 usage increases to: 3
DMM Subscriber MSISDN:42342 not paged yet, start paging.
  RAN_GERAN_A sends out paging request to IMSI 901700000010650, TMSI 0x03020100, LAC 0
  strcmp(paging_expecting_imsi, imsi) == 0
DREF VLR subscr MSISDN:42342 usage increases to: 4
  llist_count(&vsub->cs.requests) == 1
DREF VLR subscr MSISDN:42342 usage decreases to: 3
  paging_sent == 1
  paging_stopped == 0
- the subscriber and its pending request should remain
DREF VLR subscr MSISDN:42342 usage increases to: 4
  llist_count(&vsub->cs.requests) == 1
DREF VLR subscr MSISDN:42342 usage decreases to: 3
- MS replies with Paging Response, and VLR sends Auth Request with third key
  MSC <--RAN_GERAN_A-- MS: GSM48_MT_RR_PAG_RESP
  new conn
DREF unknown: MSC conn use + 1 == 1
DRLL Dispatching 04.08 message GSM48_MT_RR_PAG_RESP (0x6:0x27)
DRR PAGING RESPONSE: MI(IMSI)=901700000010650
DREF unknown: MSC conn use + 1 == 2
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_INIT}: Allocated
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_INIT}: Received Event SUBSCR_CONN_E_START
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_INIT}: state_chg to SUBSCR_CONN_S_NEW
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_INIT}: Allocated
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_INIT}: is child of Subscr_Conn(901700000010650)
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_INIT}: rev=R99 net=GERAN Auth (no Ciph)
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_INIT}: Received Event PR_ARQ_E_START
DREF VLR subscr MSISDN:42342 usage increases to: 4
DREF VLR subscr MSISDN:42342 usage increases to: 5
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_INIT}: proc_arq_vlr_fn_post_imsi()
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_INIT}: state_chg to PR_ARQ_S_WAIT_AUTH
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH}: is child of Process_Access_Request_VLR(901700000010650)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=2
- sending UMTS Auth Request for MSISDN:42342: tuple use_count=1 key_seq=2 auth_types=0x3 and...
- ...rand=efa9c29a9742148d5c9070348716e1bb
- ...autn=f9375e6d41e1000096e7fe4ff1c27e39
- ...expecting res=706f996719ba609c
DREF VLR subscr MSISDN:42342 usage decreases to: 4
DMM MSISDN:42342: bump: conn still being established (SUBSCR_CONN_S_NEW)
DREF MSISDN:42342: MSC conn use - 1 == 1
  auth_request_sent == 1
- needs auth, not yet accepted
msc_subscr_conn_is_accepted() == false
  requests shall be thwarted
DRLL Dispatching 04.08 message GSM48_MT_CC_SETUP (0x3:0x5)
DRLL subscr MSISDN:42342: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DRLL Dispatching 04.08 message unknown 0x33 (0x5:0x33)
DRLL subscr MSISDN:42342: Message not permitted for initial conn: unknown 0x33
DRLL Dispatching 04.08 message GSM48_MT_RR_SYSINFO_1 (0x6:0x19)
DRLL subscr MSISDN:42342: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DRLL Dispatching 04.08 message GSM48_PDISC_SMS:0x01 (0x9:0x1)
DRLL subscr MSISDN:42342: Message not permitted for initial conn: GSM48_PDISC_SMS:0x01
- MS sends Authen Response, VLR accepts and sends pending SMS
  MSC <--RAN_GERAN_A-- MS: GSM48_MT_MM_AUTH_RESP
DREF MSISDN:42342: MSC conn use + 1 == 2
DRLL Dispatching 04.08 message GSM48_MT_MM_AUTH_RESP (0x5:0x14)
DMM MSISDN:42342: MM R99 AUTHENTICATION RESPONSE (res = 706f996719ba609c)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(MSISDN:42342) received res: 70 6f 99 67 19 ba 60 9c 
DVLR SUBSCR(MSISDN:42342) AUTH established UMTS security context
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP}: Authentication terminating with result VLR_AUTH_RES_PASSED
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_AUTHENTICATED}: Removing from parent Process_Access_Request_VLR(901700000010650)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_AUTHENTICATED}: Freeing instance
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_AUTH}: Received Event PR_ARQ_E_AUTH_RES
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_AUTH}: got VLR_AUTH_RES_PASSED
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_node2()
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_node2_post_ciph()
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_node2_post_vlr()
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_post_pres()
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_post_trace()
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_post_imei()
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_AUTH}: proc_arq_fsm_done(VLR_PR_ARQ_RES_PASSED)
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_AUTH}: state_chg to PR_ARQ_S_DONE
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_DONE}: Process Access Request result: VLR_PR_ARQ_RES_PASSED
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_NEW}: Received Event SUBSCR_CONN_E_ACCEPTED
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_NEW}: SUBSCR_CONN_FROM_PAGING_RESP
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_NEW}: state_chg to SUBSCR_CONN_S_ACCEPTED
DPAG Paging success for MSISDN:42342 (event=0)
DPAG Calling paging cbfn.
DREF VLR subscr MSISDN:42342 usage increases to: 5
DREF MSISDN:42342: MSC conn use + 1 == 3
DMSC msc_tx 91 bytes to MSISDN:42342 via RAN_GERAN_A
- DTAP --RAN_GERAN_A--> MS: GSM48_PDISC_SMS:0x01: 09015801000791447758100650004c0005802443f2000007101000000000445079da1e1ee7416937485e9ea7c965373d1d6683c270383b3d0ed3d36ff71c949e83c22072799e9687c5ec32a81d96afcbf4b4fb0c7ac3e9e9b7db05
- DTAP matches expected message
DREF VLR subscr MSISDN:42342 usage decreases to: 4
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: Received Event SUBSCR_CONN_E_BUMP
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: bump: connection still has active transaction: GSM48_PDISC_SMS
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: Received Event SUBSCR_CONN_E_BUMP
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: bump: connection still has active transaction: GSM48_PDISC_SMS
DREF MSISDN:42342: MSC conn use - 1 == 2
  dtap_tx_confirmed == 1
  paging_stopped == 1
- SMS was delivered, no requests pending for subscr
DREF VLR subscr MSISDN:42342 usage increases to: 5
  llist_count(&vsub->cs.requests) == 0
DREF VLR subscr MSISDN:42342 usage decreases to: 4
- conn is still open to wait for SMS ack dance
  llist_count(&net->subscr_conns) == 1
- MS replies with CP-ACK for received SMS
  MSC <--RAN_GERAN_A-- MS: GSM48_PDISC_SMS:0x04
DREF MSISDN:42342: MSC conn use + 1 == 3
DRLL Dispatching 04.08 message GSM48_PDISC_SMS:0x04 (0x9:0x4)
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: Received Event SUBSCR_CONN_E_COMMUNICATING
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: state_chg to SUBSCR_CONN_S_COMMUNICATING
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_COMMUNICATING}: Received Event SUBSCR_CONN_E_BUMP
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_COMMUNICATING}: bump: connection still has active transaction: GSM48_PDISC_SMS
DREF MSISDN:42342: MSC conn use - 1 == 2
  llist_count(&net->subscr_conns) == 1
- MS also sends RP-ACK, MSC in turn sends CP-ACK for that
  MSC <--RAN_GERAN_A-- MS: GSM48_PDISC_SMS:0x01
DREF MSISDN:42342: MSC conn use + 1 == 3
DRLL Dispatching 04.08 message GSM48_PDISC_SMS:0x01 (0x9:0x1)
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_COMMUNICATING}: Received Event SUBSCR_CONN_E_COMMUNICATING
DMSC msc_tx 2 bytes to MSISDN:42342 via RAN_GERAN_A
- DTAP --RAN_GERAN_A--> MS: GSM48_PDISC_SMS:0x04: 0904
- DTAP matches expected message
DREF VLR subscr MSISDN:42342 usage decreases to: 3
DREF VLR subscr MSISDN:42342 usage decreases to: 2
DREF MSISDN:42342: MSC conn use - 1 == 2
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_COMMUNICATING}: Received Event SUBSCR_CONN_E_BUMP
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_COMMUNICATING}: bump: releasing conn
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_COMMUNICATING}: state_chg to SUBSCR_CONN_S_RELEASED
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_DONE}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_DONE}: Removing from parent Subscr_Conn(901700000010650)
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_DONE}: Freeing instance
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_DONE}: Deallocated
DMM msc_subscr_conn_close(vsub=MSISDN:42342, cause=2): no conn fsm, releasing directly without release event.
DREF MSISDN:42342: MSC conn use - 1 == 1
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_RELEASED}: Freeing instance
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_RELEASED}: Deallocated
DREF MSISDN:42342: MSC conn use - 1 == 0
DRLL subscr MSISDN:42342: Freeing subscriber connection
DREF VLR subscr MSISDN:42342 usage decreases to: 1
  dtap_tx_confirmed == 1
- SMS is done, conn is gone
  llist_count(&net->subscr_conns) == 0
---
- subscriber detaches
  MSC <--RAN_GERAN_A-- MS: GSM48_MT_MM_IMSI_DETACH_IND
  new conn
DREF unknown: MSC conn use + 1 == 1
DRLL Dispatching 04.08 message GSM48_MT_MM_IMSI_DETACH_IND (0x5:0x1)
DMM IMSI DETACH INDICATION: MI(IMSI)=901700000010650
DREF VLR subscr MSISDN:42342 usage increases to: 2
DMM IMSI DETACH for MSISDN:42342
DREF VLR subscr MSISDN:42342 usage decreases to: 1
DREF VLR subscr MSISDN:42342 usage decreases to: 0
DREF freeing VLR subscr MSISDN:42342
DMM msc_subscr_conn_close(vsub=unknown, cause=0): no conn fsm, releasing directly without release event.
DREF unknown: MSC conn use - 1 == 0
DRLL Freeing subscriber connection with NULL subscriber
  llist_count(&net->subscr_conns) == 0
===== test_umts_authen_geran: SUCCESS

full talloc report on 'msgb' (total      0 bytes in   1 blocks)
talloc_total_blocks(tall_bsc_ctx) == 9

===== test_umts_authen_utran
- Location Update request causes a GSUP Send Auth Info request to HLR
  MSC <--RAN_UTRAN_IU-- MS: GSM48_MT_MM_LOC_UPD_REQUEST
  new conn
DREF unknown: MSC conn use + 1 == 1
DRLL Dispatching 04.08 message GSM48_MT_MM_LOC_UPD_REQUEST (0x5:0x8)
DREF unknown: MSC conn use + 1 == 2
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_INIT}: Allocated
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_INIT}: Received Event SUBSCR_CONN_E_START
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_INIT}: state_chg to SUBSCR_CONN_S_NEW
DMM LOCATION UPDATING REQUEST: MI(IMSI)=901700000010650 type=NORMAL
DMM LU/new-LAC: 0/0
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_IDLE}: Allocated
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_IDLE}: is child of Subscr_Conn(901700000010650)
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_IDLE}: rev=R99 net=UTRAN Auth+Ciph
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_IDLE}: Received Event VLR_ULA_E_UPDATE_LA
DREF VLR subscr unknown usage increases to: 1
DVLR set IMSI on subscriber; IMSI=901700000010650 id=901700000010650
DVLR New subscr, IMSI: 901700000010650
DREF VLR subscr IMSI:901700000010650 usage increases to: 2
DREF VLR subscr IMSI:901700000010650 usage decreases to: 1
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_IDLE}: vlr_loc_upd_node1()
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_IDLE}: state_chg to VLR_ULA_S_WAIT_AUTH
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH}: is child of vlr_lu_fsm(901700000010650)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
DVLR GSUP tx: 08010809710000000156f0
GSUP --> HLR: OSMO_GSUP_MSGT_SEND_AUTH_INFO_REQUEST: 08010809710000000156f0
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_NEEDS_AUTH_WAIT_AI
DMM IMSI:901700000010650: bump: conn still being established (SUBSCR_CONN_S_NEW)
DREF IMSI:901700000010650: MSC conn use - 1 == 1
  lu_result_sent == 0
- from HLR, rx _SEND_AUTH_INFO_RESULT; VLR sends Auth Req to MS
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: 0a010809710000000156f00362201039fa2f4e3d523d8619a73b4f65c3e14d21049b36efdf2208059a4f668f6fbe39231027497388b6cb044648f396aa155b95ef2410f64735036e5871319c679f4742a75ea125108704f5ba55f30000d2ee44b22c8ea9192708e229c19e791f2e4103622010c187a53a5e6b9d573cac7c74451fd46d210485aa31302208d3d50a000bf04f6e23101159ec926a50e98c034a6b7d7c9f418d2410df3a03d9ca5335641efc8e36d76cd20b25101843a645b98d00005b2d666af46c45d927087db47cf7f81e4dc703622010efa9c29a9742148d5c9070348716e1bb210469d5f9fb22083df176f0c29f1a3d2310eb50e770ddcc3060101d2f43b6c2b884241076542abce5ff9345b0e8947f4c6e019c2510f9375e6d41e1000096e7fe4ff1c27e392708706f996719ba609c03622010f023d5a3b24726e0631b64b3840f82532104d570c03f2208ec011be8919883d62310c4e58af4ba43f3bcd904e16984f086d724100593f65e752e5cb7f473862bda05aa0a2510541ff1f077270000c5ea00d658bc7e9a27083fd26072eaa2a04d036220102f8f90c780d6a9c0c53da7ac57b6707e2104b072446f220823f39f9f425ad6e6231065af0527fda95b0dc5ae4aa515cdf32f2410537c3b35a3b13b08d08eeb28098f45cc25104bf4e564f75300009bc796706bc6574427080edb0eadbea94ac2
DVLR GSUP rx 511: 0a010809710000000156f00362201039fa2f4e3d523d8619a73b4f65c3e14d21049b36efdf2208059a4f668f6fbe39231027497388b6cb044648f396aa155b95ef2410f64735036e5871319c679f4742a75ea125108704f5ba55f30000d2ee44b22c8ea9192708e229c19e791f2e4103622010c187a53a5e6b9d573cac7c74451fd46d210485aa31302208d3d50a000bf04f6e23101159ec926a50e98c034a6b7d7c9f418d2410df3a03d9ca5335641efc8e36d76cd20b25101843a645b98d00005b2d666af46c45d927087db47cf7f81e4dc703622010efa9c29a9742148d5c9070348716e1bb210469d5f9fb22083df176f0c29f1a3d2310eb50e770ddcc3060101d2f43b6c2b884241076542abce5ff9345b0e8947f4c6e019c2510f9375e6d41e1000096e7fe4ff1c27e392708706f996719ba609c03622010f023d5a3b24726e0631b64b3840f82532104d570c03f2208ec011be8919883d62310c4e58af4ba43f3bcd904e16984f086d724100593f65e752e5cb7f473862bda05aa0a2510541ff1f077270000c5ea00d658bc7e9a27083fd26072eaa2a04d036220102f8f90c780d6a9c0c53da7ac57b6707e2104b072446f220823f39f9f425ad6e6231065af0527fda95b0dc5ae4aa515cdf32f2410537c3b35a3b13b08d08eeb28098f45cc25104bf4e564f75300009bc796706bc6574427080edb0eadbea94ac2
DREF VLR subscr IMSI:901700000010650 usage increases to: 2
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: Received Event VLR_AUTH_E_HLR_SAI_ACK
DVLR SUBSCR(IMSI:901700000010650) Received 5 auth tuples
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=0
- sending UMTS Auth Request for IMSI:901700000010650: tuple use_count=1 key_seq=0 auth_types=0x3 and...
- ...rand=39fa2f4e3d523d8619a73b4f65c3e14d
- ...autn=8704f5ba55f30000d2ee44b22c8ea919
- ...expecting res=e229c19e791f2e41
DREF VLR subscr IMSI:901700000010650 usage decreases to: 1
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: vlr_gsupc_read_cb() returns 0
  auth_request_sent == 1
  lu_result_sent == 0
- MS sends Authen Response, VLR accepts and sends SecurityModeControl
  MSC <--RAN_UTRAN_IU-- MS: GSM48_MT_MM_AUTH_RESP
DREF IMSI:901700000010650: MSC conn use + 1 == 2
DRLL Dispatching 04.08 message GSM48_MT_MM_AUTH_RESP (0x5:0x14)
DMM IMSI:901700000010650: MM R99 AUTHENTICATION RESPONSE (res = e229c19e791f2e41)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(IMSI:901700000010650) received res: e2 29 c1 9e 79 1f 2e 41 
DVLR SUBSCR(IMSI:901700000010650) AUTH established UMTS security context
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP}: Authentication terminating with result VLR_AUTH_RES_PASSED
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_AUTHENTICATED}: Removing from parent vlr_lu_fsm(901700000010650)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_AUTHENTICATED}: Freeing instance
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_AUTH}: Received Event VLR_ULA_E_AUTH_RES
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_post_auth()
- sending SecurityModeControl for IMSI:901700000010650
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_AUTH}: state_chg to VLR_ULA_S_WAIT_CIPH
DMM IMSI:901700000010650: bump: conn still being established (SUBSCR_CONN_S_NEW)
DREF IMSI:901700000010650: MSC conn use - 1 == 1
  cipher_mode_cmd_sent == 1
  lu_result_sent == 0
- MS sends SecurityModeControl acceptance, VLR accepts and sends GSUP LU Req to HLR
DMM <- SECURITY MODE COMPLETE IMSI:901700000010650
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_CIPH}: Received Event VLR_ULA_E_CIPH_RES
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_CIPH}: vlr_loc_upd_post_ciph()
DIUCS IMSI:901700000010650: tx CommonID 901700000010650
- Iu Common ID --RAN_UTRAN_IU--> MS (IMSI=901700000010650)
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_CIPH}: vlr_loc_upd_node_4()
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_CIPH}: state_chg to VLR_ULA_S_WAIT_HLR_UPD
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_INIT}: Allocated
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_INIT}: is child of vlr_lu_fsm(901700000010650)
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_INIT}: Received Event UPD_HLR_VLR_E_START
DVLR GSUP tx: 04010809710000000156f0
GSUP --> HLR: OSMO_GSUP_MSGT_UPDATE_LOCATION_REQUEST: 04010809710000000156f0
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_INIT}: state_chg to UPD_HLR_VLR_S_WAIT_FOR_DATA
  gsup_tx_confirmed == 1
  lu_result_sent == 0
- HLR sends _INSERT_DATA_REQUEST, VLR responds with _INSERT_DATA_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: 10010809710000000156f00804032443f2
DVLR GSUP rx 17: 10010809710000000156f00804032443f2
DREF VLR subscr IMSI:901700000010650 usage increases to: 2
DVLR IMSI:901700000010650 has MSISDN:42342
DVLR GSUP tx: 12010809710000000156f0
GSUP --> HLR: OSMO_GSUP_MSGT_INSERT_DATA_RESULT: 12010809710000000156f0
DREF VLR subscr MSISDN:42342 usage decreases to: 1
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: vlr_gsupc_read_cb() returns 0
  lu_result_sent == 0
- HLR also sends GSUP _UPDATE_LOCATION_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: 06010809710000000156f0
DVLR GSUP rx 11: 06010809710000000156f0
DREF VLR subscr MSISDN:42342 usage increases to: 2
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_HLR_LU_RES
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_WAIT_FOR_DATA}: Received Event UPD_HLR_VLR_E_UPD_LOC_ACK
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_WAIT_FOR_DATA}: state_chg to UPD_HLR_VLR_S_DONE
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_DONE}: Removing from parent vlr_lu_fsm(901700000010650)
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_DONE}: Freeing instance
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_DONE}: Deallocated
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_UPD_HLR_COMPL
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_HLR_UPD}: state_chg to VLR_ULA_S_WAIT_LU_COMPL
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_INIT}: Allocated
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_INIT}: is child of vlr_lu_fsm(901700000010650)
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_INIT}: Received Event LU_COMPL_VLR_E_START
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_INIT}: state_chg to LU_COMPL_VLR_S_WAIT_SUB_PRES
DVLR sub_pres_vlr_fsm(901700000010650){SUB_PRES_VLR_S_INIT}: Allocated
DVLR sub_pres_vlr_fsm(901700000010650){SUB_PRES_VLR_S_INIT}: is child of lu_compl_vlr_fsm(901700000010650)
DVLR sub_pres_vlr_fsm(901700000010650){SUB_PRES_VLR_S_INIT}: Received Event SUB_PRES_VLR_E_START
DVLR sub_pres_vlr_fsm(901700000010650){SUB_PRES_VLR_S_INIT}: state_chg to SUB_PRES_VLR_S_DONE
DVLR sub_pres_vlr_fsm(901700000010650){SUB_PRES_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR sub_pres_vlr_fsm(901700000010650){SUB_PRES_VLR_S_DONE}: Removing from parent lu_compl_vlr_fsm(901700000010650)
DVLR sub_pres_vlr_fsm(901700000010650){SUB_PRES_VLR_S_DONE}: Freeing instance
DVLR sub_pres_vlr_fsm(901700000010650){SUB_PRES_VLR_S_DONE}: Deallocated
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_WAIT_SUB_PRES}: Received Event LU_COMPL_VLR_E_SUB_PRES_COMPL
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_WAIT_SUB_PRES}: lu_compl_vlr_new_tmsi()
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_WAIT_SUB_PRES}: state_chg to LU_COMPL_VLR_S_WAIT_TMSI_CNF
- sending LU Accept for MSISDN:42342, with TMSI 0x03020100
DREF VLR subscr MSISDN:42342 usage decreases to: 1
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: vlr_gsupc_read_cb() returns 0
  lu_result_sent == 1
- a LU Accept with a new TMSI was sent, waiting for TMSI Realloc Compl
  llist_count(&net->subscr_conns) == 1
msc_subscr_conn_is_accepted() == false
  requests shall be thwarted
DRLL Dispatching 04.08 message GSM48_MT_CC_SETUP (0x3:0x5)
DRLL subscr MSISDN:42342: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DRLL Dispatching 04.08 message unknown 0x33 (0x5:0x33)
DRLL subscr MSISDN:42342: Message not permitted for initial conn: unknown 0x33
DRLL Dispatching 04.08 message GSM48_MT_RR_SYSINFO_1 (0x6:0x19)
DRLL subscr MSISDN:42342: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DRLL Dispatching 04.08 message GSM48_PDISC_SMS:0x01 (0x9:0x1)
DRLL subscr MSISDN:42342: Message not permitted for initial conn: GSM48_PDISC_SMS:0x01
- even though the TMSI is not acked, we can already find the subscr with it
DREF VLR subscr MSISDN:42342 usage increases to: 2
  vsub != NULL == 1
  strcmp(vsub->imsi, imsi) == 0
  vsub->tmsi_new == 0x03020100
  vsub->tmsi == 0xffffffff
DREF VLR subscr MSISDN:42342 usage decreases to: 1
- MS sends TMSI Realloc Complete
  MSC <--RAN_UTRAN_IU-- MS: GSM48_MT_MM_TMSI_REALL_COMPL
DREF MSISDN:42342: MSC conn use + 1 == 2
DRLL Dispatching 04.08 message GSM48_MT_MM_TMSI_REALL_COMPL (0x5:0x1b)
DMM TMSI Reallocation Completed. Subscriber: MSISDN:42342
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_NEW_TMSI_ACK
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_WAIT_TMSI_CNF}: Received Event LU_COMPL_VLR_E_NEW_TMSI_ACK
DREF VLR subscr MSISDN:42342 usage increases to: 2
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_WAIT_TMSI_CNF}: state_chg to LU_COMPL_VLR_S_DONE
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_LU_COMPL_SUCCESS
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_DONE}: Removing from parent vlr_lu_fsm(901700000010650)
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_DONE}: Freeing instance
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_DONE}: Deallocated
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_LU_COMPL}: state_chg to VLR_ULA_S_DONE
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_NEW}: Received Event SUBSCR_CONN_E_ACCEPTED
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_NEW}: SUBSCR_CONN_FROM_LU
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_NEW}: state_chg to SUBSCR_CONN_S_ACCEPTED
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: Received Event SUBSCR_CONN_E_BUMP
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: bump: releasing conn
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: state_chg to SUBSCR_CONN_S_RELEASED
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_DONE}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_DONE}: Removing from parent Subscr_Conn(901700000010650)
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_DONE}: fsm_lu_cleanup called with cause OSMO_FSM_TERM_PARENT
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_DONE}: Freeing instance
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_DONE}: Deallocated
DMM msc_subscr_conn_close(vsub=MSISDN:42342, cause=2): no conn fsm, releasing directly without release event.
- Iu Release --RAN_UTRAN_IU--> MS
DREF MSISDN:42342: MSC conn use - 1 == 1
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_RELEASED}: Freeing instance
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_RELEASED}: Deallocated
DREF MSISDN:42342: MSC conn use - 1 == 0
DRLL subscr MSISDN:42342: Freeing subscriber connection
DREF VLR subscr MSISDN:42342 usage decreases to: 1
- LU was successful, and the conn has already been closed
  llist_count(&net->subscr_conns) == 0
---
- after a while, a new conn sends a CM Service Request. VLR responds with Auth Req, 2nd auth vector
  MSC <--RAN_UTRAN_IU-- MS: GSM48_MT_MM_CM_SERV_REQ
  new conn
DREF unknown: MSC conn use + 1 == 1
DRLL Dispatching 04.08 message GSM48_MT_MM_CM_SERV_REQ (0x5:0x24)
DMM <- CM SERVICE REQUEST serv_type=0x08 MI(IMSI)=901700000010650
DREF unknown: MSC conn use + 1 == 2
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_INIT}: Allocated
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_INIT}: Received Event SUBSCR_CONN_E_START
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_INIT}: state_chg to SUBSCR_CONN_S_NEW
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_INIT}: Allocated
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_INIT}: is child of Subscr_Conn(901700000010650)
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_INIT}: rev=R99 net=UTRAN Auth+Ciph
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_INIT}: Received Event PR_ARQ_E_START
DREF VLR subscr MSISDN:42342 usage increases to: 2
DREF VLR subscr MSISDN:42342 usage increases to: 3
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_INIT}: proc_arq_vlr_fn_post_imsi()
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_INIT}: state_chg to PR_ARQ_S_WAIT_AUTH
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH}: is child of Process_Access_Request_VLR(901700000010650)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=1
- sending UMTS Auth Request for MSISDN:42342: tuple use_count=1 key_seq=1 auth_types=0x3 and...
- ...rand=c187a53a5e6b9d573cac7c74451fd46d
- ...autn=1843a645b98d00005b2d666af46c45d9
- ...expecting res=7db47cf7f81e4dc7
DREF VLR subscr MSISDN:42342 usage decreases to: 2
DMM MSISDN:42342: bump: conn still being established (SUBSCR_CONN_S_NEW)
DREF MSISDN:42342: MSC conn use - 1 == 1
  cm_service_result_sent == 0
  auth_request_sent == 1
- needs auth, not yet accepted
msc_subscr_conn_is_accepted() == false
  requests shall be thwarted
DRLL Dispatching 04.08 message GSM48_MT_CC_SETUP (0x3:0x5)
DRLL subscr MSISDN:42342: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DRLL Dispatching 04.08 message unknown 0x33 (0x5:0x33)
DRLL subscr MSISDN:42342: Message not permitted for initial conn: unknown 0x33
DRLL Dispatching 04.08 message GSM48_MT_RR_SYSINFO_1 (0x6:0x19)
DRLL subscr MSISDN:42342: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DRLL Dispatching 04.08 message GSM48_PDISC_SMS:0x01 (0x9:0x1)
DRLL subscr MSISDN:42342: Message not permitted for initial conn: GSM48_PDISC_SMS:0x01
- MS sends Authen Response, VLR accepts and sends SecurityModeControl
  MSC <--RAN_UTRAN_IU-- MS: GSM48_MT_MM_AUTH_RESP
DREF MSISDN:42342: MSC conn use + 1 == 2
DRLL Dispatching 04.08 message GSM48_MT_MM_AUTH_RESP (0x5:0x14)
DMM MSISDN:42342: MM R99 AUTHENTICATION RESPONSE (res = 7db47cf7f81e4dc7)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(MSISDN:42342) received res: 7d b4 7c f7 f8 1e 4d c7 
DVLR SUBSCR(MSISDN:42342) AUTH established UMTS security context
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP}: Authentication terminating with result VLR_AUTH_RES_PASSED
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_AUTHENTICATED}: Removing from parent Process_Access_Request_VLR(901700000010650)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_AUTHENTICATED}: Freeing instance
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_AUTH}: Received Event PR_ARQ_E_AUTH_RES
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_AUTH}: got VLR_AUTH_RES_PASSED
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_node2()
- sending SecurityModeControl for MSISDN:42342
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_AUTH}: state_chg to PR_ARQ_S_WAIT_CIPH
DMM MSISDN:42342: bump: conn still being established (SUBSCR_CONN_S_NEW)
DREF MSISDN:42342: MSC conn use - 1 == 1
  cipher_mode_cmd_sent == 1
  cm_service_result_sent == 0
- MS sends SecurityModeControl acceptance, VLR accepts; above Ciphering is an implicit CM Service Accept
DMM <- SECURITY MODE COMPLETE MSISDN:42342
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_CIPH}: Received Event PR_ARQ_E_CIPH_RES
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_node2_post_ciph()
DIUCS MSISDN:42342: tx CommonID 901700000010650
- Iu Common ID --RAN_UTRAN_IU--> MS (IMSI=901700000010650)
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_node2_post_vlr()
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_post_pres()
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_post_trace()
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_post_imei()
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_CIPH}: proc_arq_fsm_done(VLR_PR_ARQ_RES_PASSED)
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_CIPH}: state_chg to PR_ARQ_S_DONE
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_DONE}: Process Access Request result: VLR_PR_ARQ_RES_PASSED
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_NEW}: Received Event SUBSCR_CONN_E_ACCEPTED
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_NEW}: SUBSCR_CONN_FROM_CM_SERVICE_REQ
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_NEW}: state_chg to SUBSCR_CONN_S_ACCEPTED
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: received_cm_service_request = true
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: Received Event SUBSCR_CONN_E_BUMP
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: bump: still awaiting first request after a CM Service Request
  cm_service_result_sent == 0
- a USSD request is serviced
  expecting USSD:
  Your extension is 42342
  MSC <--RAN_UTRAN_IU-- MS: GSM48_PDISC_NC_SS:0x3b
DREF MSISDN:42342: MSC conn use + 1 == 2
DRLL Dispatching 04.08 message GSM48_PDISC_NC_SS:0x3b (0xb:0x3b)
DMM MSISDN:42342: rx msg GSM48_PDISC_NC_SS:0x3b: received_cm_service_request changes to false
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: Received Event SUBSCR_CONN_E_COMMUNICATING
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: state_chg to SUBSCR_CONN_S_COMMUNICATING
DMM USSD: Own number requested
DMM MSISDN:42342: MSISDN = 42342
DMSC msc_tx 43 bytes to MSISDN:42342 via RAN_UTRAN_IU
- DTAP --RAN_UTRAN_IU--> MS: GSM48_PDISC_NC_SS:0x2a: 8b2a1c27a225020100302002013b301b04010f0416d9775d0e2ae3e965f73cfd7683d273104d36a3c91a0d
- DTAP matches expected message
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_COMMUNICATING}: Received Event SUBSCR_CONN_E_BUMP
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_COMMUNICATING}: bump: releasing conn
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_COMMUNICATING}: state_chg to SUBSCR_CONN_S_RELEASED
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_DONE}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_DONE}: Removing from parent Subscr_Conn(901700000010650)
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_DONE}: Freeing instance
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_DONE}: Deallocated
DMM msc_subscr_conn_close(vsub=MSISDN:42342, cause=2): no conn fsm, releasing directly without release event.
- Iu Release --RAN_UTRAN_IU--> MS
DREF MSISDN:42342: MSC conn use - 1 == 1
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_RELEASED}: Freeing instance
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_RELEASED}: Deallocated
DREF MSISDN:42342: MSC conn use - 1 == 0
DRLL subscr MSISDN:42342: Freeing subscriber connection
DREF VLR subscr MSISDN:42342 usage decreases to: 1
- all requests serviced, conn has been released
  llist_count(&net->subscr_conns) == 0
---
- an SMS is sent, MS is paged
DREF VLR subscr MSISDN:42342 usage increases to: 2
  llist_count(&vsub->cs.requests) == 0
DREF VLR subscr MSISDN:42342 usage increases to: 3
DMM Subscriber MSISDN:42342 not paged yet, start paging.
  RAN_UTRAN_IU sends out paging request to IMSI 901700000010650, TMSI 0x03020100, LAC 0
  strcmp(paging_expecting_imsi, imsi) == 0
DREF VLR subscr MSISDN:42342 usage increases to: 4
  llist_count(&vsub->cs.requests) == 1
DREF VLR subscr MSISDN:42342 usage decreases to: 3
  paging_sent == 1
  paging_stopped == 0
- the subscriber and its pending request should remain
DREF VLR subscr MSISDN:42342 usage increases to: 4
  llist_count(&vsub->cs.requests) == 1
DREF VLR subscr MSISDN:42342 usage decreases to: 3
- MS replies with Paging Response, and VLR sends Auth Request with third key
  MSC <--RAN_UTRAN_IU-- MS: GSM48_MT_RR_PAG_RESP
  new conn
DREF unknown: MSC conn use + 1 == 1
DRLL Dispatching 04.08 message GSM48_MT_RR_PAG_RESP (0x6:0x27)
DRR PAGING RESPONSE: MI(IMSI)=901700000010650
DREF unknown: MSC conn use + 1 == 2
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_INIT}: Allocated
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_INIT}: Received Event SUBSCR_CONN_E_START
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_INIT}: state_chg to SUBSCR_CONN_S_NEW
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_INIT}: Allocated
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_INIT}: is child of Subscr_Conn(901700000010650)
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_INIT}: rev=R99 net=UTRAN Auth+Ciph
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_INIT}: Received Event PR_ARQ_E_START
DREF VLR subscr MSISDN:42342 usage increases to: 4
DREF VLR subscr MSISDN:42342 usage increases to: 5
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_INIT}: proc_arq_vlr_fn_post_imsi()
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_INIT}: state_chg to PR_ARQ_S_WAIT_AUTH
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH}: is child of Process_Access_Request_VLR(901700000010650)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=2
- sending UMTS Auth Request for MSISDN:42342: tuple use_count=1 key_seq=2 auth_types=0x3 and...
- ...rand=efa9c29a9742148d5c9070348716e1bb
- ...autn=f9375e6d41e1000096e7fe4ff1c27e39
- ...expecting res=706f996719ba609c
DREF VLR subscr MSISDN:42342 usage decreases to: 4
DMM MSISDN:42342: bump: conn still being established (SUBSCR_CONN_S_NEW)
DREF MSISDN:42342: MSC conn use - 1 == 1
  auth_request_sent == 1
- needs auth, not yet accepted
msc_subscr_conn_is_accepted() == false
  requests shall be thwarted
DRLL Dispatching 04.08 message GSM48_MT_CC_SETUP (0x3:0x5)
DRLL subscr MSISDN:42342: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DRLL Dispatching 04.08 message unknown 0x33 (0x5:0x33)
DRLL subscr MSISDN:42342: Message not permitted for initial conn: unknown 0x33
DRLL Dispatching 04.08 message GSM48_MT_RR_SYSINFO_1 (0x6:0x19)
DRLL subscr MSISDN:42342: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DRLL Dispatching 04.08 message GSM48_PDISC_SMS:0x01 (0x9:0x1)
DRLL subscr MSISDN:42342: Message not permitted for initial conn: GSM48_PDISC_SMS:0x01
- MS sends Authen Response, VLR accepts and sends SecurityModeControl
  MSC <--RAN_UTRAN_IU-- MS: GSM48_MT_MM_AUTH_RESP
DREF MSISDN:42342: MSC conn use + 1 == 2
DRLL Dispatching 04.08 message GSM48_MT_MM_AUTH_RESP (0x5:0x14)
DMM MSISDN:42342: MM R99 AUTHENTICATION RESPONSE (res = 706f996719ba609c)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(MSISDN:42342) received res: 70 6f 99 67 19 ba 60 9c 
DVLR SUBSCR(MSISDN:42342) AUTH established UMTS security context
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP}: Authentication terminating with result VLR_AUTH_RES_PASSED
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_AUTHENTICATED}: Removing from parent Process_Access_Request_VLR(901700000010650)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_AUTHENTICATED}: Freeing instance
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_AUTH}: Received Event PR_ARQ_E_AUTH_RES
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_AUTH}: got VLR_AUTH_RES_PASSED
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_node2()
- sending SecurityModeControl for MSISDN:42342
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_AUTH}: state_chg to PR_ARQ_S_WAIT_CIPH
DMM MSISDN:42342: bump: conn still being established (SUBSCR_CONN_S_NEW)
DREF MSISDN:42342: MSC conn use - 1 == 1
  cipher_mode_cmd_sent == 1
  paging_stopped == 0
- MS sends SecurityModeControl acceptance, VLR accepts and sends SMS
DMM <- SECURITY MODE COMPLETE MSISDN:42342
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_CIPH}: Received Event PR_ARQ_E_CIPH_RES
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_node2_post_ciph()
DIUCS MSISDN:42342: tx CommonID 901700000010650
- Iu Common ID --RAN_UTRAN_IU--> MS (IMSI=901700000010650)
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_node2_post_vlr()
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_post_pres()
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_post_trace()
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_post_imei()
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_CIPH}: proc_arq_fsm_done(VLR_PR_ARQ_RES_PASSED)
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_WAIT_CIPH}: state_chg to PR_ARQ_S_DONE
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_DONE}: Process Access Request result: VLR_PR_ARQ_RES_PASSED
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_NEW}: Received Event SUBSCR_CONN_E_ACCEPTED
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_NEW}: SUBSCR_CONN_FROM_PAGING_RESP
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_NEW}: state_chg to SUBSCR_CONN_S_ACCEPTED
DPAG Paging success for MSISDN:42342 (event=0)
DPAG Calling paging cbfn.
DREF VLR subscr MSISDN:42342 usage increases to: 5
DREF MSISDN:42342: MSC conn use + 1 == 2
DMSC msc_tx 91 bytes to MSISDN:42342 via RAN_UTRAN_IU
- DTAP --RAN_UTRAN_IU--> MS: GSM48_PDISC_SMS:0x01: 09015801000791447758100650004c0005802443f2000007101000000000445079da1e1ee7416937485e9ea7c965373d1d6683c270383b3d0ed3d36ff71c949e83c22072799e9687c5ec32a81d96afcbf4b4fb0c7ac3e9e9b7db05
- DTAP matches expected message
DREF VLR subscr MSISDN:42342 usage decreases to: 4
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: Received Event SUBSCR_CONN_E_BUMP
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: bump: connection still has active transaction: GSM48_PDISC_SMS
  paging_stopped == 1
- SMS was delivered, no requests pending for subscr
DREF VLR subscr MSISDN:42342 usage increases to: 5
  llist_count(&vsub->cs.requests) == 0
DREF VLR subscr MSISDN:42342 usage decreases to: 4
- conn is still open to wait for SMS ack dance
  llist_count(&net->subscr_conns) == 1
- MS replies with CP-ACK for received SMS
  MSC <--RAN_UTRAN_IU-- MS: GSM48_PDISC_SMS:0x04
DREF MSISDN:42342: MSC conn use + 1 == 3
DRLL Dispatching 04.08 message GSM48_PDISC_SMS:0x04 (0x9:0x4)
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: Received Event SUBSCR_CONN_E_COMMUNICATING
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: state_chg to SUBSCR_CONN_S_COMMUNICATING
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_COMMUNICATING}: Received Event SUBSCR_CONN_E_BUMP
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_COMMUNICATING}: bump: connection still has active transaction: GSM48_PDISC_SMS
DREF MSISDN:42342: MSC conn use - 1 == 2
  llist_count(&net->subscr_conns) == 1
- MS also sends RP-ACK, MSC in turn sends CP-ACK for that
  MSC <--RAN_UTRAN_IU-- MS: GSM48_PDISC_SMS:0x01
DREF MSISDN:42342: MSC conn use + 1 == 3
DRLL Dispatching 04.08 message GSM48_PDISC_SMS:0x01 (0x9:0x1)
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_COMMUNICATING}: Received Event SUBSCR_CONN_E_COMMUNICATING
DMSC msc_tx 2 bytes to MSISDN:42342 via RAN_UTRAN_IU
- DTAP --RAN_UTRAN_IU--> MS: GSM48_PDISC_SMS:0x04: 0904
- DTAP matches expected message
DREF VLR subscr MSISDN:42342 usage decreases to: 3
DREF VLR subscr MSISDN:42342 usage decreases to: 2
DREF MSISDN:42342: MSC conn use - 1 == 2
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_COMMUNICATING}: Received Event SUBSCR_CONN_E_BUMP
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_COMMUNICATING}: bump: releasing conn
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_COMMUNICATING}: state_chg to SUBSCR_CONN_S_RELEASED
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_DONE}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_DONE}: Removing from parent Subscr_Conn(901700000010650)
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_DONE}: Freeing instance
DVLR Process_Access_Request_VLR(901700000010650){PR_ARQ_S_DONE}: Deallocated
DMM msc_subscr_conn_close(vsub=MSISDN:42342, cause=2): no conn fsm, releasing directly without release event.
- Iu Release --RAN_UTRAN_IU--> MS
DREF MSISDN:42342: MSC conn use - 1 == 1
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_RELEASED}: Freeing instance
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_RELEASED}: Deallocated
DREF MSISDN:42342: MSC conn use - 1 == 0
DRLL subscr MSISDN:42342: Freeing subscriber connection
DREF VLR subscr MSISDN:42342 usage decreases to: 1
  dtap_tx_confirmed == 1
- SMS is done, conn is gone
  llist_count(&net->subscr_conns) == 0
---
- subscriber detaches
  MSC <--RAN_UTRAN_IU-- MS: GSM48_MT_MM_IMSI_DETACH_IND
  new conn
DREF unknown: MSC conn use + 1 == 1
DRLL Dispatching 04.08 message GSM48_MT_MM_IMSI_DETACH_IND (0x5:0x1)
DMM IMSI DETACH INDICATION: MI(IMSI)=901700000010650
DREF VLR subscr MSISDN:42342 usage increases to: 2
DMM IMSI DETACH for MSISDN:42342
DREF VLR subscr MSISDN:42342 usage decreases to: 1
DREF VLR subscr MSISDN:42342 usage decreases to: 0
DREF freeing VLR subscr MSISDN:42342
DMM msc_subscr_conn_close(vsub=unknown, cause=0): no conn fsm, releasing directly without release event.
- Iu Release --RAN_UTRAN_IU--> MS
DREF unknown: MSC conn use - 1 == 0
DRLL Freeing subscriber connection with NULL subscriber
  llist_count(&net->subscr_conns) == 0
===== test_umts_authen_utran: SUCCESS

full talloc report on 'msgb' (total      0 bytes in   1 blocks)
talloc_total_blocks(tall_bsc_ctx) == 9

===== test_umts_authen_resync_geran
- Location Update request causes a GSUP Send Auth Info request to HLR
  MSC <--RAN_GERAN_A-- MS: GSM48_MT_MM_LOC_UPD_REQUEST
  new conn
DREF unknown: MSC conn use + 1 == 1
DRLL Dispatching 04.08 message GSM48_MT_MM_LOC_UPD_REQUEST (0x5:0x8)
DREF unknown: MSC conn use + 1 == 2
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_INIT}: Allocated
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_INIT}: Received Event SUBSCR_CONN_E_START
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_INIT}: state_chg to SUBSCR_CONN_S_NEW
DMM LOCATION UPDATING REQUEST: MI(IMSI)=901700000010650 type=NORMAL
DMM LU/new-LAC: 0/0
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_IDLE}: Allocated
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_IDLE}: is child of Subscr_Conn(901700000010650)
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_IDLE}: rev=R99 net=GERAN Auth (no Ciph)
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_IDLE}: Received Event VLR_ULA_E_UPDATE_LA
DREF VLR subscr unknown usage increases to: 1
DVLR set IMSI on subscriber; IMSI=901700000010650 id=901700000010650
DVLR New subscr, IMSI: 901700000010650
DREF VLR subscr IMSI:901700000010650 usage increases to: 2
DREF VLR subscr IMSI:901700000010650 usage decreases to: 1
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_IDLE}: vlr_loc_upd_node1()
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_IDLE}: state_chg to VLR_ULA_S_WAIT_AUTH
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH}: is child of vlr_lu_fsm(901700000010650)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
DVLR GSUP tx: 08010809710000000156f0
GSUP --> HLR: OSMO_GSUP_MSGT_SEND_AUTH_INFO_REQUEST: 08010809710000000156f0
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_NEEDS_AUTH_WAIT_AI
DMM IMSI:901700000010650: bump: conn still being established (SUBSCR_CONN_S_NEW)
DREF IMSI:901700000010650: MSC conn use - 1 == 1
  lu_result_sent == 0
- from HLR, rx _SEND_AUTH_INFO_RESULT; VLR sends Auth Req to MS
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: 0a010809710000000156f00362201039fa2f4e3d523d8619a73b4f65c3e14d21049b36efdf2208059a4f668f6fbe39231027497388b6cb044648f396aa155b95ef2410f64735036e5871319c679f4742a75ea125108704f5ba55f30000d2ee44b22c8ea9192708e229c19e791f2e41
DVLR GSUP rx 111: 0a010809710000000156f00362201039fa2f4e3d523d8619a73b4f65c3e14d21049b36efdf2208059a4f668f6fbe39231027497388b6cb044648f396aa155b95ef2410f64735036e5871319c679f4742a75ea125108704f5ba55f30000d2ee44b22c8ea9192708e229c19e791f2e41
DREF VLR subscr IMSI:901700000010650 usage increases to: 2
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: Received Event VLR_AUTH_E_HLR_SAI_ACK
DVLR SUBSCR(IMSI:901700000010650) Received 1 auth tuples
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=0
- sending UMTS Auth Request for IMSI:901700000010650: tuple use_count=1 key_seq=0 auth_types=0x3 and...
- ...rand=39fa2f4e3d523d8619a73b4f65c3e14d
- ...autn=8704f5ba55f30000d2ee44b22c8ea919
- ...expecting res=e229c19e791f2e41
DREF VLR subscr IMSI:901700000010650 usage decreases to: 1
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: vlr_gsupc_read_cb() returns 0
  auth_request_sent == 1
  lu_result_sent == 0
- MS sends Authen Failure with Resync cause, VLR sends GSUP to HLR to resync
  MSC <--RAN_GERAN_A-- MS: GSM48_MT_MM_AUTH_FAIL
DREF IMSI:901700000010650: MSC conn use + 1 == 2
DRLL Dispatching 04.08 message GSM48_MT_MM_AUTH_FAIL (0x5:0x1c)
DMM IMSI:901700000010650: MM R99 AUTHENTICATION SYNCH (AUTS = 979498b1f72d3e28c59fa2e72f9c)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_FAIL
DVLR GSUP tx: 08010809710000000156f0260e979498b1f72d3e28c59fa2e72f9c201039fa2f4e3d523d8619a73b4f65c3e14d
GSUP --> HLR: OSMO_GSUP_MSGT_SEND_AUTH_INFO_REQUEST: 08010809710000000156f0260e979498b1f72d3e28c59fa2e72f9c201039fa2f4e3d523d8619a73b4f65c3e14d
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_NEEDS_AUTH_WAIT_SAI_RESYNC
DMM IMSI:901700000010650: bump: conn still being established (SUBSCR_CONN_S_NEW)
DREF IMSI:901700000010650: MSC conn use - 1 == 1
  gsup_tx_confirmed == 1
  auth_request_sent == 0
  lu_result_sent == 0
- HLR replies with new tuples
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: 0a010809710000000156f0036220100f1feb1623e1bf626334e37ec448ac182104efde99da220814778c855c52373023108a90c769b7272f3bb7a1c1fbb1ea9349241043ffc1cf8c89a7fd6ab94bd8d6162cbf251002a83f62e9470000660d51afc75f169d27081df5f0b4f22b696e03622010ac21d34937b4e1142a2c757af294931921047818bfdc2208d175571f41f314a42310ff8edbceb6dd24799c77c3b9a6790c102410157c39022ca9d885a7f0766a7dfee44825108a43b91898e500002cf354c6f5d1f8c32708f748a7078f5018db
DVLR GSUP rx 211: 0a010809710000000156f0036220100f1feb1623e1bf626334e37ec448ac182104efde99da220814778c855c52373023108a90c769b7272f3bb7a1c1fbb1ea9349241043ffc1cf8c89a7fd6ab94bd8d6162cbf251002a83f62e9470000660d51afc75f169d27081df5f0b4f22b696e03622010ac21d34937b4e1142a2c757af294931921047818bfdc2208d175571f41f314a42310ff8edbceb6dd24799c77c3b9a6790c102410157c39022ca9d885a7f0766a7dfee44825108a43b91898e500002cf354c6f5d1f8c32708f748a7078f5018db
DREF VLR subscr IMSI:901700000010650 usage increases to: 2
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH_WAIT_SAI_RESYNC}: Received Event VLR_AUTH_E_HLR_SAI_ACK
DVLR SUBSCR(IMSI:901700000010650) Received 2 auth tuples
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH_WAIT_SAI_RESYNC}: state_chg to VLR_SUB_AS_WAIT_RESP_RESYNC
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP_RESYNC}: got auth tuple: use_count=1 key_seq=0
- sending UMTS Auth Request for IMSI:901700000010650: tuple use_count=1 key_seq=0 auth_types=0x3 and...
- ...rand=0f1feb1623e1bf626334e37ec448ac18
- ...autn=02a83f62e9470000660d51afc75f169d
- ...expecting res=1df5f0b4f22b696e
DREF VLR subscr IMSI:901700000010650 usage decreases to: 1
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: vlr_gsupc_read_cb() returns 0
  auth_request_sent == 1
  lu_result_sent == 0
- MS sends Authen Response, VLR accepts and sends GSUP LU Req to HLR
  MSC <--RAN_GERAN_A-- MS: GSM48_MT_MM_AUTH_RESP
DREF IMSI:901700000010650: MSC conn use + 1 == 2
DRLL Dispatching 04.08 message GSM48_MT_MM_AUTH_RESP (0x5:0x14)
DMM IMSI:901700000010650: MM R99 AUTHENTICATION RESPONSE (res = 1df5f0b4f22b696e)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP_RESYNC}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(IMSI:901700000010650) received res: 1d f5 f0 b4 f2 2b 69 6e 
DVLR SUBSCR(IMSI:901700000010650) AUTH established UMTS security context
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP_RESYNC}: Authentication terminating with result VLR_AUTH_RES_PASSED
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP_RESYNC}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_AUTHENTICATED}: Removing from parent vlr_lu_fsm(901700000010650)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_AUTHENTICATED}: Freeing instance
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_AUTH}: Received Event VLR_ULA_E_AUTH_RES
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_post_auth()
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_post_ciph()
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_node_4()
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_AUTH}: state_chg to VLR_ULA_S_WAIT_HLR_UPD
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_INIT}: Allocated
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_INIT}: is child of vlr_lu_fsm(901700000010650)
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_INIT}: Received Event UPD_HLR_VLR_E_START
DVLR GSUP tx: 04010809710000000156f0
GSUP --> HLR: OSMO_GSUP_MSGT_UPDATE_LOCATION_REQUEST: 04010809710000000156f0
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_INIT}: state_chg to UPD_HLR_VLR_S_WAIT_FOR_DATA
DMM IMSI:901700000010650: bump: conn still being established (SUBSCR_CONN_S_NEW)
DREF IMSI:901700000010650: MSC conn use - 1 == 1
  gsup_tx_confirmed == 1
  lu_result_sent == 0
- HLR sends _INSERT_DATA_REQUEST, VLR responds with _INSERT_DATA_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: 10010809710000000156f00804032443f2
DVLR GSUP rx 17: 10010809710000000156f00804032443f2
DREF VLR subscr IMSI:901700000010650 usage increases to: 2
DVLR IMSI:901700000010650 has MSISDN:42342
DVLR GSUP tx: 12010809710000000156f0
GSUP --> HLR: OSMO_GSUP_MSGT_INSERT_DATA_RESULT: 12010809710000000156f0
DREF VLR subscr MSISDN:42342 usage decreases to: 1
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: vlr_gsupc_read_cb() returns 0
  lu_result_sent == 0
- HLR also sends GSUP _UPDATE_LOCATION_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: 06010809710000000156f0
DVLR GSUP rx 11: 06010809710000000156f0
DREF VLR subscr MSISDN:42342 usage increases to: 2
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_HLR_LU_RES
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_WAIT_FOR_DATA}: Received Event UPD_HLR_VLR_E_UPD_LOC_ACK
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_WAIT_FOR_DATA}: state_chg to UPD_HLR_VLR_S_DONE
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_DONE}: Removing from parent vlr_lu_fsm(901700000010650)
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_DONE}: Freeing instance
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_DONE}: Deallocated
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_UPD_HLR_COMPL
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_HLR_UPD}: state_chg to VLR_ULA_S_WAIT_LU_COMPL
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_INIT}: Allocated
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_INIT}: is child of vlr_lu_fsm(901700000010650)
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_INIT}: Received Event LU_COMPL_VLR_E_START
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_INIT}: state_chg to LU_COMPL_VLR_S_WAIT_SUB_PRES
DVLR sub_pres_vlr_fsm(901700000010650){SUB_PRES_VLR_S_INIT}: Allocated
DVLR sub_pres_vlr_fsm(901700000010650){SUB_PRES_VLR_S_INIT}: is child of lu_compl_vlr_fsm(901700000010650)
DVLR sub_pres_vlr_fsm(901700000010650){SUB_PRES_VLR_S_INIT}: Received Event SUB_PRES_VLR_E_START
DVLR sub_pres_vlr_fsm(901700000010650){SUB_PRES_VLR_S_INIT}: state_chg to SUB_PRES_VLR_S_DONE
DVLR sub_pres_vlr_fsm(901700000010650){SUB_PRES_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR sub_pres_vlr_fsm(901700000010650){SUB_PRES_VLR_S_DONE}: Removing from parent lu_compl_vlr_fsm(901700000010650)
DVLR sub_pres_vlr_fsm(901700000010650){SUB_PRES_VLR_S_DONE}: Freeing instance
DVLR sub_pres_vlr_fsm(901700000010650){SUB_PRES_VLR_S_DONE}: Deallocated
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_WAIT_SUB_PRES}: Received Event LU_COMPL_VLR_E_SUB_PRES_COMPL
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_WAIT_SUB_PRES}: lu_compl_vlr_new_tmsi()
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_WAIT_SUB_PRES}: state_chg to LU_COMPL_VLR_S_WAIT_TMSI_CNF
- sending LU Accept for MSISDN:42342, with TMSI 0x03020100
DREF VLR subscr MSISDN:42342 usage decreases to: 1
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: vlr_gsupc_read_cb() returns 0
  lu_result_sent == 1
- a LU Accept with a new TMSI was sent, waiting for TMSI Realloc Compl
  llist_count(&net->subscr_conns) == 1
msc_subscr_conn_is_accepted() == false
  requests shall be thwarted
DRLL Dispatching 04.08 message GSM48_MT_CC_SETUP (0x3:0x5)
DRLL subscr MSISDN:42342: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DRLL Dispatching 04.08 message unknown 0x33 (0x5:0x33)
DRLL subscr MSISDN:42342: Message not permitted for initial conn: unknown 0x33
DRLL Dispatching 04.08 message GSM48_MT_RR_SYSINFO_1 (0x6:0x19)
DRLL subscr MSISDN:42342: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DRLL Dispatching 04.08 message GSM48_PDISC_SMS:0x01 (0x9:0x1)
DRLL subscr MSISDN:42342: Message not permitted for initial conn: GSM48_PDISC_SMS:0x01
- even though the TMSI is not acked, we can already find the subscr with it
DREF VLR subscr MSISDN:42342 usage increases to: 2
  vsub != NULL == 1
  strcmp(vsub->imsi, imsi) == 0
  vsub->tmsi_new == 0x03020100
  vsub->tmsi == 0xffffffff
DREF VLR subscr MSISDN:42342 usage decreases to: 1
- MS sends TMSI Realloc Complete
  MSC <--RAN_GERAN_A-- MS: GSM48_MT_MM_TMSI_REALL_COMPL
DREF MSISDN:42342: MSC conn use + 1 == 2
DRLL Dispatching 04.08 message GSM48_MT_MM_TMSI_REALL_COMPL (0x5:0x1b)
DMM TMSI Reallocation Completed. Subscriber: MSISDN:42342
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_NEW_TMSI_ACK
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_WAIT_TMSI_CNF}: Received Event LU_COMPL_VLR_E_NEW_TMSI_ACK
DREF VLR subscr MSISDN:42342 usage increases to: 2
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_WAIT_TMSI_CNF}: state_chg to LU_COMPL_VLR_S_DONE
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_LU_COMPL_SUCCESS
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_DONE}: Removing from parent vlr_lu_fsm(901700000010650)
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_DONE}: Freeing instance
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_DONE}: Deallocated
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_LU_COMPL}: state_chg to VLR_ULA_S_DONE
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_NEW}: Received Event SUBSCR_CONN_E_ACCEPTED
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_NEW}: SUBSCR_CONN_FROM_LU
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_NEW}: state_chg to SUBSCR_CONN_S_ACCEPTED
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: Received Event SUBSCR_CONN_E_BUMP
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: bump: releasing conn
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: state_chg to SUBSCR_CONN_S_RELEASED
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_DONE}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_DONE}: Removing from parent Subscr_Conn(901700000010650)
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_DONE}: fsm_lu_cleanup called with cause OSMO_FSM_TERM_PARENT
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_DONE}: Freeing instance
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_DONE}: Deallocated
DMM msc_subscr_conn_close(vsub=MSISDN:42342, cause=2): no conn fsm, releasing directly without release event.
DREF MSISDN:42342: MSC conn use - 1 == 1
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_RELEASED}: Freeing instance
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_RELEASED}: Deallocated
DREF MSISDN:42342: MSC conn use - 1 == 0
DRLL subscr MSISDN:42342: Freeing subscriber connection
DREF VLR subscr MSISDN:42342 usage decreases to: 1
- LU was successful, and the conn has already been closed
  llist_count(&net->subscr_conns) == 0
DREF freeing VLR subscr MSISDN:42342
===== test_umts_authen_resync_geran: SUCCESS

full talloc report on 'msgb' (total      0 bytes in   1 blocks)
talloc_total_blocks(tall_bsc_ctx) == 9

===== test_umts_authen_resync_utran
- Location Update request causes a GSUP Send Auth Info request to HLR
  MSC <--RAN_UTRAN_IU-- MS: GSM48_MT_MM_LOC_UPD_REQUEST
  new conn
DREF unknown: MSC conn use + 1 == 1
DRLL Dispatching 04.08 message GSM48_MT_MM_LOC_UPD_REQUEST (0x5:0x8)
DREF unknown: MSC conn use + 1 == 2
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_INIT}: Allocated
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_INIT}: Received Event SUBSCR_CONN_E_START
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_INIT}: state_chg to SUBSCR_CONN_S_NEW
DMM LOCATION UPDATING REQUEST: MI(IMSI)=901700000010650 type=NORMAL
DMM LU/new-LAC: 0/0
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_IDLE}: Allocated
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_IDLE}: is child of Subscr_Conn(901700000010650)
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_IDLE}: rev=R99 net=UTRAN Auth+Ciph
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_IDLE}: Received Event VLR_ULA_E_UPDATE_LA
DREF VLR subscr unknown usage increases to: 1
DVLR set IMSI on subscriber; IMSI=901700000010650 id=901700000010650
DVLR New subscr, IMSI: 901700000010650
DREF VLR subscr IMSI:901700000010650 usage increases to: 2
DREF VLR subscr IMSI:901700000010650 usage decreases to: 1
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_IDLE}: vlr_loc_upd_node1()
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_IDLE}: state_chg to VLR_ULA_S_WAIT_AUTH
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH}: is child of vlr_lu_fsm(901700000010650)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
DVLR GSUP tx: 08010809710000000156f0
GSUP --> HLR: OSMO_GSUP_MSGT_SEND_AUTH_INFO_REQUEST: 08010809710000000156f0
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_NEEDS_AUTH_WAIT_AI
DMM IMSI:901700000010650: bump: conn still being established (SUBSCR_CONN_S_NEW)
DREF IMSI:901700000010650: MSC conn use - 1 == 1
  lu_result_sent == 0
- from HLR, rx _SEND_AUTH_INFO_RESULT; VLR sends Auth Req to MS
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: 0a010809710000000156f00362201039fa2f4e3d523d8619a73b4f65c3e14d21049b36efdf2208059a4f668f6fbe39231027497388b6cb044648f396aa155b95ef2410f64735036e5871319c679f4742a75ea125108704f5ba55f30000d2ee44b22c8ea9192708e229c19e791f2e41
DVLR GSUP rx 111: 0a010809710000000156f00362201039fa2f4e3d523d8619a73b4f65c3e14d21049b36efdf2208059a4f668f6fbe39231027497388b6cb044648f396aa155b95ef2410f64735036e5871319c679f4742a75ea125108704f5ba55f30000d2ee44b22c8ea9192708e229c19e791f2e41
DREF VLR subscr IMSI:901700000010650 usage increases to: 2
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: Received Event VLR_AUTH_E_HLR_SAI_ACK
DVLR SUBSCR(IMSI:901700000010650) Received 1 auth tuples
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=0
- sending UMTS Auth Request for IMSI:901700000010650: tuple use_count=1 key_seq=0 auth_types=0x3 and...
- ...rand=39fa2f4e3d523d8619a73b4f65c3e14d
- ...autn=8704f5ba55f30000d2ee44b22c8ea919
- ...expecting res=e229c19e791f2e41
DREF VLR subscr IMSI:901700000010650 usage decreases to: 1
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: vlr_gsupc_read_cb() returns 0
  auth_request_sent == 1
  lu_result_sent == 0
- MS sends Authen Failure with Resync cause, VLR sends GSUP to HLR to resync
  MSC <--RAN_UTRAN_IU-- MS: GSM48_MT_MM_AUTH_FAIL
DREF IMSI:901700000010650: MSC conn use + 1 == 2
DRLL Dispatching 04.08 message GSM48_MT_MM_AUTH_FAIL (0x5:0x1c)
DMM IMSI:901700000010650: MM R99 AUTHENTICATION SYNCH (AUTS = 979498b1f72d3e28c59fa2e72f9c)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_FAIL
DVLR GSUP tx: 08010809710000000156f0260e979498b1f72d3e28c59fa2e72f9c201039fa2f4e3d523d8619a73b4f65c3e14d
GSUP --> HLR: OSMO_GSUP_MSGT_SEND_AUTH_INFO_REQUEST: 08010809710000000156f0260e979498b1f72d3e28c59fa2e72f9c201039fa2f4e3d523d8619a73b4f65c3e14d
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_NEEDS_AUTH_WAIT_SAI_RESYNC
DMM IMSI:901700000010650: bump: conn still being established (SUBSCR_CONN_S_NEW)
DREF IMSI:901700000010650: MSC conn use - 1 == 1
  gsup_tx_confirmed == 1
  auth_request_sent == 0
  lu_result_sent == 0
- HLR replies with new tuples
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: 0a010809710000000156f0036220100f1feb1623e1bf626334e37ec448ac182104efde99da220814778c855c52373023108a90c769b7272f3bb7a1c1fbb1ea9349241043ffc1cf8c89a7fd6ab94bd8d6162cbf251002a83f62e9470000660d51afc75f169d27081df5f0b4f22b696e03622010ac21d34937b4e1142a2c757af294931921047818bfdc2208d175571f41f314a42310ff8edbceb6dd24799c77c3b9a6790c102410157c39022ca9d885a7f0766a7dfee44825108a43b91898e500002cf354c6f5d1f8c32708f748a7078f5018db
DVLR GSUP rx 211: 0a010809710000000156f0036220100f1feb1623e1bf626334e37ec448ac182104efde99da220814778c855c52373023108a90c769b7272f3bb7a1c1fbb1ea9349241043ffc1cf8c89a7fd6ab94bd8d6162cbf251002a83f62e9470000660d51afc75f169d27081df5f0b4f22b696e03622010ac21d34937b4e1142a2c757af294931921047818bfdc2208d175571f41f314a42310ff8edbceb6dd24799c77c3b9a6790c102410157c39022ca9d885a7f0766a7dfee44825108a43b91898e500002cf354c6f5d1f8c32708f748a7078f5018db
DREF VLR subscr IMSI:901700000010650 usage increases to: 2
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH_WAIT_SAI_RESYNC}: Received Event VLR_AUTH_E_HLR_SAI_ACK
DVLR SUBSCR(IMSI:901700000010650) Received 2 auth tuples
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_NEEDS_AUTH_WAIT_SAI_RESYNC}: state_chg to VLR_SUB_AS_WAIT_RESP_RESYNC
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP_RESYNC}: got auth tuple: use_count=1 key_seq=0
- sending UMTS Auth Request for IMSI:901700000010650: tuple use_count=1 key_seq=0 auth_types=0x3 and...
- ...rand=0f1feb1623e1bf626334e37ec448ac18
- ...autn=02a83f62e9470000660d51afc75f169d
- ...expecting res=1df5f0b4f22b696e
DREF VLR subscr IMSI:901700000010650 usage decreases to: 1
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: vlr_gsupc_read_cb() returns 0
  auth_request_sent == 1
  lu_result_sent == 0
- MS sends Authen Response, VLR accepts and sends SecurityModeControl
  MSC <--RAN_UTRAN_IU-- MS: GSM48_MT_MM_AUTH_RESP
DREF IMSI:901700000010650: MSC conn use + 1 == 2
DRLL Dispatching 04.08 message GSM48_MT_MM_AUTH_RESP (0x5:0x14)
DMM IMSI:901700000010650: MM R99 AUTHENTICATION RESPONSE (res = 1df5f0b4f22b696e)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP_RESYNC}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(IMSI:901700000010650) received res: 1d f5 f0 b4 f2 2b 69 6e 
DVLR SUBSCR(IMSI:901700000010650) AUTH established UMTS security context
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP_RESYNC}: Authentication terminating with result VLR_AUTH_RES_PASSED
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_WAIT_RESP_RESYNC}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_AUTHENTICATED}: Removing from parent vlr_lu_fsm(901700000010650)
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_AUTHENTICATED}: Freeing instance
DVLR VLR_Authenticate(901700000010650){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_AUTH}: Received Event VLR_ULA_E_AUTH_RES
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_post_auth()
- sending SecurityModeControl for IMSI:901700000010650
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_AUTH}: state_chg to VLR_ULA_S_WAIT_CIPH
DMM IMSI:901700000010650: bump: conn still being established (SUBSCR_CONN_S_NEW)
DREF IMSI:901700000010650: MSC conn use - 1 == 1
  cipher_mode_cmd_sent == 1
  lu_result_sent == 0
- MS sends SecurityModeControl acceptance, VLR accepts and sends GSUP LU Req to HLR
DMM <- SECURITY MODE COMPLETE IMSI:901700000010650
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_CIPH}: Received Event VLR_ULA_E_CIPH_RES
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_CIPH}: vlr_loc_upd_post_ciph()
DIUCS IMSI:901700000010650: tx CommonID 901700000010650
- Iu Common ID --RAN_UTRAN_IU--> MS (IMSI=901700000010650)
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_CIPH}: vlr_loc_upd_node_4()
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_CIPH}: state_chg to VLR_ULA_S_WAIT_HLR_UPD
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_INIT}: Allocated
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_INIT}: is child of vlr_lu_fsm(901700000010650)
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_INIT}: Received Event UPD_HLR_VLR_E_START
DVLR GSUP tx: 04010809710000000156f0
GSUP --> HLR: OSMO_GSUP_MSGT_UPDATE_LOCATION_REQUEST: 04010809710000000156f0
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_INIT}: state_chg to UPD_HLR_VLR_S_WAIT_FOR_DATA
  gsup_tx_confirmed == 1
  lu_result_sent == 0
- HLR sends _INSERT_DATA_REQUEST, VLR responds with _INSERT_DATA_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: 10010809710000000156f00804032443f2
DVLR GSUP rx 17: 10010809710000000156f00804032443f2
DREF VLR subscr IMSI:901700000010650 usage increases to: 2
DVLR IMSI:901700000010650 has MSISDN:42342
DVLR GSUP tx: 12010809710000000156f0
GSUP --> HLR: OSMO_GSUP_MSGT_INSERT_DATA_RESULT: 12010809710000000156f0
DREF VLR subscr MSISDN:42342 usage decreases to: 1
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: vlr_gsupc_read_cb() returns 0
  lu_result_sent == 0
- HLR also sends GSUP _UPDATE_LOCATION_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: 06010809710000000156f0
DVLR GSUP rx 11: 06010809710000000156f0
DREF VLR subscr MSISDN:42342 usage increases to: 2
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_HLR_LU_RES
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_WAIT_FOR_DATA}: Received Event UPD_HLR_VLR_E_UPD_LOC_ACK
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_WAIT_FOR_DATA}: state_chg to UPD_HLR_VLR_S_DONE
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_DONE}: Removing from parent vlr_lu_fsm(901700000010650)
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_DONE}: Freeing instance
DVLR upd_hlr_vlr_fsm(901700000010650){UPD_HLR_VLR_S_DONE}: Deallocated
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_UPD_HLR_COMPL
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_HLR_UPD}: state_chg to VLR_ULA_S_WAIT_LU_COMPL
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_INIT}: Allocated
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_INIT}: is child of vlr_lu_fsm(901700000010650)
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_INIT}: Received Event LU_COMPL_VLR_E_START
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_INIT}: state_chg to LU_COMPL_VLR_S_WAIT_SUB_PRES
DVLR sub_pres_vlr_fsm(901700000010650){SUB_PRES_VLR_S_INIT}: Allocated
DVLR sub_pres_vlr_fsm(901700000010650){SUB_PRES_VLR_S_INIT}: is child of lu_compl_vlr_fsm(901700000010650)
DVLR sub_pres_vlr_fsm(901700000010650){SUB_PRES_VLR_S_INIT}: Received Event SUB_PRES_VLR_E_START
DVLR sub_pres_vlr_fsm(901700000010650){SUB_PRES_VLR_S_INIT}: state_chg to SUB_PRES_VLR_S_DONE
DVLR sub_pres_vlr_fsm(901700000010650){SUB_PRES_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR sub_pres_vlr_fsm(901700000010650){SUB_PRES_VLR_S_DONE}: Removing from parent lu_compl_vlr_fsm(901700000010650)
DVLR sub_pres_vlr_fsm(901700000010650){SUB_PRES_VLR_S_DONE}: Freeing instance
DVLR sub_pres_vlr_fsm(901700000010650){SUB_PRES_VLR_S_DONE}: Deallocated
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_WAIT_SUB_PRES}: Received Event LU_COMPL_VLR_E_SUB_PRES_COMPL
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_WAIT_SUB_PRES}: lu_compl_vlr_new_tmsi()
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_WAIT_SUB_PRES}: state_chg to LU_COMPL_VLR_S_WAIT_TMSI_CNF
- sending LU Accept for MSISDN:42342, with TMSI 0x03020100
DREF VLR subscr MSISDN:42342 usage decreases to: 1
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: vlr_gsupc_read_cb() returns 0
  lu_result_sent == 1
- a LU Accept with a new TMSI was sent, waiting for TMSI Realloc Compl
  llist_count(&net->subscr_conns) == 1
msc_subscr_conn_is_accepted() == false
  requests shall be thwarted
DRLL Dispatching 04.08 message GSM48_MT_CC_SETUP (0x3:0x5)
DRLL subscr MSISDN:42342: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DRLL Dispatching 04.08 message unknown 0x33 (0x5:0x33)
DRLL subscr MSISDN:42342: Message not permitted for initial conn: unknown 0x33
DRLL Dispatching 04.08 message GSM48_MT_RR_SYSINFO_1 (0x6:0x19)
DRLL subscr MSISDN:42342: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DRLL Dispatching 04.08 message GSM48_PDISC_SMS:0x01 (0x9:0x1)
DRLL subscr MSISDN:42342: Message not permitted for initial conn: GSM48_PDISC_SMS:0x01
- even though the TMSI is not acked, we can already find the subscr with it
DREF VLR subscr MSISDN:42342 usage increases to: 2
  vsub != NULL == 1
  strcmp(vsub->imsi, imsi) == 0
  vsub->tmsi_new == 0x03020100
  vsub->tmsi == 0xffffffff
DREF VLR subscr MSISDN:42342 usage decreases to: 1
- MS sends TMSI Realloc Complete
  MSC <--RAN_UTRAN_IU-- MS: GSM48_MT_MM_TMSI_REALL_COMPL
DREF MSISDN:42342: MSC conn use + 1 == 2
DRLL Dispatching 04.08 message GSM48_MT_MM_TMSI_REALL_COMPL (0x5:0x1b)
DMM TMSI Reallocation Completed. Subscriber: MSISDN:42342
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_NEW_TMSI_ACK
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_WAIT_TMSI_CNF}: Received Event LU_COMPL_VLR_E_NEW_TMSI_ACK
DREF VLR subscr MSISDN:42342 usage increases to: 2
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_WAIT_TMSI_CNF}: state_chg to LU_COMPL_VLR_S_DONE
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_LU_COMPL_SUCCESS
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_DONE}: Removing from parent vlr_lu_fsm(901700000010650)
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_DONE}: Freeing instance
DVLR lu_compl_vlr_fsm(901700000010650){LU_COMPL_VLR_S_DONE}: Deallocated
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_WAIT_LU_COMPL}: state_chg to VLR_ULA_S_DONE
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_NEW}: Received Event SUBSCR_CONN_E_ACCEPTED
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_NEW}: SUBSCR_CONN_FROM_LU
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_NEW}: state_chg to SUBSCR_CONN_S_ACCEPTED
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: Received Event SUBSCR_CONN_E_BUMP
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: bump: releasing conn
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_ACCEPTED}: state_chg to SUBSCR_CONN_S_RELEASED
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_DONE}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_DONE}: Removing from parent Subscr_Conn(901700000010650)
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_DONE}: fsm_lu_cleanup called with cause OSMO_FSM_TERM_PARENT
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_DONE}: Freeing instance
DVLR vlr_lu_fsm(901700000010650){VLR_ULA_S_DONE}: Deallocated
DMM msc_subscr_conn_close(vsub=MSISDN:42342, cause=2): no conn fsm, releasing directly without release event.
- Iu Release --RAN_UTRAN_IU--> MS
DREF MSISDN:42342: MSC conn use - 1 == 1
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_RELEASED}: Freeing instance
DMM Subscr_Conn(901700000010650){SUBSCR_CONN_S_RELEASED}: Deallocated
DREF MSISDN:42342: MSC conn use - 1 == 0
DRLL subscr MSISDN:42342: Freeing subscriber connection
DREF VLR subscr MSISDN:42342 usage decreases to: 1
- LU was successful, and the conn has already been closed
  llist_count(&net->subscr_conns) == 0
DREF freeing VLR subscr MSISDN:42342
===== test_umts_authen_resync_utran: SUCCESS

full talloc report on 'msgb' (total      0 bytes in   1 blocks)
talloc_total_blocks(tall_bsc_ctx) == 9

full talloc report on 'msgb' (total      0 bytes in   1 blocks)
talloc_total_blocks(tall_bsc_ctx) == 9

