line: 'one CR'
line: 'two CR'
line: ''
line: 'one CRLF'
line: 'two CRLF'
line: ''
line: 'one LF'
line: 'two LF'
line: ''
line: 'mixed (4 lines)'
line: ''
line: ''
line: ''
Testing AUEP1
Testing AUEP2
Testing MDCX1
Testing MDCX2
Testing CRCX
Dummy packets: 1
Detected packet duration: 40
Requested packetetization period: 20-20
Connection mode: 1: RECV
Testing MDCX3
Dummy packets: 1
Packet duration not set
Requested packetization period not set
Connection mode not set
Testing MDCX4
Dummy packets: 1
Detected packet duration: 40
Requested packetetization period: 20-20
Connection mode: 3: SEND RECV
Testing MDCX4_PT1
Dummy packets: 1
Detected packet duration: 40
Requested packetetization period: 20-40
Connection mode: 3: SEND RECV
Testing MDCX4_PT2
Dummy packets: 1
Detected packet duration: 40
Requested packetetization period: 20-20
Connection mode: 3: SEND RECV
Testing MDCX4_PT3
Dummy packets: 1
Detected packet duration: 40
Requested packetization period not set
Connection mode: 3: SEND RECV
Testing MDCX4_SO
Detected packet duration: 40
Requested packetetization period: 20-20
Connection mode: 2: SEND
Testing MDCX4_RO
Dummy packets: 1
Packet duration not set
Requested packetetization period: 20-20
Connection mode: 1: RECV
Testing DLCX
Detected packet duration: 20
Requested packetization period not set
Connection mode: 0: NONE
Testing CRCX_ZYN
Dummy packets: 1
Packet duration not set
Requested packetization period not set
Connection mode: 1: RECV
Testing EMPTY
Testing SHORT1
Testing SHORT2
Testing SHORT3
Testing SHORT4
Testing RQNT1
Testing RQNT2
Testing DLCX
Detected packet duration: 20
Requested packetization period not set
Connection mode: 0: NONE
Testing CRCX
Dummy packets: 1
Detected packet duration: 40
Requested packetetization period: 20-20
Connection mode: 1: RECV
Testing MDCX3
Dummy packets: 1
Packet duration not set
Requested packetization period not set
Connection mode not set
Testing DLCX
Detected packet duration: 20
Requested packetization period not set
Connection mode: 0: NONE
Testing CRCX
Re-transmitting CRCX
Testing RQNT1
Re-transmitting RQNT1
Testing RQNT2
Re-transmitting RQNT2
Testing MDCX3
Re-transmitting MDCX3
Testing DLCX
Re-transmitting DLCX
Testing packet loss calculation.
Testing stat parsing
Parsing result: 0
Parsing result: 0
Testing packet error detection, patch SSRC.
Output SSRC changed to 11223344
In TS: 0, dTS: 0, Seq: 0
Out TS change: 0, dTS: 0, Seq change: 0, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = 0
In TS: 160, dTS: 160, Seq: 1
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = 0
In TS: 320, dTS: 160, Seq: 2
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = 0
In TS: 320, dTS: 160, Seq: 3
Out TS change: 0, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 10, Transit = 160
In TS: 480, dTS: 160, Seq: 4
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 9, Transit = 160
In TS: 640, dTS: 160, Seq: 5
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 8, Transit = 160
In TS: 960, dTS: 320, Seq: 6
Out TS change: 320, dTS: 320, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 18, Transit = 0
In TS: 1120, dTS: 160, Seq: 7
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 17, Transit = 0
In TS: 1280, dTS: 160, Seq: 8
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 16, Transit = 0
In TS: 1400, dTS: 120, Seq: 9
Out TS change: 120, dTS: 120, Seq change: 1, TS Err change: in +1, out +1
Stats: Jitter = 17, Transit = 40
In TS: 1560, dTS: 160, Seq: 10
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 16, Transit = 40
In TS: 1720, dTS: 160, Seq: 11
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 15, Transit = 40
In TS: 34688, dTS: 0, Seq: 12
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = -32768
In TS: 34848, dTS: 160, Seq: 13
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = -32768
In TS: 35008, dTS: 160, Seq: 14
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = -32768
In TS: 35128, dTS: 120, Seq: 15
Out TS change: 120, dTS: 120, Seq change: 1, TS Err change: in +1, out +1
Stats: Jitter = 2, Transit = -32728
In TS: 35288, dTS: 160, Seq: 16
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 2, Transit = -32728
In TS: 35448, dTS: 160, Seq: 17
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 2, Transit = -32728
In TS: 35768, dTS: 160, Seq: 19
Out TS change: 320, dTS: 160, Seq change: 2, TS Err change: in +0, out +0
Stats: Jitter = 12, Transit = -32888
In TS: 35928, dTS: 160, Seq: 20
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 11, Transit = -32888
In TS: 36088, dTS: 160, Seq: 21
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 20, Transit = -33048
In TS: 36088, dTS: 160, Seq: 21
Out TS change: 0, dTS: 160, Seq change: 0, TS Err change: in +0, out +0
Stats: Jitter = 29, Transit = -32888
In TS: 36248, dTS: 160, Seq: 22
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 27, Transit = -32888
In TS: 36408, dTS: 160, Seq: 23
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 25, Transit = -32888
In TS: 36568, dTS: 160, Seq: 23
Out TS change: 160, dTS: 160, Seq change: 0, TS Err change: in +1, out +1
Stats: Jitter = 24, Transit = -32888
In TS: 36728, dTS: 160, Seq: 24
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 22, Transit = -32888
In TS: 36888, dTS: 160, Seq: 25
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 21, Transit = -32888
In TS: 160000, dTS: 0, Seq: 1000
Out TS change: 12000, dTS: 12000, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = -144000
In TS: 160160, dTS: 160, Seq: 1001
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = -144000
In TS: 160320, dTS: 160, Seq: 1002
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = -144000
Testing packet error detection.
Output SSRC changed to 11223344
In TS: 0, dTS: 0, Seq: 0
Out TS change: 0, dTS: 0, Seq change: 0, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = 0
In TS: 160, dTS: 160, Seq: 1
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = 0
In TS: 320, dTS: 160, Seq: 2
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = 0
In TS: 320, dTS: 160, Seq: 3
Out TS change: 0, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 10, Transit = 160
In TS: 480, dTS: 160, Seq: 4
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 9, Transit = 160
In TS: 640, dTS: 160, Seq: 5
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 8, Transit = 160
In TS: 960, dTS: 320, Seq: 6
Out TS change: 320, dTS: 320, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 18, Transit = 0
In TS: 1120, dTS: 160, Seq: 7
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 17, Transit = 0
In TS: 1280, dTS: 160, Seq: 8
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 16, Transit = 0
In TS: 1400, dTS: 120, Seq: 9
Out TS change: 120, dTS: 120, Seq change: 1, TS Err change: in +1, out +1
Stats: Jitter = 17, Transit = 40
In TS: 1560, dTS: 160, Seq: 10
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 16, Transit = 40
In TS: 1720, dTS: 160, Seq: 11
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 15, Transit = 40
Output SSRC changed to 10203040
In TS: 34688, dTS: 0, Seq: 12
Out TS change: 32968, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = -32768
In TS: 34848, dTS: 160, Seq: 13
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = -32768
In TS: 35008, dTS: 160, Seq: 14
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = -32768
In TS: 35128, dTS: 120, Seq: 15
Out TS change: 120, dTS: 120, Seq change: 1, TS Err change: in +1, out +1
Stats: Jitter = 2, Transit = -32728
In TS: 35288, dTS: 160, Seq: 16
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 2, Transit = -32728
In TS: 35448, dTS: 160, Seq: 17
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 2, Transit = -32728
In TS: 35768, dTS: 160, Seq: 19
Out TS change: 320, dTS: 160, Seq change: 2, TS Err change: in +0, out +0
Stats: Jitter = 12, Transit = -32888
In TS: 35928, dTS: 160, Seq: 20
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 11, Transit = -32888
In TS: 36088, dTS: 160, Seq: 21
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 20, Transit = -33048
In TS: 36088, dTS: 160, Seq: 21
Out TS change: 0, dTS: 160, Seq change: 0, TS Err change: in +0, out +0
Stats: Jitter = 29, Transit = -32888
In TS: 36248, dTS: 160, Seq: 22
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 27, Transit = -32888
In TS: 36408, dTS: 160, Seq: 23
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 25, Transit = -32888
In TS: 36568, dTS: 160, Seq: 23
Out TS change: 160, dTS: 160, Seq change: 0, TS Err change: in +1, out +1
Stats: Jitter = 24, Transit = -32888
In TS: 36728, dTS: 160, Seq: 24
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 22, Transit = -32888
In TS: 36888, dTS: 160, Seq: 25
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 21, Transit = -32888
Output SSRC changed to 50607080
In TS: 160000, dTS: 0, Seq: 1000
Out TS change: 123112, dTS: 160, Seq change: 975, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = -144000
In TS: 160160, dTS: 160, Seq: 1001
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = -144000
In TS: 160320, dTS: 160, Seq: 1002
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = -144000
Testing packet error detection, patch timestamps.
Output SSRC changed to 11223344
In TS: 0, dTS: 0, Seq: 0
Out TS change: 0, dTS: 0, Seq change: 0, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = 0
In TS: 160, dTS: 160, Seq: 1
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = 0
In TS: 320, dTS: 160, Seq: 2
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = 0
In TS: 320, dTS: 160, Seq: 3
Out TS change: 0, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 10, Transit = 160
In TS: 480, dTS: 160, Seq: 4
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 9, Transit = 160
In TS: 640, dTS: 160, Seq: 5
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 8, Transit = 160
In TS: 960, dTS: 320, Seq: 6
Out TS change: 320, dTS: 320, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 18, Transit = 0
In TS: 1120, dTS: 160, Seq: 7
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 17, Transit = 0
In TS: 1280, dTS: 160, Seq: 8
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 16, Transit = 0
In TS: 1400, dTS: 120, Seq: 9
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +1, out +0
Stats: Jitter = 17, Transit = 40
In TS: 1560, dTS: 160, Seq: 10
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 16, Transit = 40
In TS: 1720, dTS: 160, Seq: 11
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 15, Transit = 40
Output SSRC changed to 10203040
In TS: 34688, dTS: 0, Seq: 12
Out TS change: 32968, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = -32768
In TS: 34848, dTS: 160, Seq: 13
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = -32768
In TS: 35008, dTS: 160, Seq: 14
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = -32768
In TS: 35128, dTS: 120, Seq: 15
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +1, out +0
Stats: Jitter = 2, Transit = -32728
In TS: 35288, dTS: 160, Seq: 16
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 2, Transit = -32728
In TS: 35448, dTS: 160, Seq: 17
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 2, Transit = -32728
In TS: 35768, dTS: 160, Seq: 19
Out TS change: 320, dTS: 160, Seq change: 2, TS Err change: in +0, out +0
Stats: Jitter = 12, Transit = -32888
In TS: 35928, dTS: 160, Seq: 20
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 11, Transit = -32888
In TS: 36088, dTS: 160, Seq: 21
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 20, Transit = -33048
In TS: 36088, dTS: 160, Seq: 21
Out TS change: 0, dTS: 160, Seq change: 0, TS Err change: in +0, out +0
Stats: Jitter = 29, Transit = -32888
In TS: 36248, dTS: 160, Seq: 22
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 27, Transit = -32888
In TS: 36408, dTS: 160, Seq: 23
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 25, Transit = -32888
In TS: 36568, dTS: 160, Seq: 23
Out TS change: 160, dTS: 160, Seq change: 0, TS Err change: in +1, out +1
Stats: Jitter = 24, Transit = -32888
In TS: 36728, dTS: 160, Seq: 24
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 22, Transit = -32888
In TS: 36888, dTS: 160, Seq: 25
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 21, Transit = -32888
Output SSRC changed to 50607080
In TS: 160000, dTS: 0, Seq: 1000
Out TS change: 123112, dTS: 160, Seq change: 975, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = -144000
In TS: 160160, dTS: 160, Seq: 1001
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = -144000
In TS: 160320, dTS: 160, Seq: 1002
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = -144000
Testing packet error detection, patch SSRC, patch timestamps.
Output SSRC changed to 11223344
In TS: 0, dTS: 0, Seq: 0
Out TS change: 0, dTS: 0, Seq change: 0, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = 0
In TS: 160, dTS: 160, Seq: 1
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = 0
In TS: 320, dTS: 160, Seq: 2
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = 0
In TS: 320, dTS: 160, Seq: 3
Out TS change: 0, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 10, Transit = 160
In TS: 480, dTS: 160, Seq: 4
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 9, Transit = 160
In TS: 640, dTS: 160, Seq: 5
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 8, Transit = 160
In TS: 960, dTS: 320, Seq: 6
Out TS change: 320, dTS: 320, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 18, Transit = 0
In TS: 1120, dTS: 160, Seq: 7
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 17, Transit = 0
In TS: 1280, dTS: 160, Seq: 8
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 16, Transit = 0
In TS: 1400, dTS: 120, Seq: 9
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +1, out +0
Stats: Jitter = 17, Transit = 40
In TS: 1560, dTS: 160, Seq: 10
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 16, Transit = 40
In TS: 1720, dTS: 160, Seq: 11
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 15, Transit = 40
In TS: 34688, dTS: 0, Seq: 12
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = -32768
In TS: 34848, dTS: 160, Seq: 13
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = -32768
In TS: 35008, dTS: 160, Seq: 14
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = -32768
In TS: 35128, dTS: 120, Seq: 15
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +1, out +0
Stats: Jitter = 2, Transit = -32728
In TS: 35288, dTS: 160, Seq: 16
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 2, Transit = -32728
In TS: 35448, dTS: 160, Seq: 17
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 2, Transit = -32728
In TS: 35768, dTS: 160, Seq: 19
Out TS change: 320, dTS: 160, Seq change: 2, TS Err change: in +0, out +0
Stats: Jitter = 12, Transit = -32888
In TS: 35928, dTS: 160, Seq: 20
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 11, Transit = -32888
In TS: 36088, dTS: 160, Seq: 21
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 20, Transit = -33048
In TS: 36088, dTS: 160, Seq: 21
Out TS change: 0, dTS: 160, Seq change: 0, TS Err change: in +0, out +0
Stats: Jitter = 29, Transit = -32888
In TS: 36248, dTS: 160, Seq: 22
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 27, Transit = -32888
In TS: 36408, dTS: 160, Seq: 23
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 25, Transit = -32888
In TS: 36568, dTS: 160, Seq: 23
Out TS change: 160, dTS: 160, Seq change: 0, TS Err change: in +1, out +1
Stats: Jitter = 24, Transit = -32888
In TS: 36728, dTS: 160, Seq: 24
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 22, Transit = -32888
In TS: 36888, dTS: 160, Seq: 25
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 21, Transit = -32888
In TS: 160000, dTS: 0, Seq: 1000
Out TS change: 12000, dTS: 12000, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = -144000
In TS: 160160, dTS: 160, Seq: 1001
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = -144000
In TS: 160320, dTS: 160, Seq: 1002
Out TS change: 160, dTS: 160, Seq change: 1, TS Err change: in +0, out +0
Stats: Jitter = 0, Transit = -144000
Testing multiple payload types
Testing no sequence flow on initial packet
Testing no rtpmap name
Done
