Generated by EAGLE CAM Processor 7.6.0

Drill Station Info File: /space/home_laforge/projects/git/osmo-small-hardware/mpcie-breakout/mpcie-breakout.dri

 Date              : 08.10.16 21:44
 Drills            : generated
 Device            : Excellon drill station, coordinate format 2.5 inch

Parameter settings:

 Tolerance Drill + :  0.00 %
 Tolerance Drill - :  0.00 %
 Rotate            : no
 Mirror            : no
 Optimize          : yes
 Auto fit          : yes
 OffsetX           : 0inch
 OffsetY           : 0inch
 Layers            : Drills Holes

Drill File Info:

 Data Mode         : Absolute
 Units             : 1/100000 Inch

Drills used:

 Code  Size       used

 T01   0.0118inch   103
 T02   0.0240inch     4
 T03   0.0354inch     2
 T04   0.0360inch     7
 T05   0.0400inch    24
 T06   0.0433inch     2
 T07   0.0630inch     3
 T08   0.0709inch     1

Total number of drills: 146

Plotfiles:

 /space/home_laforge/projects/git/osmo-small-hardware/mpcie-breakout/mpcie-breakout.TXT
