Generated by EAGLE CAM Processor 6.4.0

Drill Station Info File: /home/laforge/projects/git/osmo-lea6t-gps/hardware/gerber/ublox-lea6-test.dri

 Date              : 26.11.13 11:11
 Drills            : /home/laforge/projects/git/osmo-lea6t-gps/hardware/gerber/ublox-lea6-test.drl
 Device            : Excellon drill station with user supplied rack file

Parameter settings:

 Tolerance Drill + :  3.00 %
 Tolerance Drill - :  3.00 %
 Rotate            : no
 Mirror            : no
 Optimize          : yes
 Auto fit          : yes
 OffsetX           : 0inch
 OffsetY           : 0inch
 Layers            : Drills Holes

Drill File Info:

 Data Mode         : Absolute
 Units             : 1/10000 Inch

Drill Tolerances:

 -- Requested --  -- Used Drill --

 Size       used  Code  Size

 40.000mil    12  T06   1.020mm
 18.000mil    10  T03   0.460mm
 16.000mil    40  T02   0.410mm
 12.000mil    41  T01   0.300mm

Drills used:

 Code  Size       used

 T01   0.300mm      41
 T02   0.410mm      40
 T03   0.460mm      10
 T04   0.900mm       2
 T05   1.000mm       4
 T06   1.020mm      12

Total number of drills: 109

Plotfiles:

 /home/laforge/projects/git/osmo-lea6t-gps/hardware/gerber/ublox-lea6-test.txt
