-- $Id: MAP-BS-Code.asn 28149 2009-04-25 17:45:34Z etxrab $
-- 3GPP TS 29.002 V8.9.0 (2009-04) 
-- 17.7.10	Bearer Service Codes
 
MAP-BS-Code {
   itu-t identified-organization (4) etsi (0) mobileDomain (0)
   gsm-Network (1) modules (3) map-BS-Code (20) version11 (11)}

DEFINITIONS

::=

BEGIN

BearerServiceCode ::= OCTET STRING (SIZE (1))
	-- This type is used to represent the code identifying a single
	-- bearer service, a group of bearer services, or all bearer
	-- services. The services are defined in TS 3GPP TS 22.002 [3].
	-- The internal structure is defined as follows:
	--
	-- plmn-specific bearer services:
	-- bits 87654321: defined by the HPLMN operator

	-- rest of bearer services:
	-- bit 8: 0 (unused)
	-- bits 7654321: group (bits 7654), and rate, if applicable
	-- (bits 321)

Ext-BearerServiceCode ::= OCTET STRING (SIZE (1..5))
	-- This type is used to represent the code identifying a single
	-- bearer service, a group of bearer services, or all bearer
	-- services. The services are defined in TS 3GPP TS 22.002 [3].
	-- The internal structure is defined as follows:
	--
	-- OCTET 1:
	-- plmn-specific bearer services:
	-- bits 87654321: defined by the HPLMN operator
	--
	-- rest of bearer services:
	-- bit 8: 0 (unused)
	-- bits 7654321: group (bits 7654), and rate, if applicable
	-- (bits 321)

	-- OCTETS 2-5: reserved for future use. If received the
    -- Ext-TeleserviceCode shall be
	-- treated according to the exception handling defined for the
	-- operation that uses this type. 


	-- Ext-BearerServiceCode includes all values defined for BearerServiceCode.

allBearerServices	BearerServiceCode ::= '00000000'B

allDataCDA-Services	BearerServiceCode ::= '00010000'B
dataCDA-300bps		BearerServiceCode ::= '00010001'B
dataCDA-1200bps	BearerServiceCode ::= '00010010'B
dataCDA-1200-75bps	BearerServiceCode ::= '00010011'B
dataCDA-2400bps	BearerServiceCode ::= '00010100'B
dataCDA-4800bps	BearerServiceCode ::= '00010101'B
dataCDA-9600bps	BearerServiceCode ::= '00010110'B
general-dataCDA	BearerServiceCode ::= '00010111'B

allDataCDS-Services	BearerServiceCode ::= '00011000'B
dataCDS-1200bps	BearerServiceCode ::= '00011010'B
dataCDS-2400bps	BearerServiceCode ::= '00011100'B
dataCDS-4800bps	BearerServiceCode ::= '00011101'B
dataCDS-9600bps	BearerServiceCode ::= '00011110'B
general-dataCDS	BearerServiceCode ::= '00011111'B

allPadAccessCA-Services	BearerServiceCode ::= '00100000'B
padAccessCA-300bps	BearerServiceCode ::= '00100001'B
padAccessCA-1200bps	BearerServiceCode ::= '00100010'B
padAccessCA-1200-75bps	BearerServiceCode ::= '00100011'B
padAccessCA-2400bps	BearerServiceCode ::= '00100100'B
padAccessCA-4800bps	BearerServiceCode ::= '00100101'B
padAccessCA-9600bps	BearerServiceCode ::= '00100110'B
general-padAccessCA	BearerServiceCode ::= '00100111'B

allDataPDS-Services	BearerServiceCode ::= '00101000'B
dataPDS-2400bps	BearerServiceCode ::= '00101100'B
dataPDS-4800bps	BearerServiceCode ::= '00101101'B
dataPDS-9600bps	BearerServiceCode ::= '00101110'B
general-dataPDS	BearerServiceCode ::= '00101111'B

allAlternateSpeech-DataCDA	BearerServiceCode ::= '00110000'B

allAlternateSpeech-DataCDS	BearerServiceCode ::= '00111000'B

allSpeechFollowedByDataCDA	BearerServiceCode ::= '01000000'B

allSpeechFollowedByDataCDS	BearerServiceCode ::= '01001000'B

-- The following non-hierarchical Compound Bearer Service
-- Groups are defined in TS 3GPP TS 22.030:
allDataCircuitAsynchronous	BearerServiceCode ::= '01010000'B
	-- covers "allDataCDA-Services", "allAlternateSpeech-DataCDA" and
	-- "allSpeechFollowedByDataCDA"
allAsynchronousServices	BearerServiceCode ::= '01100000'B
	-- covers "allDataCDA-Services", "allAlternateSpeech-DataCDA",
	-- "allSpeechFollowedByDataCDA" and "allPadAccessCDA-Services"
allDataCircuitSynchronous	BearerServiceCode ::= '01011000'B
	-- covers "allDataCDS-Services", "allAlternateSpeech-DataCDS" and
	-- "allSpeechFollowedByDataCDS"
allSynchronousServices	BearerServiceCode ::= '01101000'B
	-- covers "allDataCDS-Services", "allAlternateSpeech-DataCDS",
	-- "allSpeechFollowedByDataCDS" and "allDataPDS-Services"
--
-- Compound Bearer Service Group Codes are only used in call
-- independent supplementary service operations, i.e. they
-- are not used in InsertSubscriberData or in
-- DeleteSubscriberData messages.

allPLMN-specificBS	BearerServiceCode ::= '11010000'B
plmn-specificBS-1	BearerServiceCode ::= '11010001'B
plmn-specificBS-2	BearerServiceCode ::= '11010010'B
plmn-specificBS-3	BearerServiceCode ::= '11010011'B
plmn-specificBS-4	BearerServiceCode ::= '11010100'B
plmn-specificBS-5	BearerServiceCode ::= '11010101'B
plmn-specificBS-6	BearerServiceCode ::= '11010110'B
plmn-specificBS-7	BearerServiceCode ::= '11010111'B
plmn-specificBS-8	BearerServiceCode ::= '11011000'B
plmn-specificBS-9	BearerServiceCode ::= '11011001'B
plmn-specificBS-A	BearerServiceCode ::= '11011010'B
plmn-specificBS-B	BearerServiceCode ::= '11011011'B
plmn-specificBS-C	BearerServiceCode ::= '11011100'B
plmn-specificBS-D	BearerServiceCode ::= '11011101'B
plmn-specificBS-E	BearerServiceCode ::= '11011110'B
plmn-specificBS-F	BearerServiceCode ::= '11011111'B

END

