-- Pretty-printed by Asnp, the pretty-printer of France Telecom R&D (http://asn1.elibel.tm.fr/asnp/)
MAP-BS-Code {itu-t identified-organization(4) etsi(0) mobileDomain(0)
  gsm-Network(1) modules(3) map-BS-Code(20) version8(8)} DEFINITIONS ::=
BEGIN

BearerServiceCode ::= OCTET STRING(SIZE (1))

-- This type is used to represent the code identifying a single
-- bearer service, a group of bearer services, or all bearer
-- services. The services are defined in TS 3GPP TS 22.002 [3].
-- The internal structure is defined as follows:
--
-- plmn-specific bearer services:
-- bits 87654321: defined by the HPLMN operator
-- rest of bearer services:
-- bit 8: 0 (unused)
-- bits 7654321: group (bits 7654), and rate, if applicable
-- (bits 321)
Ext-BearerServiceCode ::= OCTET STRING(SIZE (1..5))

-- This type is used to represent the code identifying a single
-- bearer service, a group of bearer services, or all bearer
-- services. The services are defined in TS 3GPP TS 22.002 [3].
-- The internal structure is defined as follows:
--
-- OCTET 1:
-- plmn-specific bearer services:
-- bits 87654321: defined by the HPLMN operator
--
-- rest of bearer services:
-- bit 8: 0 (unused)
-- bits 7654321: group (bits 7654), and rate, if applicable
-- (bits 321)
-- OCTETS 2-5: reserved for future use. If received the
-- Ext-TeleserviceCode shall be
-- treated according to the exception handling defined for the
-- operation that uses this type.
-- Ext-BearerServiceCode includes all values defined for BearerServiceCode.
allBearerServices BearerServiceCode ::=
  '00000000'B

allDataCDA-Services BearerServiceCode ::= '00010000'B

dataCDA-300bps BearerServiceCode ::= '00010001'B

dataCDA-1200bps BearerServiceCode ::= '00010010'B

dataCDA-1200-75bps BearerServiceCode ::= '00010011'B

dataCDA-2400bps BearerServiceCode ::= '00010100'B

dataCDA-4800bps BearerServiceCode ::= '00010101'B

dataCDA-9600bps BearerServiceCode ::= '00010110'B

general-dataCDA BearerServiceCode ::= '00010111'B

allDataCDS-Services BearerServiceCode ::= '00011000'B

dataCDS-1200bps BearerServiceCode ::= '00011010'B

dataCDS-2400bps BearerServiceCode ::= '00011100'B

dataCDS-4800bps BearerServiceCode ::= '00011101'B

dataCDS-9600bps BearerServiceCode ::= '00011110'B

general-dataCDS BearerServiceCode ::= '00011111'B

allPadAccessCA-Services BearerServiceCode ::= '00100000'B

padAccessCA-300bps BearerServiceCode ::= '00100001'B

padAccessCA-1200bps BearerServiceCode ::= '00100010'B

padAccessCA-1200-75bps BearerServiceCode ::= '00100011'B

padAccessCA-2400bps BearerServiceCode ::= '00100100'B

padAccessCA-4800bps BearerServiceCode ::= '00100101'B

padAccessCA-9600bps BearerServiceCode ::= '00100110'B

general-padAccessCA BearerServiceCode ::= '00100111'B

allDataPDS-Services BearerServiceCode ::= '00101000'B

dataPDS-2400bps BearerServiceCode ::= '00101100'B

dataPDS-4800bps BearerServiceCode ::= '00101101'B

dataPDS-9600bps BearerServiceCode ::= '00101110'B

general-dataPDS BearerServiceCode ::= '00101111'B

allAlternateSpeech-DataCDA BearerServiceCode ::= '00110000'B

allAlternateSpeech-DataCDS BearerServiceCode ::= '00111000'B

allSpeechFollowedByDataCDA BearerServiceCode ::= '01000000'B

allSpeechFollowedByDataCDS BearerServiceCode ::= '01001000'B

-- The following non-hierarchical Compound Bearer Service
-- Groups are defined in TS 3GPP TS 22.030:
allDataCircuitAsynchronous BearerServiceCode ::=
  '01010000'B

-- covers "allDataCDA-Services", "allAlternateSpeech-DataCDA" and
-- "allSpeechFollowedByDataCDA"
allAsynchronousServices BearerServiceCode ::=
  '01100000'B

-- covers "allDataCDA-Services", "allAlternateSpeech-DataCDA",
-- "allSpeechFollowedByDataCDA" and "allPadAccessCDA-Services"
allDataCircuitSynchronous BearerServiceCode ::=
  '01011000'B

-- covers "allDataCDS-Services", "allAlternateSpeech-DataCDS" and
-- "allSpeechFollowedByDataCDS"
allSynchronousServices BearerServiceCode ::=
  '01101000'B

-- covers "allDataCDS-Services", "allAlternateSpeech-DataCDS",
-- "allSpeechFollowedByDataCDS" and "allDataPDS-Services"
--
-- Compound Bearer Service Group Codes are only used in call
-- independent supplementary service operations, i.e. they
-- are not used in InsertSubscriberData or in
-- DeleteSubscriberData messages.
allPLMN-specificBS BearerServiceCode ::=
  '11010000'B

plmn-specificBS-1 BearerServiceCode ::= '11010001'B

plmn-specificBS-2 BearerServiceCode ::= '11010010'B

plmn-specificBS-3 BearerServiceCode ::= '11010011'B

plmn-specificBS-4 BearerServiceCode ::= '11010100'B

plmn-specificBS-5 BearerServiceCode ::= '11010101'B

plmn-specificBS-6 BearerServiceCode ::= '11010110'B

plmn-specificBS-7 BearerServiceCode ::= '11010111'B

plmn-specificBS-8 BearerServiceCode ::= '11011000'B

plmn-specificBS-9 BearerServiceCode ::= '11011001'B

plmn-specificBS-A BearerServiceCode ::= '11011010'B

plmn-specificBS-B BearerServiceCode ::= '11011011'B

plmn-specificBS-C BearerServiceCode ::= '11011100'B

plmn-specificBS-D BearerServiceCode ::= '11011101'B

plmn-specificBS-E BearerServiceCode ::= '11011110'B

plmn-specificBS-F BearerServiceCode ::= '11011111'B

END

