-- Pretty-printed by Asnp, the pretty-printer of France Telecom R&D (http://asn1.elibel.tm.fr/asnp/)
MAP-ST-DataTypes {itu-t identified-organization(4) etsi(0) mobileDomain(0)
  gsm-Network(1) modules(3) map-ST-DataTypes(27) version8(8)} DEFINITIONS
IMPLICIT TAGS ::=
BEGIN

EXPORTS
  SecureTransportArg, SecureTransportRes, SecurityHeader, ProtectedPayload;

IMPORTS
  IMSI
    FROM MAP-CommonDataTypes {itu-t identified-organization(4) etsi(0)
      mobileDomain(0) gsm-Network(1) modules(3) map-CommonDataTypes(18)
      version8(8)};

SecureTransportArg ::= SEQUENCE {
  securityHeader    SecurityHeader,
  protectedPayload  ProtectedPayload OPTIONAL}

-- The protectedPayload carries the result of applying the security function
-- defined in 3GPP TS 33.200 to the encoding of the argument of the securely
-- transported operation
SecureTransportRes ::= SEQUENCE {
  securityHeader    SecurityHeader,
  protectedPayload  ProtectedPayload OPTIONAL}

-- The protectedPayload carries the result of applying the security function
-- defined in 3GPP TS 33.200 to the encoding of the result of the securely
-- transported operation
SecurityHeader ::= SEQUENCE {
  securityParametersIndex      SecurityParametersIndex,
  originalComponentIdentifier  OriginalComponentIdentifier,
  initialisationVector         InitialisationVector OPTIONAL,
  ...}

ProtectedPayload ::= OCTET STRING(SIZE (1..3438))

-- In protection mode 0 (noProtection) the ProtectedPayload carries the transfer
-- syntax value of the component parameter identified by the
-- originalComponentIdentifier.
-- In protection mode 1 (integrityAuthenticity) the protectedPayload carries
-- the transfer syntax value of the component
-- parameter identified by the originalComponentIdentifier, followed by
-- the 32 bit integrity check value.
-- The integrity check value is the result of applying the hash algorithm
-- to the concatenation of the transfer syntax value of the SecurityHeader,
-- and the transfer syntax value of the component parameter.
-- In protection mode 2 (confidentialityIntegrityAuthenticity) the protected
-- payload carries the encrypted transfer syntax
-- value of the component parameter identified by the
-- originalComponentIdentifier, followed by the 32 bit integrity check value.
-- The integrity check value is the result of applying the hash algorithm
-- to the concatenation of the transfer syntax value of the SecurityHeader,
-- and the encrypted transfer syntax value of the component parameter.
-- See 33.200.
-- The length of the protectedPayload is adjusted according to the capabilities of
-- the lower protocol layers
SecurityParametersIndex ::= OCTET STRING(SIZE (4))

InitialisationVector ::= OCTET STRING(SIZE (14))

-- the internal structure is defined as follows:
-- Octets 1 to 4 : TVP. The TVP is a 32 bit time stamp. Its value is binary coded
-- and indicates the number of intervals of 100 milliseconds
-- elapsed since 1st January 2002, 0:00:00 UTC
-- Octets 5 to 10: NE-Id. The NE-Id uniquely identifies the sending network entity
-- within the PLMN. It is the entity's E.164 number without CC and
-- NDC. It is TBCD-coded, padded with zeros.
-- Octets 11 to 14: PROP. This 32 bit value is used to make the
-- InitialisationVector unique within the same TVP period.
-- The content is not standardized.
OriginalComponentIdentifier ::= CHOICE {
  operationCode  [0]  OperationCode,
  errorCode      [1]  ErrorCode,
  userInfo       [2]  NULL}

OperationCode ::= CHOICE {localValue   INTEGER,
                          globalValue  OBJECT IDENTIFIER}

ErrorCode ::= CHOICE {localValue   INTEGER,
                      globalValue  OBJECT IDENTIFIER}

END

