#################################################################################
#
# config file for YSF TX 
#
#################################################################################
# 
# YSF Encoder (C) Copyright 2017 Max H. Parke KA1RBI
# 
# This file is part of OP25
# 
# This is free software; you can redistribute it and/or modify
# it under the terms of the GNU General Public License as published by
# the Free Software Foundation; either version 3, or (at your option)
# any later version.
# 
# This software is distributed in the hope that it will be useful,
# but WITHOUT ANY WARRANTY; without even the implied warranty of
# MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
# GNU General Public License for more details.
# 
# You should have received a copy of the GNU General Public License
# along with this software; see the file COPYING.  If not, write to
# the Free Software Foundation, Inc., 51 Franklin Street,
# Boston, MA 02110-1301, USA.
#################################################################################
#
# NOTE 
#
# Syntax is unforgiving - no whitespace allowed (outside of comments)
#
# REFER TO THE Yaesu_Amateur_Radio_Digital_Specs PDF for details on field defs
# 
#################################################################################
# ft = number of frames for rolling embedded data (callsign data) in halfrate mode
# (3 bits)
ft=1
# message routing field (3 bits)
mr=0
# sq type (1 bit)
sq=0
# sc type (7 bits)
sc=0
# deviation flag (1 bit)
dev=0
# voip path (1 bit)
voip=0
#################################################################################
# call sign data fields (10 byte, except rem12 and rem34 are five byte)
#################################################################################
dest=**********
src=KA1RBI
down=down1
up=up1
rem12=rem12
rem34=rem34
