Test `CSD 9600/V.110/transparent' passed
Test `Speech, all codecs' passed
Simple TMSI encoding test....passed
Simple IMSI encoding test....passed: [10] 17 08 99 10 07 00 00 00 64 02 

Testing Mobile Identity conversions
- IMSI 123456789012345
  -> MI-TLV-hex='17081932547698103254'
  -> MI-str="123456789012345" rc=16
  -> MI-name="IMSI-123456789012345"
- IMSI 12345678901234
  -> MI-TLV-hex='170811325476981032f4'
  -> MI-str="12345678901234" rc=15
  -> MI-name="IMSI-12345678901234"
- IMSI 423423
  -> MI-TLV-hex='1704413224f3'
  -> MI-str="423423" rc=7
  -> MI-name="IMSI-423423"
- unknown 0x9 423423
  -> MI-TLV-hex='1704413224f3'
  -> MI-str="423423" rc=7
  -> MI-name="IMSI-423423"
- IMSI 4234235
  -> MI-TLV-hex='170449322453'
  -> MI-str="4234235" rc=8
  -> MI-name="IMSI-4234235"
- IMSI 4234235
  -> MI-TLV-hex='170449322453'
  -> MI-str="423" rc=4
  -> MI-name="IMSI-4234235"
- IMEI 123456789012345
  -> MI-TLV-hex='17081a32547698103254'
  -> MI-str="123456789012345" rc=16
  -> MI-name="IMEI-123456789012345"
- IMEI 98765432109876
  -> MI-TLV-hex='170892785634129078f6'
  -> MI-str="98765432109876" rc=15
  -> MI-name="IMEI-98765432109876"
- IMEI 987654321098765
  -> MI-TLV-hex='17089a78563412907856'
  -> MI-str="987654321098765" rc=16
  -> MI-name="IMEI-987654321098765"
- IMEI-SV 9876543210987654
  -> MI-TLV-hex='17099378563412907856f4'
  -> MI-str="9876543210987654" rc=17
  -> MI-name="IMEI-SV-9876543210987654"
- IMEI-SV 9876543210987654
  -> MI-TLV-hex='17099378563412907856f4'
  -> MI-str="9876543210987654" rc=17
  -> MI-name="IMEI-SV-9876543210987654"
- TMSI 305419896
  -> MI-TLV-hex='1705f412345678'
  -> MI-str="305419896" rc=9
  -> MI-name="TMSI-0x12345678"
- TMSI 12648430
  -> MI-TLV-hex='1705f400c0ffee'
  -> MI-str="12648430" rc=8
  -> MI-name="TMSI-0x00C0FFEE"
- TMSI 0
  -> MI-TLV-hex='1705f400000000'
  -> MI-str="0" rc=1
  -> MI-name="TMSI-0x00000000"
- TMSI 305419896
  -> MI-TLV-hex='1705f412345678'
  -> MI-str="3054" rc=9
  -> MI-name="TMSI-0x12345678"
- NONE 123
  -> MI-TLV-hex='17021832'
  -> MI-str="" rc=1
  -> MI-name="unknown"
- NONE 1234
  -> MI-TLV-hex='17031032f4'
  -> MI-str="" rc=1
  -> MI-name="unknown"
- unknown 0x8 1234
  -> MI-TLV-hex='17031032f4'
  -> MI-str="" rc=1
  -> MI-name="unknown"

Decoding zero length Mobile Identities
- MI type: IMSI
  - writing to zero-length string:
    rc=0
    nothing written
  - writing to 1-byte-length string:
    rc=1
    returned empty string
  - decode zero-length mi:
    rc=1
    returned empty string
- MI type: TMSI
  - writing to zero-length string:
    rc=0
    nothing written
  - writing to 1-byte-length string:
    rc=1
    returned empty string
  - decode zero-length mi:
    rc=1
    returned empty string
- MI type: NONE
  - writing to zero-length string:
    rc=0
    nothing written
  - writing to 1-byte-length string:
    rc=1
    returned empty string
  - decode zero-length mi:
    rc=1
    returned empty string
- MI type: IMSI | GSM_MI_ODD
  - writing to zero-length string:
    rc=0
    nothing written
  - writing to 1-byte-length string:
    rc=1
    returned empty string
  - decode zero-length mi:
    rc=1
    returned empty string
- MI type: TMSI | GSM_MI_ODD
  - writing to zero-length string:
    rc=0
    nothing written
  - writing to 1-byte-length string:
    rc=1
    returned empty string
  - decode zero-length mi:
    rc=1
    returned empty string
- MI type: NONE | GSM_MI_ODD
  - writing to zero-length string:
    rc=0
    nothing written
  - writing to 1-byte-length string:
    rc=1
    returned empty string
  - decode zero-length mi:
    rc=1
    returned empty string

test_struct_mobile_identity()
LU with IMSI 901700000004620: rc = 0, mi = IMSI-901700000004620 ok
LU with TMSI 0x0980ad8a: rc = 0, mi = TMSI-0x0980AD8A ok
LU with invalid MI type: rc = -22 ok
LU with truncated IMSI MI: rc = -74 ok
LU with too short IMSI MI (12345): rc = -74 ok
LU with just long enough IMSI MI 123456: rc = 0, mi = IMSI-123456 ok
LU with max length IMSI MI 123456789012345: rc = 0, mi = IMSI-123456789012345 ok
LU with just too long IMSI MI 1234567890123456: rc = -74 ok
LU with truncated TMSI MI: rc = -74 ok
LU with odd length TMSI: rc = -74 ok
LU with too long TMSI MI: rc = -74 ok
LU with too short TMSI: rc = -74 ok
CM Service Request with IMSI 123456: rc = 0, mi = IMSI-123456 ok
CM Service Request with TMSI 0x5a42e404: rc = 0, mi = TMSI-0x5A42E404 ok
CM Service Request with shorter CM2, with IMSI 123456: rc = 0, mi = IMSI-123456 ok
CM Service Request with longer CM2, with IMSI 123456: rc = 0, mi = IMSI-123456 ok
CM Service Request with shorter CM2, with TMSI 0x00000000: rc = 0, mi = TMSI-0x00000000 ok
CM Service Request with invalid MI type: rc = -22 ok
CM Service Request with truncated IMSI MI: rc = -74 ok
CM Service Request with truncated TMSI MI: rc = -74 ok
CM Service Request with odd length TMSI: rc = -74 ok
CM Service Request with too long TMSI MI: rc = -74 ok
CM Service Request with too short TMSI: rc = -74 ok
CM Service Reestablish Request with TMSI 0x5a42e404: rc = 0, mi = TMSI-0x5A42E404 ok
Paging Response with IMSI 1234567: rc = 0, mi = IMSI-1234567 ok
Paging Response with TMSI 0xb48883de: rc = 0, mi = TMSI-0xB48883DE ok
Paging Response with TMSI, with unused nibble not 0xf: rc = -74 ok
Paging Response with too short IMEI (1234567): rc = -74 ok
Paging Response with IMEI 123456789012345: rc = 0, mi = IMEI-123456789012345 ok
Paging Response with IMEI 12345678901234 (no Luhn checksum): rc = 0, mi = IMEI-12345678901234 ok
Paging Response with IMEISV 1234567890123456: rc = 0, mi = IMEI-SV-1234567890123456 ok
Paging Response with too short IMEISV 123456789012345: rc = -74 ok
Paging Response with too long IMEISV 12345678901234567: rc = -74 ok
Paging Response with IMSI 123456789012345 and flipped ODD bit: rc = -74 ok
IMSI-Detach with IMSI 901700000004620: rc = 0, mi = IMSI-901700000004620 ok
IMSI-Detach with TMSI 0x0980ad8a: rc = 0, mi = TMSI-0x0980AD8A ok
IMSI-Detach with invalid MI type: rc = -22 ok
IMSI-Detach with truncated IMSI MI: rc = -74 ok
IMSI-Detach with too short IMSI MI (12345): rc = -74 ok
IMSI-Detach with just long enough IMSI MI 123456: rc = 0, mi = IMSI-123456 ok
IMSI-Detach with max length IMSI MI 123456789012345: rc = 0, mi = IMSI-123456789012345 ok
IMSI-Detach with just too long IMSI MI 1234567890123456: rc = -74 ok
IMSI-Detach with truncated TMSI MI: rc = -74 ok
IMSI-Detach with odd length TMSI: rc = -74 ok
IMSI-Detach with too long TMSI MI: rc = -74 ok
IMSI-Detach with too short TMSI: rc = -74 ok
Identity Response with IMSI 901700000004620: rc = 0, mi = IMSI-901700000004620 ok
Identity Response with IMEI 123456789012345: rc = 0, mi = IMEI-123456789012345 ok
Identity Response with IMEISV 9876543210987654: rc = 0, mi = IMEI-SV-9876543210987654 ok

BSD number encoding / decoding test
- Running test: regular 9-digit MSISDN
  - Encoding ASCII (buffer limit=0) '123456789'...
    - Expected: (rc=6) '0521436587f9'
    -   Actual: (rc=6) '0521436587f9'
  - Decoding HEX (buffer limit=0) '0521436587f9'...
    - Expected: (rc=0) '123456789'
    -   Actual: (rc=0) '123456789'
- Running test: regular 6-digit MSISDN with optional header (LHV)
  - Encoding ASCII (buffer limit=0) '123456'...
    - Expected: (rc=8) '07ffffffff214365'
    -   Actual: (rc=8) '07ffffffff214365'
  - Decoding HEX (buffer limit=0) '07deadbeef214365'...
    - Expected: (rc=0) '123456'
    -   Actual: (rc=0) '123456'
- Running test: long 15-digit (maximum) MSISDN
  - Encoding ASCII (buffer limit=0) '123456789012345'...
    - Expected: (rc=9) '0821436587092143f5'
    -   Actual: (rc=9) '0821436587092143f5'
  - Decoding HEX (buffer limit=0) '0821436587092143f5'...
    - Expected: (rc=0) '123456789012345'
    -   Actual: (rc=0) '123456789012345'
- Running test: long 15-digit (maximum) MSISDN, limited buffer
  - Encoding ASCII (buffer limit=9) '123456789012345'...
    - Expected: (rc=9) '0821436587092143f5'
    -   Actual: (rc=9) '0821436587092143f5'
  - Decoding HEX (buffer limit=16) '0821436587092143f5'...
    - Expected: (rc=0) '123456789012345'
    -   Actual: (rc=0) '123456789012345'
- Running test: to be truncated 20-digit MSISDN
  - Encoding ASCII (buffer limit=9) '12345678901234567890'...
    - Expected: (rc=-5) ''
    -   Actual: (rc=-5) ''
  - Decoding HEX (buffer limit=16) '0a21436587092143658709'...
    - Expected: (rc=-28) '123456789012345'
    -   Actual: (rc=-28) '123456789012345'
- Running test: LV incorrect length
  - Decoding HEX (buffer limit=0) '05214365'...
    - Expected: (rc=-22) '(none)'
    -   Actual: (rc=-22) '(none)'
- Running test: empty input buffer
  - Encoding ASCII (buffer limit=0) ''...
    - Expected: (rc=1) '00'
    -   Actual: (rc=1) '00'
  - Decoding HEX (buffer limit=0) ''...
    - Expected: (rc=-5) '(none)'
    -   Actual: (rc=-5) '(none)'
- Running test: decoding buffer is one byte too small (OS#4049)
  - Decoding HEX (buffer limit=4) '022143'...
    - Expected: (rc=-28) '123'
    -   Actual: (rc=-28) '123'

Constructed RA:
077-121-666-5
MCC+MNC in BCD: 70 17 21 
077-121-666-5 (3-digit MNC)
RA test...passed
Constructed RA:
084-98-11-89
MCC+MNC in BCD: 80 f4 89 
084-98-11-89
RA test...passed
Constructed RA:
000-00-0-0
MCC+MNC in BCD: 00 f0 00 
000-00-0-0
RA test...passed
Constructed RA:
000-000-0-0 (3-digit MNC)
MCC+MNC in BCD: 00 00 00 
000-000-0-0 (3-digit MNC)
RA test...passed
Constructed RA:
999-999-65535-255
MCC+MNC in BCD: 99 99 99 
999-999-65535-255 (3-digit MNC)
RA test...passed
Constructed RA:
001-02-23-42
MCC+MNC in BCD: 00 f1 20 
001-02-23-42
RA test...passed
Constructed RA:
001-002-23-42 (3-digit MNC)
MCC+MNC in BCD: 00 21 00 
001-002-23-42 (3-digit MNC)
RA test...passed
Constructed RA:
012-34-56-78
MCC+MNC in BCD: 10 f2 43 
012-34-56-78
RA test...passed
Constructed RA:
012-034-23-42 (3-digit MNC)
MCC+MNC in BCD: 10 42 30 
012-034-23-42 (3-digit MNC)
RA test...passed
Constructed RA:
123-456-23-42
MCC+MNC in BCD: 21 63 54 
123-456-23-42 (3-digit MNC)
RA test...passed
Constructed RA:
123-456-23-42 (3-digit MNC)
MCC+MNC in BCD: 21 63 54 
123-456-23-42 (3-digit MNC)
RA test...passed
- gsm48_generate_lai() from 077-121-666-0
  Encoded 70 17 21 02 9a 
  gsm48_decode_lai() gives  077-121-666-0
  passed
- gsm48_generate_lai2() from 077-121-666
  Encoded 70 17 21 02 9a 
  gsm48_decode_lai2() gives  077-121-666 (3-digit MNC)
  passed
- gsm48_generate_lai() from 084-98-11-0
  Encoded 80 f4 89 00 0b 
  gsm48_decode_lai() gives  084-98-11-0
  passed
- gsm48_generate_lai2() from 084-98-11
  Encoded 80 f4 89 00 0b 
  gsm48_decode_lai2() gives  084-98-11
  passed
- gsm48_generate_lai() from 000-00-0-0
  Encoded 00 f0 00 00 00 
  gsm48_decode_lai() gives  000-00-0-0
  passed
- gsm48_generate_lai2() from 000-00-0
  Encoded 00 f0 00 00 00 
  gsm48_decode_lai2() gives  000-00-0
  passed
- gsm48_generate_lai() from 000-000-0-0 (3-digit MNC)
  Encoded 00 f0 00 00 00 
  gsm48_decode_lai() gives  000-00-0-0
  passed
- gsm48_generate_lai2() from 000-000-0 (3-digit MNC)
  Encoded 00 00 00 00 00 
  gsm48_decode_lai2() gives  000-000-0 (3-digit MNC)
  passed
- gsm48_generate_lai() from 999-999-65535-0
  Encoded 99 99 99 ff ff 
  gsm48_decode_lai() gives  999-999-65535-0
  passed
- gsm48_generate_lai2() from 999-999-65535
  Encoded 99 99 99 ff ff 
  gsm48_decode_lai2() gives  999-999-65535 (3-digit MNC)
  passed
- gsm48_generate_lai() from 001-02-23-0
  Encoded 00 f1 20 00 17 
  gsm48_decode_lai() gives  001-02-23-0
  passed
- gsm48_generate_lai2() from 001-02-23
  Encoded 00 f1 20 00 17 
  gsm48_decode_lai2() gives  001-02-23
  passed
- gsm48_generate_lai() from 001-002-23-0 (3-digit MNC)
  Encoded 00 f1 20 00 17 
  gsm48_decode_lai() gives  001-02-23-0
  passed
- gsm48_generate_lai2() from 001-002-23 (3-digit MNC)
  Encoded 00 21 00 00 17 
  gsm48_decode_lai2() gives  001-002-23 (3-digit MNC)
  passed
- gsm48_generate_lai() from 012-34-56-0
  Encoded 10 f2 43 00 38 
  gsm48_decode_lai() gives  012-34-56-0
  passed
- gsm48_generate_lai2() from 012-34-56
  Encoded 10 f2 43 00 38 
  gsm48_decode_lai2() gives  012-34-56
  passed
- gsm48_generate_lai() from 012-034-23-0 (3-digit MNC)
  Encoded 10 f2 43 00 17 
  gsm48_decode_lai() gives  012-34-23-0
  passed
- gsm48_generate_lai2() from 012-034-23 (3-digit MNC)
  Encoded 10 42 30 00 17 
  gsm48_decode_lai2() gives  012-034-23 (3-digit MNC)
  passed
- gsm48_generate_lai() from 123-456-23-0
  Encoded 21 63 54 00 17 
  gsm48_decode_lai() gives  123-456-23-0
  passed
- gsm48_generate_lai2() from 123-456-23
  Encoded 21 63 54 00 17 
  gsm48_decode_lai2() gives  123-456-23 (3-digit MNC)
  passed
- gsm48_generate_lai() from 123-456-23-0 (3-digit MNC)
  Encoded 21 63 54 00 17 
  gsm48_decode_lai() gives  123-456-23-0
  passed
- gsm48_generate_lai2() from 123-456-23 (3-digit MNC)
  Encoded 21 63 54 00 17 
  gsm48_decode_lai2() gives  123-456-23 (3-digit MNC)
  passed
=====cm3_1=====
mult_band_supp=06
a5_bits=00
assoc_radio_cap_1=04
assoc_radio_cap_2=01

r_support.present=0
r_support.r_gsm_assoc_radio_cap=00

hscsd_mult_slot_cap.present=0
hscsd_mult_slot_cap.mslot_class=00

ucs2_treatment=0
extended_meas_cap=0

ms_meas_cap.present=0
ms_meas_cap.sms_value=00
ms_meas_cap.sm_value=00

ms_pos_method_cap.present=1
ms_pos_method_cap.method=01

ecsd_multislot_cap.present=0
ecsd_multislot_cap.mslot_class=00

psk8_struct.present=1
psk8_struct.mod_cap=1
psk8_struct.rf_pwr_cap_1.present=1
psk8_struct.rf_pwr_cap_1.value=02
psk8_struct.rf_pwr_cap_2.present=1
psk8_struct.rf_pwr_cap_2.value=02

gsm_400_bands_supp.present=0
gsm_400_bands_supp.value=00
gsm_400_bands_supp.assoc_radio_cap=00

gsm_850_assoc_radio_cap.present=1
gsm_850_assoc_radio_cap.value=04

gsm_1900_assoc_radio_cap.present=0
gsm_1900_assoc_radio_cap.value=00

umts_fdd_rat_cap=0
umts_tdd_rat_cap=0
cdma200_rat_cap=0

dtm_gprs_multislot_cap.present=0
dtm_gprs_multislot_cap.mslot_class=00
dtm_gprs_multislot_cap.single_slot_dtm=0
dtm_gprs_multislot_cap.dtm_egprs_multislot_cap.present=0
dtm_gprs_multislot_cap.dtm_egprs_multislot_cap.mslot_class=00

single_band_supp.present=0
single_band_supp.value=0

gsm_750_assoc_radio_cap.present=0
gsm_750_assoc_radio_cap.value=00

umts_1_28_mcps_tdd_rat_cap=0
geran_feature_package=1

extended_dtm_gprs_multislot_cap.present=0
extended_dtm_gprs_multislot_cap.mslot_class=00
extended_dtm_gprs_multislot_cap.dtm_egprs_multislot_cap.present=0
extended_dtm_gprs_multislot_cap.dtm_egprs_multislot_cap.mslot_class=00

high_multislot_cap.present=0
high_multislot_cap.value=00

geran_feature_package_2=0
gmsk_multislot_power_prof=00
psk8_multislot_power_prof=00

t_gsm_400_bands_supp.present=0
t_gsm_400_bands_supp.value=00
t_gsm_400_bands_supp.assoc_radio_cap=00

dl_advanced_rx_perf=01
dtm_enhancements_cap=1

dtm_gprs_high_multislot_cap.present=0
dtm_gprs_high_multislot_cap.mslot_class=00
dtm_gprs_high_multislot_cap.offset_required=0
dtm_gprs_high_multislot_cap.dtm_egprs_high_multislot_cap.present=0
dtm_gprs_high_multislot_cap.dtm_egprs_high_multislot_cap.mslot_class=00

repeated_acch_capability=1

gsm_710_assoc_radio_cap.present=0
gsm_710_assoc_radio_cap.value=00

t_gsm_810_assoc_radio_cap.present=0
t_gsm_810_assoc_radio_cap.value=00

ciphering_mode_setting_cap=0
add_pos_cap=0
e_utra_fdd_supp=0
e_utra_tdd_supp=0
e_utra_meas_rep_supp=0
prio_resel_supp=1
utra_csg_cells_rep=0
vamos_level=01
tighter_capability=01
sel_ciph_dl_sacch=0
cs_ps_srvcc_geran_utra=00
cs_ps_srvcc_geran_eutra=00
geran_net_sharing=0
e_utra_wb_rsrq_meas_supp=0
er_band_support=0
utra_mult_band_ind_supp=0
e_utra_mult_band_ind_supp=0
extended_tsc_set_cap_supp=0
extended_earfcn_val_range=0

=====cm3_2=====
mult_band_supp=05
a5_bits=05
assoc_radio_cap_1=05
assoc_radio_cap_2=05

r_support.present=0
r_support.r_gsm_assoc_radio_cap=00

hscsd_mult_slot_cap.present=1
hscsd_mult_slot_cap.mslot_class=0a

ucs2_treatment=1
extended_meas_cap=0

ms_meas_cap.present=1
ms_meas_cap.sms_value=05
ms_meas_cap.sm_value=05

ms_pos_method_cap.present=0
ms_pos_method_cap.method=00

ecsd_multislot_cap.present=1
ecsd_multislot_cap.mslot_class=0a

psk8_struct.present=1
psk8_struct.mod_cap=0
psk8_struct.rf_pwr_cap_1.present=1
psk8_struct.rf_pwr_cap_1.value=01
psk8_struct.rf_pwr_cap_2.present=0
psk8_struct.rf_pwr_cap_2.value=00

gsm_400_bands_supp.present=1
gsm_400_bands_supp.value=01
gsm_400_bands_supp.assoc_radio_cap=05

gsm_850_assoc_radio_cap.present=0
gsm_850_assoc_radio_cap.value=00

gsm_1900_assoc_radio_cap.present=1
gsm_1900_assoc_radio_cap.value=05

umts_fdd_rat_cap=0
umts_tdd_rat_cap=1
cdma200_rat_cap=0

dtm_gprs_multislot_cap.present=1
dtm_gprs_multislot_cap.mslot_class=01
dtm_gprs_multislot_cap.single_slot_dtm=0
dtm_gprs_multislot_cap.dtm_egprs_multislot_cap.present=1
dtm_gprs_multislot_cap.dtm_egprs_multislot_cap.mslot_class=01

single_band_supp.present=0
single_band_supp.value=0

gsm_750_assoc_radio_cap.present=1
gsm_750_assoc_radio_cap.value=05

umts_1_28_mcps_tdd_rat_cap=0
geran_feature_package=1

extended_dtm_gprs_multislot_cap.present=0
extended_dtm_gprs_multislot_cap.mslot_class=00
extended_dtm_gprs_multislot_cap.dtm_egprs_multislot_cap.present=0
extended_dtm_gprs_multislot_cap.dtm_egprs_multislot_cap.mslot_class=00

high_multislot_cap.present=1
high_multislot_cap.value=01

geran_feature_package_2=1
gmsk_multislot_power_prof=01
psk8_multislot_power_prof=01

t_gsm_400_bands_supp.present=0
t_gsm_400_bands_supp.value=00
t_gsm_400_bands_supp.assoc_radio_cap=00

dl_advanced_rx_perf=01
dtm_enhancements_cap=0

dtm_gprs_high_multislot_cap.present=1
dtm_gprs_high_multislot_cap.mslot_class=02
dtm_gprs_high_multislot_cap.offset_required=1
dtm_gprs_high_multislot_cap.dtm_egprs_high_multislot_cap.present=0
dtm_gprs_high_multislot_cap.dtm_egprs_high_multislot_cap.mslot_class=00

repeated_acch_capability=1

gsm_710_assoc_radio_cap.present=0
gsm_710_assoc_radio_cap.value=00

t_gsm_810_assoc_radio_cap.present=1
t_gsm_810_assoc_radio_cap.value=05

ciphering_mode_setting_cap=0
add_pos_cap=1
e_utra_fdd_supp=0
e_utra_tdd_supp=0
e_utra_meas_rep_supp=0
prio_resel_supp=0
utra_csg_cells_rep=0
vamos_level=00
tighter_capability=00
sel_ciph_dl_sacch=0
cs_ps_srvcc_geran_utra=00
cs_ps_srvcc_geran_eutra=00
geran_net_sharing=0
e_utra_wb_rsrq_meas_supp=0
er_band_support=0
utra_mult_band_ind_supp=0
e_utra_mult_band_ind_supp=0
extended_tsc_set_cap_supp=0
extended_earfcn_val_range=0

=====cm3_3=====
mult_band_supp=02
a5_bits=0a
assoc_radio_cap_1=0a
assoc_radio_cap_2=00

r_support.present=1
r_support.r_gsm_assoc_radio_cap=02

hscsd_mult_slot_cap.present=1
hscsd_mult_slot_cap.mslot_class=0a

ucs2_treatment=1
extended_meas_cap=0

ms_meas_cap.present=1
ms_meas_cap.sms_value=05
ms_meas_cap.sm_value=05

ms_pos_method_cap.present=0
ms_pos_method_cap.method=00

ecsd_multislot_cap.present=1
ecsd_multislot_cap.mslot_class=0a

psk8_struct.present=1
psk8_struct.mod_cap=0
psk8_struct.rf_pwr_cap_1.present=1
psk8_struct.rf_pwr_cap_1.value=01
psk8_struct.rf_pwr_cap_2.present=0
psk8_struct.rf_pwr_cap_2.value=00

gsm_400_bands_supp.present=1
gsm_400_bands_supp.value=01
gsm_400_bands_supp.assoc_radio_cap=05

gsm_850_assoc_radio_cap.present=0
gsm_850_assoc_radio_cap.value=00

gsm_1900_assoc_radio_cap.present=1
gsm_1900_assoc_radio_cap.value=05

umts_fdd_rat_cap=0
umts_tdd_rat_cap=1
cdma200_rat_cap=0

dtm_gprs_multislot_cap.present=1
dtm_gprs_multislot_cap.mslot_class=01
dtm_gprs_multislot_cap.single_slot_dtm=0
dtm_gprs_multislot_cap.dtm_egprs_multislot_cap.present=1
dtm_gprs_multislot_cap.dtm_egprs_multislot_cap.mslot_class=01

single_band_supp.present=0
single_band_supp.value=0

gsm_750_assoc_radio_cap.present=1
gsm_750_assoc_radio_cap.value=05

umts_1_28_mcps_tdd_rat_cap=0
geran_feature_package=1

extended_dtm_gprs_multislot_cap.present=0
extended_dtm_gprs_multislot_cap.mslot_class=00
extended_dtm_gprs_multislot_cap.dtm_egprs_multislot_cap.present=0
extended_dtm_gprs_multislot_cap.dtm_egprs_multislot_cap.mslot_class=00

high_multislot_cap.present=1
high_multislot_cap.value=01

geran_feature_package_2=1
gmsk_multislot_power_prof=01
psk8_multislot_power_prof=01

t_gsm_400_bands_supp.present=0
t_gsm_400_bands_supp.value=00
t_gsm_400_bands_supp.assoc_radio_cap=00

dl_advanced_rx_perf=01
dtm_enhancements_cap=0

dtm_gprs_high_multislot_cap.present=1
dtm_gprs_high_multislot_cap.mslot_class=02
dtm_gprs_high_multislot_cap.offset_required=1
dtm_gprs_high_multislot_cap.dtm_egprs_high_multislot_cap.present=0
dtm_gprs_high_multislot_cap.dtm_egprs_high_multislot_cap.mslot_class=00

repeated_acch_capability=1

gsm_710_assoc_radio_cap.present=0
gsm_710_assoc_radio_cap.value=00

t_gsm_810_assoc_radio_cap.present=1
t_gsm_810_assoc_radio_cap.value=04

ciphering_mode_setting_cap=0
add_pos_cap=0
e_utra_fdd_supp=0
e_utra_tdd_supp=0
e_utra_meas_rep_supp=0
prio_resel_supp=0
utra_csg_cells_rep=0
vamos_level=00
tighter_capability=00
sel_ciph_dl_sacch=0
cs_ps_srvcc_geran_utra=00
cs_ps_srvcc_geran_eutra=00
geran_net_sharing=0
e_utra_wb_rsrq_meas_supp=0
er_band_support=0
utra_mult_band_ind_supp=0
e_utra_mult_band_ind_supp=0
extended_tsc_set_cap_supp=0
extended_earfcn_val_range=0

Element is: 2 => freqs[i] = 121
Element is: 2 => freqs[i] = 1
Element is: 0 => freqs[i] = 68
w[0]=122
w[1]=2
w[2]=69
w[3]=204
w[4]=75
w[5]=66
w[6]=60
w[7]=70
w[8]=83
w[9]=3
w[10]=24
w[11]=67
w[12]=54
w[13]=64
w[14]=70
w[15]=9
Range512: 89 4b 2a 95 65 95 55 2c a9 55 aa 55 6a 95 59 55 
Range test 0: range 511, num ARFCNs 12
range=511, arfcns_used=11, f0=1, f0_included=1
chan_list = 88 00 98 34 85 36 7c 50 22 dc 5e ec 00 00 00 00 
Decoded freqs 12 (expected 12)
Decoded: 1 12 31 51 57 91 97 98 113 117 120 125 
Range test 1: range 511, num ARFCNs 17
range=511, arfcns_used=16, f0=1, f0_included=1
chan_list = 88 00 82 7f 01 3f 7e 04 0b ff ff fc 10 41 07 e0 
Decoded freqs 17 (expected 17)
Decoded: 1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 
Range test 2: range 511, num ARFCNs 18
range=511, arfcns_used=17, f0=1, f0_included=1
chan_list = 88 00 82 7f 01 7f 7e 04 0b ff ff fc 10 41 07 ff 
Decoded freqs 18 (expected 18)
Decoded: 1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 
Range test 3: range 511, num ARFCNs 18
range=511, arfcns_used=17, f0=1, f0_included=1
chan_list = 88 00 94 3a 44 32 d7 2a 43 2a 13 94 e5 38 39 f6 
Decoded freqs 18 (expected 18)
Decoded: 1 17 31 45 58 79 81 97 113 127 213 277 287 311 331 391 417 511 
Range test 4: range 511, num ARFCNs 6
range=511, arfcns_used=5, f0=1, f0_included=1
chan_list = 88 00 8b 3c 88 b9 6b 00 00 00 00 00 00 00 00 00 
Decoded freqs 6 (expected 6)
Decoded: 1 17 31 45 58 79 
Range test 5: range 511, num ARFCNs 6
range=511, arfcns_used=5, f0=10, f0_included=1
chan_list = 88 05 08 fc 88 b9 6b 00 00 00 00 00 00 00 00 00 
Decoded freqs 6 (expected 6)
Decoded: 10 17 31 45 58 79 
Range test 6: range 1023, num ARFCNs 17
range=1023, arfcns_used=16, f0=0, f0_included=1
chan_list = 84 71 e4 ab b9 58 05 cb 39 17 fd b0 75 62 0f 2f 
Decoded freqs 17 (expected 17)
Decoded: 0 17 31 45 58 79 81 97 113 127 213 277 287 311 331 391 1023 
Range test 7: range 1023, num ARFCNs 16
range=1023, arfcns_used=16, f0=0, f0_included=0
chan_list = 80 71 e4 ab b9 58 05 cb 39 17 fd b0 75 62 0f 2f 
Decoded freqs 16 (expected 16)
Decoded: 17 31 45 58 79 81 97 113 127 213 277 287 311 331 391 1023 
Random range test: range 127, max num ARFCNs 29
Random range test: range 255, max num ARFCNs 22
Random range test: range 511, max num ARFCNs 18
Random range test: range 1023, max num ARFCNs 16
