--- test_bssmap_le_enc_dec
[0] RESET: ok (encoded len = 6)
[1] RESET ACKNOWLEDGE: ok (encoded len = 3)
[2] PERFORM LOCATION REQUEST: ok (encoded len = 41)
[3] PERFORM LOCATION RESPONSE: ok (encoded len = 13)
[4] PERFORM LOCATION RESPONSE: ok (encoded len = 6)
[5] PERFORM LOCATION RESPONSE: ok (encoded len = 7)
[6] PERFORM LOCATION ABORT: ok (encoded len = 6)
[7] CONNECTION ORIENTED INFORMATON: ok (encoded len = 8)
[8] CONNECTION ORIENTED INFORMATON: ok (encoded len = 13)
[9] CONNECTION ORIENTED INFORMATON: ok (encoded len = 10)
