===== BSSGP flow-control test START
size-max=100 oct, leak-rate=100 oct/s, queue-len=5 msgs, pdu_len=10 oct, pdu_cnt=20

0: FC IN Nr 1
0: FC OUT Nr 1
 -> 0: ok
0: FC IN Nr 2
0: FC OUT Nr 2
 -> 0: ok
0: FC IN Nr 3
0: FC OUT Nr 3
 -> 0: ok
0: FC IN Nr 4
0: FC OUT Nr 4
 -> 0: ok
0: FC IN Nr 5
0: FC OUT Nr 5
 -> 0: ok
0: FC IN Nr 6
0: FC OUT Nr 6
 -> 0: ok
0: FC IN Nr 7
0: FC OUT Nr 7
 -> 0: ok
0: FC IN Nr 8
0: FC OUT Nr 8
 -> 0: ok
0: FC IN Nr 9
0: FC OUT Nr 9
 -> 0: ok
0: FC IN Nr 10
0: FC OUT Nr 10
 -> 0: ok
0: FC IN Nr 11
 -> 0: ok
0: FC IN Nr 12
 -> 0: ok
0: FC IN Nr 13
 -> 0: ok
0: FC IN Nr 14
 -> 0: ok
0: FC IN Nr 15
 -> 0: ok
0: FC IN Nr 16
 -> -28: queue full, msg dropped.
0: FC IN Nr 17
 -> -28: queue full, msg dropped.
0: FC IN Nr 18
 -> -28: queue full, msg dropped.
0: FC IN Nr 19
 -> -28: queue full, msg dropped.
0: FC IN Nr 20
 -> -28: queue full, msg dropped.
10: FC OUT Nr 11
20: FC OUT Nr 12
30: FC OUT Nr 13
40: FC OUT Nr 14
50: FC OUT Nr 15
msgb ctx: 0 b in 1 blocks (0 b in 1 block == just the context)
===== BSSGP flow-control test END

===== BSSGP flow-control test START
size-max=100 oct, leak-rate=100 oct/s, queue-len=100 msgs, pdu_len=10 oct, pdu_cnt=20

0: FC IN Nr 1
0: FC OUT Nr 1
 -> 0: ok
0: FC IN Nr 2
0: FC OUT Nr 2
 -> 0: ok
0: FC IN Nr 3
0: FC OUT Nr 3
 -> 0: ok
0: FC IN Nr 4
0: FC OUT Nr 4
 -> 0: ok
0: FC IN Nr 5
0: FC OUT Nr 5
 -> 0: ok
0: FC IN Nr 6
0: FC OUT Nr 6
 -> 0: ok
0: FC IN Nr 7
0: FC OUT Nr 7
 -> 0: ok
0: FC IN Nr 8
0: FC OUT Nr 8
 -> 0: ok
0: FC IN Nr 9
0: FC OUT Nr 9
 -> 0: ok
0: FC IN Nr 10
0: FC OUT Nr 10
 -> 0: ok
0: FC IN Nr 11
 -> 0: ok
0: FC IN Nr 12
 -> 0: ok
0: FC IN Nr 13
 -> 0: ok
0: FC IN Nr 14
 -> 0: ok
0: FC IN Nr 15
 -> 0: ok
0: FC IN Nr 16
 -> 0: ok
0: FC IN Nr 17
 -> 0: ok
0: FC IN Nr 18
 -> 0: ok
0: FC IN Nr 19
 -> 0: ok
0: FC IN Nr 20
 -> 0: ok
10: FC OUT Nr 11
20: FC OUT Nr 12
30: FC OUT Nr 13
40: FC OUT Nr 14
50: FC OUT Nr 15
60: FC OUT Nr 16
70: FC OUT Nr 17
80: FC OUT Nr 18
90: FC OUT Nr 19
100: FC OUT Nr 20
msgb ctx: 0 b in 1 blocks (0 b in 1 block == just the context)
===== BSSGP flow-control test END

===== BSSGP flow-control test START
size-max=100 oct, leak-rate=100 oct/s, queue-len=5 msgs, pdu_len=1000 oct, pdu_cnt=20

0: FC IN Nr 1
 -> -5: PDU too large, msg dropped.
0: FC IN Nr 2
 -> -5: PDU too large, msg dropped.
0: FC IN Nr 3
 -> -5: PDU too large, msg dropped.
0: FC IN Nr 4
 -> -5: PDU too large, msg dropped.
0: FC IN Nr 5
 -> -5: PDU too large, msg dropped.
0: FC IN Nr 6
 -> -5: PDU too large, msg dropped.
0: FC IN Nr 7
 -> -5: PDU too large, msg dropped.
0: FC IN Nr 8
 -> -5: PDU too large, msg dropped.
0: FC IN Nr 9
 -> -5: PDU too large, msg dropped.
0: FC IN Nr 10
 -> -5: PDU too large, msg dropped.
0: FC IN Nr 11
 -> -5: PDU too large, msg dropped.
0: FC IN Nr 12
 -> -5: PDU too large, msg dropped.
0: FC IN Nr 13
 -> -5: PDU too large, msg dropped.
0: FC IN Nr 14
 -> -5: PDU too large, msg dropped.
0: FC IN Nr 15
 -> -5: PDU too large, msg dropped.
0: FC IN Nr 16
 -> -5: PDU too large, msg dropped.
0: FC IN Nr 17
 -> -5: PDU too large, msg dropped.
0: FC IN Nr 18
 -> -5: PDU too large, msg dropped.
0: FC IN Nr 19
 -> -5: PDU too large, msg dropped.
0: FC IN Nr 20
 -> -5: PDU too large, msg dropped.
msgb ctx: 0 b in 1 blocks (0 b in 1 block == just the context)
===== BSSGP flow-control test END

===== BSSGP flow-control test START
size-max=100 oct, leak-rate=100 oct/s, queue-len=5 msgs, pdu_len=10 oct, pdu_cnt=20

0: FC IN Nr 1
0: FC OUT Nr 1
 -> 0: ok
0: FC IN Nr 2
0: FC OUT Nr 2
 -> 0: ok
0: FC IN Nr 3
0: FC OUT Nr 3
 -> 0: ok
0: FC IN Nr 4
0: FC OUT Nr 4
 -> 0: ok
0: FC IN Nr 5
0: FC OUT Nr 5
 -> 0: ok
0: FC IN Nr 6
0: FC OUT Nr 6
 -> 0: ok
0: FC IN Nr 7
0: FC OUT Nr 7
 -> 0: ok
0: FC IN Nr 8
0: FC OUT Nr 8
 -> 0: ok
0: FC IN Nr 9
0: FC OUT Nr 9
 -> 0: ok
0: FC IN Nr 10
0: FC OUT Nr 10
 -> 0: ok
0: FC IN Nr 11
 -> 0: ok
0: FC IN Nr 12
 -> 0: ok
0: FC IN Nr 13
 -> 0: ok
0: FC IN Nr 14
 -> 0: ok
0: FC IN Nr 15
 -> 0: ok
0: FC IN Nr 16
 -> -28: queue full, msg dropped.
0: FC IN Nr 17
 -> -28: queue full, msg dropped.
0: FC IN Nr 18
 -> -28: queue full, msg dropped.
0: FC IN Nr 19
 -> -28: queue full, msg dropped.
0: FC IN Nr 20
 -> -28: queue full, msg dropped.
10: FC OUT Nr 11
20: FC OUT Nr 12
30: FC OUT Nr 13
40: FC OUT Nr 14
50: FC OUT Nr 15
msgb ctx: 0 b in 1 blocks (0 b in 1 block == just the context)
===== BSSGP flow-control test END

