############################################################################
# configs/eagle100/thttpd/defconfig
#
#   Copyright (C) 2009-2010, 2012 Gregory Nutt. All rights reserved.
#   Author: Gregory Nutt <gnutt@nuttx.org>
#
# Redistribution and use in source and binary forms, with or without
# modification, are permitted provided that the following conditions
# are met:
#
# 1. Redistributions of source code must retain the above copyright
#    notice, this list of conditions and the following disclaimer.
# 2. Redistributions in binary form must reproduce the above copyright
#    notice, this list of conditions and the following disclaimer in
#    the documentation and/or other materials provided with the
#    distribution.
# 3. Neither the name NuttX nor the names of its contributors may be
#    used to endorse or promote products derived from this software
#    without specific prior written permission.
#
# THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS
# "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT
# LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS
# FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE
# COPYRIGHT OWNER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT,
# INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING,
# BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS
# OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED
# AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT
# LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN
# ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
# POSSIBILITY OF SUCH DAMAGE.
#
############################################################################
#
# architecture selection
#
# CONFIG_ARCH - identifies the arch subdirectory and, hence, the
#   processor architecture.
# CONFIG_ARCH_family - for use in C code.  This identifies the
#   particular chip family that the architecture is implemented
#   in.
# CONFIG_ARCH_architecture - for use in C code.  This identifies the
#   specific architecture within the chip familyl.
# CONFIG_ARCH_CHIP - Identifies the arch/*/chip subdirectory
# CONFIG_ARCH_CHIP_name - For use in C code
# CONFIG_ARCH_BOARD - identifies the configs subdirectory and, hence,
#   the board that supports the particular chip or SoC.
# CONFIG_ARCH_BOARD_name - for use in C code
# CONFIG_ENDIAN_BIG - define if big endian (default is little endian)
# CONFIG_BOARD_LOOPSPERMSEC - for delay loops
# CONFIG_DRAM_SIZE - Describes the installed DRAM.
# CONFIG_DRAM_START - The start address of DRAM (physical)
# CONFIG_DRAM_END - Last address+1 of installed RAM
# CONFIG_ARCH_IRQPRIO - The LM3S6918 supports interrupt prioritization
# CONFIG_ARCH_INTERRUPTSTACK - This architecture supports an interrupt
#   stack. If defined, this symbol is the size of the interrupt
#   stack in bytes.  If not defined, the user task stacks will be
#   used during interrupt handling.
# CONFIG_ARCH_STACKDUMP - Do stack dumps after assertions
# CONFIG_ARCH_BOOTLOADER - Configure to use the MicroMint Eagle-100
#   Ethernet bootloader.
# CONFIG_ARCH_LEDS -  Use LEDs to show state. Unique to board architecture.
# CONFIG_ARCH_CALIBRATION - Enables some build in instrumentation that
#   cause a 100 second delay during boot-up.  This 100 second delay
#   serves no purpose other than it allows you to calibratre
#   CONFIG_BOARD_LOOPSPERMSEC.  You simply use a stop watch to measure
#   the 100 second delay then adjust CONFIG_BOARD_LOOPSPERMSEC until
#   the delay actually is 100 seconds.
#
CONFIG_ARCH=arm
CONFIG_ARCH_ARM=y
CONFIG_ARCH_CORTEXM3=y
CONFIG_ARCH_CHIP=lm3s
CONFIG_ARCH_CHIP_LM3S6918=y
CONFIG_ARCH_BOARD=eagle100
CONFIG_ARCH_BOARD_EAGLE100=y
CONFIG_BOARD_LOOPSPERMSEC=4531
CONFIG_DRAM_SIZE=0x00010000
CONFIG_DRAM_START=0x20000000
CONFIG_DRAM_END=(CONFIG_DRAM_START+CONFIG_DRAM_SIZE)
CONFIG_ARCH_IRQPRIO=y
CONFIG_ARCH_INTERRUPTSTACK=n
CONFIG_ARCH_STACKDUMP=y
CONFIG_ARCH_BOOTLOADER=y
CONFIG_ARCH_LEDS=y
CONFIG_ARCH_CALIBRATION=n

#
# Disable support for interrupts on GPIOJ which does not
# exist on the LM3S6918.  Additional interrupt support can be
# disabled if desired to reduce memory footprint.
CONFIG_LM3S_DISABLE_GPIOA_IRQS=n
CONFIG_LM3S_DISABLE_GPIOB_IRQS=n
CONFIG_LM3S_DISABLE_GPIOC_IRQS=n
CONFIG_LM3S_DISABLE_GPIOD_IRQS=n
CONFIG_LM3S_DISABLE_GPIOE_IRQS=n
CONFIG_LM3S_DISABLE_GPIOF_IRQS=n
CONFIG_LM3S_DISABLE_GPIOG_IRQS=n
CONFIG_LM3S_DISABLE_GPIOH_IRQS=n
CONFIG_LM3S_DISABLE_GPIOJ_IRQS=y

#
# LM3S6918 specific serial device driver settings
#
# CONFIG_UARTn_DISABLE - select to disable all support for
#   the UART
# CONFIG_UARTn_SERIAL_CONSOLE - selects the UARTn for the
#   console and ttys0 (default is the UART0).
# CONFIG_UARTn_RXBUFSIZE - Characters are buffered as received.
#   This specific the size of the receive buffer
# CONFIG_UARTn_TXBUFSIZE - Characters are buffered before
#   being sent.  This specific the size of the transmit buffer
# CONFIG_UARTn_BAUD - The configure BAUD of the UART.  Must be
# CONFIG_UARTn_BITS - The number of bits.  Must be either 7 or 8.
# CONFIG_UARTn_PARTIY - 0=no parity, 1=odd parity, 2=even parity
# CONFIG_UARTn_2STOP - Two stop bits
#
CONFIG_UART0_DISABLE=n
CONFIG_UART1_DISABLE=y
CONFIG_UART0_SERIAL_CONSOLE=y
CONFIG_UART1_SERIAL_CONSOLE=n
CONFIG_UART0_TXBUFSIZE=256
CONFIG_UART1_TXBUFSIZE=256
CONFIG_UART0_RXBUFSIZE=256
CONFIG_UART1_RXBUFSIZE=256
CONFIG_UART0_BAUD=115200
CONFIG_UART1_BAUD=115200
CONFIG_UART0_BITS=8
CONFIG_UART1_BITS=8
CONFIG_UART0_PARITY=0
CONFIG_UART1_PARITY=0
CONFIG_UART0_2STOP=0
CONFIG_UART1_2STOP=0

#
# LM3S6918 specific SSI device driver settings
#
# CONFIG_SSIn_DISABLE - select to disable all support for
#   the SSI
# CONFIG_SSI_POLLWAIT - Select to disable interrupt driven SSI support
#   Poll-waiting is recommended if the interrupt rate would be to
#   high in the interrupt driven case.
# CONFIG_SSI_TXLIMIT - Write this many words to the Tx FIFO before
#   emptying the Rx FIFO.  If the SPI frequency is high and this
#   value is large, then larger values of this setting may cause
#   Rx FIFO overrun errors.  Default: half of the Tx FIFO size (4).
#
CONFIG_SSI0_DISABLE=n
CONFIG_SSI1_DISABLE=y
CONFIG_SSI_POLLWAIT=y
#CONFIG_SSI_TXLIMIT=4

#
# LM3S6918 specific serial device driver settings
#
# CONFIG_LM3S_ETHERNET - This must be set (along with CONFIG_NET)
#   to build the LM3S Ethernet driver
# CONFIG_LM3S_ETHLEDS - Enable to use Ethernet LEDs on the board.
# CONFIG_LM3S_BOARDMAC - If the board-specific logic can provide
#   a MAC address (via lm3s_ethernetmac()), then this should be selected.
# CONFIG_LM3S_ETHHDUPLEX - Set to force half duplex operation
# CONFIG_LM3S_ETHNOAUTOCRC - Set to suppress auto-CRC generation
# CONFIG_LM3S_ETHNOPAD - Set to suppress Tx padding
# CONFIG_LM3S_MULTICAST - Set to enable multicast frames
# CONFIG_LM3S_PROMISCUOUS - Set to enable promiscuous mode
# CONFIG_LM3S_BADCRC - Set to enable bad CRC rejection.
# CONFIG_LM3S_DUMPPACKET - Dump each packet received/sent to the console.
#
CONFIG_LM3S_ETHERNET=y
CONFIG_LM3S_ETHLEDS=n
CONFIG_LM3S_BOARDMAC=y
CONFIG_LM3S_ETHHDUPLEX=n
CONFIG_LM3S_ETHNOAUTOCRC=n
CONFIG_LM3S_ETHNOPAD=n
CONFIG_LM3S_MULTICAST=n
CONFIG_LM3S_PROMISCUOUS=n
CONFIG_LM3S_BADCRC=n
CONFIG_LM3S_DUMPPACKET=n

#
# General build options
#
# CONFIG_RRLOAD_BINARY - make the rrload binary format used with
#   BSPs from www.ridgerun.com using the tools/mkimage.sh script
# CONFIG_INTELHEX_BINARY - make the Intel HEX binary format
#   used with many different loaders using the GNU objcopy program
#   Should not be selected if you are not using the GNU toolchain.
# CONFIG_MOTOROLA_SREC - make the Motorola S-Record binary format
#   used with many different loaders using the GNU objcopy program
#   Should not be selected if you are not using the GNU toolchain.
# CONFIG_RAW_BINARY - make a raw binary format file used with many
#   different loaders using the GNU objcopy program.  This option
#   should not be selected if you are not using the GNU toolchain.
# CONFIG_HAVE_LIBM - toolchain supports libm.a
#
CONFIG_RRLOAD_BINARY=n
CONFIG_INTELHEX_BINARY=n
CONFIG_MOTOROLA_SREC=n
CONFIG_RAW_BINARY=y
CONFIG_HAVE_LIBM=n

#
# General OS setup
#
# CONFIG_APPS_DIR - Identifies the relative path to the directory
#   that builds the application to link with NuttX.  Default: ../apps
# CONFIG_DEBUG - enables built-in debug options
# CONFIG_DEBUG_VERBOSE - enables verbose debug output
# CONFIG_DEBUG_SYMBOLS - build without optimization and with
#   debug symbols (needed for use with a debugger).
# CONFIG_MM_REGIONS - If the architecture includes multiple
#   regions of memory to allocate from, this specifies the
#   number of memory regions that the memory manager must
#   handle and enables the API mm_addregion(start, end);
# CONFIG_ARCH_LOWPUTC - architecture supports low-level, boot
#   time console output
# CONFIG_MSEC_PER_TICK - The default system timer is 100Hz
#   or MSEC_PER_TICK=10.  This setting may be defined to
#   inform NuttX that the processor hardware is providing
#   system timer interrupts at some interrupt interval other
#   than 10 msec.
# CONFIG_RR_INTERVAL - The round robin timeslice will be set
#   this number of milliseconds;  Round robin scheduling can
#   be disabled by setting this value to zero.
# CONFIG_SCHED_INSTRUMENTATION - enables instrumentation in 
#   scheduler to monitor system performance
# CONFIG_TASK_NAME_SIZE - Spcifies that maximum size of a
#   task name to save in the TCB.  Useful if scheduler
#   instrumentation is selected.  Set to zero to disable.
# CONFIG_START_YEAR, CONFIG_START_MONTH, CONFIG_START_DAY -
#   Used to initialize the internal time logic.
# CONFIG_GREGORIAN_TIME - Enables Gregorian time conversions.
#   You would only need this if you are concerned about accurate
#   time conversions in the past or in the distant future.
# CONFIG_JULIAN_TIME - Enables Julian time conversions. You
#   would only need this if you are concerned about accurate
#   time conversion in the distand past.  You must also define
#   CONFIG_GREGORIAN_TIME in order to use Julian time.
# CONFIG_DEV_CONSOLE - Set if architecture-specific logic
#   provides /dev/console.  Enables stdout, stderr, stdin.
# CONFIG_DEV_LOWCONSOLE - Use the simple, low-level serial console
#   driver (minimul support)
# CONFIG_MUTEX_TYPES: Set to enable support for recursive and
#   errorcheck mutexes. Enables pthread_mutexattr_settype().
# CONFIG_PRIORITY_INHERITANCE : Set to enable support for priority
#   inheritance on mutexes and semaphores. 
# CONFIG_SEM_PREALLOCHOLDERS: This setting is only used if priority
#   inheritance is enabled.  It defines the maximum number of
#   different threads (minus one) that can take counts on a
#   semaphore with priority inheritance support.  This may be 
#   set to zero if priority inheritance is disabled OR if you
#   are only using semaphores as mutexes (only one holder) OR
#   if no more than two threads participate using a counting
#   semaphore.
# CONFIG_SEM_NNESTPRIO.  If priority inheritance is enabled,
#   then this setting is the maximum number of higher priority
#   threads (minus 1) than can be waiting for another thread
#   to release a count on a semaphore.  This value may be set
#   to zero if no more than one thread is expected to wait for
#   a semaphore.
# CONFIG_FDCLONE_DISABLE. Disable cloning of all file descriptors
#   by task_create() when a new task is started.  If set, all
#   files/drivers will appear to be closed in the new task.
# CONFIG_FDCLONE_STDIO. Disable cloning of all but the first
#   three file descriptors (stdin, stdout, stderr) by task_create()
#   when a new task is started. If set, all files/drivers will
#   appear to be closed in the new task except for stdin, stdout,
#   and stderr.
# CONFIG_SDCLONE_DISABLE. Disable cloning of all socket
#   desciptors by task_create() when a new task is started. If
#   set, all sockets will appear to be closed in the new task.
#
#CONFIG_APPS_DIR=
CONFIG_DEBUG=n
CONFIG_DEBUG_VERBOSE=n
CONFIG_DEBUG_SYMBOLS=n
CONFIG_DEBUG_NET=y
CONFIG_MM_REGIONS=1
CONFIG_ARCH_LOWPUTC=y
CONFIG_RR_INTERVAL=200
CONFIG_SCHED_INSTRUMENTATION=n
CONFIG_TASK_NAME_SIZE=0
CONFIG_START_YEAR=2009
CONFIG_START_MONTH=7
CONFIG_START_DAY=12
CONFIG_GREGORIAN_TIME=n
CONFIG_JULIAN_TIME=n
CONFIG_DEV_CONSOLE=y
CONFIG_DEV_LOWCONSOLE=y
CONFIG_MUTEX_TYPES=n
CONFIG_PRIORITY_INHERITANCE=n
CONFIG_SEM_PREALLOCHOLDERS=0
CONFIG_SEM_NNESTPRIO=0
CONFIG_FDCLONE_DISABLE=n
CONFIG_FDCLONE_STDIO=n
CONFIG_SDCLONE_DISABLE=n

#
# Settings for examples/nxflat
# CONFIG_NXFLAT. Enable support for the NXFLAT binary format.
#  This format will support execution of NuttX binaries located
#  in a ROMFS filesystem (see examples/nxflat).
# CONFIG_NXFLAT_DUMPBUFFER. Dump a most buffers that NXFFLAT deals
#  with.  CONFIG_DEBUG, CONFIG_DEBUG_VERBOSE, and
#  CONFIG_DEBUG_BINFMT have to be defined or
#  CONFIG_NXFLAT_DUMPBUFFER does nothing.
# CONFIG_SYMTAB_ORDEREDBYNAME. Select if the system symbol table
#  is ordered by symbol name
#
CONFIG_NXFLAT=y
CONFIG_NXFLAT_DUMPBUFFER=n
CONFIG_SYMTAB_ORDEREDBYNAME=y

#
# The following can be used to disable categories of
# APIs supported by the OS.  If the compiler supports
# weak functions, then it should not be necessary to
# disable functions unless you want to restrict usage
# of those APIs.
#
# There are certain dependency relationships in these
# features.
#
# o mq_notify logic depends on signals to awaken tasks
#   waiting for queues to become full or empty.
# o pthread_condtimedwait() depends on signals to wake
#   up waiting tasks.
#
CONFIG_DISABLE_CLOCK=n
CONFIG_DISABLE_POSIX_TIMERS=y
CONFIG_DISABLE_PTHREAD=y
CONFIG_DISABLE_SIGNALS=n
CONFIG_DISABLE_MQUEUE=y
CONFIG_DISABLE_MOUNTPOINT=n
CONFIG_DISABLE_ENVIRON=n
CONFIG_DISABLE_POLL=n

#
# Misc libc settings
#
# CONFIG_NOPRINTF_FIELDWIDTH - sprintf-related logic is a
#   little smaller if we do not support fieldwidthes
#
CONFIG_NOPRINTF_FIELDWIDTH=n

#
# Allow for architecture optimized implementations
#
# The architecture can provide optimized versions of the
# following to improve system performance
#
CONFIG_ARCH_MEMCPY=n
CONFIG_ARCH_MEMCMP=n
CONFIG_ARCH_MEMMOVE=n
CONFIG_ARCH_MEMSET=n
CONFIG_ARCH_STRCMP=n
CONFIG_ARCH_STRCPY=n
CONFIG_ARCH_STRNCPY=n
CONFIG_ARCH_STRLEN=n
CONFIG_ARCH_STRNLEN=n
CONFIG_ARCH_BZERO=n

#
# Sizes of configurable things (0 disables)
#
# CONFIG_MAX_TASKS - The maximum number of simultaneously
#   active tasks.  This value must be a power of two.
# CONFIG_MAX_TASK_ARGS - This controls the maximum number of
#   of parameters that a task may receive (i.e., maxmum value
#   of 'argc')
# CONFIG_NPTHREAD_KEYS - The number of items of thread-
#   specific data that can be retained
# CONFIG_NFILE_DESCRIPTORS - The maximum number of file
#   descriptors (one for each open)
# CONFIG_NFILE_STREAMS - The maximum number of streams that
#   can be fopen'ed
# CONFIG_NAME_MAX - The maximum size of a file name.
# CONFIG_STDIO_BUFFER_SIZE - Size of the buffer to allocate
#   on fopen. (Only if CONFIG_NFILE_STREAMS > 0)
# CONFIG_NUNGET_CHARS - Number of characters that can be
#   buffered by ungetc() (Only if CONFIG_NFILE_STREAMS > 0)
# CONFIG_PREALLOC_MQ_MSGS - The number of pre-allocated message
#   structures.  The system manages a pool of preallocated
#   message structures to minimize dynamic allocations
# CONFIG_MQ_MAXMSGSIZE - Message structures are allocated with
#   a fixed payload size given by this settin (does not include
#   other message structure overhead.
# CONFIG_MAX_WDOGPARMS - Maximum number of parameters that
#   can be passed to a watchdog handler
# CONFIG_PREALLOC_WDOGS - The number of pre-allocated watchdog
#   structures.  The system manages a pool of preallocated
#   watchdog structures to minimize dynamic allocations
# CONFIG_PREALLOC_TIMERS - The number of pre-allocated POSIX
#   timer structures.  The system manages a pool of preallocated
#   timer structures to minimize dynamic allocations.  Set to
#   zero for all dynamic allocations.
#
CONFIG_MAX_TASKS=16
CONFIG_MAX_TASK_ARGS=4
CONFIG_NPTHREAD_KEYS=0
CONFIG_NFILE_DESCRIPTORS=8
CONFIG_NFILE_STREAMS=8
CONFIG_NAME_MAX=32
CONFIG_STDIO_BUFFER_SIZE=64
CONFIG_NUNGET_CHARS=0
CONFIG_PREALLOC_MQ_MSGS=0
CONFIG_MQ_MAXMSGSIZE=0
CONFIG_MAX_WDOGPARMS=2
CONFIG_PREALLOC_WDOGS=8
CONFIG_PREALLOC_TIMERS=8

#
# Filesystem configuration
#
# CONFIG_FS_FAT - Enable FAT filesystem support
# CONFIG_FAT_SECTORSIZE - Max supported sector size
# CONFIG_FS_ROMFS - Enable ROMFS filesystem support
CONFIG_FS_FAT=n
CONFIG_FS_ROMFS=y

#
# SPI-based MMC/SD driver
#
# CONFIG_MMCSD_NSLOTS
#   Number of MMC/SD slots supported by the driver
# CONFIG_MMCSD_READONLY
#   Provide read-only access (default is read/write)
# CONFIG_MMCSD_SPICLOCK - Maximum SPI clock to drive MMC/SD card.
#   Default is 20MHz.
#
CONFIG_MMCSD_NSLOTS=1
CONFIG_MMCSD_READONLY=n
CONFIG_MMCSD_SPICLOCK=12500000

#
# TCP/IP and UDP support via uIP
# CONFIG_NET - Enable or disable all network features
# CONFIG_NET_IPv6 - Build in support for IPv6
# CONFIG_NSOCKET_DESCRIPTORS - Maximum number of socket descriptors per task/thread.
# CONFIG_NET_SOCKOPTS - Enable or disable support for socket options
# CONFIG_NET_BUFSIZE - uIP buffer size
# CONFIG_NET_TCP - TCP support on or off
# CONFIG_NET_TCP_CONNS - Maximum number of TCP connections (all tasks)
# CONFIG_NET_TCP_READAHEAD_BUFSIZE - Size of TCP read-ahead buffers
# CONFIG_NET_NTCP_READAHEAD_BUFFERS - Number of TCP read-ahead buffers (may be zero)
# CONFIG_NET_TCPBACKLOG - Incoming connections pend in a backlog until
#   accept() is called. The size of the backlog is selected when listen() is called.
# CONFIG_NET_MAX_LISTENPORTS - Maximum number of listening TCP ports (all tasks)
# CONFIG_NET_UDP - UDP support on or off
# CONFIG_NET_UDP_CHECKSUMS - UDP checksums on or off
# CONFIG_NET_UDP_CONNS - The maximum amount of concurrent UDP connections
# CONFIG_NET_ICMP - ICMP ping response support on or off
# CONFIG_NET_ICMP_PING - ICMP ping request support on or off
# CONFIG_NET_PINGADDRCONF - Use "ping" packet for setting IP address
# CONFIG_NET_STATISTICS - uIP statistics on or off
# CONFIG_NET_RECEIVE_WINDOW - The size of the advertised receiver's window
# CONFIG_NET_ARPTAB_SIZE - The size of the ARP table
# CONFIG_NET_BROADCAST - Broadcast support
# CONFIG_NET_FWCACHE_SIZE - number of packets to remember when looking for duplicates
#
CONFIG_NET=y
CONFIG_NET_IPv6=n
CONFIG_NSOCKET_DESCRIPTORS=16
CONFIG_NET_SOCKOPTS=y
CONFIG_NET_BUFSIZE=420
CONFIG_NET_TCP=y
CONFIG_NET_TCP_CONNS=16
CONFIG_NET_NTCP_READAHEAD_BUFFERS=8
CONFIG_NET_TCPBACKLOG=y
CONFIG_NET_MAX_LISTENPORTS=8
CONFIG_NET_UDP=n
CONFIG_NET_UDP_CHECKSUMS=y
#CONFIG_NET_UDP_CONNS=10
CONFIG_NET_ICMP=y
CONFIG_NET_ICMP_PING=n
#CONFIG_NET_PINGADDRCONF=0
CONFIG_NET_STATISTICS=n
#CONFIG_NET_RECEIVE_WINDOW=
#CONFIG_NET_ARPTAB_SIZE=8
CONFIG_NET_BROADCAST=n
#CONFIG_NET_FWCACHE_SIZE=2

#
# UIP Network Utilities
# CONFIG_NET_DHCP_LIGHT - Reduces size of DHCP
# CONFIG_NET_RESOLV_ENTRIES - Number of resolver entries
#
CONFIG_NET_DHCP_LIGHT=n
CONFIG_NET_RESOLV_ENTRIES=4

#
# THTTPD settings
#
# CONFIG_THTTPD_PORT - THTTPD Server port number
# CONFIG_THTTPD_IPADDR - Server IP address (no host name)
# CONFIG_THTTPD_SERVER_ADDRESS - SERVER_ADDRESS: response
# CONFIG_THTTPD_SERVER_SOFTWARE - SERVER_SOFTWARE: response
# CONFIG_THTTPD_PATH - Server working directory
# CONFIG_THTTPD_CGI_PATH - Path to CGI executables
# CONFIG_THTTPD_CGI_PATTERN - Only CGI programs matching this
#   pattern will be executed.  In fact, if this value is not defined
#   then no CGI logic will be built.
# CONFIG_THTTPD_CGI_PRIORITY - Provides the priority of CGI child tasks
# CONFIG_THTTPD_CGI_STACKSIZE - Provides the initial stack size of
#   CGI child task (will be overridden by the stack size in the NXFLAT
#   header)
# CONFIG_THTTPD_CGI_BYTECOUNT - Byte output limit for CGI tasks.
# CONFIG_THTTPD_CGI_TIMELIMIT - How many seconds to allow CGI programs
#   to run before killing them.
# CONFIG_THTTPD_CHARSET- The default character set name to use with
#   text MIME types.
# CONFIG_THTTPD_IOBUFFERSIZE - 
# CONFIG_THTTPD_INDEX_NAMES - A list of index filenames to check. The
#   files are searched for in this order.
# CONFIG_AUTH_FILE - The file to use for authentication. If this is
#   defined then thttpd checks for this file in the local directory
#   before every fetch. If the file exists then authentication is done,
#   otherwise the fetch proceeds as usual. If you leave this undefined
#   then thttpd will not implement authentication at all and will not
#   check for auth files, which saves a bit of CPU time. A typical
#   value is ".htpasswd"
# CONFIG_THTTPD_LISTEN_BACKLOG - The listen() backlog queue length.
# CONFIG_THTTPD_LINGER_MSEC - How many milliseconds to leave a connection
#   open while doing a lingering close.
# CONFIG_THTTPD_OCCASIONAL_MSEC - How often to run the occasional
#   cleanup job.
# CONFIG_THTTPD_IDLE_READ_LIMIT_SEC - How many seconds to allow for
#  reading the initial request on a new connection.
# CONFIG_THTTPD_IDLE_SEND_LIMIT_SEC - How many seconds before an
#   idle connection gets closed.
# CONFIG_THTTPD_TILDE_MAP1 and CONFIG_THTTPD_TILDE_MAP2 - Tilde mapping.
#   Many URLs use ~username to indicate a user's home directory. thttpd
#   provides two options for mapping this construct to an  actual filename.
#   1) Map ~username to <prefix>/username. This is the recommended choice.
#     Each user gets a subdirectory in the main web tree, and the tilde
#     construct points there. The prefix could be something like "users",
#     or it could be empty.
#   2) Map ~username to <user's homedir>/<postfix>. The postfix would be
#     the name of a subdirectory off of the user's actual home dir,
#     something like "public_html".
#   You can also leave both options undefined, and thttpd will not do
#   anything special about tildes. Enabling both options is an error.
#   Typical values, if they're defined, are "users" for
#   CONFIG_THTTPD_TILDE_MAP1 and "public_html"forCONFIG_THTTPD_TILDE_MAP2. 
# CONFIG_THTTPD_GENERATE_INDICES
# CONFIG_THTTPD_URLPATTERN - If defined, then it will be used to match
#   and verify referrers.
CONFIG_THTTPD_PORT=80
CONFIG_THTTPD_IPADDR=(10<<24|0<<16|0<<8|2)
CONFIG_THTTPD_SERVER_ADDRESS="http://www.nuttx.org"
CONFIG_THTTPD_SERVER_SOFTWARE="thttpd/2.25b 29dec2003-NuttX"
CONFIG_THTTPD_PATH="/mnt/www"
CONFIG_THTTPD_CGI_PATH="/mnt/www/cgi-bin"
CONFIG_THTTPD_CGI_PATTERN="/mnt/www/cgi-bin/*"
CONFIG_THTTPD_CGI_PRIORITY=50
CONFIG_THTTPD_CGI_STACKSIZE=1024
CONFIG_THTTPD_CGI_BYTECOUNT=20000
CONFIG_THTTPD_CGI_TIMELIMIT=0
CONFIG_THTTPD_CHARSET="iso-8859-1"
CONFIG_THTTPD_IOBUFFERSIZE=1024
#CONFIG_THTTPD_INDEX_NAMES
CONFIG_AUTH_FILE=n
CONFIG_THTTPD_LISTEN_BACKLOG=8
CONFIG_THTTPD_LINGER_MSEC=500
CONFIG_THTTPD_OCCASIONAL_MSEC=120
CONFIG_THTTPD_IDLE_READ_LIMIT_SEC=300
CONFIG_THTTPD_IDLE_SEND_LIMIT_SEC=300
CONFIG_THTTPD_TILDE_MAP1=n
CONFIG_THTTPD_TILDE_MAP2=n
CONFIG_THTTPD_GENERATE_INDICES=n
CONFIG_THTTPD_URLPATTERN=n

#
# Additional settings for examples/thttpd
#
CONFIG_EXAMPLE_THTTPD_NOMAC=n
CONFIG_EXAMPLE_THTTPD_DRIPADDR=(10<<24|0<<16|0<<8|1)
CONFIG_EXAMPLE_THTTPD_NETMASK=(255<<24|255<<16|255<<8|0)

#
# Settings for examples/uip
#
CONFIG_EXAMPLE_UIP_IPADDR=(10<<24|0<<16|0<<8|2)
CONFIG_EXAMPLE_UIP_DRIPADDR=(10<<24|0<<16|0<<8|1)
CONFIG_EXAMPLE_UIP_NETMASK=(255<<24|255<<16|255<<8|0)
CONFIG_EXAMPLE_UIP_DHCPC=n

#
# Settings for examples/nettest
CONFIG_EXAMPLE_NETTEST_SERVER=n
CONFIG_EXAMPLE_NETTEST_PERFORMANCE=n
CONFIG_EXAMPLE_NETTEST_NOMAC=n
CONFIG_EXAMPLE_NETTEST_IPADDR=(10<<24|0<<16|0<<8|2)
CONFIG_EXAMPLE_NETTEST_DRIPADDR=(10<<24|0<<16|0<<8|1)
CONFIG_EXAMPLE_NETTEST_NETMASK=(255<<24|255<<16|255<<8|0)
CONFIG_EXAMPLE_NETTEST_CLIENTIP=(10<<24|0<<16|0<<8|1)

#
# Settings for examples/ostest
#
CONFIG_EXAMPLES_OSTEST_LOOPS=1
CONFIG_EXAMPLES_OSTEST_STACKSIZE=2048
CONFIG_EXAMPLES_OSTEST_NBARRIER_THREADS=3

#
# Settings for apps/nshlib
#
# CONFIG_NSH_FILEIOSIZE - Size of a static I/O buffer
# CONFIG_NSH_STRERROR - Use strerror(errno)
# CONFIG_NSH_LINELEN - Maximum length of one command line
# CONFIG_NSH_NESTDEPTH - Max number of nested if-then[-else]-fi
# CONFIG_NSH_DISABLESCRIPT - Disable scripting support
# CONFIG_NSH_DISABLEBG - Disable background commands
# CONFIG_NSH_ROMFSETC - Use startup script in /etc
# CONFIG_NSH_CONSOLE - Use serial console front end
# CONFIG_NSH_TELNET - Use telnetd console front end
# CONFIG_NSH_ARCHINIT - Platform provides architecture
#   specific initialization (nsh_archinitialize()).
#
# If CONFIG_NSH_TELNET is selected:
# CONFIG_NSH_IOBUFFER_SIZE -- Telnetd I/O buffer size
# CONFIG_NSH_DHCPC - Obtain address using DHCP
# CONFIG_NSH_IPADDR - Provides static IP address
# CONFIG_NSH_DRIPADDR - Provides static router IP address
# CONFIG_NSH_NETMASK - Provides static network mask
# CONFIG_NSH_NOMAC - Use a bogus MAC address
#
# If CONFIG_NSH_ROMFSETC is selected:
# CONFIG_NSH_ROMFSMOUNTPT - ROMFS mountpoint
# CONFIG_NSH_INITSCRIPT - Relative path to init script
# CONFIG_NSH_ROMFSDEVNO - ROMFS RAM device minor
# CONFIG_NSH_ROMFSSECTSIZE - ROMF sector size
# CONFIG_NSH_FATDEVNO - FAT FS RAM device minor
# CONFIG_NSH_FATSECTSIZE - FAT FS sector size
# CONFIG_NSH_FATNSECTORS - FAT FS number of sectors
# CONFIG_NSH_FATMOUNTPT - FAT FS mountpoint
#
CONFIG_NSH_FILEIOSIZE=512
CONFIG_NSH_STRERROR=n
CONFIG_NSH_LINELEN=64
CONFIG_NSH_NESTDEPTH=3
CONFIG_NSH_DISABLESCRIPT=n
CONFIG_NSH_DISABLEBG=n
CONFIG_NSH_ROMFSETC=n
CONFIG_NSH_CONSOLE=y
CONFIG_NSH_TELNET=n
CONFIG_NSH_ARCHINIT=n
CONFIG_NSH_IOBUFFER_SIZE=512
CONFIG_NSH_DHCPC=n
CONFIG_NSH_NOMAC=n
CONFIG_NSH_IPADDR=(10<<24|0<<16|0<<8|2)
CONFIG_NSH_DRIPADDR=(10<<24|0<<16|0<<8|1)
CONFIG_NSH_NETMASK=(255<<24|255<<16|255<<8|0)
CONFIG_NSH_ROMFSMOUNTPT="/etc"
CONFIG_NSH_INITSCRIPT="init.d/rcS"
CONFIG_NSH_ROMFSDEVNO=0
CONFIG_NSH_ROMFSSECTSIZE=64
CONFIG_NSH_FATDEVNO=1
CONFIG_NSH_FATSECTSIZE=512
CONFIG_NSH_FATNSECTORS=1024
CONFIG_NSH_FATMOUNTPT=/tmp

#
# Architecture-specific NSH options
#
CONFIG_NSH_MMCSDSPIPORTNO=0
CONFIG_NSH_MMCSDSLOTNO=0
CONFIG_NSH_MMCSDMINOR=0

#
# Stack and heap information
#
# CONFIG_BOOT_RUNFROMFLASH - Some configurations support XIP
#   operation from FLASH but must copy initialized .data sections to RAM.
#   (should also be =n for the Eagle100 which always runs from flash)
# CONFIG_BOOT_COPYTORAM -  Some configurations boot in FLASH
#   but copy themselves entirely into RAM for better performance.
# CONFIG_CUSTOM_STACK - The up_ implementation will handle
#   all stack operations outside of the nuttx model.
# CONFIG_STACK_POINTER - The initial stack pointer (arm7tdmi only)
# CONFIG_IDLETHREAD_STACKSIZE - The size of the initial stack.
#  This is the thread that (1) performs the inital boot of the system up
#  to the point where user_start() is spawned, and (2) there after is the
#  IDLE thread that executes only when there is no other thread ready to
#  run.
# CONFIG_USERMAIN_STACKSIZE - The size of the stack to allocate
#  for the main user thread that begins at the user_start() entry point.
# CONFIG_PTHREAD_STACK_MIN - Minimum pthread stack size
# CONFIG_PTHREAD_STACK_DEFAULT - Default pthread stack size
# CONFIG_HEAP_BASE - The beginning of the heap
# CONFIG_HEAP_SIZE - The size of the heap
#
CONFIG_BOOT_RUNFROMFLASH=n
CONFIG_BOOT_COPYTORAM=n
CONFIG_CUSTOM_STACK=n
CONFIG_STACK_POINTER=
CONFIG_IDLETHREAD_STACKSIZE=1024
CONFIG_USERMAIN_STACKSIZE=8192
CONFIG_PTHREAD_STACK_MIN=256
CONFIG_PTHREAD_STACK_DEFAULT=2048
CONFIG_HEAP_BASE=
CONFIG_HEAP_SIZE=
