############################################################################
# configs/sure-pic32mx/usbnsh/defconfig
#
#   Copyright (C) 2012 Gregory Nutt. All rights reserved.
#   Author: Gregory Nutt <gnutt@nuttx.org>
#
# Redistribution and use in source and binary forms, with or without
# modification, are permitted provided that the following conditions
# are met:
#
# 1. Redistributions of source code must retain the above copyright
#    notice, this list of conditions and the following disclaimer.
# 2. Redistributions in binary form must reproduce the above copyright
#    notice, this list of conditions and the following disclaimer in
#    the documentation and/or other materials provided with the
#    distribution.
# 3. Neither the name NuttX nor the names of its contributors may be
#    used to endorse or promote products derived from this software
#    without specific prior written permission.
#
# THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS
# "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT
# LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS
# FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE
# COPYRIGHT OWNER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT,
# INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING,
# BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS
# OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED
# AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT
# LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN
# ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
# POSSIBILITY OF SUCH DAMAGE.
#
############################################################################
#
# architecture selection
#
# CONFIG_ARCH - identifies the arch subdirectory and, hence, the
#   processor architecture.
# CONFIG_ARCH_family - for use in C code.  This identifies the
#   particular chip family that the architecture is implemented
#   in.
# CONFIG_ARCH_architecture - for use in C code.  This identifies the
#   specific architecture within the chip family.
# CONFIG_ARCH_CHIP - Identifies the arch/*/chip subdirectory
# CONFIG_ARCH_CHIP_name - For use in C code
# CONFIG_ARCH_BOARD - identifies the configs subdirectory and, hence,
#   the board that supports the particular chip or SoC.
# CONFIG_ARCH_BOARD_name - for use in C code
# CONFIG_ENDIAN_BIG - define if big endian (default is little endian)
#   NOTE: The PIC32MX is always little endian.
# CONFIG_BOARD_LOOPSPERMSEC.  You simply use a stop watch to measure
#   the 100 second delay then adjust CONFIG_BOARD_LOOPSPERMSEC until
#   the delay actually is 100 seconds.
# CONFIG_DRAM_SIZE - Describes the installed DRAM.
# CONFIG_DRAM_START - The start address of DRAM (physical)
# CONFIG_ARCH_NOINTC - define if the architecture does not
#   support an interrupt controller or otherwise cannot support
#   APIs like up_enable_irq() and up_disable_irq().
# CONFIG_ARCH_VECNOTIRQ - Usually the interrupt vector number provided
#   to interfaces like irq_attach() and irq_detach are the same as IRQ
#   numbers that are provied to IRQ management functions like
#   up_enable_irq() and up_disable_irq().  But that is not true for all
#   interrupt controller implementations.  For example, the PIC32MX
#   interrupt controller manages interrupt sources that have a many-to-one
#   relationship to interrupt vectors. In such cases, CONFIG_ARCH_VECNOTIRQ
#   must defined so that the OS logic will know not to assume it can use
#   a vector number to enable or disable interrupts.
# CONFIG_ARCH_IRQPRIO - The PIC32MX supports interrupt prioritization
# CONFIG_ARCH_INTERRUPTSTACK - This architecture supports an interrupt
#   stack. If defined, this symbol is the size of the interrupt
#   stack in bytes.  If not defined, the user task stacks will be
#   used during interrupt handling.
# CONFIG_ARCH_STACKDUMP - Do stack dumps after assertions
# CONFIG_ARCH_BOOTLOADER - Set if you are using a bootloader.
# CONFIG_ARCH_LEDS -  Use LEDs to show state. Unique to board architecture.
# CONFIG_ARCH_BUTTONS -  Enable support for buttons. Unique to board architecture.
# CONFIG_ARCH_CALIBRATION - Enables some build in instrumentation that
#   cause a 100 second delay during boot-up.  This 100 second delay
#   serves no purpose other than it allows you to calibrate
# CONFIG_ARCH_DMA - Support DMA initialization
#
CONFIG_ARCH="mips"
CONFIG_ARCH_MIPS=y
CONFIG_ARCH_MIPS32=y
CONFIG_ARCH_CHIP="pic32mx"
CONFIG_ARCH_CHIP_PIC32MX440F512H=y
CONFIG_ARCH_BOARD="sure-pic32mx"
CONFIG_ARCH_BOARD_SUREPIC32MX=y
CONFIG_ARCH_DBDP11215=y
CONFIG_ARCH_DBDP11212=n
CONFIG_BOARD_LOOPSPERMSEC=4275
CONFIG_DRAM_SIZE=32768
CONFIG_DRAM_START=0xa0000000
CONFIG_ARCH_NOINTC=n
CONFIG_ARCH_VECNOTIRQ=y
CONFIG_ARCH_IRQPRIO=y
CONFIG_ARCH_INTERRUPTSTACK=n
CONFIG_ARCH_STACKDUMP=y
CONFIG_ARCH_BOOTLOADER=n
CONFIG_ARCH_LEDS=y
CONFIG_ARCH_BUTTONS=n
CONFIG_ARCH_CALIBRATION=n
CONFIG_ARCH_DMA=n

#
# Enable support for RAM-based functions
# (If selected, then modifications are needed in ld.script as well)
#
CONFIG_PIC32MX_RAMFUNCS=n

#
# Identify toolchain and linker options
#
CONFIG_PIC32MX_MICROCHIPW=n
CONFIG_PIC32MX_MICROCHIPL=n
CONFIG_PIC32MX_MICROCHIPW_LITE=y
CONFIG_PIC32MX_MICROCHIPL_LITE=n

#
#  Individual subsystems can be enabled:
#

CONFIG_PIC32MX_WDT=n
CONFIG_PIC32MX_RTCC=n
CONFIG_PIC32MX_TIMER1=n
CONFIG_PIC32MX_TIMER2=n
CONFIG_PIC32MX_TIMER3=n
CONFIG_PIC32MX_TIMER4=n
CONFIG_PIC32MX_TIMER5=n
CONFIG_PIC32MX_IC1=n
CONFIG_PIC32MX_IC2=n
CONFIG_PIC32MX_IC3=n
CONFIG_PIC32MX_IC4=n
CONFIG_PIC32MX_IC5=n
CONFIG_PIC32MX_OC1=n
CONFIG_PIC32MX_OC2=n
CONFIG_PIC32MX_OC3=n
CONFIG_PIC32MX_OC4=n
CONFIG_PIC32MX_OC5=n
CONFIG_PIC32MX_I2C1=n
CONFIG_PIC32MX_I2C2=n
CONFIG_PIC32MX_SPI2=n
CONFIG_PIC32MX_UART1=n
CONFIG_PIC32MX_UART2=y
CONFIG_PIC32MX_PMP=n
CONFIG_PIC32MX_ADC=n
CONFIG_PIC32MX_CVR=n
CONFIG_PIC32MX_CM1=n
CONFIG_PIC32MX_CM2=n
CONFIG_PIC32MX_OSC=y
CONFIG_PIC32MX_DDP=n
CONFIG_PIC32MX_FLASH=n
CONFIG_PIC32MX_BMX=n
CONFIG_PIC32MX_DMA=n
CONFIG_PIC32MX_CHE=n
CONFIG_PIC32MX_USBDEV=y
CONFIG_PIC32MX_USBHOST=n
CONFIG_PIC32MX_IOPORTA=y
CONFIG_PIC32MX_IOPORTB=y
CONFIG_PIC32MX_IOPORTC=y
CONFIG_PIC32MX_IOPORTD=y
CONFIG_PIC32MX_IOPORTE=y
CONFIG_PIC32MX_IOPORTF=y
CONFIG_PIC32MX_IOPORTG=y

#
# PIC32MX Configuration Settings
#
# DEVCFG0:
#   CONFIG_PIC32MX_DEBUGGER - Background Debugger Enable. Default 3 (disabled). The
#     value 2 enables.
#   CONFIG_PIC32MX_ICESEL - In-Circuit Emulator/Debugger Communication Channel Select
#     Default 1 (PG2)
#   CONFIG_PIC32MX_PROGFLASHWP  - Program FLASH write protect.  Default 0xff (disabled)
#   CONFIG_PIC32MX_BOOTFLASHWP - Default 1 (disabled)
#   CONFIG_PIC32MX_CODEWP - Default 1 (disabled)
# DEVCFG1: (All settings determined by selections in board.h)
# DEVCFG2: (All settings determined by selections in board.h)
# DEVCFG3: 
#  CONFIG_PIC32MX_USBIDO - USB USBID Selection.  Default 1 if USB enabled
#    (USBID pin is controlled by the USB module), but 0 (GPIO) otherwise.
#  CONFIG_PIC32MX_VBUSIO - USB VBUSON Selection (Default 1 if USB enabled
#    (VBUSON pin is controlled by the USB module, but 0 (GPIO) otherwise.
#  CONFIG_PIC32MX_WDENABLE - Enabled watchdog on power up.  Default 0 (watchdog
#    can be enabled later by software).
#
CONFIG_PIC32MX_DEBUGGER=2
CONFIG_PIC32MX_ICESEL=1

#
# PIC32MX specific serial device driver settings
#
# CONFIG_UARTn_SERIAL_CONSOLE - selects the UARTn for the
#   console and ttys0 (default is the UART1).
# CONFIG_UARTn_RXBUFSIZE - Characters are buffered as received.
#   This specific the size of the receive buffer
# CONFIG_UARTn_TXBUFSIZE - Characters are buffered before
#   being sent.  This specific the size of the transmit buffer
# CONFIG_UARTn_BAUD - The configure BAUD of the UART.  Must be
# CONFIG_UARTn_BITS - The number of bits.  Must be either 7 or 8.
# CONFIG_UARTn_PARTIY - 0=no parity, 1=odd parity, 2=even parity
# CONFIG_UARTn_2STOP - Two stop bits
#
CONFIG_UART1_SERIAL_CONSOLE=n
CONFIG_UART2_SERIAL_CONSOLE=n

CONFIG_UART1_TXBUFSIZE=256
CONFIG_UART2_TXBUFSIZE=256

CONFIG_UART1_RXBUFSIZE=256
CONFIG_UART2_RXBUFSIZE=256

CONFIG_UART1_BAUD=115200
CONFIG_UART2_BAUD=115200

CONFIG_UART1_BITS=8
CONFIG_UART2_BITS=8

CONFIG_UART1_PARITY=0
CONFIG_UART2_PARITY=0

CONFIG_UART1_2STOP=0
CONFIG_UART2_2STOP=0

#
# PIC32MX-specific USB device setup
#
CONFIG_PIC32MX_USBDEV_REGDEBUG=n
CONFIG_PIC32MX_USBDEV_BDTDEBUG=n
 
#
# General build options
#
# CONFIG_RRLOAD_BINARY - make the rrload binary format used with
#   BSPs from www.ridgerun.com using the tools/mkimage.sh script
# CONFIG_INTELHEX_BINARY - make the Intel HEX binary format
#   used with many different loaders using the GNU objcopy program
#   Should not be selected if you are not using the GNU toolchain.
# CONFIG_MOTOROLA_SREC - make the Motorola S-Record binary format
#   used with many different loaders using the GNU objcopy program
#   Should not be selected if you are not using the GNU toolchain.
# CONFIG_RAW_BINARY - make a raw binary format file used with many
#   different loaders using the GNU objcopy program.  This option
#   should not be selected if you are not using the GNU toolchain.
# CONFIG_HAVE_LIBM - toolchain supports libm.a
#
CONFIG_RRLOAD_BINARY=n
CONFIG_INTELHEX_BINARY=y
CONFIG_MOTOROLA_SREC=n
CONFIG_RAW_BINARY=n
CONFIG_HAVE_LIBM=n

#
# General OS setup
#
# CONFIG_APPS_DIR - Identifies the relative path to the directory
#   that builds the application to link with NuttX.  Default: ../apps
# CONFIG_DEBUG - enables built-in debug options
# CONFIG_DEBUG_VERBOSE - enables verbose debug output
# CONFIG_DEBUG_SYMBOLS - build without optimization and with
#   debug symbols (needed for use with a debugger).
# CONFIG_HAVE_CXX - Enable support for C++
# CONFIG_HAVE_CXXINITIALIZE - The platform-specific logic includes support
#   for initialization of static C++ instances for this architecture
#   and for the selected toolchain (via up_cxxinitialize()).
# CONFIG_MM_REGIONS - If the architecture includes multiple
#   regions of memory to allocate from, this specifies the
#   number of memory regions that the memory manager must
#   handle and enables the API mm_addregion(start, end);
# CONFIG_ARCH_LOWPUTC - architecture supports low-level, boot
#   time console output
# CONFIG_MSEC_PER_TICK - The default system timer is 100Hz
#   or MSEC_PER_TICK=10.  This setting may be defined to
#   inform NuttX that the processor hardware is providing
#   system timer interrupts at some interrupt interval other
#   than 10 msec.
# CONFIG_RR_INTERVAL - The round robin timeslice will be set
#   this number of milliseconds;  Round robin scheduling can
#   be disabled by setting this value to zero.
# CONFIG_SCHED_INSTRUMENTATION - enables instrumentation in 
#   scheduler to monitor system performance
# CONFIG_TASK_NAME_SIZE - Spcifies that maximum size of a
#   task name to save in the TCB.  Useful if scheduler
#   instrumentation is selected.  Set to zero to disable.
# CONFIG_START_YEAR, CONFIG_START_MONTH, CONFIG_START_DAY -
#   Used to initialize the internal time logic.
# CONFIG_GREGORIAN_TIME - Enables Gregorian time conversions.
#   You would only need this if you are concerned about accurate
#   time conversions in the past or in the distant future.
# CONFIG_JULIAN_TIME - Enables Julian time conversions. You
#   would only need this if you are concerned about accurate
#   time conversion in the distand past.  You must also define
#   CONFIG_GREGORIAN_TIME in order to use Julian time.
# CONFIG_DEV_CONSOLE - Set if architecture-specific logic
#   provides /dev/console.  Enables stdout, stderr, stdin.
# CONFIG_DEV_LOWCONSOLE - Use the simple, low-level serial console
#   driver (minimul support)
# CONFIG_MUTEX_TYPES: Set to enable support for recursive and
#   errorcheck mutexes. Enables pthread_mutexattr_settype().
# CONFIG_PRIORITY_INHERITANCE : Set to enable support for priority
#   inheritance on mutexes and semaphores. 
# CONFIG_SEM_PREALLOCHOLDERS: This setting is only used if priority
#   inheritance is enabled.  It defines the maximum number of
#   different threads (minus one) that can take counts on a
#   semaphore with priority inheritance support.  This may be 
#   set to zero if priority inheritance is disabled OR if you
#   are only using semaphores as mutexes (only one holder) OR
#   if no more than two threads participate using a counting
#   semaphore.
# CONFIG_SEM_NNESTPRIO.  If priority inheritance is enabled,
#   then this setting is the maximum number of higher priority
#   threads (minus 1) than can be waiting for another thread
#   to release a count on a semaphore.  This value may be set
#   to zero if no more than one thread is expected to wait for
#   a semaphore.
# CONFIG_FDCLONE_DISABLE. Disable cloning of all file descriptors
#   by task_create() when a new task is started.  If set, all
#   files/drivers will appear to be closed in the new task.
# CONFIG_FDCLONE_STDIO. Disable cloning of all but the first
#   three file descriptors (stdin, stdout, stderr) by task_create()
#   when a new task is started. If set, all files/drivers will
#   appear to be closed in the new task except for stdin, stdout,
#   and stderr.
# CONFIG_SDCLONE_DISABLE. Disable cloning of all socket
#   desciptors by task_create() when a new task is started. If
#   set, all sockets will appear to be closed in the new task.
# CONFIG_SCHED_WORKQUEUE.  Create a dedicated "worker" thread to
#  handle delayed processing from interrupt handlers.  This feature
#  is required for some drivers but, if there are not complaints,
#  can be safely disabled.  The worker thread also performs
#  garbage collection -- completing any delayed memory deallocations
#  from interrupt handlers.  If the worker thread is disabled,
#  then that clean will be performed by the IDLE thread instead
#  (which runs at the lowest of priority and may not be appropriate
#  if memory reclamation is of high priority).  If CONFIG_SCHED_WORKQUEUE
#  is enabled, then the following options can also be used:
# CONFIG_SCHED_WORKPRIORITY - The execution priority of the worker
#  thread.  Default: 50
# CONFIG_SCHED_WORKPERIOD - How often the worker thread checks for
#  work in units of microseconds.  Default: 50000 (50 MS).
# CONFIG_SCHED_WORKSTACKSIZE - The stack size allocated for the worker
#  thread.  Default: CONFIG_IDLETHREAD_STACKSIZE.
# CONFIG_SIG_SIGWORK - The signal number that will be used to wake-up
#  the worker thread.  Default: 4
# CONFIG_SCHED_WAITPID - Enable the waitpid() API
# CONFIG_SCHED_ATEXIT - Enabled the atexit() API
#
#CONFIG_APPS_DIR=

CONFIG_DEBUG=n
CONFIG_DEBUG_VERBOSE=n
CONFIG_DEBUG_SYMBOLS=n
CONFIG_DEBUG_SCHED=n
CONFIG_DEBUG_USB=n

CONFIG_HAVE_CXX=n
CONFIG_HAVE_CXXINITIALIZE=n
CONFIG_MM_REGIONS=1
CONFIG_ARCH_LOWPUTC=y
CONFIG_RR_INTERVAL=0
CONFIG_SCHED_INSTRUMENTATION=n
CONFIG_TASK_NAME_SIZE=0
CONFIG_START_YEAR=2012
CONFIG_START_MONTH=3
CONFIG_START_DAY=6
CONFIG_GREGORIAN_TIME=n
CONFIG_JULIAN_TIME=n
CONFIG_DEV_CONSOLE=y
CONFIG_DEV_LOWCONSOLE=n
CONFIG_MUTEX_TYPES=n
CONFIG_PRIORITY_INHERITANCE=n
CONFIG_SEM_PREALLOCHOLDERS=0
CONFIG_SEM_NNESTPRIO=0
CONFIG_FDCLONE_DISABLE=n
CONFIG_FDCLONE_STDIO=n
CONFIG_SDCLONE_DISABLE=y
CONFIG_SCHED_WORKQUEUE=n
CONFIG_SCHED_WORKPRIORITY=50
CONFIG_SCHED_WORKPERIOD=50000
CONFIG_SCHED_WORKSTACKSIZE=1024
CONFIG_SIG_SIGWORK=4
CONFIG_SCHED_WAITPID=y
CONFIG_SCHED_ATEXIT=n

#
# Settings for nxflat
# CONFIG_NXFLAT. Enable support for the NXFLAT binary format.
#  This format will support execution of NuttX binaries located
#  in a ROMFS filesystem (see examples/nxflat).
# CONFIG_NXFLAT_DUMPBUFFER. Dump a most buffers that NXFFLAT deals
#  with.  CONFIG_DEBUG, CONFIG_DEBUG_VERBOSE, and
#  CONFIG_DEBUG_BINFMT have to be defined or
#  CONFIG_NXFLAT_DUMPBUFFER does nothing.
# CONFIG_SYMTAB_ORDEREDBYNAME. Select if the system symbol table
#  is ordered by symbol name
#
CONFIG_NXFLAT=n
CONFIG_NXFLAT_DUMPBUFFER=n
CONFIG_SYMTAB_ORDEREDBYNAME=y

#
# The following can be used to disable categories of
# APIs supported by the OS.  If the compiler supports
# weak functions, then it should not be necessary to
# disable functions unless you want to restrict usage
# of those APIs.
#
# There are certain dependency relationships in these
# features.
#
# o mq_notify logic depends on signals to awaken tasks
#   waiting for queues to become full or empty.
# o pthread_condtimedwait() depends on signals to wake
#   up waiting tasks.
#
CONFIG_DISABLE_CLOCK=n
CONFIG_DISABLE_POSIX_TIMERS=n
CONFIG_DISABLE_PTHREAD=n
CONFIG_DISABLE_SIGNALS=n
CONFIG_DISABLE_MQUEUE=n
CONFIG_DISABLE_MOUNTPOINT=n
CONFIG_DISABLE_ENVIRON=n
CONFIG_DISABLE_POLL=y

#
# Misc libc settings
#
# CONFIG_NOPRINTF_FIELDWIDTH - sprintf-related logic is a
#   little smaller if we do not support fieldwidthes
#
CONFIG_NOPRINTF_FIELDWIDTH=n

#
# Allow for architecture optimized implementations
#
# The architecture can provide optimized versions of the
# following to improve system performance
#
CONFIG_ARCH_MEMCPY=n
CONFIG_ARCH_MEMCMP=n
CONFIG_ARCH_MEMMOVE=n
CONFIG_ARCH_MEMSET=n
CONFIG_ARCH_STRCMP=n
CONFIG_ARCH_STRCPY=n
CONFIG_ARCH_STRNCPY=n
CONFIG_ARCH_STRLEN=n
CONFIG_ARCH_STRNLEN=n
CONFIG_ARCH_BZERO=n

#
# Sizes of configurable things (0 disables)
#
# CONFIG_MAX_TASKS - The maximum number of simultaneously
#   active tasks.  This value must be a power of two.
# CONFIG_MAX_TASK_ARGS - This controls the maximum number of
#   of parameters that a task may receive (i.e., maxmum value
#   of 'argc')
# CONFIG_NPTHREAD_KEYS - The number of items of thread-
#   specific data that can be retained
# CONFIG_NFILE_DESCRIPTORS - The maximum number of file
#   descriptors (one for each open)
# CONFIG_NFILE_STREAMS - The maximum number of streams that
#   can be fopen'ed
# CONFIG_NAME_MAX - The maximum size of a file name.
# CONFIG_STDIO_BUFFER_SIZE - Size of the buffer to allocate
#   on fopen. (Only if CONFIG_NFILE_STREAMS > 0)
# CONFIG_STDIO_LINEBUFFER - If standard C buffered I/O is enabled
#   (CONFIG_STDIO_BUFFER_SIZE > 0), then this option may be added
#   to force automatic, line-oriented flushing the output buffer
#   for putc(), fputc(), putchar(), puts(), fputs(), printf(),
#   fprintf(), and vfprintf().  When a newline is encountered in
#   the output string, the output buffer will be flushed.  This
#   (slightly) increases the NuttX footprint but supports the kind
#   of behavior that people expect for printf().
# CONFIG_NUNGET_CHARS - Number of characters that can be
#   buffered by ungetc() (Only if CONFIG_NFILE_STREAMS > 0)
# CONFIG_PREALLOC_MQ_MSGS - The number of pre-allocated message
#   structures.  The system manages a pool of preallocated
#   message structures to minimize dynamic allocations
# CONFIG_MQ_MAXMSGSIZE - Message structures are allocated with
#   a fixed payload size given by this settin (does not include
#   other message structure overhead.
# CONFIG_MAX_WDOGPARMS - Maximum number of parameters that
#   can be passed to a watchdog handler
# CONFIG_PREALLOC_WDOGS - The number of pre-allocated watchdog
#   structures.  The system manages a pool of preallocated
#   watchdog structures to minimize dynamic allocations
# CONFIG_PREALLOC_TIMERS - The number of pre-allocated POSIX
#   timer structures.  The system manages a pool of preallocated
#   timer structures to minimize dynamic allocations.  Set to
#   zero for all dynamic allocations.
#
CONFIG_MAX_TASKS=16
CONFIG_MAX_TASK_ARGS=4
CONFIG_NPTHREAD_KEYS=4
CONFIG_NFILE_DESCRIPTORS=8
CONFIG_NFILE_STREAMS=8
CONFIG_NAME_MAX=32
CONFIG_STDIO_BUFFER_SIZE=64
CONFIG_STDIO_LINEBUFFER=y
CONFIG_NUNGET_CHARS=2
CONFIG_PREALLOC_MQ_MSGS=4
CONFIG_MQ_MAXMSGSIZE=32
CONFIG_MAX_WDOGPARMS=2
CONFIG_PREALLOC_WDOGS=4
CONFIG_PREALLOC_TIMERS=4

#
# Filesystem configuration
#
# CONFIG_FS_FAT - Enable FAT filesystem support
# CONFIG_FAT_SECTORSIZE - Max supported sector size
# CONFIG_FAT_LCNAMES - Enable use of the NT-style upper/lower case 8.3
#   file name support.
# CONFIG_FAT_LFN - Enable FAT long file names.  NOTE:  Microsoft claims
#   patents on FAT long file name technology.  Please read the
#   disclaimer in the top-level COPYING file and only enable this
#   feature if you understand these issues.
# CONFIG_FAT_MAXFNAME - If CONFIG_FAT_LFN is defined, then the
#   default, maximum long file name is 255 bytes.  This can eat up
#   a lot of memory (especially stack space).  If you are willing
#   to live with some non-standard, short long file names, then
#   define this value.  A good choice would be the same value as
#   selected for CONFIG_NAME_MAX which will limit the visibility
#   of longer file names anyway.
# CONFIG_FS_NXFFS: Enable NuttX FLASH file system (NXFF) support.
# CONFIG_NXFFS_ERASEDSTATE: The erased state of FLASH. 
#   This must have one of the values of 0xff or 0x00.
#   Default: 0xff.
# CONFIG_NXFFS_PACKTHRESHOLD: When packing flash file data,
#   don't both with file chunks smaller than this number of data bytes.
# CONFIG_NXFFS_MAXNAMLEN: The maximum size of an NXFFS file name.
#   Default: 255.
# CONFIG_NXFFS_PACKTHRESHOLD: When packing flash file data,
#   don't both with file chunks smaller than this number of data bytes.
#   Default: 32.
# CONFIG_NXFFS_TAILTHRESHOLD: clean-up can either mean
#   packing files together toward the end of the file or, if file are
#   deleted at the end of the file, clean up can simply mean erasing
#   the end of FLASH memory so that it can be re-used again.  However,
#   doing this can also harm the life of the FLASH part because it can
#   mean that the tail end of the FLASH is re-used too often. This
#   threshold determines if/when it is worth erased the tail end of FLASH
#   and making it available for re-use (and possible over-wear).
#   Default: 8192.
# CONFIG_FS_ROMFS - Enable ROMFS filesystem support
# CONFIG_FS_RAMMAP - For file systems that do not support XIP, this
#   option will enable a limited form of memory mapping that is
#   implemented by copying whole files into memory.
#
CONFIG_FS_FAT=y
CONFIG_FAT_LCNAMES=y
CONFIG_FAT_LFN=y
CONFIG_FAT_MAXFNAME=32
CONFIG_FS_NXFFS=n
CONFIG_FS_ROMFS=n

#
# SPI-based MMC/SD driver
#
# CONFIG_MMCSD_NSLOTS
#   Number of MMC/SD slots supported by the driver
# CONFIG_MMCSD_READONLY
#   Provide read-only access (default is read/write)
# CONFIG_MMCSD_SPICLOCK - Maximum SPI clock to drive MMC/SD card.
#   Default is 20MHz.
#
CONFIG_MMCSD_NSLOTS=1
CONFIG_MMCSD_READONLY=n
CONFIG_MMCSD_SPICLOCK=12500000

#
# Block driver buffering
#
# CONFIG_FS_READAHEAD
#   Enable read-ahead buffering
# CONFIG_FS_WRITEBUFFER
#   Enable write buffering
#
CONFIG_FS_READAHEAD=n
CONFIG_FS_WRITEBUFFER=n

#
# SDIO-based MMC/SD driver
#
# CONFIG_SDIO_DMA
#   SDIO driver supports DMA
# CONFIG_MMCSD_MMCSUPPORT
#   Enable support for MMC cards
# CONFIG_MMCSD_HAVECARDDETECT
#   SDIO driver card detection is 100% accurate
#
CONFIG_SDIO_DMA=n
CONFIG_MMCSD_MMCSUPPORT=n
CONFIG_MMCSD_HAVECARDDETECT=n

#
# TCP/IP and UDP support via uIP
# CONFIG_NET - Enable or disable all network features
# CONFIG_NET_IPv6 - Build in support for IPv6
# CONFIG_NSOCKET_DESCRIPTORS - Maximum number of socket descriptors per task/thread.
# CONFIG_NET_SOCKOPTS - Enable or disable support for socket options
# CONFIG_NET_BUFSIZE - uIP buffer size
# CONFIG_NET_TCP - TCP support on or off
# CONFIG_NET_TCP_CONNS - Maximum number of TCP connections (all tasks)
# CONFIG_NET_TCP_READAHEAD_BUFSIZE - Size of TCP read-ahead buffers
# CONFIG_NET_NTCP_READAHEAD_BUFFERS - Number of TCP read-ahead buffers (may be zero)
# CONFIG_NET_TCPBACKLOG - Incoming connections pend in a backlog until
#   accept() is called. The size of the backlog is selected when listen() is called.
# CONFIG_NET_MAX_LISTENPORTS - Maximum number of listening TCP ports (all tasks)
# CONFIG_NET_UDP - UDP support on or off
# CONFIG_NET_UDP_CHECKSUMS - UDP checksums on or off
# CONFIG_NET_UDP_CONNS - The maximum amount of concurrent UDP connections
# CONFIG_NET_ICMP - ICMP ping response support on or off
# CONFIG_NET_ICMP_PING - ICMP ping request support on or off
# CONFIG_NET_PINGADDRCONF - Use "ping" packet for setting IP address
# CONFIG_NET_STATISTICS - uIP statistics on or off
# CONFIG_NET_RECEIVE_WINDOW - The size of the advertised receiver's window
# CONFIG_NET_ARPTAB_SIZE - The size of the ARP table
# CONFIG_NET_BROADCAST - Broadcast support
# CONFIG_NET_FWCACHE_SIZE - number of packets to remember when looking for duplicates
#
CONFIG_NET=n
CONFIG_NET_IPv6=n
CONFIG_NSOCKET_DESCRIPTORS=0
CONFIG_NET_SOCKOPTS=y
CONFIG_NET_BUFSIZE=420
CONFIG_NET_TCP=n
CONFIG_NET_TCP_CONNS=40
CONFIG_NET_MAX_LISTENPORTS=40
CONFIG_NET_UDP=n
CONFIG_NET_UDP_CHECKSUMS=y
#CONFIG_NET_UDP_CONNS=10
CONFIG_NET_ICMP=n
CONFIG_NET_ICMP_PING=n
#CONFIG_NET_PINGADDRCONF=0
CONFIG_NET_STATISTICS=y
#CONFIG_NET_RECEIVE_WINDOW=
#CONFIG_NET_ARPTAB_SIZE=8
CONFIG_NET_BROADCAST=n
#CONFIG_NET_FWCACHE_SIZE=2

#
# UIP Network Utilities
# CONFIG_NET_DHCP_LIGHT - Reduces size of DHCP
# CONFIG_NET_RESOLV_ENTRIES - Number of resolver entries
#
CONFIG_NET_DHCP_LIGHT=n
CONFIG_NET_RESOLV_ENTRIES=4

#
# USB Device Configuration
#
# CONFIG_USBDEV
#   Enables USB device support
# CONFIG_USBDEV_ISOCHRONOUS
#   Build in extra support for isochronous endpoints
# CONFIG_USBDEV_DUALSPEED
#   Hardware handles high and full speed operation (USB 2.0)
# CONFIG_USBDEV_SELFPOWERED
#   Will cause USB features to indicate that the device is
#   self-powered
# CONFIG_USBDEV_MAXPOWER
#   Maximum power consumption in mA
# CONFIG_USBDEV_TRACE
#   Enables USB tracing for debug
# CONFIG_USBDEV_TRACE_NRECORDS
#   Number of trace entries to remember
#
CONFIG_USBDEV=y
CONFIG_USBDEV_ISOCHRONOUS=n
CONFIG_USBDEV_DUALSPEED=n
CONFIG_USBDEV_SELFPOWERED=y
CONFIG_USBDEV_REMOTEWAKEUP=n
CONFIG_USBDEV_MAXPOWER=100
CONFIG_USBDEV_TRACE=n
CONFIG_USBDEV_TRACE_NRECORDS=128

#
# USB Serial Device Configuration
#
# CONFIG_PL2303
#   Enable compilation of the USB serial driver
# CONFIG_PL2303_EPINTIN
#   The logical 7-bit address of a hardware endpoint that supports
#   interrupt IN operation
# CONFIG_PL2303_EPBULKOUT
#   The logical 7-bit address of a hardware endpoint that supports
#   bulk OUT operation
# CONFIG_PL2303_EPBULKIN
#   The logical 7-bit address of a hardware endpoint that supports
#   bulk IN operation
# # CONFIG_PL2303_NWRREQS and CONFIG_PL2303_NRDREQS
#   The number of write/read requests that can be in flight
# CONFIG_PL2303_VENDORID and CONFIG_PL2303_VENDORSTR
#   The vendor ID code/string
# CONFIG_PL2303_PRODUCTID and CONFIG_PL2303_PRODUCTSTR
#   The product ID code/string
# CONFIG_PL2303_RXBUFSIZE and CONFIG_PL2303_TXBUFSIZE
#   Size of the serial receive/transmit buffers
#
CONFIG_PL2303=n
CONFIG_PL2303_EPINTIN=1
CONFIG_PL2303_EPBULKOUT=2
CONFIG_PL2303_EPBULKIN=5
CONFIG_PL2303_NWRREQS=4
CONFIG_PL2303_NRDREQS=4
CONFIG_PL2303_VENDORID=0x067b
CONFIG_PL2303_PRODUCTID=0x2303
CONFIG_PL2303_VENDORSTR="Nuttx"
CONFIG_PL2303_PRODUCTSTR="USBdev Serial"
CONFIG_PL2303_RXBUFSIZE=512
CONFIG_PL2303_TXBUFSIZE=512

#
# USB serial device class driver (Standard CDC ACM class)
#
# CONFIG_CDCACM
#   Enable compilation of the USB serial driver
# CONFIG_CDCACM_CONSOLE
#   Configures the CDC/ACM serial port as the console device.
# CONFIG_CDCACM_EP0MAXPACKET
#   Endpoint 0 max packet size. Default 64
# CONFIG_CDCACM_EPINTIN
#   The logical 7-bit address of a hardware endpoint that supports
#   interrupt IN operation.  Default 2.
# CONFIG_CDCACM_EPINTIN_FSSIZE
#   Max package size for the interrupt IN endpoint if full speed mode.
#   Default 64.
# CONFIG_CDCACM_EPINTIN_HSSIZE
#   Max package size for the interrupt IN endpoint if high speed mode.
#   Default 64
# CONFIG_CDCACM_EPBULKOUT
#   The logical 7-bit address of a hardware endpoint that supports
#   bulk OUT operation
# CONFIG_CDCACM_EPBULKOUT_FSSIZE
#   Max package size for the bulk OUT endpoint if full speed mode.
#   Default 64.
# CONFIG_CDCACM_EPBULKOUT_HSSIZE
#   Max package size for the bulk OUT  endpoint if high speed mode.
#   Default 512.
# CONFIG_CDCACM_EPBULKIN
#   The logical 7-bit address of a hardware endpoint that supports
#   bulk IN operation
# CONFIG_CDCACM_EPBULKIN_FSSIZE
#   Max package size for the bulk IN endpoint if full speed mode.
#   Default 64.
# CONFIG_CDCACM_EPBULKIN_HSSIZE
#   Max package size for the bulk IN  endpoint if high speed mode.
#   Default 512.
# CONFIG_CDCACM_NWRREQS and CONFIG_CDCACM_NRDREQS
#   The number of write/read requests that can be in flight.
#   Default 256.
# CONFIG_CDCACM_VENDORID and CONFIG_CDCACM_VENDORSTR
#   The vendor ID code/string.  Default 0x0525 and "NuttX"
#   0x0525 is the Netchip vendor and should not be used in any
#   products.  This default VID was selected for compatibility with
#   the Linux CDC ACM default VID.
# CONFIG_CDCACM_PRODUCTID and CONFIG_CDCACM_PRODUCTSTR
#   The product ID code/string. Default 0xa4a7 and "CDC/ACM Serial"
#   0xa4a7 was selected for compatibility with the Linux CDC ACM
#   default PID.
# CONFIG_CDCACM_RXBUFSIZE and CONFIG_CDCACM_TXBUFSIZE
#   Size of the serial receive/transmit buffers. Default 256.
#
CONFIG_CDCACM=y
CONFIG_CDCACM_CONSOLE=y
#CONFIG_CDCACM_EP0MAXPACKET
#CONFIG_CDCACM_EPINTIN
#CONFIG_CDCACM_EPINTIN_FSSIZE
#CONFIG_CDCACM_EPINTIN_HSSIZE
#CONFIG_CDCACM_EPBULKOUT
#CONFIG_CDCACM_EPBULKOUT_FSSIZE
#CONFIG_CDCACM_EPBULKOUT_HSSIZE
#CONFIG_CDCACM_EPBULKIN
#CONFIG_CDCACM_EPBULKIN_FSSIZE
#CONFIG_CDCACM_EPBULKIN_HSSIZE
#CONFIG_CDCACM_NWRREQS
#CONFIG_CDCACM_NRDREQS
#CONFIG_CDCACM_VENDORID
#CONFIG_CDCACM_VENDORSTR
#CONFIG_CDCACM_PRODUCTID
#CONFIG_CDCACM_PRODUCTSTR
#CONFIG_CDCACM_RXBUFSIZE
#CONFIG_CDCACM_TXBUFSIZE

#
# USB Storage Device Configuration
#
# CONFIG_USBMSC
#   Enable compilation of the USB storage driver
# CONFIG_USBMSC_EP0MAXPACKET
#   Max packet size for endpoint 0
# CONFIG_USBMSC_EPBULKOUT and CONFIG_USBMSC_EPBULKIN
#   The logical 7-bit address of a hardware endpoints that support
#   bulk OUT and IN operations
# CONFIG_USBMSC_NWRREQS and CONFIG_USBMSC_NRDREQS
#   The number of write/read requests that can be in flight
# CONFIG_USBMSC_BULKINREQLEN and CONFIG_USBMSC_BULKOUTREQLEN
#   The size of the buffer in each write/read request.  This
#   value needs to be at least as large as the endpoint
#   maxpacket and ideally as large as a block device sector.
# CONFIG_USBMSC_VENDORID and CONFIG_USBMSC_VENDORSTR
#   The vendor ID code/string
# CONFIG_USBMSC_PRODUCTID and CONFIG_USBMSC_PRODUCTSTR
#   The product ID code/string
# CONFIG_USBMSC_REMOVABLE
#   Select if the media is removable
#
CONFIG_USBMSC=n
CONFIG_USBMSC_EP0MAXPACKET=64
CONFIG_USBMSC_EPBULKOUT=1
CONFIG_USBMSC_EPBULKIN=2
CONFIG_USBMSC_NRDREQS=8
CONFIG_USBMSC_NWRREQS=2
CONFIG_USBMSC_BULKINREQLEN=256
CONFIG_USBMSC_BULKOUTREQLEN=64
CONFIG_USBMSC_VENDORID=0x584e
CONFIG_USBMSC_VENDORSTR="NuttX"
CONFIG_USBMSC_PRODUCTID=0x5342
CONFIG_USBMSC_PRODUCTSTR="USBdev Storage"
CONFIG_USBMSC_VERSIONNO=0x0399
CONFIG_USBMSC_REMOVABLE=y

#
# Settings for examples/uip
#
CONFIG_EXAMPLE_UIP_IPADDR=0x0a000002
CONFIG_EXAMPLE_UIP_DRIPADDR=0x0a000001
CONFIG_EXAMPLE_UIP_NETMASK=0xffffff00
CONFIG_EXAMPLE_UIP_DHCPC=n

#
# Settings for examples/nettest
#
# CONFIG_EXAMPLE_NETTEST_SERVER - The target board can act
#   as either the client side or server side of the test
# CONFIG_EXAMPLE_NETTEST_PERFORMANCE - If set, then the
#   client side simply receives messages forever, allowing
#   measurement of throughput
# CONFIG_EXAMPLE_NETTEST_NOMAC - Set if the hardware has
#   no MAC address; one will be assigned
# CONFIG_EXAMPLE_NETTEST_IPADDR - Target board IP address
# CONFIG_EXAMPLE_NETTEST_DRIPADDR - Default router address
# CONFIG_EXAMPLE_NETTEST_NETMASK - Network mask
# CONFIG_EXAMPLE_NETTEST_CLIENTIP - IP address of the
#   client side of the test (may be target or host)
#
CONFIG_EXAMPLE_NETTEST_SERVER=n
CONFIG_EXAMPLE_NETTEST_PERFORMANCE=n
CONFIG_EXAMPLE_NETTEST_NOMAC=y
CONFIG_EXAMPLE_NETTEST_IPADDR=0x0a000002
CONFIG_EXAMPLE_NETTEST_DRIPADDR=0x0a000001
CONFIG_EXAMPLE_NETTEST_NETMASK=0xffffff00
CONFIG_EXAMPLE_NETTEST_CLIENTIP=0x0a000001

#
# Settings for examples/ostest
#
CONFIG_EXAMPLES_OSTEST_LOOPS=1
CONFIG_EXAMPLES_OSTEST_STACKSIZE=2048
CONFIG_EXAMPLES_OSTEST_NBARRIER_THREADS=3

#
# Settings for apps/nshlib
#
# CONFIG_NSH_BUILTIN_APPS - Support external registered,
#   "named" applications that can be executed from the NSH
#   command line (see apps/README.txt for more information).
# CONFIG_NSH_FILEIOSIZE - Size of a static I/O buffer
# CONFIG_NSH_STRERROR - Use strerror(errno)
# CONFIG_NSH_LINELEN - Maximum length of one command line
# CONFIG_NSH_NESTDEPTH - Max number of nested if-then[-else]-fi
# CONFIG_NSH_DISABLESCRIPT - Disable scripting support
# CONFIG_NSH_DISABLEBG - Disable background commands
# CONFIG_NSH_ROMFSETC - Use startup script in /etc
# CONFIG_NSH_CONSOLE - Use serial console front end
# CONFIG_NSH_TELNET - Use telnetd console front end
# CONFIG_NSH_ARCHINIT - Platform provides architecture
#   specific initialization (nsh_archinitialize()).
#
# If CONFIG_NSH_TELNET is selected:
# CONFIG_NSH_IOBUFFER_SIZE -- Telnetd I/O buffer size
# CONFIG_NSH_DHCPC - Obtain address using DHCP
# CONFIG_NSH_IPADDR - Provides static IP address
# CONFIG_NSH_DRIPADDR - Provides static router IP address
# CONFIG_NSH_NETMASK - Provides static network mask
# CONFIG_NSH_NOMAC - Use a bogus MAC address
#
# If CONFIG_NSH_ROMFSETC is selected:
# CONFIG_NSH_ROMFSMOUNTPT - ROMFS mountpoint
# CONFIG_NSH_INITSCRIPT - Relative path to init script
# CONFIG_NSH_ROMFSDEVNO - ROMFS RAM device minor
# CONFIG_NSH_ROMFSSECTSIZE - ROMF sector size
# CONFIG_NSH_FATDEVNO - FAT FS RAM device minor
# CONFIG_NSH_FATSECTSIZE - FAT FS sector size
# CONFIG_NSH_FATNSECTORS - FAT FS number of sectors
# CONFIG_NSH_FATMOUNTPT - FAT FS mountpoint
#
CONFIG_NSH_BUILTIN_APPS=y
CONFIG_NSH_FILEIOSIZE=512
CONFIG_NSH_STRERROR=n
CONFIG_NSH_LINELEN=64
CONFIG_NSH_NESTDEPTH=3
CONFIG_NSH_DISABLESCRIPT=n
CONFIG_NSH_DISABLEBG=n
CONFIG_NSH_ROMFSETC=n
CONFIG_NSH_CONSOLE=y
CONFIG_NSH_TELNET=n
CONFIG_NSH_ARCHINIT=y
CONFIG_NSH_IOBUFFER_SIZE=512
CONFIG_NSH_DHCPC=n
CONFIG_NSH_NOMAC=n
CONFIG_NSH_IPADDR=0x0a000002
CONFIG_NSH_DRIPADDR=0x0a000001
CONFIG_NSH_NETMASK=0xffffff00
CONFIG_NSH_ROMFSMOUNTPT="/etc"
CONFIG_NSH_INITSCRIPT="init.d/rcS"
CONFIG_NSH_ROMFSDEVNO=0
CONFIG_NSH_ROMFSSECTSIZE=64
CONFIG_NSH_FATDEVNO=1
CONFIG_NSH_FATSECTSIZE=512
CONFIG_NSH_FATNSECTORS=1024
CONFIG_NSH_FATMOUNTPT=/tmp

#
# Architecture-specific NSH options
#
CONFIG_NSH_MMCSDSPIPORTNO=2
CONFIG_NSH_MMCSDSLOTNO=0
CONFIG_NSH_MMCSDMINOR=0

#
# Settings for examples/usbserial
#
# CONFIG_EXAMPLES_USBSERIAL_INONLY
#    Only verify IN (device-to-host) data transfers.  Default: both
# CONFIG_EXAMPLES_USBSERIAL_OUTONLY
#    Only verify OUT (host-to-device) data transfers.  Default: both
# CONFIG_EXAMPLES_USBSERIAL_ONLYSMALL
#    Send only small, single packet messages.  Default: Send large and small.
# CONFIG_EXAMPLES_USBSERIAL_ONLYBIG
#    Send only large, multi-packet messages.  Default: Send large and small.
#
CONFIG_EXAMPLES_USBSERIAL_INONLY=n
CONFIG_EXAMPLES_USBSERIAL_OUTONLY=n
CONFIG_EXAMPLES_USBSERIAL_ONLYSMALL=n
CONFIG_EXAMPLES_USBSERIAL_ONLYBIG=n

CONFIG_EXAMPLES_USBSERIAL_TRACEINIT=n
CONFIG_EXAMPLES_USBSERIAL_TRACECLASS=n
CONFIG_EXAMPLES_USBSERIAL_TRACETRANSFERS=n
CONFIG_EXAMPLES_USBSERIAL_TRACECONTROLLER=n
CONFIG_EXAMPLES_USBSERIAL_TRACEINTERRUPTS=n

#
# Settings for examples/usbstorage
#
# CONFIG_EXAMPLES_USBMSC_NLUNS
#    Defines the number of logical units (LUNs) exported by the USB storage
#    driver.  Each LUN corresponds to one exported block driver (or partition
#    of a block driver).  May be 1, 2, or 3.  Default is 1.
# CONFIG_EXAMPLES_USBMSC_DEVMINOR1
#    The minor device number of the block driver for the first LUN. For
#    example, N in /dev/mmcsdN.  Used for registering the block driver. Default
#    is zero.
# CONFIG_EXAMPLES_USBMSC_DEVPATH1
#    The full path to the registered block driver.  Default is "/dev/mmcsd0"
#  CONFIG_EXAMPLES_USBMSC_DEVMINOR2 and CONFIG_EXAMPLES_USBMSC_DEVPATH2
#    Similar parameters that would have to be provided if CONFIG_EXAMPLES_USBMSC_NLUNS
#    is 2 or 3.  No defaults.
#  CONFIG_EXAMPLES_USBMSC_DEVMINOR3 and CONFIG_EXAMPLES_USBMSC_DEVPATH3
#    Similar parameters that would have to be provided if CONFIG_EXAMPLES_USBMSC_NLUNS
#    is 3.  No defaults.
#
#  If CONFIG_USBDEV_TRACE is enabled (or CONFIG_DEBUG and CONFIG_DEBUG_USB), then
#  the example code will also manage the USB trace output.  The amount of trace output
#  can be controlled using:
#
#  CONFIG_EXAMPLES_USBMSC_TRACEINIT
#    Show initialization events
#  CONFIG_EXAMPLES_USBMSC_TRACECLASS
#    Show class driver events
#  CONFIG_EXAMPLES_USBMSC_TRACETRANSFERS
#    Show data transfer events
#  CONFIG_EXAMPLES_USBMSC_TRACECONTROLLER
#    Show controller events
#  CONFIG_EXAMPLES_USBMSC_TRACEINTERRUPTS
#    Show interrupt-related events.
#
CONFIG_EXAMPLES_USBMSC_NLUNS=1
CONFIG_EXAMPLES_USBMSC_DEVMINOR1=0
CONFIG_EXAMPLES_USBMSC_DEVPATH1="/dev/mmcsd0"
CONFIG_EXAMPLES_USBMSC_TRACEINIT=n
CONFIG_EXAMPLES_USBMSC_TRACECLASS=n
CONFIG_EXAMPLES_USBMSC_TRACETRANSFERS=n
CONFIG_EXAMPLES_USBMSC_TRACECONTROLLER=n
CONFIG_EXAMPLES_USBMSC_TRACEINTERRUPTS=n

#
# Settings for examples/usbterm
#
# CONFIG_EXAMPLES_USBTERM_BUILTIN - Build the usbterm example as an NSH
#   built-in command.  NOTE:  This is not fully functional as of this
#   writing.. It should work, but there is no mechanism in place yet
#   to exit the USB terminal program and return to NSH.
# CONFIG_EXAMPLES_USBTERM_DEVINIT - If defined, then the example will
#   call a user provided function as part of its initialization:
#      int usbterm_devinit(void);
#   And another user provided function at termination:
#      void usbterm_devuninit(void);
# CONFIG_EXAMPLES_USBTERM_BUFLEN - The size of the input and output
#   buffers used for receiving data. Default 256 bytes.
#
# If CONFIG_USBDEV_TRACE is enabled (or CONFIG_DEBUG and CONFIG_DEBUG_USB, or
# CONFIG_USBDEV_TRACE), then the example code will also manage the USB trace
# output.  The amount of trace output can be controlled using:
#
# CONFIG_EXAMPLES_USBTERM_TRACEINIT
#   Show initialization events
# CONFIG_EXAMPLES_USBTERM_TRACECLASS
#   Show class driver events
# CONFIG_EXAMPLES_USBTERM_TRACETRANSFERS
#   Show data transfer events
# CONFIG_EXAMPLES_USBTERM_TRACECONTROLLER
#   Show controller events
# CONFIG_EXAMPLES_USBTERM_TRACEINTERRUPTS
#   Show interrupt-related events.
#
CONFIG_EXAMPLES_USBTERM_BUILTIN=y
CONFIG_EXAMPLES_USBTERM_DEVINIT=y
#CONFIG_EXAMPLES_USBTERM_BUFLEN
CONFIG_EXAMPLES_USBTERM_TRACEINIT=n
CONFIG_EXAMPLES_USBTERM_TRACECLASS=n
CONFIG_EXAMPLES_USBTERM_TRACETRANSFERS=n
CONFIG_EXAMPLES_USBTERM_TRACECONTROLLER=n
CONFIG_EXAMPLES_USBTERM_TRACEINTERRUPTS=n

#
# Settings for examples/cdcacm
#
# Configuration prequisites:
#
#   CONFIG_USBDEV=y         : USB device support must be enabled
#   CONFIG_CDCACM=y         : The CDC/ACM driver must be built
#   CONFIG_NSH_BUILTIN_APPS : NSH built-in application support must be enabled
#
# Configuration options specific to this example:
#
# CONFIG_EXAMPLES_CDCACM_DEVMINOR
#  The minor number of the CDC/ACM device.
# CONFIG_EXAMPLES_CDCACM_TRACEINIT
#   Show initialization events
# CONFIG_EXAMPLES_CDCACM_TRACECLASS
#   Show class driver events
# CONFIG_EXAMPLES_CDCACM_TRACETRANSFERS
#   Show data transfer events
# CONFIG_EXAMPLES_CDCACM_TRACECONTROLLER
#   Show controller events
# CONFIG_EXAMPLES_CDCACM_TRACEINTERRUPTS
#   Show interrupt-related events.
#
CONFIG_EXAMPLES_CDCACM_DEVMINOR=0
CONFIG_EXAMPLES_CDCACM_TRACEINIT=n
CONFIG_EXAMPLES_CDCACM_TRACECLASS=n
CONFIG_EXAMPLES_CDCACM_TRACETRANSFERS=n
CONFIG_EXAMPLES_CDCACM_TRACECONTROLLER=n
CONFIG_EXAMPLES_CDCACM_TRACEINTERRUPTS=n

#
# Stack and heap information
#
# CONFIG_BOOT_RUNFROMFLASH - Some configurations support XIP
#   operation from FLASH but must copy initialized .data sections to RAM.
#   (should also be =n for the PIC32MX which always runs from flash)
# CONFIG_BOOT_COPYTORAM -  Some configurations boot in FLASH
#   but copy themselves entirely into RAM for better performance.
# CONFIG_CUSTOM_STACK - The up_ implementation will handle
#   all stack operations outside of the nuttx model.
# CONFIG_STACK_POINTER - The initial stack pointer (arm7tdmi only)
# CONFIG_IDLETHREAD_STACKSIZE - The size of the initial stack.
#  This is the thread that (1) performs the inital boot of the system up
#  to the point where user_start() is spawned, and (2) there after is the
#  IDLE thread that executes only when there is no other thread ready to
#  run.
# CONFIG_USERMAIN_STACKSIZE - The size of the stack to allocate
#  for the main user thread that begins at the user_start() entry point.
# CONFIG_PTHREAD_STACK_MIN - Minimum pthread stack size
# CONFIG_PTHREAD_STACK_DEFAULT - Default pthread stack size
# CONFIG_HEAP_BASE - The beginning of the heap
# CONFIG_HEAP_SIZE - The size of the heap
#
CONFIG_BOOT_RUNFROMFLASH=n
CONFIG_BOOT_COPYTORAM=n
CONFIG_CUSTOM_STACK=n
#CONFIG_STACK_POINTER
CONFIG_IDLETHREAD_STACKSIZE=2048
CONFIG_USERMAIN_STACKSIZE=2048
CONFIG_PTHREAD_STACK_MIN=256
CONFIG_PTHREAD_STACK_DEFAULT=2048
CONFIG_HEAP_BASE=
CONFIG_HEAP_SIZE=
