
#================================================
# WANPIPE1 Configuration File
#================================================
#
# Date: Fri Jun 25 16:47:33 EDT 2004
#
# Note: This file was generated automatically
#       by /usr/sbin/wancfg program.
#
#       If you want to edit this file, it is
#       recommended that you use wancfg program
#       to do so.
#================================================
# Sangoma Technologies Inc.
#================================================

[devices]
wanpipe1 = WAN_AFT_TE1, Comment  #WAN_AFT_TE1 - Indicates A104/8 card
                                 #WAN_AFT     - Indicates A101/2 card


[interfaces]
w1g1 = wanpipe1, , STACK, Comment               	#do not change
w1lapd = wanpipe1, 1 ,API, lip_lapd, lapd.w1g1,         #do not change


[wanpipe1]
#-------- DEVICE / DRIVER BINDING ----------------------------------

CARD_TYPE       = AFT   #AFT: Same for all aft cards must
                        #This value must be hardcoed to AFT for all
                        #aft cards.

S514CPU         = A     #Used by A101/2 driver to determine T1/E1 port
                        #A - port 1
                        #B - port 2
                        #For A104 driver: Always set this value to A!

CommPort        = PRI   #Only used by S514 cards.
                        #PRI - S514 primary port
                        #SEC - S514 secondary port
                        #
                        #OBSELETE for AFT cards (can be removed)

#-------- PCI SETUP ----------------------------------------------


AUTO_PCISLOT    = NO    #Auto detect PCI/BUS info for this card type
                        #NO - disable this option
                        #YES- enable this option
                        #     if enabled bottom two options
                        #     PCISLOT and PCIBUS will not be used.
                        #     Therefore one can set the to arbitrary value
                        #     or remove them all together.

PCISLOT         = 1     #PCI SLOT Number:
                        #Valid values = any number

PCIBUS          = 3     #PCI BUS Number:
                        #Valid values = any number



#--------------FRONT END SETUP -----------------------------------

FE_MEDIA        = T1    #Front End Type:
                        #T1 - set front end for T1 mode
                        #E1 - set front end for E1 mode

FE_LCODE        = B8ZS  #Front End Line Coding
                        #If T1:  B8ZS or AMI
                        #   E1:  HDB3 or AMI

FE_FRAME        = ESF   #Front End Framing
                        #If T1:  ESF or D4
                        #   E1:  CRC4 or NCRC4

FE_LINE         = 1       #Front End Line number.
                          #Used by A104 driver to determine T1/E1 port
                          #Valid values are: 1-4
                          #
                          #The A101/2 driver doesn't use this option
                          #so one should hardcode it to 1 or
                          #remove it all together.


TE_CLOCK        = NORMAL  #T1/E1 Clock Source
                          #NORMAL - slave clock, clock is received from telco
                          #         This is always the DEFAULT
                          #MASTER - master clcok, use hw oscillator clock
                          #         Only used in back to back mode or
                          #         when specified by telco.

TE_REF_CLOCK    = 0       #T1/E1 Reference Clock Source
                          #This option allows one to use the incoming clock
                          #from a different port as a clock source to this
                          #port.  FOR THIS OPTION TO WORK: TE_CLOCK=MASTER
                          #Valid options: 0   - disable
                          #               1-4 - use clock from particular port

ACTIVE_CH       = ALL     #Specify T1/E1 Active channels (timeslots)
                          #Since AFT cards support channelization this
                          #option MUST BE HARDCODED TO:  ALL!

TE_HIGHIMPEDANCE        = NO  #Set the Front Ent chip in High Impedance mode
                              #used for datascoping:
                              #NO - Disable high impedance mode (DEFAULT)
                              #YES - Enable hight impedance mode
                              #      (only if you know what you are doing)

IGNORE_FRONT_END = NO
LBO             = 0DB     #Front End Line Buildout
                          # 0db     (Default)
                          # 7.5dB
                          # 15dB
                          # 22.5dB
                          # 0-110ft
                          # 110-220ft
                          # 220-330ft
                          # 330-440ft
                          # 440-550ft
                          # 550-660ft

FE_TXTRISTATE   = NO      #Front End Tri-State Mode
                          #Disable front end chip TX mode
                          #Used for datascoping or connecting multiple ports
                          #together where one port is operating normally and others
                          #are tristated, thus only receiving.
                          #NO - Disable tristae mode
                          #YES- Enable tristate mode

MTU             = 1500    #Global MTU Value
                          #Note: This value is overwritten by the
                          #      interface MTU value below if it exists.
                          #Values: any number [ suggested 128 - 4086 ]


UDPPORT         = 9000    #OBSELETE option
                          #Old wanpipemon used sockets to connect to
                          #device driver.

TTL             = 255     #OBSELETE option
                          #Old wanpipemon used sockets to connect to
                          #device driver.

IGNORE_FRONT_END = NO     #Ignore Fronte End State
                          #NO - Do not ignore front end state,
                          #     therefore if state changes, change the
                          #     state of the above protocol.
                          #YES- Igonore front end state
                          #     Thus if front end goes down, the protocol
                          #     will not know.


#--------------------------------------------
#Q921/LAPD  Profile Configuration
#--------------------------------------------

[lapd.w1g1]
LAP_STATION	= DTE     
T1	= 2
T2	= 0
T3	= 6
T4	= 3
N2	= 5
LAP_MODE = 128
LAP_WINDOW  = 7
MAX_PKT_SIZE = 1024



#--------------------------------------------
#Hardware Interface Configuration
#--------------------------------------------


[w1g1]
HDLC_STREAMING	= YES 	#Enable hardware hdlc engine
			#(Do not change)

ACTIVE_CH       = 24	#DCHAN on T1/E1 Span
			#For T1 select 24
			#For E1 seelct 16
			#(Confirm with telco)

[w1lapd]
