; Each section in this file describes a SIGTRAN connection
; Connections are referenced from other configurations describing the upper layer

;[name-of-connection]
; The name of the section identifies the connection

; type: keyword: Socket type - sctp, tcp, udp, unix
;type=sctp

; stream: bool: Socket connection type.
; Designed for SCTP sockets to create a stream socket or a sequenced packet socket
; NOTE: for M2PA if stream is false the M2PA autostart should be on true on both ends,
;  if stream is true the M2PA autostart must be true only at one end
;stream=true for TCP or UNIX sockets, false for other types

; local: string: Primary local address
; Format is ipv4:port like: 1.1.1.1:3566
;local=

; localN: string: Additional local addresses, SCTP only
; Multiple addresses can be specified by incrementing the 1-based index at the end of 'local'
; The address format is ip:port like:
;  local1=1.2.3.4:3566
;  local2=2.3.4.5:3566
;local1=

; remote: string: Primary remote address
; Format is ipv4:port like: 2.2.2.2:3566
;remote=

; remoteN: string: Additional remote addresses, SCTP only
; Multiple addresses can be specified by incrementing the 1-based index at the end of 'remote'
; The address format is ip:port like:
;  remote1=5.6.7.8:3566
;  remote2=6.7.8.9:3566
;remote1=

; endpoint: bool: Set to true if this is an endpoint that actively tries to connect,
;  false to listen for remote connections
;endpoint=false
