; This file keep signalling channel configuration
; Each section (except for 'general' section) configure a call controller (trunk)
;  or a signalling component
; For call controllers (trunks), the name of the section will be used to route
;  outgoing calls


; IMPORTANT:
;  The configuration has changed between Yate 2 and 3, you must check the
;  configuration against the relevant sample if upgrading.


[general]
; This section keep general or default settings for the signalling module:

; debuglevel: int: Debug level for the plugin
; This parameter is applied on reload
;debuglevel=

; debuglevel_engine: int: Debug level for the signalling engine
; This parameter is applied on reload
;debuglevel_engine=

; dtmfinband: boolean: Enable to try to send the DTMF data in band when an audio
;  channel is available. If disabled or no audio channel available, the DTMF will
;  be sent through the signalling channel if any
;dtmfinband=no

; floodevents: int: How many events retrieved in a row trigger a flood warning
; Can be overridden in each ss7-isup, isdn-pri-... or isdn-bri-... section
;floodevents=20

; datafile: string: File to save/restore trunks data (circuits lock status)
; Defaults to ysigdata.conf located in current config directory
; If set the file must contain the path (relative or absolute)
; This parameter is applied on reload
;datafile=

; Each section except [general] can have some common parameters

; To disable the component without deleting the entire section.
; The default is to enable the component
; enable: bool: Allow creation of the component corresponding to the section
;enable=yes

; Debug name as reported in Yate logs, default is derived from component name
; This parameter is used only when a component is created
; debugname: string: Debug name of the created component
;debugname=

; Debug level to apply on creation or reload
; debuglevel: int: Debug level of the component
;debuglevel=


; Example of an ISDN trunk
;[trunk1]

; type: keyword: Specify the trunk type 
; Allowed values:
;  isdn-bri-net:  ISDN network side of a data link over basic rate HDLC interface(s)
;  isdn-bri-cpe:  ISDN CPE (user) side of a data link over basic rate HDLC interface(s)
;  isdn-pri-net:  ISDN network side of a data link over one or more primary HDLC interface(s)
;  isdn-pri-cpe:  ISDN CPE (user) side of a data link over one or more primary HDLC interface(s)
; NOTE: isdn-pri-net and isdn-pri-cpe are identical, except for the side of the link
;type=

; switchtype: string: The switch type of this group
; This parameter defines a set of flags modifying the call controller's behaviour
; Allowed values: euro-isdn-e1, euro-isdn-t1, national-isdn, dms100, lucent5e, att4ess, qsig, unknown
;switchtype=unknown

; sig: string: Specify the span(s) containing the signalling channel (D)
; For example wanpipe1 or any other section specified in any of the telephony
;   modules like wpcard or zapcard
;sig=

; voice: string: Specify the span(s) containing the voice channels (B)
; Multiple cards may be specified by simply separating them with a comma (',')
;  character
; Defaults to the value of "sig" and then to trunk name if missing
; It is mandatory to have voice circuits configured
; NOTE: The default has changed from Yate 2 because of architecture differences
;voice=

; offset: int: Offset of voice circuit codes relative to low level circuit number
;offset=0

; range: string: Arbitrary ranges of circuits for outbound calls (can be repeated)
; Possible formats:
;  range=name:list of circuits (like 1,3,5-9)
;  range=name:strategy:list of circuits (like 1,3,5-9)

; number: string: Prefix of numbers we accept call setups for, empty to accept all
; Only used by isdn-pri-cpe, makes sense when NET side is Point-to-Multipoint
; Setups are ignored if called number is present but doesn't start with this prefix
;number=

; rxunderrun: int: Maximum interval in ms between two packets before we report
;  an underrun condition, zero to disable or 2500+
;rxunderrun=0

; strategy: string: The strategy used to allocate voice channels for outgoing calls
; Allowed values:
;  - increment  Incremental search an idle channel starting with the last allocated channel
;  - decrement  Decremental search an idle channel starting with the last allocated channel
;  - lowest     Incremental search an idle channel starting with the first channel in group
;  - highest    Decremental search an idle channel starting with the last channel in group
;  - random     Randomly choose an idle channel
; Defaults to increment
;strategy=increment

; strategy-restrict: string: Define channel allocation restrictions and behaviour
; This option is ignored when strategy is random
; Allowed values:
;    even           Allocate only even channels
;    odd            Allocate only odd channels
;    even-fallback  Allocate even channels, fall back to odd channels
;    odd-fallback   Allocate odd channels, fall back to even channels
;strategy-restrict=

; channelsync: integer: The interval (in seconds) at which the call controller
;  will try to re-sync idle channels
; The call controller will notify the other side of the link of idle channels
; Set to 0 to disable
; Invalid values default to minimum (60s)
;channelsync=300

; channellock: integer: Maximum time (in ms) spent trying to lock a remote channel
; Invalid values default to minimum (2500ms)
;channellock=10000

; numplan: string: Default numbering plan for outgoing calls
; Values: unknown, isdn, data, telex, national, private
; Defaults to unknown if missing or incorrect
;numplan=unknown

; numtype: string:  Default number type for outgoing calls
; Values: unknown,international,national,net-specific,subscriber,abbreviated,reserved
; Defaults to unknown if missing or incorrect
;numtype=unknown

; presentation: string: Default number presentation for outgoing calls
; Values: allowed, restricted, unavailable
; Defaults to allowed if missing or incorrect
;presentation=allowed

; screening: string:  Default number screening for outgoing calls
; Values: user-provided, user-provided-passed, user-provided-failed, network-provided
; Defaults to user-provided if missing or incorrect
;screening=user-provided

; format: string:  Default data format for outgoing calls. Values: alaw, mulaw, g721
; Defaults to alaw if missing or incorrect
; alaw is used commonly in Europe while mulaw is used commonly in US and Japan.
;format=alaw

; ringback: boolean: Offer a ringback tone even if not provided by peer channel
; If it fails the correct indication (no inband available) is signaled
;ringback=no

; floodevents: int: How many events retrieved in a row trigger a flood warning
; Default value is taken from the [general] section
;floodevents=20

; print-messages: boolean: Print decoded protocol data units to output
; This option is applied on reload
; Defaults to no
;print-messages=no

; print-frames: boolean: Print decoded Layer 2 (Q.921) frames to output
; This option is applied on reload
; Defaults to no
;print-frames=no

; extended-debug: boolean: Print extended debug data (such as raw hex data) to output
; This option is applied on reload
; Defaults to no
;extended-debug=no

; layer2dump: string: Filename to dump Q.921 packets to
;layer2dump=

; layer3dump: string: Filename to dump Q.931 packets to
;layer3dump=


; Example of an ISDN passive recorder
;[recorder1]

; type: keyword: Specify the trunk type 
; Allowed values:
;  isdn-pri-mon:  ISDN monitor of one or more primary HDLC interface(s)
;type=isdn-pri-mon

; sig-net: string: Specify the span(s) containing the signalling channel(s) for the network side of the monitored link
; For example wanpipe1 or any other section specified in any of the telephony
;   modules like wpcard or zapcard
;sig-net=

; sig-cpe: string: Specify the span(s) containing the signalling channel(s) for the user side of the monitored link
; For example wanpipe1 or any other section specified in any of the telephony
;   modules like wpcard or zapcard
;sig-cpe=

; voice-net: string: Specify the span(s) containing the voice channel(s) for the network side of the monitored link
; Multiple cards may be specified by simply separating them with a comma (',') character
; Defaults to the span specified in the sig-net parameter
;voice-net=

; voice-cpe: string: Specify the span(s) containing the voice channel(s) for the user side of the monitored link
; Multiple cards may be specified by simply separating them with a comma (',') character
; Defaults to the span specified in the sig-cpe parameter
;voice-cpe=

; detect: boolean: Change the side of the link on each captured request for watched signalling span(s)
; If disabled and the side of the link is not correct, the monitor will not be notified on
;   data link state change. This may lead to malfunction
;detect=yes

; idletimeout: integer: HDLC data link idle timeout, should be 3 * T203
; The minimum allowed value is 4000ms. Defaults to 30000 if missing or invalid
;idletimeout=30000

; muxchanbuffer: integer: The buffer size for one channel of the audio multiplexer
; Defaults to 160 if 0 or missing
;muxchanbuffer=160

; idlevalue: integer: The value used by the audio multiplexer to fill missing data
; This value is used to fill the free space when the multiplexer has to forward the received
;   data but one channel buffer is not full
; Interval: 0..255. Defaults to 255 if missing or invalid
; Ignored if type is not isdn-pri-mon
;idlevalue=255

; floodevents: int: How many events retrieved in a row trigger a flood warning
; Default value is taken from the [general] section
;floodevents=20

; layer2dump-net: string: Filename to dump NET Q.921 packets to
;layer2dump-net=

; layer2dump-cpe: string: Filename to dump CPE Q.921 packets to
;layer2dump-cpe=


; Example of a SS7 ISUP trunk
;[isup1]
; type: keyword: Specify the trunk type 
; Allowed values:
;  ss7-isup:      SS7 ISDN User Part
;type=ss7-isup

; pointcodetype: string: SS7 point code type (required)
; Allowed values:
;  ITU    ITU-T Q.704
;  ANSI   ANSI T1.111.4
;  ANSI8  8-bit SLS
;  China  GF 001-9001
;  Japan  T-Q704, NTT-Q704
;  Japan5 5-bit SLS
;pointcodetype=

; pointcode: string: Local point code to accept as destination
; If no point codes are added no calls can be made (incoming or outgoing)
;  through this trunk
; The format is network-cluster-member or number
;pointcode=

; defaultpointcode: string: Default originating point code used for outgoing calls
; It also acts as accepted point code (see pointcode)
; Only one point code can be default
; The format is network-cluster-member or number
;defaultpointcode=

; remotepointcode: string: Default destination point code used for outgoing
;  calls and maintenance messages
; If missing or invalid, no maintenance message will be sent
; The format is network-cluster-member or number
;remotepointcode=

; service: int: Service Information Field (protocol number)
; It is unlikely you will ever need to modify it
;service=5

; priority: keyword: Value of the Priority bits in the Service Information Octet
; Allowed values: regular, special, circuit, facility
;priority=regular

; netindicator: keyword: Value of Network Indicator bits in the SIO
; Allowed values: international, spareinternational, national, reservednational
;netindicator=national

; router: string: Name of the SS7 Router to attach to
; A boolean false value disables attaching a router (unlikely)
;router=ss7router

; network: string: Name of linkset to attach to if router is disabled
; This allows direct connection without MTP management (unlikely)
;network=

; userparttest: integer: Remote user part test interval in seconds
; Set to 0 to always assume the remote user part is available
; Invalid values default to minimum (10s)
;userparttest=60

; parttestmsg: keyword: ISUP message to use for user part test
; For ANSI the CVT message may be used instead on UPT
; Other possibilities are RSC and UBL but are not recommended
;parttestmsg=UPT

; lockgroup: boolean: Allow sending circuit group block/unblock requests
; Normally the remote side must support circuit group operations
;lockgroup=yes

; earlyacm: boolean: Convert received early ACM user state into progress or ringing
;earlyacm=yes

; voice: string: Specify the span(s) containing the voice channels (L1)
; Multiple cards may be specified by simply separating them with a comma (',')
;  character
; It is mandatory to have voice circuits configured
; Defaults to the trunk name if missing
;voice=

; offset: int: Offset of voice circuit codes relative to low level circuit number
;offset=0

; range: string: Arbitrary ranges of circuits for outbound calls (can be repeated)
; Possible formats:
;  range=name:list of circuits (like 1,3,5-9)
;  range=name:strategy:list of circuits (like 1,3,5-9)

; strategy: string: The strategy used to allocate voice channels for outgoing calls
; Allowed values:
;  - increment  Incremental search an idle channel starting with the last allocated channel
;  - decrement  Decremental search an idle channel starting with the last allocated channel
;  - lowest     Incremental search an idle channel starting with the first channel in group
;  - highest    Decremental search an idle channel starting with the last channel in group
;  - random     Randomly choose an idle channel
; Defaults to increment
;strategy=increment

; strategy-restrict: string: Define channel allocation restrictions and behaviour
; This option is ignored when strategy is random
; Allowed values:
;    even           Allocate only even channels
;    odd            Allocate only odd channels
;    even-fallback  Allocate even channels, fall back to odd channels
;    odd-fallback   Allocate odd channels, fall back to even channels
;strategy-restrict=

; channelsync: integer: The interval (in seconds) at which the call controller
;  will try to re-sync idle channels
; The call controller will notify the other side of the link of idle channels
; Set to 0 to disable
; Defaults to minimum value (60s) if missing or invalid
;channelsync=300

; sls: integer or keyword: Default Signaling Link Selection in outbound calls
; Allowed values:
;    auto    Let SS7 Layer3 add a proper value
;    last    Last SLS used (default for non-ITU)
;    cic     Use the circuit number as SLS (ITU style)
;    0..255  Explicit numeric value, gets truncated to the SLS bit range
; NOTE: The default has changed from Yate 2
;sls=last (cic if pointcodetype is ITU)

; numplan: string: Default numbering plan for outgoing calls
; Values: unknown, isdn, data, telex, national, private
; Defaults to unknown if missing or incorrect
;numplan=unknown

; numtype: string:  Default number type for outgoing calls
; Values: unknown,international,national,net-specific,subscriber,abbreviated,reserved
; Defaults to unknown if missing or incorrect
;numtype=unknown

; presentation: string: Default number presentation for outgoing calls
; Values: allowed, restricted, unavailable
; Defaults to allowed if missing or incorrect
;presentation=allowed

; screening: string:  Default number screening for outgoing calls
; Values: user-provided, user-provided-passed, user-provided-failed, network-provided
; Defaults to user-provided if missing or incorrect
;screening=user-provided

; inn: boolean: Routing to Internal Network Number allowed
; Defaults to no
;inn=no

; format: string: Default data format for outgoing calls. Values: alaw, mulaw, g721
; Defaults to mulaw for ANSI and Japan point codes, alaw for all others
; alaw is used commonly in Europe while mulaw is used commonly in US and Japan.
;format=

; continuity: string: Type of continuity check to perform on the circuits
; If not set calls that request continuity check will be rejected
;continuity=

; ringback: boolean: Offer a ringback tone even if not provided by peer channel
; If it fails the correct indication (no inband available) is signaled
;ringback=no

; location: string: Exchange location to be set when sending Q.850 causes
; Available values are: 
;   U    User
;   LPN  Private network serving the local user
;   LN   Public network serving the local user
;   TN   Transit network
;   RLN  Public network serving the remote user
;   RPN  Private network serving the remote user
;   INTL International network
;   BI   Network beyond the interworking point
; A default 'BI' will be used if not set or invalid
;location=

; confirm_ccr: boolean: Send a Loopback Ack (national use) in response to Continuity Check Request message
; Defaults to yes
;confirm_ccr=yes

; drop_unknown: boolean: Drop call or attempt to change circuit if an unknown
;  or unsupported message is received in an early state
;drop_unknown=yes

; needmedia: keyword: When is media absolutely required to continue the call
; In case of circuit failure the call may continue and retry circuit setup later
; Allowed values:
;    no        Media not required, always continue the call (default)
;    ringing   Media required after call is ringing
;    answered  Media required after call is answered
;    yes       Media required from the beginning
;needmedia=no

; maxcalleddigits: int: Maximum number of digits sent in Called Party Number in IAM
; Any digits exceeding this limit will be sent separately in a SAM
;maxcalleddigits=16

; ignore-unknown-digits: boolean: Ignore signal digits that are not ITU standard (A, D and E)
; The standard set includes only 0-9, B, C and the stop pulsing "."
; ISUP does not support sending the * and # signals
;ignore-unknown-digits=yes

; ignore-grs-single: boolean: Ignore (drop) circuit group reset messages with
;  range 0 (1 circuit affected)
; Defaults to no
;ignore-grs-single=no

; ignore-cgb-single: boolean: Ignore (drop) circuit group blocking requests with
;  range 0 (1 circuit in map)
; Defaults to no
;ignore-cgb-single=no

; ignore-cgu-single: boolean: Ignore (drop) circuit group unblocking requests with
;  range 0 (1 circuit in map)
; Defaults to no
;ignore-cgu-single=no

; duplicate-cgb: boolean: Duplicate all sent circuit group blocking requests
; Defaults to yes if pointcodetype is ANSI or ANSI8, no for other types
;duplicate-cgb=

; floodevents: int: How many events retrieved in a row trigger a flood warning
; Default value is taken from the [general] section
;floodevents=20

; print-messages: boolean: Print decoded protocol data units to output
; This option is applied on reload
; Defaults to no
;print-messages=no

; extended-debug: boolean: Print extended debug data (such as raw hex data) to output
; This option is applied on reload
; Defaults to no
;extended-debug=no


; Example of a SS7 MTP3 network (linkset)
;[linkset1]
; type: keyword: Specify the linkset type 
; Allowed values:
;  ss7-mtp3:      SS7 Message Transfer Part - Layer 3
;type=ss7-mtp3

; netind2pctype: string: Comma separated list of point code types used to map an
;  incoming network indicator to a specific point code type
; This option is required and is used to configure a SS7 MTP3 network
; The list must contain either a singe type or 4 values indicating the point
;  code type for International, SpareInternational, National and ReservedNational
;  network indicators
; If only a single type is specified it will be used to configure all types of
;  network indicators
; See the ISUP pointcodetype option for allowed values
; NOTE: An incoming packet with an unconfigured network indicator will be dropped
; Examples:
;  netind2pctype=ITU
;  netind2pctype=ITU,ANSI,ITU,ITU
;  netind2pctype=ANSI8,ITU,ANSI,ITU
;netind2pctype=

; netindicator: keyword: Default value of Network Indicator bits
; Allowed values: international, spareinternational, national, reservednational
;netindicator=national

; route: string: Build a destination route for the SS7 network
; The format of this option is pointcodetype,label,priority
; This parameter can be repeated to build multiple destination routes
; The network will notify the router about its destination(s) and priority
; If not specified the priority is 100. A zero priority creates an adjacent route
; Example: route=ITU,2-2-2,100
;route=

; adjacent: string: Build an adjacent route for the SS7 network (A, E and F links)
; The format of this option is pointcodetype,label
; This parameter can be repeated to declare multiple adjacent routers
; The network will notify the router about its destination(s) and priority
; The priority is always zero so an adjacent route will always match first.
; Example: adjacent=ANSI,40-50-60
;adjacent=

; local: string: Declare a local pointcode for the SS7 network
; The format of this option is pointcodetype,label
; This parameter can be repeated to declare a local point codes per type
; To be standards compliant at least one local pointcode must be declared
; Example: local=ITU,2-2-4
;local=

; allowed: string: List of point codes explicitely allowed from this SS7 network
; An empty or missing list will allow access to all known routes
; Example: allowed=ITU,2-2-2,2-2-3,1001,2001,2002
;allowed=

; router: string: Name of the SS7 Router to attach to
; A boolean false value disables attaching a router (unlikely)
; If no router is attached only a single User Part can be connected
;router=ss7router

; link: string: Name of a SS7 Layer 2 link to create in the linkset
; This parameter can be repeated to add more links to the linkset
; An explicit SLS can be provided after a comma
; Example: link=mtp2_to_hq,3
;link=

; autostart: bool: Automatically enable the linkset at startup
; This should be enabled (default) for normal operation
;autostart=yes

; checklinks: boolean: Check that the links answer to maintenance messages
;  (SLTM/SLTA) before placing them into service (normal behavior)
;checklinks=true

; forcealign: boolean: Realign links that are no longer responding to SLTM
;forcealign=true

; checkfails: integer: Interval in msec for resending SLTM messages (Q.707 T1)
; A value of zero disables link fail else the value is clamped between 4s - 12s
;checkfails=5000

; maintenance: integer: Interval in msec for sending SLTM messages (Q.707 T2)
; A value of zero disables periodic SLTM else it is clamped to range 30s - 5m
;maintenance=60000

; layer3dump: string: Filename to dump MTP3 packets to
;layer3dump=


; Example of a SS7 MTP2 link
;[link1]
; type: keyword: Specify the link type 
; Allowed values:
;  ss7-mtp2:      SS7 Message Transfer Part - Layer 2
;type=ss7-mtp2

; autostart: bool: Automatically try to align the MTP2 at startup or on failure
; This should be enabled (default) for normal operation
;autostart=yes

; emergency: boolean: Emergency align SS7 MTP2 layer at startup
;emergency=yes

; autoemergency: boolean: Emergency align link if owner linkset is down
;autoemergency=yes

; filllink: boolean: Configure MTP2 to request link fill (packet repeat) when
;  sending FISU or LSSU packets
;filllink=yes

; maxerrors: int: Number of consecutive errors that cause realignment
; This parameter is constrained between 8 and 256
; When in proving interval this setting is ignored and realignment occurs at
;  4 errors in normal proving or 1 error in emergency proving
;maxerrors=64

; rxunderrun: int: Maximum interval in ms between two packets before we report
;  an underrun condition, zero to disable or 25+
;rxunderrun=0

; layer2dump: string: Filename to dump MTP2 packets to
;layer2dump=


; Example of a SS7 router (combines discrimination and SN or STP functions)
; A router named 'ss7router' is implicitely declared with default parameters
;[ss7router]
; type: keyword: identifies the component as a SS7 Router
;type=ss7-router

; transfer: boolean: Enable the Transfer function (STP mode)
; Enabling STP allows routing messages between adjacent networks
; By default only the SN and discrimination functions are enabled
; The special "silent" value performs message transfer without advertising
;transfer=no

; local: string: Declare a default local pointcode for the attached SS7 networks
; The format of this option is pointcodetype,label
; This parameter can be repeated to declare a local point codes per type
; Example: local=ITU,2-2-4
;local=

; management: string: Name of the SS7 Management component to create
; A boolean false value will disable SS7 Management (unlikely)
;management=ss7snm

; starttime: integer: MTP restart timer (T20) in milliseconds
; It is enforced to be at least 5000 (5s)
; Defaults to 60000 (Q.704 standard value) in STP mode or 10000 in SN mode
;starttime=

; isolation: integer: MTP isolation timer (T1) in milliseconds
; The minimum value is 500 (0.5s), default 1000 (1s)
; A value of zero disables isolation checks entirely
;isolation=1000

; autostart: boolean: Perform MTP restart sequence at initialization
; According to the standard the restart is performed on first link activation
;autostart=no

; autoallow: boolean: Turn adjacent routes Allowed on first received regular MSU
; Should be used only to interoperate with broken implementations
;autoallow=no

; sendupu: boolean: Send User Part Unavailable (UPU) SNM messages
;sendupu=yes

; sendtfp: boolean: Send Transfer Prohibited (TFP) SNM messages
; This setting applies only to transfer function (STP operation mode)
;sendtfp=yes

; testroutes: integer: Signaling Route Test timer (T10) in milliseconds
; The minimum value is 10000 (10s), Q.704 recommends 30s to 60s
; A value of zero disables periodical route tests
; testroutes=50000

; testrestricted: boolean: Test restricted routes too (national option)
;testrestricted=no


; Example of a SS7 Management Part
; This component is created by the SS7 router, see its "management" setting
; A management named 'ss7snm' is implicitely declared with default parameters
;[ss7snm]
; type: keyword: identifies the component as a SS7 Management Part
;type=ss7-snm

; local: string: Declare a default local pointcode for messages to send
; The format of this option is pointcodetype,label
; This parameter can be repeated to declare a local point codes per type
; If missing the local address of the attached router is used
; Example: local=ITU,2-2-4
;local=

; priority: keyword: Value of the Priority bits in the Service Information Octet
; Allowed values: regular, special, circuit, facility
;priority=regular

; netindicator: keyword: Default value of Network Indicator bits in the SIO
; Allowed values: international, spareinternational, national, reservednational
;netindicator=national

; changemsgs: boolean: Emit and process changeover and changeback messages
; Disabling these messages forces always using time controlled diversion
;changemsgs=yes

; changesets: boolean: Emit changeover and changeback between linksets
; Requires "changemsgs" to be enabled to allow sequence controlled diversion
;  procedures to be used on another linkset if the controlled one is unavaliable
;changesets=no

; neighbours: boolean: Only accept management messages from adjacent nodes
;neighbours=yes


; Example of a SS7 SCCP
;[sccp]

; type: keyword: identifies the component as a SS7 SCCP
;type=ss7-sccp

; pointcodetype: string: SS7 point code type (required)
; Allowed values:
;  ITU    ITU-T Q.704
;  ANSI   ANSI T1.111.4
;pointcodetype=

; localpointcode: string: Local point code to accept as destination (required)
; The format is network-cluster-member or number
;localpointcode=

; router: string: Name of the SS7 Router to attach to
; A boolean false value disables attaching a router (unlikely)
;router=ss7router

; network: string: Name of linkset to attach to if router is disabled
; This allows direct connection without MTP management (unlikely)
;network=

; management: string: Name of the SS7 management to use
;management=sccp-mgm

; hopcounter: integer: Default value for hop-counter
; This value indicates the maximum number of gt translations that can be
;  made before the message reach it's destination
;hopcounter=15

; ludt-support: boolean: True to allow sccp to send Long UnitData messages
;ludt-support=false

; segmentation-timeout: integer: Time in milliseconds before a segmented
;  message is expired
; Values: 5000-20000 ms
;segmentation-timeout=5000

; extended-monitoring: boolean: Compute an extended monitoring of sccp messages
;extended-monitoring=no

; print-messages: boolean: Print decoded protocol data units to output
; This option is applied on reload
; Defaults to no
;print-messages=no

; extended-debug: boolean: Print extended debug data (such as raw hex data)
;  to output
; This option is applied on reload
; Defaults to no
;extended-debug=no

; endpoint: boolean: Force message processing if we are an endpoint
; This option will allow sccp to process failed gt translations messages
;  if a ssn is pressent
;endpoint=true;


; Example of SS7 Sccp Management
;[sccp-mgm]

; type: keyword: identifies the component as a SS7 SCCP Management
; Values : ss7-sccp-itu-mgm 
; Must correspond with the pointcode type of the sccp
;type=

; test-timer: integer: Initial time in milliseconds for Subsystem Status
;  Test to be generated
; Values : 5000-10000
; Note! This timer will increase exponentially until reaches 20000 if no
;  corresponding message is received from the test initiator
;test-timer=5000

; print-messages: boolean: True to print sccp management messages
;print-messages=false

; remote: struct: Remote SCCP witch present interest for GTT
;  (Global Title Translator)
; This parameter allow us to monitor remote sccp's state
; This option can be repeated to monitor multiple remote sccp's
; Format: remote=pc(integer):ssn1,ssn2,....
; pc : integer: Remote sccp pointcode
; ssn1 - ssnn: integer; Remote sccp subsystems witch we are monitoring
; Note! Ssn list may be empty if the remote sccp is a stp with GTT
;remote=2057:1,2,3,4

; concerned: struct: List of remote sccp's witch are concerned about local state
; This parameter allow us to inform remote sccp's when local status has changed
; This option can be repeated to inform multiple remote sccp's
; Format: remote=pc(integer):ssn1,ssn2,....
; pc : integer: Remote sccp pointcode
; ssn1 - ssnn: integer; List of local subsystems witch are of interest for the
;  remote sccp
; Note! Ssn list may be empty if the remote sccp is concerned only if local 
;  sccp is available or not
;concerned=2057:1,2,3,4

; local-subsystems: string: Coma separated list of local subsystems
; The subsystems present in this list will be monitored by this sccp management
;local-subsystems=1,2,3,4,5,..

; auto-monitor: boolean: True to auto monitor remote sccp's.
; This flag enables remote sccp auto monitoring. When a message failed to be 
;  send to a remote sccp, the sccp management will automaticaly append the 
;  destination to the monitored remote sccp destinations
;  to prevent sccp routing failure.
; NOTE! Do not use this option if your GTT (Global Title Translator)
;  can route to a large number of remote addresses
;  because a lot of memory and cpu power will be used!
;auto-monitor=false


; Example of GTT (Global Title Translator)
;[gtt]

; type: keyword: Identifies this component as a GTT
; NOTE! This type of gtt is based on yate messages system.
;type=ss7-gtt

; sccp: string: The name of the sccp to attach to this GTT
;sccp=sccp


; Example of dummy sccp user
;[sccp-userd]
; Sccp user dummy sends a message over sccp protocol.

; type: keyword: Identifies this component as a Sccp User Dummy
;type=ss7-sccpu-dummy

; sccp: string: The name of the sccp to attach to this Sccp User
;sccp=sccp

; ssn: integer: Optional ssn asociated with this user
; If this parameter is present this user will accept only the messages who
;  have the same ssn
;ssn=0


; Example of a SS7 Transaction Capabilities Application Part
; This component is created when encountering a section of this kind
;[ss7tcap]
; type: keyword: identifies the component as a SS7 Transfer Capabilities Application Part
; type = ss7-tcap-ansi for ANSI TCAP
; type = ss7-tcap-itu for ITU TCAP
;type=

; local_SSN: local SubSystem Number. Mandatory
;local_SSN=

; default_remote_SSN: remote SubSystem Number to provide to SCCP if the application does not provide one
;default_remote_SSN=

; default_remote_pointcode: remote Point Code to provide to SCCP if the application does not provide one
;default_remote_pointcode=

; pointcodetype: remote Point Code type. See above documentation for available types
;pointcodetype=

; sccp: Name of the SCCP component to create and be used by this TCAP
; A section with the name given here must exist in order to configure the SCCP level
;sccp=

; default_hopcounter: HopCounter provided to SCCP if the application does not provide one
; Values range 1-15, 0 or boolean false disables, boolean true sets to 15
; A non-zero value will force using XUDT or LUDT instead of UDT messages
;default_hopcounter=false

; transact_timeout: Time in seconds to timeout a TCAP transaction after no more activity was registered on it
; Defaults to 300 seconds
;transact_timeout=300

;print-messages: Boolean to enable/disable printing of decoding/encoding of TCAP messages
; This option applies on reload
;print-messages=false

;extended-debug: Boolean to enable/disable printing of the step-by-step decoding/encoding of TCAP messages
; This option applies on reload. print-messages must be true.
;extended-debug=false


[tcapuser_test]
; mimicks  a TCAP User, which emits and receives TCAP messages in Message form
; type is ss7-tcap-user to identify it as the specific user
;type=ss7-tcap-user

; tcap: The TCAP to which this user is to attach itself to it
;tcap=
