# Copyright (C) 1991-2005 Altera Corporation
# Your use of Altera Corporation's design tools, logic functions 
# and other software and tools, and its AMPP partner logic       
# functions, and any output files any of the foregoing           
# (including device programming or simulation files), and any    
# associated documentation or information are expressly subject  
# to the terms and conditions of the Altera Program License      
# Subscription Agreement, Altera MegaCore Function License       
# Agreement, or other applicable license agreement, including,   
# without limitation, that your use is for the sole purpose of   
# programming logic devices manufactured by Altera and sold by   
# Altera or its authorized distributors.  Please refer to the    
# applicable agreement for further details.


# The default values for assignments are stored in the file
#		mrfm_assignment_defaults.qdf
# If this file doesn't exist, and for assignments not listed, see file
#		assignment_defaults.qdf

# Altera recommends that you do not modify this file. This
# file is updated automatically by the Quartus II software
# and any changes you make may be lost or overwritten.


# Project-Wide Assignments
# ========================
set_global_assignment -name ORIGINAL_QUARTUS_VERSION 3.0
set_global_assignment -name PROJECT_CREATION_TIME_DATE "00:14:04  JULY 13, 2003"
set_global_assignment -name LAST_QUARTUS_VERSION "5.1 SP2"

# Pin & Location Assignments
# ==========================
set_global_assignment -name RESERVE_PIN "AS INPUT TRI-STATED"
set_location_assignment PIN_29 -to SCLK
set_location_assignment PIN_117 -to SDI
set_location_assignment PIN_28 -to usbclk
set_location_assignment PIN_107 -to usbctl[0]
set_location_assignment PIN_106 -to usbctl[1]
set_location_assignment PIN_105 -to usbctl[2]
set_location_assignment PIN_100 -to usbdata[0]
set_location_assignment PIN_84 -to usbdata[10]
set_location_assignment PIN_83 -to usbdata[11]
set_location_assignment PIN_82 -to usbdata[12]
set_location_assignment PIN_79 -to usbdata[13]
set_location_assignment PIN_78 -to usbdata[14]
set_location_assignment PIN_77 -to usbdata[15]
set_location_assignment PIN_99 -to usbdata[1]
set_location_assignment PIN_98 -to usbdata[2]
set_location_assignment PIN_95 -to usbdata[3]
set_location_assignment PIN_94 -to usbdata[4]
set_location_assignment PIN_93 -to usbdata[5]
set_location_assignment PIN_88 -to usbdata[6]
set_location_assignment PIN_87 -to usbdata[7]
set_location_assignment PIN_86 -to usbdata[8]
set_location_assignment PIN_85 -to usbdata[9]
set_location_assignment PIN_104 -to usbrdy[0]
set_location_assignment PIN_101 -to usbrdy[1]
set_location_assignment PIN_76 -to FX2_1
set_location_assignment PIN_75 -to FX2_2
set_location_assignment PIN_74 -to FX2_3
set_location_assignment PIN_116 -to io_rx_a[0]
set_location_assignment PIN_115 -to io_rx_a[1]
set_location_assignment PIN_114 -to io_rx_a[2]
set_location_assignment PIN_113 -to io_rx_a[3]
set_location_assignment PIN_108 -to io_rx_a[4]
set_location_assignment PIN_195 -to io_rx_a[5]
set_location_assignment PIN_196 -to io_rx_a[6]
set_location_assignment PIN_197 -to io_rx_a[7]
set_location_assignment PIN_200 -to io_rx_a[8]
set_location_assignment PIN_201 -to io_rx_a[9]
set_location_assignment PIN_202 -to io_rx_a[10]
set_location_assignment PIN_203 -to io_rx_a[11]
set_location_assignment PIN_206 -to io_rx_a[12]
set_location_assignment PIN_207 -to io_rx_a[13]
set_location_assignment PIN_208 -to io_rx_a[14]
set_location_assignment PIN_214 -to io_rx_b[0]
set_location_assignment PIN_215 -to io_rx_b[1]
set_location_assignment PIN_216 -to io_rx_b[2]
set_location_assignment PIN_217 -to io_rx_b[3]
set_location_assignment PIN_218 -to io_rx_b[4]
set_location_assignment PIN_219 -to io_rx_b[5]
set_location_assignment PIN_222 -to io_rx_b[6]
set_location_assignment PIN_223 -to io_rx_b[7]
set_location_assignment PIN_224 -to io_rx_b[8]
set_location_assignment PIN_225 -to io_rx_b[9]
set_location_assignment PIN_226 -to io_rx_b[10]
set_location_assignment PIN_227 -to io_rx_b[11]
set_location_assignment PIN_228 -to io_rx_b[12]
set_location_assignment PIN_233 -to io_rx_b[13]
set_location_assignment PIN_234 -to io_rx_b[14]
set_location_assignment PIN_175 -to io_tx_a[0]
set_location_assignment PIN_176 -to io_tx_a[1]
set_location_assignment PIN_177 -to io_tx_a[2]
set_location_assignment PIN_178 -to io_tx_a[3]
set_location_assignment PIN_179 -to io_tx_a[4]
set_location_assignment PIN_180 -to io_tx_a[5]
set_location_assignment PIN_181 -to io_tx_a[6]
set_location_assignment PIN_182 -to io_tx_a[7]
set_location_assignment PIN_183 -to io_tx_a[8]
set_location_assignment PIN_184 -to io_tx_a[9]
set_location_assignment PIN_185 -to io_tx_a[10]
set_location_assignment PIN_186 -to io_tx_a[11]
set_location_assignment PIN_187 -to io_tx_a[12]
set_location_assignment PIN_188 -to io_tx_a[13]
set_location_assignment PIN_193 -to io_tx_a[14]
set_location_assignment PIN_73 -to io_tx_b[0]
set_location_assignment PIN_68 -to io_tx_b[1]
set_location_assignment PIN_67 -to io_tx_b[2]
set_location_assignment PIN_66 -to io_tx_b[3]
set_location_assignment PIN_65 -to io_tx_b[4]
set_location_assignment PIN_64 -to io_tx_b[5]
set_location_assignment PIN_63 -to io_tx_b[6]
set_location_assignment PIN_62 -to io_tx_b[7]
set_location_assignment PIN_61 -to io_tx_b[8]
set_location_assignment PIN_60 -to io_tx_b[9]
set_location_assignment PIN_59 -to io_tx_b[10]
set_location_assignment PIN_58 -to io_tx_b[11]
set_location_assignment PIN_57 -to io_tx_b[12]
set_location_assignment PIN_56 -to io_tx_b[13]
set_location_assignment PIN_55 -to io_tx_b[14]
set_location_assignment PIN_152 -to master_clk
set_location_assignment PIN_144 -to rx_a_a[0]
set_location_assignment PIN_143 -to rx_a_a[1]
set_location_assignment PIN_141 -to rx_a_a[2]
set_location_assignment PIN_140 -to rx_a_a[3]
set_location_assignment PIN_139 -to rx_a_a[4]
set_location_assignment PIN_138 -to rx_a_a[5]
set_location_assignment PIN_137 -to rx_a_a[6]
set_location_assignment PIN_136 -to rx_a_a[7]
set_location_assignment PIN_135 -to rx_a_a[8]
set_location_assignment PIN_134 -to rx_a_a[9]
set_location_assignment PIN_133 -to rx_a_a[10]
set_location_assignment PIN_132 -to rx_a_a[11]
set_location_assignment PIN_23 -to rx_a_b[0]
set_location_assignment PIN_21 -to rx_a_b[1]
set_location_assignment PIN_20 -to rx_a_b[2]
set_location_assignment PIN_19 -to rx_a_b[3]
set_location_assignment PIN_18 -to rx_a_b[4]
set_location_assignment PIN_17 -to rx_a_b[5]
set_location_assignment PIN_16 -to rx_a_b[6]
set_location_assignment PIN_15 -to rx_a_b[7]
set_location_assignment PIN_14 -to rx_a_b[8]
set_location_assignment PIN_13 -to rx_a_b[9]
set_location_assignment PIN_12 -to rx_a_b[10]
set_location_assignment PIN_11 -to rx_a_b[11]
set_location_assignment PIN_131 -to rx_b_a[0]
set_location_assignment PIN_128 -to rx_b_a[1]
set_location_assignment PIN_127 -to rx_b_a[2]
set_location_assignment PIN_126 -to rx_b_a[3]
set_location_assignment PIN_125 -to rx_b_a[4]
set_location_assignment PIN_124 -to rx_b_a[5]
set_location_assignment PIN_123 -to rx_b_a[6]
set_location_assignment PIN_122 -to rx_b_a[7]
set_location_assignment PIN_121 -to rx_b_a[8]
set_location_assignment PIN_120 -to rx_b_a[9]
set_location_assignment PIN_119 -to rx_b_a[10]
set_location_assignment PIN_118 -to rx_b_a[11]
set_location_assignment PIN_8 -to rx_b_b[0]
set_location_assignment PIN_7 -to rx_b_b[1]
set_location_assignment PIN_6 -to rx_b_b[2]
set_location_assignment PIN_5 -to rx_b_b[3]
set_location_assignment PIN_4 -to rx_b_b[4]
set_location_assignment PIN_3 -to rx_b_b[5]
set_location_assignment PIN_2 -to rx_b_b[6]
set_location_assignment PIN_240 -to rx_b_b[7]
set_location_assignment PIN_239 -to rx_b_b[8]
set_location_assignment PIN_238 -to rx_b_b[9]
set_location_assignment PIN_237 -to rx_b_b[10]
set_location_assignment PIN_236 -to rx_b_b[11]
set_location_assignment PIN_156 -to SDO
set_location_assignment PIN_153 -to SEN_FPGA
set_location_assignment PIN_159 -to tx_a[0]
set_location_assignment PIN_160 -to tx_a[1]
set_location_assignment PIN_161 -to tx_a[2]
set_location_assignment PIN_162 -to tx_a[3]
set_location_assignment PIN_163 -to tx_a[4]
set_location_assignment PIN_164 -to tx_a[5]
set_location_assignment PIN_165 -to tx_a[6]
set_location_assignment PIN_166 -to tx_a[7]
set_location_assignment PIN_167 -to tx_a[8]
set_location_assignment PIN_168 -to tx_a[9]
set_location_assignment PIN_169 -to tx_a[10]
set_location_assignment PIN_170 -to tx_a[11]
set_location_assignment PIN_173 -to tx_a[12]
set_location_assignment PIN_174 -to tx_a[13]
set_location_assignment PIN_38 -to tx_b[0]
set_location_assignment PIN_39 -to tx_b[1]
set_location_assignment PIN_41 -to tx_b[2]
set_location_assignment PIN_42 -to tx_b[3]
set_location_assignment PIN_43 -to tx_b[4]
set_location_assignment PIN_44 -to tx_b[5]
set_location_assignment PIN_45 -to tx_b[6]
set_location_assignment PIN_46 -to tx_b[7]
set_location_assignment PIN_47 -to tx_b[8]
set_location_assignment PIN_48 -to tx_b[9]
set_location_assignment PIN_49 -to tx_b[10]
set_location_assignment PIN_50 -to tx_b[11]
set_location_assignment PIN_53 -to tx_b[12]
set_location_assignment PIN_54 -to tx_b[13]
set_location_assignment PIN_158 -to TXSYNC_A
set_location_assignment PIN_37 -to TXSYNC_B
set_location_assignment PIN_235 -to io_rx_b[15]
set_location_assignment PIN_24 -to io_tx_b[15]
set_location_assignment PIN_213 -to io_rx_a[15]
set_location_assignment PIN_194 -to io_tx_a[15]
set_location_assignment PIN_1 -to MYSTERY_SIGNAL

# Timing Assignments
# ==================
set_global_assignment -name INCLUDE_EXTERNAL_PIN_DELAYS_IN_FMAX_CALCULATIONS OFF

# Analysis & Synthesis Assignments
# ================================
set_global_assignment -name SAVE_DISK_SPACE OFF
set_global_assignment -name DEVICE_FILTER_PACKAGE "ANY QFP"
set_global_assignment -name DEVICE_FILTER_PIN_COUNT 240
set_global_assignment -name EDA_DESIGN_ENTRY_SYNTHESIS_TOOL "<None>"
set_global_assignment -name FAMILY Cyclone
set_global_assignment -name CYCLONE_OPTIMIZATION_TECHNIQUE SPEED
set_global_assignment -name STRATIX_OPTIMIZATION_TECHNIQUE SPEED
set_global_assignment -name APEX20K_OPTIMIZATION_TECHNIQUE SPEED
set_global_assignment -name TOP_LEVEL_ENTITY mrfm
set_global_assignment -name VHDL_SHOW_LMF_MAPPING_MESSAGES OFF
set_global_assignment -name USER_LIBRARIES "e:\\usrp\\fpga\\megacells"
set_global_assignment -name AUTO_ENABLE_SMART_COMPILE ON

# Fitter Assignments
# ==================
set_global_assignment -name DEVICE EP1C12Q240C8
set_global_assignment -name CYCLONE_CONFIGURATION_SCHEME "PASSIVE SERIAL"
set_global_assignment -name RESERVE_ALL_UNUSED_PINS "AS INPUT TRI-STATED"
set_global_assignment -name OPTIMIZE_HOLD_TIMING OFF
set_global_assignment -name OPTIMIZE_TIMING "NORMAL COMPILATION"
set_global_assignment -name PHYSICAL_SYNTHESIS_COMBO_LOGIC ON
set_global_assignment -name PHYSICAL_SYNTHESIS_REGISTER_DUPLICATION ON
set_global_assignment -name PHYSICAL_SYNTHESIS_REGISTER_RETIMING ON
set_global_assignment -name IO_PLACEMENT_OPTIMIZATION OFF
set_global_assignment -name PHYSICAL_SYNTHESIS_EFFORT EXTRA
set_global_assignment -name INC_PLC_MODE OFF
set_global_assignment -name ROUTING_BACK_ANNOTATION_MODE OFF
set_instance_assignment -name IO_STANDARD LVTTL -to usbdata[12]
set_global_assignment -name STRATIX_DEVICE_IO_STANDARD LVTTL
set_global_assignment -name ERROR_CHECK_FREQUENCY_DIVISOR 1

# Timing Analysis Assignments
# ===========================
set_global_assignment -name MAX_SCC_SIZE 50

# EDA Netlist Writer Assignments
# ==============================
set_global_assignment -name EDA_SIMULATION_TOOL "<None>"
set_global_assignment -name EDA_TIMING_ANALYSIS_TOOL "<NONE>"
set_global_assignment -name EDA_BOARD_DESIGN_TOOL "<NONE>"
set_global_assignment -name EDA_FORMAL_VERIFICATION_TOOL "<NONE>"
set_global_assignment -name EDA_RESYNTHESIS_TOOL "<NONE>"

# Assembler Assignments
# =====================
set_global_assignment -name USE_CONFIGURATION_DEVICE OFF
set_global_assignment -name GENERATE_RBF_FILE ON
set_global_assignment -name RESERVE_ALL_UNUSED_PINS_NO_OUTPUT_GND "AS INPUT TRI-STATED"
set_global_assignment -name AUTO_RESTART_CONFIGURATION OFF

# Simulator Assignments
# =====================
set_global_assignment -name START_TIME "0 ns"
set_global_assignment -name GLITCH_INTERVAL "1 ns"

# Design Assistant Assignments
# ============================
set_global_assignment -name DRC_REPORT_TOP_FANOUT OFF
set_global_assignment -name DRC_REPORT_FANOUT_EXCEEDING OFF
set_global_assignment -name ASSG_CAT OFF
set_global_assignment -name ASSG_RULE_MISSING_FMAX OFF
set_global_assignment -name ASSG_RULE_MISSING_TIMING OFF
set_global_assignment -name NONSYNCHSTRUCT_RULE_ASYN_RAM OFF
set_global_assignment -name CLK_CAT OFF
set_global_assignment -name CLK_RULE_COMB_CLOCK OFF
set_global_assignment -name CLK_RULE_INV_CLOCK OFF
set_global_assignment -name CLK_RULE_GATING_SCHEME OFF
set_global_assignment -name CLK_RULE_INPINS_CLKNET OFF
set_global_assignment -name CLK_RULE_CLKNET_CLKSPINES OFF
set_global_assignment -name CLK_RULE_MIX_EDGES OFF
set_global_assignment -name RESET_CAT OFF
set_global_assignment -name RESET_RULE_INPINS_RESETNET OFF
set_global_assignment -name RESET_RULE_UNSYNCH_EXRESET OFF
set_global_assignment -name RESET_RULE_IMSYNCH_EXRESET OFF
set_global_assignment -name RESET_RULE_COMB_ASYNCH_RESET OFF
set_global_assignment -name RESET_RULE_UNSYNCH_ASYNCH_DOMAIN OFF
set_global_assignment -name RESET_RULE_IMSYNCH_ASYNCH_DOMAIN OFF
set_global_assignment -name TIMING_CAT OFF
set_global_assignment -name TIMING_RULE_SHIFT_REG OFF
set_global_assignment -name TIMING_RULE_COIN_CLKEDGE OFF
set_global_assignment -name NONSYNCHSTRUCT_RULE_COMB_DRIVES_RAM_WE OFF
set_global_assignment -name NONSYNCHSTRUCT_CAT OFF
set_global_assignment -name NONSYNCHSTRUCT_RULE_COMBLOOP OFF
set_global_assignment -name NONSYNCHSTRUCT_RULE_REG_LOOP OFF
set_global_assignment -name NONSYNCHSTRUCT_RULE_DELAY_CHAIN OFF
set_global_assignment -name NONSYNCHSTRUCT_RULE_RIPPLE_CLK OFF
set_global_assignment -name NONSYNCHSTRUCT_RULE_ILLEGAL_PULSE_GEN OFF
set_global_assignment -name NONSYNCHSTRUCT_RULE_MULTI_VIBRATOR OFF
set_global_assignment -name NONSYNCHSTRUCT_RULE_SRLATCH OFF
set_global_assignment -name NONSYNCHSTRUCT_RULE_LATCH_UNIDENTIFIED OFF
set_global_assignment -name SIGNALRACE_CAT OFF
set_global_assignment -name ACLK_CAT OFF
set_global_assignment -name ACLK_RULE_NO_SZER_ACLK_DOMAIN OFF
set_global_assignment -name ACLK_RULE_SZER_BTW_ACLK_DOMAIN OFF
set_global_assignment -name ACLK_RULE_IMSZER_ADOMAIN OFF
set_global_assignment -name HCPY_CAT OFF
set_global_assignment -name HCPY_VREF_PINS OFF

# SignalTap II Assignments
# ========================
set_global_assignment -name HUB_ENTITY_NAME SLD_HUB
set_global_assignment -name HUB_INSTANCE_NAME SLD_HUB_INST
set_global_assignment -name ENABLE_SIGNALTAP OFF

# LogicLock Region Assignments
# ============================
set_global_assignment -name LOGICLOCK_INCREMENTAL_COMPILE_ASSIGNMENT OFF

# -----------------
# start CLOCK(SCLK)

	# Timing Assignments
	# ==================
set_global_assignment -name DUTY_CYCLE 50 -section_id SCLK
set_global_assignment -name FMAX_REQUIREMENT "1 MHz" -section_id SCLK
set_global_assignment -name INCLUDE_EXTERNAL_PIN_DELAYS_IN_FMAX_CALCULATIONS OFF -section_id SCLK

# end CLOCK(SCLK)
# ---------------

# -----------------------
# start CLOCK(master_clk)

	# Timing Assignments
	# ==================
set_global_assignment -name DUTY_CYCLE 50 -section_id master_clk
set_global_assignment -name FMAX_REQUIREMENT "64 MHz" -section_id master_clk
set_global_assignment -name INCLUDE_EXTERNAL_PIN_DELAYS_IN_FMAX_CALCULATIONS OFF -section_id master_clk

# end CLOCK(master_clk)
# ---------------------

# -------------------
# start CLOCK(usbclk)

	# Timing Assignments
	# ==================
set_global_assignment -name DUTY_CYCLE 50 -section_id usbclk
set_global_assignment -name FMAX_REQUIREMENT "48 MHz" -section_id usbclk
set_global_assignment -name INCLUDE_EXTERNAL_PIN_DELAYS_IN_FMAX_CALCULATIONS OFF -section_id usbclk

# end CLOCK(usbclk)
# -----------------

# ----------------------
# start ENTITY(mrfm)

	# Timing Assignments
	# ==================
set_instance_assignment -name CLOCK_SETTINGS SCLK -to SCLK
set_instance_assignment -name CLOCK_SETTINGS usbclk -to usbclk
set_instance_assignment -name CLOCK_SETTINGS master_clk -to master_clk

# end ENTITY(mrfm)
# --------------------


set_global_assignment -name PHYSICAL_SYNTHESIS_ASYNCHRONOUS_SIGNAL_PIPELINING ON
set_global_assignment -name SMART_RECOMPILE ON
set_global_assignment -name VERILOG_FILE mrfm.vh
set_global_assignment -name VERILOG_FILE biquad_2stage.v
set_global_assignment -name VERILOG_FILE mrfm_compensator.v
set_global_assignment -name VERILOG_FILE ../../sdr_lib/ram16.v
set_global_assignment -name VERILOG_FILE mrfm_proc.v
set_global_assignment -name VERILOG_FILE ../../megacells/fifo_4k.v
set_global_assignment -name VERILOG_FILE ../../sdr_lib/hb/acc.v
set_global_assignment -name VERILOG_FILE ../../sdr_lib/hb/mult.v
set_global_assignment -name VERILOG_FILE ../../sdr_lib/hb/ram16_2sum.v
set_global_assignment -name VERILOG_FILE ../../sdr_lib/hb/coeff_rom.v
set_global_assignment -name VERILOG_FILE ../../sdr_lib/hb/halfband_decim.v
set_global_assignment -name VERILOG_FILE ../../sdr_lib/hb/mac.v
set_global_assignment -name VERILOG_FILE ../../sdr_lib/hb/coeff_ram.v
set_global_assignment -name VERILOG_FILE ../../sdr_lib/tx_chain.v
set_global_assignment -name VERILOG_FILE ../../sdr_lib/rx_dcoffset.v
set_global_assignment -name VERILOG_FILE ../../sdr_lib/adc_interface.v
set_global_assignment -name VERILOG_FILE ../../sdr_lib/io_pins.v
set_global_assignment -name VERILOG_FILE ../../sdr_lib/setting_reg.v
set_global_assignment -name VERILOG_FILE ../../sdr_lib/bidir_reg.v
set_global_assignment -name VERILOG_FILE ../../sdr_lib/cic_int_shifter.v
set_global_assignment -name VERILOG_FILE ../../megacells/clk_doubler.v
set_global_assignment -name VERILOG_FILE ../../sdr_lib/gen_sync.v
set_global_assignment -name VERILOG_FILE ../../sdr_lib/master_control.v
set_global_assignment -name VERILOG_FILE ../../megacells/fifo_2k.v
set_global_assignment -name VERILOG_FILE ../../megacells/bustri.v
set_global_assignment -name VERILOG_FILE ../../sdr_lib/rx_buffer.v
set_global_assignment -name VERILOG_FILE ../../sdr_lib/tx_buffer.v
set_global_assignment -name VERILOG_FILE ../../sdr_lib/phase_acc.v
set_global_assignment -name VERILOG_FILE ../../sdr_lib/cic_interp.v
set_global_assignment -name VERILOG_FILE ../../sdr_lib/cic_decim.v
set_global_assignment -name VERILOG_FILE ../../sdr_lib/cordic_stage.v
set_global_assignment -name VERILOG_FILE ../../sdr_lib/cordic.v
set_global_assignment -name VERILOG_FILE mrfm.v
set_global_assignment -name VERILOG_FILE ../../sdr_lib/clk_divider.v
set_global_assignment -name VERILOG_FILE ../../sdr_lib/serial_io.v
set_global_assignment -name VERILOG_FILE ../../sdr_lib/strobe_gen.v
set_global_assignment -name VERILOG_FILE ../../sdr_lib/sign_extend.v
set_global_assignment -name FITTER_EFFORT "STANDARD FIT"