COMPILER_SETTINGS
{
	IO_PLACEMENT_OPTIMIZATION = OFF;
	ENABLE_DRC_SETTINGS = OFF;
	PHYSICAL_SYNTHESIS_REGISTER_RETIMING = OFF;
	PHYSICAL_SYNTHESIS_REGISTER_DUPLICATION = OFF;
	PHYSICAL_SYNTHESIS_COMBO_LOGIC = OFF;
	DRC_FANOUT_EXCEEDING = 30;
	DRC_REPORT_FANOUT_EXCEEDING = OFF;
	DRC_TOP_FANOUT = 50;
	DRC_REPORT_TOP_FANOUT = OFF;
	RUN_DRC_DURING_COMPILATION = OFF;
	ADV_NETLIST_OPT_RETIME_CORE_AND_IO = ON;
	ADV_NETLIST_OPT_SYNTH_USE_FITTER_INFO = OFF;
	ADV_NETLIST_OPT_SYNTH_GATE_RETIME = OFF;
	ADV_NETLIST_OPT_SYNTH_WYSIWYG_REMAP = OFF;
	SMART_COMPILE_IGNORES_TDC_FOR_STRATIX_PLL_CHANGES = OFF;
	MERGE_HEX_FILE = OFF;
	TRUE_WYSIWYG_FLOW = OFF;
	SEED = 1;
	FINAL_PLACEMENT_OPTIMIZATION = AUTOMATICALLY;
	FAMILY = Cyclone;
	DPRAM_DUAL_PORT_MODE_OTHER_SIGNALS_EPXA1 = "DPRAM0 TO 1 DPRAM1 TO 2";
	DPRAM_32BIT_SINGLE_PORT_MODE_OTHER_SIGNALS_EPXA1 = "MEGALAB COLUMN 1";
	DPRAM_8BIT_16BIT_SINGLE_PORT_MODE_OTHER_SIGNALS_EPXA1 = "MEGALAB COLUMN 1";
	DPRAM_DUAL_PORT_MODE_OUTPUT_EPXA1 = "DPRAM0 TO 1 DPRAM1 TO 2";
	DPRAM_32BIT_SINGLE_PORT_MODE_OUTPUT_EPXA1 = "LOWER TO 1ESB UPPER TO 1";
	DPRAM_8BIT_16BIT_SINGLE_PORT_MODE_OUTPUT_EPXA1 = "MEGALAB COLUMN 1";
	DPRAM_DUAL_PORT_MODE_INPUT_EPXA1 = "DPRAM0 TO 1 DPRAM1 TO 2";
	DPRAM_32BIT_SINGLE_PORT_MODE_INPUT_EPXA1 = "MEGALAB COLUMN 1";
	DPRAM_8BIT_16BIT_SINGLE_PORT_MODE_INPUT_EPXA1 = "MEGALAB COLUMN 1";
	DPRAM_DUAL_PORT_MODE_OTHER_SIGNALS_EPXA4_10 = "DPRAM0 TO 3 DPRAM1 TO 4";
	DPRAM_SINGLE_PORT_MODE_OTHER_SIGNALS_EPXA4_10 = "DPRAM0 TO 3 DPRAM1 TO 4";
	DPRAM_WIDE_MODE_OTHER_SIGNALS_EPXA4_10 = "MEGALAB COLUMN 3";
	DPRAM_DEEP_MODE_OTHER_SIGNALS_EPXA4_10 = "MEGALAB COLUMN 3";
	DPRAM_DUAL_PORT_MODE_OUTPUT_EPXA4_10 = "DPRAM0 TO 3 DPRAM1 TO 4ESB";
	DPRAM_SINGLE_PORT_MODE_OUTPUT_EPXA4_10 = "DPRAM0 TO 3 DPRAM1 TO 4ESB";
	DPRAM_WIDE_MODE_OUTPUT_EPXA4_10 = "LOWER TO 3 UPPER TO 4ESB";
	DPRAM_DEEP_MODE_OUTPUT_EPXA4_10 = "MEGALAB COLUMN 3";
	DPRAM_DUAL_PORT_MODE_INPUT_EPXA4_10 = "DPRAM0 TO 3 DPRAM1 TO 4";
	DPRAM_SINGLE_PORT_MODE_INPUT_EPXA4_10 = "DPRAM0 TO 3 DPRAM1 TO 4";
	DPRAM_WIDE_MODE_INPUT_EPXA4_10 = "LOWER TO 3 UPPER TO 4";
	DPRAM_DEEP_MODE_INPUT_EPXA4_10 = "MEGALAB COLUMN 3";
	DPRAM_OTHER_SIGNALS_EPXA4_10 = "DEFAULT OTHER ROUTING OPTIONS";
	DPRAM_OUTPUT_EPXA4_10 = "DEFAULT OUTPUT ROUTING OPTIONS";
	DPRAM_INPUT_EPXA4_10 = "DEFAULT INPUT ROUTING OPTIONS";
	STRIPE_TO_PLD_INTERRUPTS_EPXA4_10 = "MEGALAB COLUMN 2";
	PLD_TO_STRIPE_INTERRUPTS_EPXA4_10 = "MEGALAB COLUMN 2";
	PROCESSOR_DEBUG_EXTENSIONS_EPXA4_10 = "MEGALAB COLUMN 2";
	STRIPE_TO_PLD_BRIDGE_EPXA4_10 = "MEGALAB COLUMN 1";
	FAST_FIT_COMPILATION = OFF;
	SIGNALPROBE_DURING_NORMAL_COMPILATION = OFF;
	OPTIMIZE_IOC_REGISTER_PLACEMENT_FOR_TIMING = ON;
	OPTIMIZE_TIMING = "NORMAL COMPILATION";
	OPTIMIZE_HOLD_TIMING = OFF;
	COMPILATION_LEVEL = FULL;
	SAVE_DISK_SPACE = OFF;
	SPEED_DISK_USAGE_TRADEOFF = NORMAL;
	LOGICLOCK_INCREMENTAL_COMPILE_ASSIGNMENT = OFF;
	SIGNALPROBE_ALLOW_OVERUSE = OFF;
	FOCUS_ENTITY_NAME = |usrp_multi;
	ROUTING_BACK_ANNOTATION_MODE = OFF;
	INC_PLC_MODE = OFF;
	FIT_ONLY_ONE_ATTEMPT = OFF;
}
DEFAULT_DEVICE_OPTIONS
{
	GENERATE_CONFIG_HEXOUT_FILE = OFF;
	GENERATE_CONFIG_JBC_FILE_COMPRESSED = ON;
	GENERATE_CONFIG_JBC_FILE = OFF;
	GENERATE_CONFIG_JAM_FILE = OFF;
	GENERATE_CONFIG_ISC_FILE = OFF;
	GENERATE_CONFIG_SVF_FILE = OFF;
	GENERATE_JBC_FILE_COMPRESSED = ON;
	GENERATE_JBC_FILE = OFF;
	GENERATE_JAM_FILE = OFF;
	GENERATE_ISC_FILE = OFF;
	GENERATE_SVF_FILE = OFF;
	RESERVE_PIN = "AS INPUT TRI-STATED";
	RESERVE_ALL_UNUSED_PINS = "AS OUTPUT DRIVING GROUND";
	HEXOUT_FILE_COUNT_DIRECTION = UP;
	HEXOUT_FILE_START_ADDRESS = 0;
	GENERATE_HEX_FILE = OFF;
	GENERATE_RBF_FILE = OFF;
	GENERATE_TTF_FILE = OFF;
	RESERVE_ASDO_AFTER_CONFIGURATION = "USE AS REGULAR IO";
	RESERVE_DATA0_AFTER_CONFIGURATION = "AS INPUT TRI-STATED";
	RESERVE_DATA7_THROUGH_DATA1_AFTER_CONFIGURATION = "USE AS REGULAR IO";
	RESERVE_RDYNBUSY_AFTER_CONFIGURATION = "USE AS REGULAR IO";
	RESERVE_NWS_NRS_NCS_CS_AFTER_CONFIGURATION = "USE AS REGULAR IO";
	DISABLE_NCS_AND_OE_PULLUPS_ON_CONFIG_DEVICE = OFF;
	AUTO_INCREMENT_CONFIG_DEVICE_JTAG_USER_CODE = ON;
	EPROM_USE_CHECKSUM_AS_USERCODE = OFF;
	FLEX10K_CONFIG_DEVICE_JTAG_USER_CODE = FFFFFFFF;
	MERCURY_CONFIG_DEVICE_JTAG_USER_CODE = FFFFFFFF;
	STRATIX_CONFIG_DEVICE_JTAG_USER_CODE = FFFFFFFF;
	APEX20K_CONFIG_DEVICE_JTAG_USER_CODE = FFFFFFFF;
	STRATIX_CONFIGURATION_DEVICE = AUTO;
	CYCLONE_CONFIGURATION_DEVICE = AUTO;
	FLEX10K_CONFIGURATION_DEVICE = AUTO;
	FLEX6K_CONFIGURATION_DEVICE = AUTO;
	MERCURY_CONFIGURATION_DEVICE = AUTO;
	EXCALIBUR_CONFIGURATION_DEVICE = AUTO;
	APEX20K_CONFIGURATION_DEVICE = AUTO;
	USE_CONFIGURATION_DEVICE = ON;
	ENABLE_INIT_DONE_OUTPUT = OFF;
	FLEX10K_ENABLE_LOCK_OUTPUT = OFF;
	ENABLE_DEVICE_WIDE_OE = OFF;
	ENABLE_DEVICE_WIDE_RESET = OFF;
	RELEASE_CLEARS_BEFORE_TRI_STATES = OFF;
	AUTO_RESTART_CONFIGURATION = OFF;
	ENABLE_VREFB_PIN = OFF;
	ENABLE_VREFA_PIN = OFF;
	SECURITY_BIT = OFF;
	USER_START_UP_CLOCK = OFF;
	APEXII_CONFIGURATION_SCHEME = "PASSIVE SERIAL";
	FLEX10K_CONFIGURATION_SCHEME = "PASSIVE SERIAL";
	FLEX6K_CONFIGURATION_SCHEME = "PASSIVE SERIAL";
	MERCURY_CONFIGURATION_SCHEME = "PASSIVE SERIAL";
	EXCALIBUR_CONFIGURATION_SCHEME = "PASSIVE SERIAL";
	CYCLONE_CONFIGURATION_SCHEME = "ACTIVE SERIAL";
	STRATIX_CONFIGURATION_SCHEME = "PASSIVE SERIAL";
	APEX20K_CONFIGURATION_SCHEME = "PASSIVE SERIAL";
	STRATIX_UPDATE_MODE = STANDARD;
	USE_CHECKSUM_AS_USERCODE = OFF;
	MAX7000_USE_CHECKSUM_AS_USERCODE = OFF;
	MAX7000_JTAG_USER_CODE = FFFFFFFF;
	FLEX10K_JTAG_USER_CODE = 7F;
	MERCURY_JTAG_USER_CODE = FFFFFFFF;
	APEX20K_JTAG_USER_CODE = FFFFFFFF;
	STRATIX_JTAG_USER_CODE = FFFFFFFF;
	MAX7000S_JTAG_USER_CODE = FFFF;
	RESERVE_NCEO_AFTER_CONFIGURATION = "USE AS REGULAR IO";
	FLEX10K_ENABLE_LOW_VOLTAGE_MODE_ON_CONFIG_DEVICE = ON;
	FLEX6K_ENABLE_LOW_VOLTAGE_MODE_ON_CONFIG_DEVICE = OFF;
	ENABLE_LOW_VOLTAGE_MODE_ON_CONFIG_DEVICE = ON;
	MAX7000_ENABLE_JTAG_BST_SUPPORT = ON;
	ENABLE_JTAG_BST_SUPPORT = OFF;
	CONFIGURATION_CLOCK_DIVISOR = 1;
	CONFIGURATION_CLOCK_FREQUENCY = "10 MHZ";
	CLOCK_SOURCE = INTERNAL;
	COMPRESSION_MODE = OFF;
	ON_CHIP_BITSTREAM_DECOMPRESSION = OFF;
}
AUTO_SLD_HUB_ENTITY
{
	AUTO_INSERT_SLD_HUB_ENTITY = ENABLE;
	HUB_INSTANCE_NAME = SLD_HUB_INST;
	HUB_ENTITY_NAME = SLD_HUB;
}
SIGNALTAP_LOGIC_ANALYZER_SETTINGS
{
	ENABLE_SIGNALTAP = Off;
	AUTO_ENABLE_SMART_COMPILE = On;
}
CHIP(usrp_multi)
{
	DEVICE = EP1C12Q240C8;
	DEVICE_FILTER_PACKAGE = "ANY QFP";
	DEVICE_FILTER_PIN_COUNT = 240;
	DEVICE_FILTER_SPEED_GRADE = ANY;
	AUTO_RESTART_CONFIGURATION = OFF;
	RELEASE_CLEARS_BEFORE_TRI_STATES = OFF;
	USER_START_UP_CLOCK = OFF;
	ENABLE_DEVICE_WIDE_RESET = OFF;
	ENABLE_DEVICE_WIDE_OE = OFF;
	ENABLE_INIT_DONE_OUTPUT = OFF;
	FLEX10K_ENABLE_LOCK_OUTPUT = OFF;
	ENABLE_JTAG_BST_SUPPORT = OFF;
	MAX7000_ENABLE_JTAG_BST_SUPPORT = ON;
	APEX20K_JTAG_USER_CODE = FFFFFFFF;
	MERCURY_JTAG_USER_CODE = FFFFFFFF;
	FLEX10K_JTAG_USER_CODE = 7F;
	MAX7000_JTAG_USER_CODE = FFFFFFFF;
	MAX7000S_JTAG_USER_CODE = FFFF;
	STRATIX_JTAG_USER_CODE = FFFFFFFF;
	APEX20K_CONFIGURATION_SCHEME = "PASSIVE SERIAL";
	MERCURY_CONFIGURATION_SCHEME = "PASSIVE SERIAL";
	FLEX6K_CONFIGURATION_SCHEME = "PASSIVE SERIAL";
	FLEX10K_CONFIGURATION_SCHEME = "PASSIVE SERIAL";
	EXCALIBUR_CONFIGURATION_SCHEME = "PASSIVE SERIAL";
	APEXII_CONFIGURATION_SCHEME = "PASSIVE SERIAL";
	STRATIX_CONFIGURATION_SCHEME = "PASSIVE SERIAL";
	CYCLONE_CONFIGURATION_SCHEME = "PASSIVE SERIAL";
	USE_CONFIGURATION_DEVICE = OFF;
	APEX20K_CONFIGURATION_DEVICE = AUTO;
	MERCURY_CONFIGURATION_DEVICE = AUTO;
	FLEX6K_CONFIGURATION_DEVICE = AUTO;
	FLEX10K_CONFIGURATION_DEVICE = AUTO;
	EXCALIBUR_CONFIGURATION_DEVICE = AUTO;
	STRATIX_CONFIGURATION_DEVICE = AUTO;
	CYCLONE_CONFIGURATION_DEVICE = AUTO;
	STRATIX_UPDATE_MODE = STANDARD;
	APEX20K_CONFIG_DEVICE_JTAG_USER_CODE = FFFFFFFF;
	MERCURY_CONFIG_DEVICE_JTAG_USER_CODE = FFFFFFFF;
	FLEX10K_CONFIG_DEVICE_JTAG_USER_CODE = FFFFFFFF;
	STRATIX_CONFIG_DEVICE_JTAG_USER_CODE = FFFFFFFF;
	AUTO_INCREMENT_CONFIG_DEVICE_JTAG_USER_CODE = ON;
	DISABLE_NCS_AND_OE_PULLUPS_ON_CONFIG_DEVICE = OFF;
	COMPRESSION_MODE = OFF;
	ENABLE_LOW_VOLTAGE_MODE_ON_CONFIG_DEVICE = ON;
	FLEX6K_ENABLE_LOW_VOLTAGE_MODE_ON_CONFIG_DEVICE = OFF;
	FLEX10K_ENABLE_LOW_VOLTAGE_MODE_ON_CONFIG_DEVICE = ON;
	EPROM_USE_CHECKSUM_AS_USERCODE = OFF;
	USE_CHECKSUM_AS_USERCODE = OFF;
	MAX7000_USE_CHECKSUM_AS_USERCODE = OFF;
	GENERATE_TTF_FILE = OFF;
	GENERATE_RBF_FILE = ON;
	GENERATE_HEX_FILE = OFF;
	SECURITY_BIT = OFF;
	ENABLE_VREFA_PIN = OFF;
	ENABLE_VREFB_PIN = OFF;
	GENERATE_SVF_FILE = OFF;
	GENERATE_ISC_FILE = OFF;
	GENERATE_JAM_FILE = OFF;
	GENERATE_JBC_FILE = OFF;
	GENERATE_JBC_FILE_COMPRESSED = ON;
	GENERATE_CONFIG_SVF_FILE = OFF;
	GENERATE_CONFIG_ISC_FILE = OFF;
	GENERATE_CONFIG_JAM_FILE = OFF;
	GENERATE_CONFIG_JBC_FILE = OFF;
	GENERATE_CONFIG_JBC_FILE_COMPRESSED = ON;
	GENERATE_CONFIG_HEXOUT_FILE = OFF;
	ON_CHIP_BITSTREAM_DECOMPRESSION = OFF;
	BASE_PIN_OUT_FILE_ON_SAMEFRAME_DEVICE = OFF;
	HEXOUT_FILE_START_ADDRESS = 0;
	HEXOUT_FILE_COUNT_DIRECTION = UP;
	RESERVE_ALL_UNUSED_PINS = "AS INPUT TRI-STATED";
	STRATIX_DEVICE_IO_STANDARD = LVTTL;
	CLOCK_SOURCE = INTERNAL;
	CONFIGURATION_CLOCK_FREQUENCY = "10 MHZ";
	CONFIGURATION_CLOCK_DIVISOR = 1;
	RESERVE_NWS_NRS_NCS_CS_AFTER_CONFIGURATION = "USE AS REGULAR IO";
	RESERVE_RDYNBUSY_AFTER_CONFIGURATION = "USE AS REGULAR IO";
	RESERVE_DATA7_THROUGH_DATA1_AFTER_CONFIGURATION = "USE AS REGULAR IO";
	RESERVE_DATA0_AFTER_CONFIGURATION = "AS INPUT TRI-STATED";
	RESERVE_NCEO_AFTER_CONFIGURATION = "USE AS REGULAR IO";
	RESERVE_ASDO_AFTER_CONFIGURATION = "USE AS REGULAR IO";
	SCLK : LOCATION = Pin_101;
	SDI : LOCATION = Pin_100;
	SEN : LOCATION = Pin_98;
	SLD : LOCATION = Pin_95;
	adc1_data[0] : LOCATION = Pin_5;
	adc1_data[10] : LOCATION = Pin_235;
	adc1_data[11] : LOCATION = Pin_234;
	adc1_data[1] : LOCATION = Pin_4;
	adc1_data[2] : LOCATION = Pin_3;
	adc1_data[3] : LOCATION = Pin_2;
	adc1_data[4] : LOCATION = Pin_1;
	adc1_data[4] : IO_STANDARD = LVTTL;
	adc1_data[5] : LOCATION = Pin_240;
	adc1_data[6] : LOCATION = Pin_239;
	adc1_data[7] : LOCATION = Pin_238;
	adc1_data[8] : LOCATION = Pin_237;
	adc1_data[9] : LOCATION = Pin_236;
	adc2_data[0] : LOCATION = Pin_20;
	adc2_data[10] : LOCATION = Pin_8;
	adc2_data[11] : LOCATION = Pin_7;
	adc2_data[1] : LOCATION = Pin_19;
	adc2_data[2] : LOCATION = Pin_18;
	adc2_data[3] : LOCATION = Pin_17;
	adc2_data[4] : LOCATION = Pin_16;
	adc2_data[5] : LOCATION = Pin_15;
	adc2_data[6] : LOCATION = Pin_14;
	adc2_data[7] : LOCATION = Pin_13;
	adc2_data[8] : LOCATION = Pin_12;
	adc2_data[9] : LOCATION = Pin_11;
	adc3_data[0] : LOCATION = Pin_200;
	adc3_data[10] : LOCATION = Pin_184;
	adc3_data[11] : LOCATION = Pin_183;
	adc3_data[1] : LOCATION = Pin_197;
	adc3_data[2] : LOCATION = Pin_196;
	adc3_data[3] : LOCATION = Pin_195;
	adc3_data[4] : LOCATION = Pin_194;
	adc3_data[5] : LOCATION = Pin_193;
	adc3_data[6] : LOCATION = Pin_188;
	adc3_data[7] : LOCATION = Pin_187;
	adc3_data[8] : LOCATION = Pin_186;
	adc3_data[9] : LOCATION = Pin_185;
	adc4_data[0] : LOCATION = Pin_222;
	adc4_data[10] : LOCATION = Pin_203;
	adc4_data[11] : LOCATION = Pin_202;
	adc4_data[1] : LOCATION = Pin_219;
	adc4_data[2] : LOCATION = Pin_217;
	adc4_data[3] : LOCATION = Pin_216;
	adc4_data[4] : LOCATION = Pin_215;
	adc4_data[5] : LOCATION = Pin_214;
	adc4_data[6] : LOCATION = Pin_213;
	adc4_data[7] : LOCATION = Pin_208;
	adc4_data[8] : LOCATION = Pin_207;
	adc4_data[9] : LOCATION = Pin_206;
	adc_oeb[0] : LOCATION = Pin_228;
	adc_oeb[1] : LOCATION = Pin_21;
	adc_oeb[2] : LOCATION = Pin_181;
	adc_oeb[3] : LOCATION = Pin_218;
	adc_otr[0] : LOCATION = Pin_233;
	adc_otr[1] : LOCATION = Pin_6;
	adc_otr[2] : LOCATION = Pin_182;
	adc_otr[3] : LOCATION = Pin_201;
	adclk0 : LOCATION = Pin_224;
	adclk1 : LOCATION = Pin_226;
	clk0 : LOCATION = Pin_28;
	clk0 : RESERVE_PIN = "AS INPUT TRI-STATED";
	clk0 : IO_STANDARD = LVTTL;
	clk1 : LOCATION = Pin_29;
	clk1 : RESERVE_PIN = "AS INPUT TRI-STATED";
	clk1 : IO_STANDARD = LVTTL;
	clk3 : LOCATION = Pin_152;
	clk3 : RESERVE_PIN = "AS INPUT TRI-STATED";
	clk3 : IO_STANDARD = LVTTL;
	clk_120mhz : LOCATION = Pin_153;
	clk_120mhz : IO_STANDARD = LVTTL;
	clk_out : LOCATION = Pin_63;
	clk_out : IO_STANDARD = LVTTL;
	dac1_data[0] : LOCATION = Pin_165;
	dac1_data[10] : LOCATION = Pin_177;
	dac1_data[11] : LOCATION = Pin_178;
	dac1_data[12] : LOCATION = Pin_179;
	dac1_data[13] : LOCATION = Pin_180;
	dac1_data[1] : LOCATION = Pin_166;
	dac1_data[2] : LOCATION = Pin_167;
	dac1_data[3] : LOCATION = Pin_168;
	dac1_data[4] : LOCATION = Pin_169;
	dac1_data[5] : LOCATION = Pin_170;
	dac1_data[6] : LOCATION = Pin_173;
	dac1_data[7] : LOCATION = Pin_174;
	dac1_data[8] : LOCATION = Pin_175;
	dac1_data[9] : LOCATION = Pin_176;
	dac2_data[0] : LOCATION = Pin_159;
	dac2_data[10] : LOCATION = Pin_163;
	dac2_data[11] : LOCATION = Pin_139;
	dac2_data[12] : LOCATION = Pin_164;
	dac2_data[13] : LOCATION = Pin_138;
	dac2_data[1] : LOCATION = Pin_158;
	dac2_data[2] : LOCATION = Pin_160;
	dac2_data[3] : LOCATION = Pin_156;
	dac2_data[4] : LOCATION = Pin_161;
	dac2_data[5] : LOCATION = Pin_144;
	dac2_data[6] : LOCATION = Pin_162;
	dac2_data[7] : LOCATION = Pin_141;
	dac2_data[8] : LOCATION = Pin_143;
	dac2_data[9] : LOCATION = Pin_140;
	dac3_data[0] : LOCATION = Pin_122;
	dac3_data[10] : LOCATION = Pin_134;
	dac3_data[11] : LOCATION = Pin_135;
	dac3_data[12] : LOCATION = Pin_136;
	dac3_data[13] : LOCATION = Pin_137;
	dac3_data[1] : LOCATION = Pin_123;
	dac3_data[2] : LOCATION = Pin_124;
	dac3_data[3] : LOCATION = Pin_125;
	dac3_data[4] : LOCATION = Pin_126;
	dac3_data[5] : LOCATION = Pin_127;
	dac3_data[6] : LOCATION = Pin_128;
	dac3_data[7] : LOCATION = Pin_131;
	dac3_data[8] : LOCATION = Pin_132;
	dac3_data[9] : LOCATION = Pin_133;
	dac4_data[0] : LOCATION = Pin_104;
	dac4_data[10] : LOCATION = Pin_118;
	dac4_data[11] : LOCATION = Pin_119;
	dac4_data[12] : LOCATION = Pin_120;
	dac4_data[13] : LOCATION = Pin_121;
	dac4_data[1] : LOCATION = Pin_105;
	dac4_data[2] : LOCATION = Pin_106;
	dac4_data[3] : LOCATION = Pin_107;
	dac4_data[4] : LOCATION = Pin_108;
	dac4_data[5] : LOCATION = Pin_113;
	dac4_data[6] : LOCATION = Pin_114;
	dac4_data[7] : LOCATION = Pin_115;
	dac4_data[8] : LOCATION = Pin_116;
	dac4_data[9] : LOCATION = Pin_117;
	enable_rx : LOCATION = Pin_88;
	enable_tx : LOCATION = Pin_93;
	gndbus[0] : LOCATION = Pin_223;
	gndbus[0] : RESERVE_PIN = "AS INPUT TRI-STATED";
	gndbus[0] : IO_STANDARD = LVTTL;
	gndbus[1] : LOCATION = Pin_225;
	gndbus[1] : RESERVE_PIN = "AS INPUT TRI-STATED";
	gndbus[1] : IO_STANDARD = LVTTL;
	gndbus[2] : LOCATION = Pin_227;
	gndbus[2] : RESERVE_PIN = "AS INPUT TRI-STATED";
	gndbus[2] : IO_STANDARD = LVTTL;
	gndbus[3] : LOCATION = Pin_62;
	gndbus[3] : RESERVE_PIN = "AS INPUT TRI-STATED";
	gndbus[3] : IO_STANDARD = LVTTL;
	gndbus[4] : LOCATION = Pin_64;
	gndbus[4] : RESERVE_PIN = "AS INPUT TRI-STATED";
	gndbus[4] : IO_STANDARD = LVTTL;
	misc_pins[0] : LOCATION = Pin_87;
	misc_pins[0] : IO_STANDARD = LVTTL;
	misc_pins[10] : LOCATION = Pin_76;
	misc_pins[10] : IO_STANDARD = LVTTL;
	misc_pins[11] : LOCATION = Pin_74;
	misc_pins[11] : IO_STANDARD = LVTTL;
	misc_pins[1] : LOCATION = Pin_86;
	misc_pins[1] : IO_STANDARD = LVTTL;
	misc_pins[2] : LOCATION = Pin_85;
	misc_pins[2] : IO_STANDARD = LVTTL;
	misc_pins[3] : LOCATION = Pin_84;
	misc_pins[3] : IO_STANDARD = LVTTL;
	misc_pins[4] : LOCATION = Pin_83;
	misc_pins[4] : IO_STANDARD = LVTTL;
	misc_pins[5] : LOCATION = Pin_82;
	misc_pins[5] : IO_STANDARD = LVTTL;
	misc_pins[6] : LOCATION = Pin_79;
	misc_pins[6] : IO_STANDARD = LVTTL;
	misc_pins[7] : LOCATION = Pin_78;
	misc_pins[7] : IO_STANDARD = LVTTL;
	misc_pins[8] : LOCATION = Pin_77;
	misc_pins[8] : IO_STANDARD = LVTTL;
	misc_pins[9] : LOCATION = Pin_75;
	misc_pins[9] : IO_STANDARD = LVTTL;
	reset : LOCATION = Pin_94;
	usbclk : LOCATION = Pin_55;
	usbctl[0] : LOCATION = Pin_56;
	usbctl[1] : LOCATION = Pin_54;
	usbctl[2] : LOCATION = Pin_53;
	usbctl[3] : LOCATION = Pin_58;
	usbctl[4] : LOCATION = Pin_57;
	usbctl[5] : LOCATION = Pin_44;
	usbdata[0] : LOCATION = Pin_73;
	usbdata[10] : LOCATION = Pin_41;
	usbdata[11] : LOCATION = Pin_39;
	usbdata[12] : LOCATION = Pin_38;
	usbdata[12] : IO_STANDARD = LVTTL;
	usbdata[13] : LOCATION = Pin_37;
	usbdata[14] : LOCATION = Pin_24;
	usbdata[15] : LOCATION = Pin_23;
	usbdata[1] : LOCATION = Pin_68;
	usbdata[2] : LOCATION = Pin_67;
	usbdata[3] : LOCATION = Pin_66;
	usbdata[4] : LOCATION = Pin_65;
	usbdata[5] : LOCATION = Pin_61;
	usbdata[6] : LOCATION = Pin_60;
	usbdata[7] : LOCATION = Pin_59;
	usbdata[8] : LOCATION = Pin_43;
	usbdata[9] : LOCATION = Pin_42;
	usbrdy[0] : LOCATION = Pin_45;
	usbrdy[1] : LOCATION = Pin_46;
	usbrdy[2] : LOCATION = Pin_47;
	usbrdy[3] : LOCATION = Pin_48;
	usbrdy[4] : LOCATION = Pin_49;
	usbrdy[5] : LOCATION = Pin_50;
	clear_status : LOCATION = Pin_99;
}
