COMPILER_SETTINGS
{
	IO_PLACEMENT_OPTIMIZATION = OFF;
	ENABLE_DRC_SETTINGS = OFF;
	PHYSICAL_SYNTHESIS_REGISTER_RETIMING = OFF;
	PHYSICAL_SYNTHESIS_REGISTER_DUPLICATION = OFF;
	PHYSICAL_SYNTHESIS_COMBO_LOGIC = OFF;
	DRC_FANOUT_EXCEEDING = 30;
	DRC_REPORT_FANOUT_EXCEEDING = OFF;
	DRC_TOP_FANOUT = 50;
	DRC_REPORT_TOP_FANOUT = OFF;
	RUN_DRC_DURING_COMPILATION = OFF;
	ADV_NETLIST_OPT_RETIME_CORE_AND_IO = ON;
	ADV_NETLIST_OPT_SYNTH_USE_FITTER_INFO = OFF;
	ADV_NETLIST_OPT_SYNTH_GATE_RETIME = OFF;
	ADV_NETLIST_OPT_SYNTH_WYSIWYG_REMAP = OFF;
	SMART_COMPILE_IGNORES_TDC_FOR_STRATIX_PLL_CHANGES = OFF;
	MERGE_HEX_FILE = OFF;
	TRUE_WYSIWYG_FLOW = OFF;
	SEED = 1;
	FINAL_PLACEMENT_OPTIMIZATION = AUTOMATICALLY;
	FAMILY = Cyclone;
	DPRAM_DUAL_PORT_MODE_OTHER_SIGNALS_EPXA1 = "DPRAM0 TO 1 DPRAM1 TO 2";
	DPRAM_32BIT_SINGLE_PORT_MODE_OTHER_SIGNALS_EPXA1 = "MEGALAB COLUMN 1";
	DPRAM_8BIT_16BIT_SINGLE_PORT_MODE_OTHER_SIGNALS_EPXA1 = "MEGALAB COLUMN 1";
	DPRAM_DUAL_PORT_MODE_OUTPUT_EPXA1 = "DPRAM0 TO 1 DPRAM1 TO 2";
	DPRAM_32BIT_SINGLE_PORT_MODE_OUTPUT_EPXA1 = "LOWER TO 1ESB UPPER TO 1";
	DPRAM_8BIT_16BIT_SINGLE_PORT_MODE_OUTPUT_EPXA1 = "MEGALAB COLUMN 1";
	DPRAM_DUAL_PORT_MODE_INPUT_EPXA1 = "DPRAM0 TO 1 DPRAM1 TO 2";
	DPRAM_32BIT_SINGLE_PORT_MODE_INPUT_EPXA1 = "MEGALAB COLUMN 1";
	DPRAM_8BIT_16BIT_SINGLE_PORT_MODE_INPUT_EPXA1 = "MEGALAB COLUMN 1";
	DPRAM_DUAL_PORT_MODE_OTHER_SIGNALS_EPXA4_10 = "DPRAM0 TO 3 DPRAM1 TO 4";
	DPRAM_SINGLE_PORT_MODE_OTHER_SIGNALS_EPXA4_10 = "DPRAM0 TO 3 DPRAM1 TO 4";
	DPRAM_WIDE_MODE_OTHER_SIGNALS_EPXA4_10 = "MEGALAB COLUMN 3";
	DPRAM_DEEP_MODE_OTHER_SIGNALS_EPXA4_10 = "MEGALAB COLUMN 3";
	DPRAM_DUAL_PORT_MODE_OUTPUT_EPXA4_10 = "DPRAM0 TO 3 DPRAM1 TO 4ESB";
	DPRAM_SINGLE_PORT_MODE_OUTPUT_EPXA4_10 = "DPRAM0 TO 3 DPRAM1 TO 4ESB";
	DPRAM_WIDE_MODE_OUTPUT_EPXA4_10 = "LOWER TO 3 UPPER TO 4ESB";
	DPRAM_DEEP_MODE_OUTPUT_EPXA4_10 = "MEGALAB COLUMN 3";
	DPRAM_DUAL_PORT_MODE_INPUT_EPXA4_10 = "DPRAM0 TO 3 DPRAM1 TO 4";
	DPRAM_SINGLE_PORT_MODE_INPUT_EPXA4_10 = "DPRAM0 TO 3 DPRAM1 TO 4";
	DPRAM_WIDE_MODE_INPUT_EPXA4_10 = "LOWER TO 3 UPPER TO 4";
	DPRAM_DEEP_MODE_INPUT_EPXA4_10 = "MEGALAB COLUMN 3";
	DPRAM_OTHER_SIGNALS_EPXA4_10 = "DEFAULT OTHER ROUTING OPTIONS";
	DPRAM_OUTPUT_EPXA4_10 = "DEFAULT OUTPUT ROUTING OPTIONS";
	DPRAM_INPUT_EPXA4_10 = "DEFAULT INPUT ROUTING OPTIONS";
	STRIPE_TO_PLD_INTERRUPTS_EPXA4_10 = "MEGALAB COLUMN 2";
	PLD_TO_STRIPE_INTERRUPTS_EPXA4_10 = "MEGALAB COLUMN 2";
	PROCESSOR_DEBUG_EXTENSIONS_EPXA4_10 = "MEGALAB COLUMN 2";
	STRIPE_TO_PLD_BRIDGE_EPXA4_10 = "MEGALAB COLUMN 1";
	FAST_FIT_COMPILATION = OFF;
	SIGNALPROBE_DURING_NORMAL_COMPILATION = OFF;
	OPTIMIZE_IOC_REGISTER_PLACEMENT_FOR_TIMING = OFF;
	OPTIMIZE_TIMING = OFF;
	OPTIMIZE_HOLD_TIMING = OFF;
	COMPILATION_LEVEL = FULL;
	SAVE_DISK_SPACE = ON;
	SPEED_DISK_USAGE_TRADEOFF = NORMAL;
	LOGICLOCK_INCREMENTAL_COMPILE_ASSIGNMENT = OFF;
	SIGNALPROBE_ALLOW_OVERUSE = OFF;
	FOCUS_ENTITY_NAME = |sizetest;
	FIT_ONLY_ONE_ATTEMPT = OFF;
}
DEFAULT_DEVICE_OPTIONS
{
	GENERATE_CONFIG_HEXOUT_FILE = OFF;
	GENERATE_CONFIG_JBC_FILE_COMPRESSED = ON;
	GENERATE_CONFIG_JBC_FILE = OFF;
	GENERATE_CONFIG_JAM_FILE = OFF;
	GENERATE_CONFIG_ISC_FILE = OFF;
	GENERATE_CONFIG_SVF_FILE = OFF;
	GENERATE_JBC_FILE_COMPRESSED = ON;
	GENERATE_JBC_FILE = OFF;
	GENERATE_JAM_FILE = OFF;
	GENERATE_ISC_FILE = OFF;
	GENERATE_SVF_FILE = OFF;
	RESERVE_PIN = "AS INPUT TRI-STATED";
	RESERVE_ALL_UNUSED_PINS = "AS OUTPUT DRIVING GROUND";
	HEXOUT_FILE_COUNT_DIRECTION = UP;
	HEXOUT_FILE_START_ADDRESS = 0;
	GENERATE_HEX_FILE = OFF;
	GENERATE_RBF_FILE = OFF;
	GENERATE_TTF_FILE = OFF;
	RESERVE_ASDO_AFTER_CONFIGURATION = "USE AS REGULAR IO";
	RESERVE_DATA0_AFTER_CONFIGURATION = "AS INPUT TRI-STATED";
	RESERVE_DATA7_THROUGH_DATA1_AFTER_CONFIGURATION = "USE AS REGULAR IO";
	RESERVE_RDYNBUSY_AFTER_CONFIGURATION = "USE AS REGULAR IO";
	RESERVE_NWS_NRS_NCS_CS_AFTER_CONFIGURATION = "USE AS REGULAR IO";
	DISABLE_NCS_AND_OE_PULLUPS_ON_CONFIG_DEVICE = OFF;
	AUTO_INCREMENT_CONFIG_DEVICE_JTAG_USER_CODE = ON;
	EPROM_USE_CHECKSUM_AS_USERCODE = OFF;
	FLEX10K_CONFIG_DEVICE_JTAG_USER_CODE = FFFFFFFF;
	MERCURY_CONFIG_DEVICE_JTAG_USER_CODE = FFFFFFFF;
	STRATIX_CONFIG_DEVICE_JTAG_USER_CODE = FFFFFFFF;
	APEX20K_CONFIG_DEVICE_JTAG_USER_CODE = FFFFFFFF;
	STRATIX_CONFIGURATION_DEVICE = AUTO;
	CYCLONE_CONFIGURATION_DEVICE = AUTO;
	FLEX10K_CONFIGURATION_DEVICE = AUTO;
	FLEX6K_CONFIGURATION_DEVICE = AUTO;
	MERCURY_CONFIGURATION_DEVICE = AUTO;
	EXCALIBUR_CONFIGURATION_DEVICE = AUTO;
	APEX20K_CONFIGURATION_DEVICE = AUTO;
	USE_CONFIGURATION_DEVICE = ON;
	ENABLE_INIT_DONE_OUTPUT = OFF;
	FLEX10K_ENABLE_LOCK_OUTPUT = OFF;
	ENABLE_DEVICE_WIDE_OE = OFF;
	ENABLE_DEVICE_WIDE_RESET = OFF;
	RELEASE_CLEARS_BEFORE_TRI_STATES = OFF;
	AUTO_RESTART_CONFIGURATION = OFF;
	ENABLE_VREFB_PIN = OFF;
	ENABLE_VREFA_PIN = OFF;
	SECURITY_BIT = OFF;
	USER_START_UP_CLOCK = OFF;
	APEXII_CONFIGURATION_SCHEME = "PASSIVE SERIAL";
	FLEX10K_CONFIGURATION_SCHEME = "PASSIVE SERIAL";
	FLEX6K_CONFIGURATION_SCHEME = "PASSIVE SERIAL";
	MERCURY_CONFIGURATION_SCHEME = "PASSIVE SERIAL";
	EXCALIBUR_CONFIGURATION_SCHEME = "PASSIVE SERIAL";
	CYCLONE_CONFIGURATION_SCHEME = "ACTIVE SERIAL";
	STRATIX_CONFIGURATION_SCHEME = "PASSIVE SERIAL";
	APEX20K_CONFIGURATION_SCHEME = "PASSIVE SERIAL";
	STRATIX_UPDATE_MODE = STANDARD;
	USE_CHECKSUM_AS_USERCODE = OFF;
	MAX7000_USE_CHECKSUM_AS_USERCODE = OFF;
	MAX7000_JTAG_USER_CODE = FFFFFFFF;
	FLEX10K_JTAG_USER_CODE = 7F;
	MERCURY_JTAG_USER_CODE = FFFFFFFF;
	APEX20K_JTAG_USER_CODE = FFFFFFFF;
	STRATIX_JTAG_USER_CODE = FFFFFFFF;
	MAX7000S_JTAG_USER_CODE = FFFF;
	RESERVE_NCEO_AFTER_CONFIGURATION = "USE AS REGULAR IO";
	FLEX10K_ENABLE_LOW_VOLTAGE_MODE_ON_CONFIG_DEVICE = ON;
	FLEX6K_ENABLE_LOW_VOLTAGE_MODE_ON_CONFIG_DEVICE = OFF;
	ENABLE_LOW_VOLTAGE_MODE_ON_CONFIG_DEVICE = ON;
	MAX7000_ENABLE_JTAG_BST_SUPPORT = ON;
	ENABLE_JTAG_BST_SUPPORT = OFF;
	CONFIGURATION_CLOCK_DIVISOR = 1;
	CONFIGURATION_CLOCK_FREQUENCY = "10 MHZ";
	CLOCK_SOURCE = INTERNAL;
	COMPRESSION_MODE = OFF;
	ON_CHIP_BITSTREAM_DECOMPRESSION = OFF;
}
AUTO_SLD_HUB_ENTITY
{
	AUTO_INSERT_SLD_HUB_ENTITY = ENABLE;
	HUB_INSTANCE_NAME = SLD_HUB_INST;
	HUB_ENTITY_NAME = SLD_HUB;
}
CHIP(sizetest)
{
	DEVICE = EP1C12Q240C8;
	DEVICE_FILTER_PACKAGE = "ANY QFP";
	DEVICE_FILTER_PIN_COUNT = 240;
	DEVICE_FILTER_SPEED_GRADE = ANY;
}
SIGNALTAP_LOGIC_ANALYZER_SETTINGS
{
	ENABLE_SIGNALTAP = Off;
	AUTO_ENABLE_SMART_COMPILE = On;
}
