Cmp-Mod V01 Created by CvPCB (2011-06-08)-testing date = Sa 02 Jul 2011 17:52:11 CEST

BeginCmp
TimeStamp = /4DC804A6;
Reference = BT1;
ValeurCmp = 4.5-6V;
IdModule  = PIN_ARRAY_2X1;
EndCmp

BeginCmp
TimeStamp = /4DC8F975;
Reference = C1;
ValeurCmp = 2.2uF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4D037E30;
Reference = C3;
ValeurCmp = 100nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4DC66392;
Reference = C4;
ValeurCmp = 100nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4DC79EDF;
Reference = C5;
ValeurCmp = 33pF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4D020DD3;
Reference = C6;
ValeurCmp = 10nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4D020BDE;
Reference = C7;
ValeurCmp = 100nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4D020BEB;
Reference = C9;
ValeurCmp = 100nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4D020DCD;
Reference = C10;
ValeurCmp = 1nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4DC79ED8;
Reference = C11;
ValeurCmp = 15pF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4DC8F97A;
Reference = C12;
ValeurCmp = 2.2uF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4DC79EDC;
Reference = C13;
ValeurCmp = 15pF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4DC6A5DE;
Reference = C14;
ValeurCmp = 1uF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4D020ED8;
Reference = C15;
ValeurCmp = 100nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4DC664DD;
Reference = C16;
ValeurCmp = 100nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4CE9162F;
Reference = C17;
ValeurCmp = 10pF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4CE91633;
Reference = C18;
ValeurCmp = 10pF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4DC664E0;
Reference = C19;
ValeurCmp = 100nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4D020EDF;
Reference = C20;
ValeurCmp = 100nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4DC6A5CB;
Reference = C21;
ValeurCmp = 1uF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4DC6A5D9;
Reference = C22;
ValeurCmp = 1uF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4DC68E45;
Reference = C23;
ValeurCmp = 100nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4DFF9964;
Reference = C24;
ValeurCmp = 100nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4DC7A27C;
Reference = D1;
ValeurCmp = Schottky;
IdModule  = SOD123;
EndCmp

BeginCmp
TimeStamp = /4DCB8C13;
Reference = D2;
ValeurCmp = 1N5819;
IdModule  = SOD123;
EndCmp

BeginCmp
TimeStamp = /4DCB8C0D;
Reference = D3;
ValeurCmp = 1N5819;
IdModule  = SOD123;
EndCmp

BeginCmp
TimeStamp = /4CF54717;
Reference = D4;
ValeurCmp = RED;
IdModule  = LED-0805;
EndCmp

BeginCmp
TimeStamp = /4CF5471F;
Reference = D5;
ValeurCmp = GREEN;
IdModule  = LED-0805;
EndCmp

BeginCmp
TimeStamp = /4DC79E48;
Reference = FB1;
ValeurCmp = FILTER;
IdModule  = SM0805;
EndCmp

BeginCmp
TimeStamp = /4DC68E1D;
Reference = FB2;
ValeurCmp = FILTER;
IdModule  = SM0805;
EndCmp

BeginCmp
TimeStamp = /4DFF8B97;
Reference = IC2;
ValeurCmp = AP7332;
IdModule  = SOT26;
EndCmp

BeginCmp
TimeStamp = /4CE84486;
Reference = IC3;
ValeurCmp = AT91SAM7S;
IdModule  = TQFP_64;
EndCmp

BeginCmp
TimeStamp = /4DC6A187;
Reference = IC4;
ValeurCmp = CB3Q3244;
IdModule  = SSOP20_BDQ;
EndCmp

BeginCmp
TimeStamp = /4DFF9774;
Reference = IC5;
ValeurCmp = FPF2005;
IdModule  = SOT353;
EndCmp

BeginCmp
TimeStamp = /4CFAC6EA;
Reference = J1;
ValeurCmp = USB;
IdModule  = USB-MINI-B_54819-0519;
EndCmp

BeginCmp
TimeStamp = /4DCBE233;
Reference = J2;
ValeurCmp = JACK_2.5;
IdModule  = JACK2.5_SJ1-2503A;
EndCmp

BeginCmp
TimeStamp = /4DC68259;
Reference = JP1;
ValeurCmp = TEST;
IdModule  = PIN_ARRAY_2X1;
EndCmp

BeginCmp
TimeStamp = /4DC683ED;
Reference = JP2;
ValeurCmp = ERASE;
IdModule  = PIN_ARRAY_2X1;
EndCmp

BeginCmp
TimeStamp = /4CFCD6C9;
Reference = P1;
ValeurCmp = JTAG;
IdModule  = pin_array_10x2;
EndCmp

BeginCmp
TimeStamp = /4CE9ADCF;
Reference = P2;
ValeurCmp = DEBUG;
IdModule  = PIN_ARRAY-6X1;
EndCmp

BeginCmp
TimeStamp = /4DC51F05;
Reference = P3;
ValeurCmp = REBELSIM;
IdModule  = FFC_REBELSIM;
EndCmp

BeginCmp
TimeStamp = /4DC8FA06;
Reference = P4;
ValeurCmp = SIM;
IdModule  = SIM_AMPHENOL;
EndCmp

BeginCmp
TimeStamp = /4E0D8A18;
Reference = P5;
ValeurCmp = SAM;
IdModule  = SAM_FCI;
EndCmp

BeginCmp
TimeStamp = /4DC7A1CA;
Reference = Q1;
ValeurCmp = BC847;
IdModule  = SOT23_BC847;
EndCmp

BeginCmp
TimeStamp = /4DC7A43A;
Reference = Q2;
ValeurCmp = BC847;
IdModule  = SOT23_BC847;
EndCmp

BeginCmp
TimeStamp = /4DC79ED1;
Reference = R1;
ValeurCmp = 100K;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4DC79E9A;
Reference = R2;
ValeurCmp = 10K;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4DC79ECE;
Reference = R3;
ValeurCmp = 1K5;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4CE9A68C;
Reference = R4;
ValeurCmp = 100K;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4CE9A69A;
Reference = R5;
ValeurCmp = 100K;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4CE9A6A5;
Reference = R6;
ValeurCmp = 100K;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4CE9A6A9;
Reference = R7;
ValeurCmp = 100K;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4CE9A6AE;
Reference = R8;
ValeurCmp = 100K;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4DC79EAD;
Reference = R9;
ValeurCmp = 27R;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4DC79EA7;
Reference = R10;
ValeurCmp = 27R;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4D020DC6;
Reference = R11;
ValeurCmp = 1K5;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4D0206C7;
Reference = R12;
ValeurCmp = 100K;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4CF7BAEE;
Reference = R13;
ValeurCmp = 150R;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4DC555D0;
Reference = R14;
ValeurCmp = 150R;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4DC7A441;
Reference = R16;
ValeurCmp = 10K;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4DC799F2;
Reference = R17;
ValeurCmp = 10K;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4DC5A30D;
Reference = R18;
ValeurCmp = 10K;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4DFF73B0;
Reference = R19;
ValeurCmp = 100K;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4DFF7469;
Reference = R20;
ValeurCmp = 10k1%;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4DFF746C;
Reference = R21;
ValeurCmp = 10k1%;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4DFF9902;
Reference = R22;
ValeurCmp = 100K;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /4D020733;
Reference = SW1;
ValeurCmp = RESET;
IdModule  = PUSH_BUTTON;
EndCmp

BeginCmp
TimeStamp = /4DC6852C;
Reference = SW2;
ValeurCmp = BOOTLOADER;
IdModule  = PUSH_BUTTON;
EndCmp

BeginCmp
TimeStamp = /4DC5A250;
Reference = U1;
ValeurCmp = FLASH;
IdModule  = SOIC8;
EndCmp

BeginCmp
TimeStamp = /4CE915DE;
Reference = X1;
ValeurCmp = 18.432MHz;
IdModule  = Q_49U3HMS;
EndCmp

EndListe
