# Handover to best better cell
# The best neighbor cell is selected

create-n-bts 7
set-ts-use trx 0 0 states * TCH/F - - - - - -
meas-rep lchan 0 0 1 0 rxlev 10 rxqual 0 ta 0 neighbors 20 21 18 20 23 19
expect-ho from lchan 0 0 1 0 to lchan 5 0 1 0
expect-ts-use trx 0 0 states * - - - - - - -
expect-ts-use trx 5 0 states * TCH/F - - - - - -

