# No more parallel handovers, if max_unsync_ho is defined
# There are three mobiles that want to handover, but only two can do
# it at a time, because the maximum number is limited to two.

create-n-bts 2
network
 bts 1
  handover2 max-handovers 2
set-ts-use trx 0 0 states * TCH/F TCH/F TCH/F - - - -
meas-rep lchan 0 0 1 0 rxlev 0 rxqual 0 ta 0 neighbors 30
expect-chan lchan 1 0 1 0
expect-ho-cmd lchan 0 0 1 0
meas-rep lchan 0 0 2 0 rxlev 0 rxqual 0 ta 0 neighbors 30
expect-chan lchan 1 0 2 0
expect-ho-cmd lchan 0 0 2 0
meas-rep lchan 0 0 3 0 rxlev 0 rxqual 0 ta 0 neighbors 30
expect-no-chan

