===== test_ms_timeout_lu_auth_resp
- Total time passed: 0.000000 s
- Location Update request causes a GSUP Send Auth Info request to HLR
  MSC <--RAN_GERAN_A-- MS: GSM48_MT_MM_LOC_UPD_REQUEST
  new conn
DREF unknown: MSC conn use + 1 == 1
DRLL Dispatching 04.08 message GSM48_MT_MM_LOC_UPD_REQUEST (0x5:0x8)
DREF unknown: MSC conn use + 1 == 2
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_INIT}: Allocated
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_INIT}: Received Event SUBSCR_CONN_E_START
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_INIT}: state_chg to SUBSCR_CONN_S_NEW
DMM LOCATION UPDATING REQUEST: MI(IMSI)=901700000004620 type=IMSI ATTACH
DMM LU/new-LAC: 1/0
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_IDLE}: Allocated
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_IDLE}: is child of Subscr_Conn(901700000004620)
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_IDLE}: rev=GSM net=GERAN Auth (no Ciph)
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_IDLE}: Received Event VLR_ULA_E_UPDATE_LA
DREF VLR subscr unknown usage increases to: 1
DVLR set IMSI on subscriber; IMSI=901700000004620 id=901700000004620
DVLR New subscr, IMSI: 901700000004620
DREF VLR subscr IMSI:901700000004620 usage increases to: 2
DREF VLR subscr IMSI:901700000004620 usage decreases to: 1
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_IDLE}: vlr_loc_upd_node1()
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_IDLE}: state_chg to VLR_ULA_S_WAIT_AUTH
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_NEEDS_AUTH}: is child of vlr_lu_fsm(901700000004620)
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
DVLR GSUP tx: 08010809710000004026f0
GSUP --> HLR: OSMO_GSUP_MSGT_SEND_AUTH_INFO_REQUEST: 08010809710000004026f0
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_NEEDS_AUTH_WAIT_AI
DMM IMSI:901700000004620: bump: conn still being established (SUBSCR_CONN_S_NEW)
DREF IMSI:901700000004620: MSC conn use - 1 == 1
  lu_result_sent == 0
- from HLR, rx _SEND_AUTH_INFO_RESULT; VLR sends Auth Req to MS
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: 0a010809710000004026f003222010585df1ae287f6e273dce07090d61320b21042d8b2c3e220861855fb81fc2a800
DVLR GSUP rx 47: 0a010809710000004026f003222010585df1ae287f6e273dce07090d61320b21042d8b2c3e220861855fb81fc2a800
DREF VLR subscr IMSI:901700000004620 usage increases to: 2
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: Received Event VLR_AUTH_E_HLR_SAI_ACK
DVLR SUBSCR(IMSI:901700000004620) Received 1 auth tuples
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=0
- sending GSM Auth Request for IMSI:901700000004620: tuple use_count=1 key_seq=0 auth_types=0x1 and...
- ...rand=585df1ae287f6e273dce07090d61320b
- ...expecting sres=2d8b2c3e
DREF VLR subscr IMSI:901700000004620 usage decreases to: 1
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: vlr_gsupc_read_cb() returns 0
  auth_request_sent == 1
  lu_result_sent == 0
---
- MS fails to send an Authentication Response
- At first, we're still waiting
- Total time passed: 0.000423 s
  llist_count(&net->subscr_conns) == 1
  lu_result_sent == 0
- Total time passed: 1.000658 s
  llist_count(&net->subscr_conns) == 1
  lu_result_sent == 0
- Total time passed: 2.000893 s
  llist_count(&net->subscr_conns) == 1
  lu_result_sent == 0
- Total time passed: 3.001128 s
  llist_count(&net->subscr_conns) == 1
  lu_result_sent == 0
- Total time passed: 4.001363 s
  llist_count(&net->subscr_conns) == 1
  lu_result_sent == 0
- Total time passed: 5.001598 s
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_NEW}: Timeout of T0
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_WAIT_AUTH}: Connection timed out
- sending LU Reject for IMSI:901700000004620, cause 22
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_WAIT_AUTH}: state_chg to VLR_ULA_S_DONE
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_NEW}: Received Event SUBSCR_CONN_E_CN_CLOSE
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_NEW}: SUBSCR_CONN_FROM_LU
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_NEW}: Close event, cause 1
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_NEW}: state_chg to SUBSCR_CONN_S_RELEASED
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_DONE}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_WAIT_RESP}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_WAIT_RESP}: Removing from parent vlr_lu_fsm(901700000004620)
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_WAIT_RESP}: Freeing instance
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_WAIT_RESP}: Deallocated
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_DONE}: Removing from parent Subscr_Conn(901700000004620)
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_DONE}: fsm_lu_cleanup called with cause OSMO_FSM_TERM_PARENT
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_DONE}: Freeing instance
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_DONE}: Deallocated
DMM msc_subscr_conn_close(vsub=IMSI:901700000004620, cause=2): no conn fsm, releasing directly without release event.
- BSSAP Clear --RAN_GERAN_A--> MS
DREF IMSI:901700000004620: MSC conn use - 1 == 0
DRLL subscr IMSI:901700000004620: Freeing subscriber connection
DREF VLR subscr IMSI:901700000004620 usage decreases to: 0
DREF freeing VLR subscr IMSI:901700000004620
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_RELEASED}: Freeing instance
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_RELEASED}: Deallocated
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_RELEASED}: Received Event SUBSCR_CONN_E_CN_CLOSE
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_RELEASED}: Event SUBSCR_CONN_E_CN_CLOSE not permitted
- SUBSCR_CONN_TIMEOUT has passed, conn is gone.
  bssap_clear_sent == 1
  llist_count(&net->subscr_conns) == 0
  lu_result_sent == 2
===== test_ms_timeout_lu_auth_resp: SUCCESS

full talloc report on 'msgb' (total      0 bytes in   1 blocks)
talloc_total_blocks(tall_bsc_ctx) == 9

===== test_ms_timeout_cm_auth_resp
- Total time passed: 0.000000 s
- Location Update request causes a GSUP Send Auth Info request to HLR
  MSC <--RAN_GERAN_A-- MS: GSM48_MT_MM_LOC_UPD_REQUEST
  new conn
DREF unknown: MSC conn use + 1 == 1
DRLL Dispatching 04.08 message GSM48_MT_MM_LOC_UPD_REQUEST (0x5:0x8)
DREF unknown: MSC conn use + 1 == 2
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_INIT}: Allocated
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_INIT}: Received Event SUBSCR_CONN_E_START
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_INIT}: state_chg to SUBSCR_CONN_S_NEW
DMM LOCATION UPDATING REQUEST: MI(IMSI)=901700000004620 type=IMSI ATTACH
DMM LU/new-LAC: 1/0
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_IDLE}: Allocated
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_IDLE}: is child of Subscr_Conn(901700000004620)
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_IDLE}: rev=GSM net=GERAN Auth (no Ciph)
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_IDLE}: Received Event VLR_ULA_E_UPDATE_LA
DREF VLR subscr unknown usage increases to: 1
DVLR set IMSI on subscriber; IMSI=901700000004620 id=901700000004620
DVLR New subscr, IMSI: 901700000004620
DREF VLR subscr IMSI:901700000004620 usage increases to: 2
DREF VLR subscr IMSI:901700000004620 usage decreases to: 1
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_IDLE}: vlr_loc_upd_node1()
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_IDLE}: state_chg to VLR_ULA_S_WAIT_AUTH
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_NEEDS_AUTH}: is child of vlr_lu_fsm(901700000004620)
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
DVLR GSUP tx: 08010809710000004026f0
GSUP --> HLR: OSMO_GSUP_MSGT_SEND_AUTH_INFO_REQUEST: 08010809710000004026f0
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_NEEDS_AUTH_WAIT_AI
DMM IMSI:901700000004620: bump: conn still being established (SUBSCR_CONN_S_NEW)
DREF IMSI:901700000004620: MSC conn use - 1 == 1
  lu_result_sent == 0
- from HLR, rx _SEND_AUTH_INFO_RESULT; VLR sends Auth Req to MS
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: 0a010809710000004026f003222010585df1ae287f6e273dce07090d61320b21042d8b2c3e220861855fb81fc2a8000322201012aca96fb4ffdea5c985cbafa9b6e18b210420bde240220807fa7502e07e1c0003222010e7c03ba7cf0e2fde82b2dc4d63077d422104a29514ae2208e2b234f80788640003222010fa8f20b781b5881329d4fea26b1a3c5121045afc8d7222082392f14f709ae000032220100fd4cc8dbe8715d1f439e304edfd68dc2104bc8d1c5b2208da7cdd6bfe2d7000
DVLR GSUP rx 191: 0a010809710000004026f003222010585df1ae287f6e273dce07090d61320b21042d8b2c3e220861855fb81fc2a8000322201012aca96fb4ffdea5c985cbafa9b6e18b210420bde240220807fa7502e07e1c0003222010e7c03ba7cf0e2fde82b2dc4d63077d422104a29514ae2208e2b234f80788640003222010fa8f20b781b5881329d4fea26b1a3c5121045afc8d7222082392f14f709ae000032220100fd4cc8dbe8715d1f439e304edfd68dc2104bc8d1c5b2208da7cdd6bfe2d7000
DREF VLR subscr IMSI:901700000004620 usage increases to: 2
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: Received Event VLR_AUTH_E_HLR_SAI_ACK
DVLR SUBSCR(IMSI:901700000004620) Received 5 auth tuples
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=0
- sending GSM Auth Request for IMSI:901700000004620: tuple use_count=1 key_seq=0 auth_types=0x1 and...
- ...rand=585df1ae287f6e273dce07090d61320b
- ...expecting sres=2d8b2c3e
DREF VLR subscr IMSI:901700000004620 usage decreases to: 1
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: vlr_gsupc_read_cb() returns 0
  auth_request_sent == 1
  lu_result_sent == 0
- MS sends Authen Response, VLR accepts and sends GSUP LU Req to HLR
  MSC <--RAN_GERAN_A-- MS: GSM48_MT_MM_AUTH_RESP
DREF IMSI:901700000004620: MSC conn use + 1 == 2
DRLL Dispatching 04.08 message GSM48_MT_MM_AUTH_RESP (0x5:0x14)
DMM IMSI:901700000004620: MM GSM AUTHENTICATION RESPONSE (sres = 2d8b2c3e)
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(IMSI:901700000004620) received res: 2d 8b 2c 3e 
DVLR SUBSCR(IMSI:901700000004620) AUTH established GSM security context
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_WAIT_RESP}: Authentication terminating with result VLR_AUTH_RES_PASSED
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_AUTHENTICATED}: Removing from parent vlr_lu_fsm(901700000004620)
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_AUTHENTICATED}: Freeing instance
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_WAIT_AUTH}: Received Event VLR_ULA_E_AUTH_RES
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_post_auth()
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_post_ciph()
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_node_4()
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_WAIT_AUTH}: state_chg to VLR_ULA_S_WAIT_HLR_UPD
DVLR upd_hlr_vlr_fsm(901700000004620){UPD_HLR_VLR_S_INIT}: Allocated
DVLR upd_hlr_vlr_fsm(901700000004620){UPD_HLR_VLR_S_INIT}: is child of vlr_lu_fsm(901700000004620)
DVLR upd_hlr_vlr_fsm(901700000004620){UPD_HLR_VLR_S_INIT}: Received Event UPD_HLR_VLR_E_START
DVLR GSUP tx: 04010809710000004026f0
GSUP --> HLR: OSMO_GSUP_MSGT_UPDATE_LOCATION_REQUEST: 04010809710000004026f0
DVLR upd_hlr_vlr_fsm(901700000004620){UPD_HLR_VLR_S_INIT}: state_chg to UPD_HLR_VLR_S_WAIT_FOR_DATA
DMM IMSI:901700000004620: bump: conn still being established (SUBSCR_CONN_S_NEW)
DREF IMSI:901700000004620: MSC conn use - 1 == 1
  lu_result_sent == 0
- HLR sends _INSERT_DATA_REQUEST, VLR responds with _INSERT_DATA_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: 10010809710000004026f00804036470f1
DVLR GSUP rx 17: 10010809710000004026f00804036470f1
DREF VLR subscr IMSI:901700000004620 usage increases to: 2
DVLR IMSI:901700000004620 has MSISDN:46071
DVLR GSUP tx: 12010809710000004026f0
GSUP --> HLR: OSMO_GSUP_MSGT_INSERT_DATA_RESULT: 12010809710000004026f0
DREF VLR subscr MSISDN:46071 usage decreases to: 1
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: vlr_gsupc_read_cb() returns 0
  lu_result_sent == 0
- HLR also sends GSUP _UPDATE_LOCATION_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: 06010809710000004026f0
DVLR GSUP rx 11: 06010809710000004026f0
DREF VLR subscr MSISDN:46071 usage increases to: 2
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_HLR_LU_RES
DVLR upd_hlr_vlr_fsm(901700000004620){UPD_HLR_VLR_S_WAIT_FOR_DATA}: Received Event UPD_HLR_VLR_E_UPD_LOC_ACK
DVLR upd_hlr_vlr_fsm(901700000004620){UPD_HLR_VLR_S_WAIT_FOR_DATA}: state_chg to UPD_HLR_VLR_S_DONE
DVLR upd_hlr_vlr_fsm(901700000004620){UPD_HLR_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR upd_hlr_vlr_fsm(901700000004620){UPD_HLR_VLR_S_DONE}: Removing from parent vlr_lu_fsm(901700000004620)
DVLR upd_hlr_vlr_fsm(901700000004620){UPD_HLR_VLR_S_DONE}: Freeing instance
DVLR upd_hlr_vlr_fsm(901700000004620){UPD_HLR_VLR_S_DONE}: Deallocated
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_UPD_HLR_COMPL
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_WAIT_HLR_UPD}: state_chg to VLR_ULA_S_WAIT_LU_COMPL
DVLR lu_compl_vlr_fsm(901700000004620){LU_COMPL_VLR_S_INIT}: Allocated
DVLR lu_compl_vlr_fsm(901700000004620){LU_COMPL_VLR_S_INIT}: is child of vlr_lu_fsm(901700000004620)
DVLR lu_compl_vlr_fsm(901700000004620){LU_COMPL_VLR_S_INIT}: Received Event LU_COMPL_VLR_E_START
DVLR lu_compl_vlr_fsm(901700000004620){LU_COMPL_VLR_S_INIT}: state_chg to LU_COMPL_VLR_S_WAIT_SUB_PRES
DVLR sub_pres_vlr_fsm(901700000004620){SUB_PRES_VLR_S_INIT}: Allocated
DVLR sub_pres_vlr_fsm(901700000004620){SUB_PRES_VLR_S_INIT}: is child of lu_compl_vlr_fsm(901700000004620)
DVLR sub_pres_vlr_fsm(901700000004620){SUB_PRES_VLR_S_INIT}: Received Event SUB_PRES_VLR_E_START
DVLR sub_pres_vlr_fsm(901700000004620){SUB_PRES_VLR_S_INIT}: state_chg to SUB_PRES_VLR_S_DONE
DVLR sub_pres_vlr_fsm(901700000004620){SUB_PRES_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR sub_pres_vlr_fsm(901700000004620){SUB_PRES_VLR_S_DONE}: Removing from parent lu_compl_vlr_fsm(901700000004620)
DVLR sub_pres_vlr_fsm(901700000004620){SUB_PRES_VLR_S_DONE}: Freeing instance
DVLR sub_pres_vlr_fsm(901700000004620){SUB_PRES_VLR_S_DONE}: Deallocated
DVLR lu_compl_vlr_fsm(901700000004620){LU_COMPL_VLR_S_WAIT_SUB_PRES}: Received Event LU_COMPL_VLR_E_SUB_PRES_COMPL
- sending LU Accept for MSISDN:46071
DREF VLR subscr MSISDN:46071 usage increases to: 3
DVLR lu_compl_vlr_fsm(901700000004620){LU_COMPL_VLR_S_WAIT_SUB_PRES}: state_chg to LU_COMPL_VLR_S_DONE
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_LU_COMPL_SUCCESS
DVLR lu_compl_vlr_fsm(901700000004620){LU_COMPL_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DVLR lu_compl_vlr_fsm(901700000004620){LU_COMPL_VLR_S_DONE}: Removing from parent vlr_lu_fsm(901700000004620)
DVLR lu_compl_vlr_fsm(901700000004620){LU_COMPL_VLR_S_DONE}: Freeing instance
DVLR lu_compl_vlr_fsm(901700000004620){LU_COMPL_VLR_S_DONE}: Deallocated
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_WAIT_LU_COMPL}: state_chg to VLR_ULA_S_DONE
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_NEW}: Received Event SUBSCR_CONN_E_ACCEPTED
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_NEW}: SUBSCR_CONN_FROM_LU
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_NEW}: state_chg to SUBSCR_CONN_S_ACCEPTED
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_ACCEPTED}: Received Event SUBSCR_CONN_E_BUMP
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_ACCEPTED}: bump: releasing conn
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_ACCEPTED}: state_chg to SUBSCR_CONN_S_RELEASED
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_DONE}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_DONE}: Removing from parent Subscr_Conn(901700000004620)
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_DONE}: fsm_lu_cleanup called with cause OSMO_FSM_TERM_PARENT
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_DONE}: Freeing instance
DVLR vlr_lu_fsm(901700000004620){VLR_ULA_S_DONE}: Deallocated
DMM msc_subscr_conn_close(vsub=MSISDN:46071, cause=2): no conn fsm, releasing directly without release event.
- BSSAP Clear --RAN_GERAN_A--> MS
DREF MSISDN:46071: MSC conn use - 1 == 0
DRLL subscr MSISDN:46071: Freeing subscriber connection
DREF VLR subscr MSISDN:46071 usage decreases to: 2
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_RELEASED}: Freeing instance
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_RELEASED}: Deallocated
DREF VLR subscr MSISDN:46071 usage decreases to: 1
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: vlr_gsupc_read_cb() returns 0
  bssap_clear_sent == 1
- LU was successful, and the conn has already been closed
  lu_result_sent == 1
  llist_count(&net->subscr_conns) == 0
---
- after a while, a new conn sends a CM Service Request. VLR responds with Auth Req, 2nd auth vector
  MSC <--RAN_GERAN_A-- MS: GSM48_MT_MM_CM_SERV_REQ
  new conn
DREF unknown: MSC conn use + 1 == 1
DRLL Dispatching 04.08 message GSM48_MT_MM_CM_SERV_REQ (0x5:0x24)
DMM <- CM SERVICE REQUEST serv_type=0x08 MI(IMSI)=901700000004620
DREF unknown: MSC conn use + 1 == 2
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_INIT}: Allocated
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_INIT}: Received Event SUBSCR_CONN_E_START
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_INIT}: state_chg to SUBSCR_CONN_S_NEW
DVLR Process_Access_Request_VLR(901700000004620){PR_ARQ_S_INIT}: Allocated
DVLR Process_Access_Request_VLR(901700000004620){PR_ARQ_S_INIT}: is child of Subscr_Conn(901700000004620)
DVLR Process_Access_Request_VLR(901700000004620){PR_ARQ_S_INIT}: rev=GSM net=GERAN Auth (no Ciph)
DVLR Process_Access_Request_VLR(901700000004620){PR_ARQ_S_INIT}: Received Event PR_ARQ_E_START
DREF VLR subscr MSISDN:46071 usage increases to: 2
DREF VLR subscr MSISDN:46071 usage increases to: 3
DVLR Process_Access_Request_VLR(901700000004620){PR_ARQ_S_INIT}: proc_arq_vlr_fn_post_imsi()
DVLR Process_Access_Request_VLR(901700000004620){PR_ARQ_S_INIT}: state_chg to PR_ARQ_S_WAIT_AUTH
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_NEEDS_AUTH}: is child of Process_Access_Request_VLR(901700000004620)
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=1
- sending GSM Auth Request for MSISDN:46071: tuple use_count=1 key_seq=1 auth_types=0x1 and...
- ...rand=12aca96fb4ffdea5c985cbafa9b6e18b
- ...expecting sres=20bde240
DREF VLR subscr MSISDN:46071 usage decreases to: 2
DMM MSISDN:46071: bump: conn still being established (SUBSCR_CONN_S_NEW)
DREF MSISDN:46071: MSC conn use - 1 == 1
  cm_service_result_sent == 0
  auth_request_sent == 1
---
- MS fails to send an Authentication Response
- At first, we're still waiting
- Total time passed: 0.000423 s
  llist_count(&net->subscr_conns) == 1
  cm_service_result_sent == 0
- Total time passed: 1.000658 s
  llist_count(&net->subscr_conns) == 1
  cm_service_result_sent == 0
- Total time passed: 2.000893 s
  llist_count(&net->subscr_conns) == 1
  cm_service_result_sent == 0
- Total time passed: 3.001128 s
  llist_count(&net->subscr_conns) == 1
  cm_service_result_sent == 0
- Total time passed: 4.001363 s
  llist_count(&net->subscr_conns) == 1
  cm_service_result_sent == 0
- Total time passed: 5.001598 s
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_NEW}: Timeout of T0
DVLR Process_Access_Request_VLR(901700000004620){PR_ARQ_S_WAIT_AUTH}: Connection timed out
DVLR Process_Access_Request_VLR(901700000004620){PR_ARQ_S_WAIT_AUTH}: proc_arq_fsm_done(VLR_PR_ARQ_RES_TIMEOUT)
DVLR Process_Access_Request_VLR(901700000004620){PR_ARQ_S_WAIT_AUTH}: state_chg to PR_ARQ_S_DONE
DVLR Process_Access_Request_VLR(901700000004620){PR_ARQ_S_DONE}: Process Access Request result: VLR_PR_ARQ_RES_TIMEOUT
- sending CM Service Reject for MSISDN:46071, result VLR_PR_ARQ_RES_TIMEOUT
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_NEW}: Received Event SUBSCR_CONN_E_CN_CLOSE
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_NEW}: SUBSCR_CONN_FROM_CM_SERVICE_REQ
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_NEW}: Close event, cause 2
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_NEW}: state_chg to SUBSCR_CONN_S_RELEASED
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR Process_Access_Request_VLR(901700000004620){PR_ARQ_S_DONE}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_WAIT_RESP}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_WAIT_RESP}: Removing from parent Process_Access_Request_VLR(901700000004620)
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_WAIT_RESP}: Freeing instance
DVLR VLR_Authenticate(901700000004620){VLR_SUB_AS_WAIT_RESP}: Deallocated
DVLR Process_Access_Request_VLR(901700000004620){PR_ARQ_S_DONE}: Removing from parent Subscr_Conn(901700000004620)
DVLR Process_Access_Request_VLR(901700000004620){PR_ARQ_S_DONE}: Freeing instance
DVLR Process_Access_Request_VLR(901700000004620){PR_ARQ_S_DONE}: Deallocated
DMM msc_subscr_conn_close(vsub=MSISDN:46071, cause=2): no conn fsm, releasing directly without release event.
- BSSAP Clear --RAN_GERAN_A--> MS
DREF MSISDN:46071: MSC conn use - 1 == 0
DRLL subscr MSISDN:46071: Freeing subscriber connection
DREF VLR subscr MSISDN:46071 usage decreases to: 1
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_RELEASED}: Freeing instance
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_RELEASED}: Deallocated
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_RELEASED}: Received Event SUBSCR_CONN_E_CN_CLOSE
DMM Subscr_Conn(901700000004620){SUBSCR_CONN_S_RELEASED}: Event SUBSCR_CONN_E_CN_CLOSE not permitted
- SUBSCR_CONN_TIMEOUT has passed, conn is gone.
  bssap_clear_sent == 1
  llist_count(&net->subscr_conns) == 0
  cm_service_result_sent == 2
DREF freeing VLR subscr MSISDN:46071
===== test_ms_timeout_cm_auth_resp: SUCCESS

full talloc report on 'msgb' (total      0 bytes in   1 blocks)
talloc_total_blocks(tall_bsc_ctx) == 9

full talloc report on 'msgb' (total      0 bytes in   1 blocks)
talloc_total_blocks(tall_bsc_ctx) == 9

