<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<settings>
<setting alwaysvectorfont="no"/>
<setting verticaltext="up"/>
</settings>
<grid distance="0.254" unitdist="mm" unit="mm" style="lines" multiple="1" display="no" altdistance="0.025" altunitdist="inch" altunit="inch"/>
<layers>
<layer number="1" name="Top" color="4" fill="1" visible="yes" active="yes"/>
<layer number="2" name="Route2" color="1" fill="3" visible="no" active="no"/>
<layer number="3" name="Route3" color="4" fill="3" visible="no" active="no"/>
<layer number="4" name="Route4" color="1" fill="4" visible="no" active="no"/>
<layer number="5" name="Route5" color="4" fill="4" visible="no" active="no"/>
<layer number="6" name="Route6" color="1" fill="8" visible="no" active="no"/>
<layer number="7" name="Route7" color="4" fill="8" visible="no" active="no"/>
<layer number="8" name="Route8" color="1" fill="2" visible="no" active="no"/>
<layer number="9" name="Route9" color="4" fill="2" visible="no" active="no"/>
<layer number="10" name="Route10" color="1" fill="7" visible="no" active="no"/>
<layer number="11" name="Route11" color="4" fill="7" visible="no" active="no"/>
<layer number="12" name="Route12" color="1" fill="5" visible="no" active="no"/>
<layer number="13" name="Route13" color="4" fill="5" visible="no" active="no"/>
<layer number="14" name="Route14" color="1" fill="6" visible="no" active="no"/>
<layer number="15" name="Route15" color="4" fill="6" visible="no" active="no"/>
<layer number="16" name="Bottom" color="1" fill="1" visible="yes" active="yes"/>
<layer number="17" name="Pads" color="2" fill="1" visible="yes" active="yes"/>
<layer number="18" name="Vias" color="2" fill="1" visible="yes" active="yes"/>
<layer number="19" name="Unrouted" color="6" fill="1" visible="yes" active="yes"/>
<layer number="20" name="Dimension" color="15" fill="1" visible="yes" active="yes"/>
<layer number="21" name="tPlace" color="7" fill="1" visible="yes" active="yes"/>
<layer number="22" name="bPlace" color="7" fill="1" visible="yes" active="yes"/>
<layer number="23" name="tOrigins" color="15" fill="1" visible="yes" active="yes"/>
<layer number="24" name="bOrigins" color="15" fill="1" visible="yes" active="yes"/>
<layer number="25" name="tNames" color="7" fill="1" visible="yes" active="yes"/>
<layer number="26" name="bNames" color="7" fill="1" visible="yes" active="yes"/>
<layer number="27" name="tValues" color="7" fill="1" visible="no" active="yes"/>
<layer number="28" name="bValues" color="7" fill="1" visible="no" active="yes"/>
<layer number="29" name="tStop" color="7" fill="3" visible="no" active="yes"/>
<layer number="30" name="bStop" color="7" fill="6" visible="no" active="yes"/>
<layer number="31" name="tCream" color="7" fill="4" visible="no" active="yes"/>
<layer number="32" name="bCream" color="7" fill="5" visible="no" active="yes"/>
<layer number="33" name="tFinish" color="6" fill="3" visible="no" active="yes"/>
<layer number="34" name="bFinish" color="6" fill="6" visible="no" active="yes"/>
<layer number="35" name="tGlue" color="7" fill="4" visible="no" active="yes"/>
<layer number="36" name="bGlue" color="7" fill="5" visible="no" active="yes"/>
<layer number="37" name="tTest" color="7" fill="1" visible="no" active="yes"/>
<layer number="38" name="bTest" color="7" fill="1" visible="no" active="yes"/>
<layer number="39" name="tKeepout" color="4" fill="11" visible="yes" active="yes"/>
<layer number="40" name="bKeepout" color="1" fill="11" visible="yes" active="yes"/>
<layer number="41" name="tRestrict" color="4" fill="10" visible="yes" active="yes"/>
<layer number="42" name="bRestrict" color="1" fill="10" visible="yes" active="yes"/>
<layer number="43" name="vRestrict" color="2" fill="10" visible="yes" active="yes"/>
<layer number="44" name="Drills" color="7" fill="1" visible="no" active="yes"/>
<layer number="45" name="Holes" color="7" fill="1" visible="no" active="yes"/>
<layer number="46" name="Milling" color="3" fill="1" visible="no" active="yes"/>
<layer number="47" name="Measures" color="7" fill="1" visible="no" active="yes"/>
<layer number="48" name="Document" color="7" fill="1" visible="yes" active="yes"/>
<layer number="49" name="Reference" color="7" fill="1" visible="yes" active="yes"/>
<layer number="50" name="dxf" color="7" fill="1" visible="no" active="no"/>
<layer number="51" name="tDocu" color="7" fill="1" visible="yes" active="yes"/>
<layer number="52" name="bDocu" color="7" fill="1" visible="yes" active="yes"/>
<layer number="53" name="tGND_GNDA" color="7" fill="9" visible="no" active="no"/>
<layer number="54" name="bGND_GNDA" color="1" fill="9" visible="no" active="no"/>
<layer number="56" name="wert" color="7" fill="1" visible="no" active="no"/>
<layer number="57" name="tCAD" color="6" fill="1" visible="no" active="no"/>
<layer number="59" name="tMark" color="7" fill="1" visible="no" active="no"/>
<layer number="60" name="bMark" color="7" fill="1" visible="no" active="no"/>
<layer number="90" name="Modules" color="5" fill="1" visible="no" active="no"/>
<layer number="91" name="Nets" color="2" fill="1" visible="no" active="no"/>
<layer number="92" name="Busses" color="1" fill="1" visible="no" active="no"/>
<layer number="93" name="Pins" color="2" fill="1" visible="no" active="no"/>
<layer number="94" name="Symbols" color="4" fill="1" visible="no" active="no"/>
<layer number="95" name="Names" color="7" fill="1" visible="no" active="no"/>
<layer number="96" name="Values" color="7" fill="1" visible="no" active="no"/>
<layer number="97" name="Info" color="7" fill="1" visible="no" active="no"/>
<layer number="98" name="Guide" color="6" fill="1" visible="no" active="no"/>
<layer number="99" name="SpiceOrder" color="7" fill="1" visible="no" active="no"/>
<layer number="100" name="Muster" color="7" fill="1" visible="yes" active="yes"/>
<layer number="101" name="Patch_Top" color="12" fill="4" visible="yes" active="yes"/>
<layer number="102" name="Mittellin" color="7" fill="1" visible="yes" active="yes"/>
<layer number="103" name="Stiffner" color="7" fill="1" visible="yes" active="yes"/>
<layer number="104" name="Name" color="7" fill="1" visible="yes" active="yes"/>
<layer number="105" name="Beschreib" color="7" fill="1" visible="yes" active="yes"/>
<layer number="106" name="BGA-Top" color="7" fill="1" visible="yes" active="yes"/>
<layer number="107" name="BD-Top" color="7" fill="1" visible="yes" active="yes"/>
<layer number="108" name="tBridges" color="7" fill="1" visible="yes" active="yes"/>
<layer number="109" name="tBPL" color="7" fill="1" visible="yes" active="yes"/>
<layer number="110" name="bBPL" color="7" fill="1" visible="yes" active="yes"/>
<layer number="111" name="MPL" color="7" fill="1" visible="yes" active="yes"/>
<layer number="112" name="tSilk" color="7" fill="1" visible="yes" active="yes"/>
<layer number="113" name="Laser Schnitt" color="12" fill="1" visible="no" active="no"/>
<layer number="114" name="Laser Fläche Gravur" color="15" fill="1" visible="no" active="no"/>
<layer number="115" name="Laser Bohrungen" color="9" fill="1" visible="no" active="no"/>
<layer number="116" name="Patch_BOT" color="7" fill="1" visible="yes" active="yes"/>
<layer number="118" name="Rect_Pads" color="7" fill="1" visible="no" active="no"/>
<layer number="119" name="_bPlace" color="7" fill="1" visible="yes" active="yes"/>
<layer number="120" name="Descript" color="7" fill="1" visible="yes" active="yes"/>
<layer number="121" name="sName" color="7" fill="1" visible="yes" active="yes"/>
<layer number="122" name="_bPlace" color="7" fill="1" visible="yes" active="yes"/>
<layer number="123" name="tTestmark" color="7" fill="1" visible="yes" active="yes"/>
<layer number="124" name="bTestmark" color="7" fill="1" visible="yes" active="yes"/>
<layer number="125" name="_tNames" color="7" fill="1" visible="yes" active="yes"/>
<layer number="126" name="_bNames" color="7" fill="1" visible="yes" active="yes"/>
<layer number="127" name="_tValues" color="7" fill="1" visible="yes" active="yes"/>
<layer number="128" name="_bValues" color="7" fill="1" visible="yes" active="yes"/>
<layer number="129" name="Mask" color="7" fill="1" visible="yes" active="yes"/>
<layer number="130" name="vermassung" color="7" fill="1" visible="yes" active="yes"/>
<layer number="131" name="tAdjust" color="7" fill="1" visible="yes" active="yes"/>
<layer number="132" name="bAdjust" color="7" fill="1" visible="yes" active="yes"/>
<layer number="133" name="Ritzung" color="1" fill="0" visible="no" active="no"/>
<layer number="134" name="Fräsung" color="2" fill="0" visible="no" active="no"/>
<layer number="140" name="land_pattern" color="6" fill="1" visible="yes" active="yes"/>
<layer number="141" name="freihand" color="7" fill="1" visible="yes" active="yes"/>
<layer number="142" name="BMRestrict" color="1" fill="9" visible="no" active="no"/>
<layer number="144" name="Drill_legend" color="7" fill="1" visible="yes" active="yes"/>
<layer number="147" name="deckel_neu" color="14" fill="1" visible="yes" active="yes"/>
<layer number="148" name="Document_mirrored" color="7" fill="1" visible="no" active="no"/>
<layer number="150" name="Notes" color="7" fill="1" visible="yes" active="yes"/>
<layer number="151" name="HeatSink" color="7" fill="1" visible="yes" active="yes"/>
<layer number="152" name="_bDocu" color="7" fill="1" visible="yes" active="yes"/>
<layer number="153" name="FabDoc1" color="7" fill="1" visible="yes" active="yes"/>
<layer number="154" name="FabDoc2" color="7" fill="1" visible="yes" active="yes"/>
<layer number="155" name="FabDoc3" color="7" fill="1" visible="yes" active="yes"/>
<layer number="156" name="gesam-Maß" color="1" fill="7" visible="no" active="no"/>
<layer number="157" name="FaceMchng" color="3" fill="1" visible="no" active="no"/>
<layer number="158" name="FaceMMeas" color="3" fill="1" visible="no" active="no"/>
<layer number="159" name="Geh-Bear2" color="1" fill="7" visible="no" active="no"/>
<layer number="160" name="Ritzen" color="10" fill="0" visible="yes" active="yes"/>
<layer number="161" name="Fräsen" color="11" fill="0" visible="yes" active="yes"/>
<layer number="170" name="ProgrammierAdapter" color="7" fill="1" visible="no" active="no"/>
<layer number="194" name="Schematicdocumentation" color="7" fill="1" visible="yes" active="yes"/>
<layer number="195" name="Netlinks" color="7" fill="1" visible="yes" active="yes"/>
<layer number="199" name="EXTD_ERC" color="7" fill="1" visible="yes" active="yes"/>
<layer number="200" name="200bmp" color="1" fill="10" visible="yes" active="yes"/>
<layer number="201" name="201bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="202" name="202bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="203" name="203bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="204" name="204bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="205" name="205bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="206" name="206bmp" color="7" fill="10" visible="yes" active="yes"/>
<layer number="207" name="207bmp" color="8" fill="10" visible="yes" active="yes"/>
<layer number="208" name="208bmp" color="9" fill="10" visible="yes" active="yes"/>
<layer number="209" name="209bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="210" name="210bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="211" name="211bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="212" name="212bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="213" name="213bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="214" name="214bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="215" name="215bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="216" name="216bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="217" name="217bmp" color="18" fill="1" visible="no" active="no"/>
<layer number="218" name="218bmp" color="19" fill="1" visible="no" active="no"/>
<layer number="219" name="219bmp" color="20" fill="1" visible="no" active="no"/>
<layer number="220" name="220bmp" color="21" fill="1" visible="no" active="no"/>
<layer number="221" name="221bmp" color="22" fill="1" visible="no" active="no"/>
<layer number="222" name="222bmp" color="23" fill="1" visible="no" active="no"/>
<layer number="223" name="223bmp" color="24" fill="1" visible="no" active="no"/>
<layer number="224" name="224bmp" color="25" fill="1" visible="no" active="no"/>
<layer number="225" name="225bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="226" name="226bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="227" name="227bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="228" name="228bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="229" name="229bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="230" name="230bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="231" name="231bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="232" name="Eagle3D_PG2" color="7" fill="1" visible="no" active="no"/>
<layer number="233" name="Eagle3D_PG3" color="7" fill="1" visible="no" active="no"/>
<layer number="248" name="Housing" color="7" fill="1" visible="yes" active="yes"/>
<layer number="249" name="Edge" color="7" fill="1" visible="yes" active="yes"/>
<layer number="250" name="Descript" color="7" fill="1" visible="yes" active="yes"/>
<layer number="251" name="SMDround" color="7" fill="1" visible="yes" active="yes"/>
<layer number="252" name="BR-BS" color="7" fill="1" visible="yes" active="yes"/>
<layer number="253" name="BR-LS" color="7" fill="1" visible="yes" active="yes"/>
<layer number="254" name="cooling" color="7" fill="1" visible="yes" active="yes"/>
<layer number="255" name="routoute" color="7" fill="1" visible="yes" active="yes"/>
</layers>
<board>
<plain>
<wire x1="0" y1="0" x2="50" y2="0" width="0" layer="20"/>
<wire x1="50" y1="0" x2="50" y2="100" width="0" layer="20"/>
<wire x1="50" y1="100" x2="0" y2="100" width="0" layer="20"/>
<wire x1="0" y1="100" x2="0" y2="0" width="0" layer="20"/>
<text x="48.037" y="63.1055" size="1.016" layer="26" font="vector" ratio="14" rot="MR0">osmo-clock-converter
(C) 2019 by
Harald Welte
Mfg: sysmocom GmbH
OSHW / CC-BY-SA</text>
<text x="30.449" y="63.1055" size="1.016" layer="25" font="vector" ratio="14">osmo-clock-converter
(C) 2019 by
Harald Welte
Mfg: sysmocom GmbH
OSHW / CC-BY-SA</text>
<text x="37.857" y="61.0855" size="1.016" layer="25" font="vector" ratio="14">&gt;REVISION</text>
<text x="30.462" y="61.0855" size="1.016" layer="25" font="vector" ratio="14">Version:</text>
</plain>
<libraries>
<library name="rc-sysmocom">
<packages>
<package name="_0603">
<description>&lt;b&gt;0603&lt;/b&gt;</description>
<wire x1="-0.432" y1="-0.306" x2="0.432" y2="-0.306" width="0.1016" layer="51"/>
<wire x1="0.432" y1="0.306" x2="-0.432" y2="0.306" width="0.1016" layer="51"/>
<wire x1="-1.4605" y1="0.635" x2="1.4605" y2="0.635" width="0.2032" layer="21"/>
<wire x1="1.4605" y1="0.635" x2="1.4605" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="1.4605" y1="-0.635" x2="-1.4605" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-1.4605" y1="-0.635" x2="-1.4605" y2="0.635" width="0.2032" layer="21"/>
<smd name="1" x="-0.762" y="0" dx="0.9" dy="0.8" layer="1" roundness="30" cream="no"/>
<smd name="2" x="0.762" y="0" dx="0.9" dy="0.8" layer="1" roundness="30" cream="no"/>
<text x="-1.5875" y="0.9525" size="1.016" layer="25" font="vector" ratio="14">&gt;NAME</text>
<text x="-1.5875" y="-1.4923" size="0.508" layer="27" font="vector" ratio="10">&gt;VALUE</text>
<rectangle x1="0.4318" y1="-0.4" x2="0.8382" y2="0.4" layer="51"/>
<rectangle x1="-0.8382" y1="-0.4" x2="-0.4318" y2="0.4" layer="51"/>
<rectangle x1="-0.1999" y1="-0.4001" x2="0.1999" y2="0.4001" layer="35"/>
<polygon width="0.127" layer="31">
<vertex x="0.635" y="0.3175"/>
<vertex x="1.11125" y="0.3175"/>
<vertex x="1.11125" y="-0.3175"/>
<vertex x="0.635" y="-0.3175"/>
<vertex x="0.396875" y="0"/>
</polygon>
<polygon width="0.127" layer="31">
<vertex x="-1.11125" y="0.3175"/>
<vertex x="-0.635" y="0.3175"/>
<vertex x="-0.396875" y="0"/>
<vertex x="-0.635" y="-0.3175"/>
<vertex x="-1.11125" y="-0.3175"/>
</polygon>
</package>
<package name="_0805">
<description>&lt;b&gt;0805&lt;/b&gt;</description>
<wire x1="-0.41" y1="0.585" x2="0.41" y2="0.585" width="0.1016" layer="51"/>
<wire x1="-0.41" y1="-0.585" x2="0.41" y2="-0.585" width="0.1016" layer="51"/>
<wire x1="-1.905" y1="0.889" x2="1.905" y2="0.889" width="0.2032" layer="21"/>
<wire x1="1.905" y1="0.889" x2="1.905" y2="-0.889" width="0.2032" layer="21"/>
<wire x1="1.905" y1="-0.889" x2="-1.905" y2="-0.889" width="0.2032" layer="21"/>
<wire x1="-1.905" y1="-0.889" x2="-1.905" y2="0.889" width="0.2032" layer="21"/>
<smd name="1" x="-1.016" y="0" dx="1.2" dy="1.3" layer="1" roundness="30" cream="no"/>
<smd name="2" x="1.016" y="0" dx="1.2" dy="1.3" layer="1" roundness="30" cream="no"/>
<text x="-1.905" y="1.27" size="1.016" layer="25" font="vector" ratio="14">&gt;NAME</text>
<text x="-1.9049" y="-1.651" size="0.508" layer="27" font="vector" ratio="10">&gt;VALUE</text>
<rectangle x1="0.4064" y1="-0.65" x2="1.0564" y2="0.65" layer="51"/>
<rectangle x1="-1.0668" y1="-0.65" x2="-0.4168" y2="0.65" layer="51"/>
<rectangle x1="-0.1999" y1="-0.5001" x2="0.1999" y2="0.5001" layer="35"/>
<polygon width="0.127" layer="31">
<vertex x="-1.508125" y="0.555625"/>
<vertex x="-0.873125" y="0.555625"/>
<vertex x="-0.47625" y="0"/>
<vertex x="-0.873125" y="-0.555625"/>
<vertex x="-1.508125" y="-0.555625"/>
</polygon>
<polygon width="0.127" layer="31">
<vertex x="0.47625" y="0"/>
<vertex x="0.873125" y="0.555625"/>
<vertex x="1.508125" y="0.555625"/>
<vertex x="1.508125" y="-0.555625"/>
<vertex x="0.873125" y="-0.555625"/>
</polygon>
</package>
</packages>
</library>
<library name="laforge">
<description>&lt;b&gt;PCB Matrix Packages&lt;/b&gt;&lt;p&gt;</description>
<packages>
<package name="0603">
<wire x1="-0.356" y1="0.432" x2="0.356" y2="0.432" width="0.1016" layer="51"/>
<wire x1="-0.356" y1="-0.419" x2="0.356" y2="-0.419" width="0.1016" layer="51"/>
<smd name="1" x="-0.85" y="0" dx="1.1" dy="1" layer="1"/>
<smd name="2" x="0.85" y="0" dx="1.1" dy="1" layer="1"/>
<text x="-0.635" y="0.635" size="1.27" layer="25">&gt;NAME</text>
<text x="-0.635" y="-1.905" size="1.27" layer="27">&gt;VALUE</text>
<rectangle x1="-0.8382" y1="-0.4699" x2="-0.3381" y2="0.4801" layer="51"/>
<rectangle x1="0.3302" y1="-0.4699" x2="0.8303" y2="0.4801" layer="51"/>
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<wire x1="-1.905" y1="1.27" x2="-0.635" y2="1.27" width="0.1524" layer="21"/>
<wire x1="-0.635" y1="1.27" x2="0" y2="0.635" width="0.1524" layer="21"/>
<wire x1="0" y1="0.635" x2="0" y2="-0.635" width="0.1524" layer="21"/>
<wire x1="0" y1="-0.635" x2="-0.635" y2="-1.27" width="0.1524" layer="21"/>
<wire x1="-2.54" y1="0.635" x2="-2.54" y2="-0.635" width="0.1524" layer="21"/>
<wire x1="-1.905" y1="1.27" x2="-2.54" y2="0.635" width="0.1524" layer="21"/>
<wire x1="-2.54" y1="-0.635" x2="-1.905" y2="-1.27" width="0.1524" layer="21"/>
<wire x1="-0.635" y1="-1.27" x2="-1.905" y2="-1.27" width="0.1524" layer="21"/>
<wire x1="0" y1="0.635" x2="0.635" y2="1.27" width="0.1524" layer="21"/>
<wire x1="0.635" y1="1.27" x2="1.905" y2="1.27" width="0.1524" layer="21"/>
<wire x1="1.905" y1="1.27" x2="2.54" y2="0.635" width="0.1524" layer="21"/>
<wire x1="2.54" y1="0.635" x2="2.54" y2="-0.635" width="0.1524" layer="21"/>
<wire x1="2.54" y1="-0.635" x2="1.905" y2="-1.27" width="0.1524" layer="21"/>
<wire x1="1.905" y1="-1.27" x2="0.635" y2="-1.27" width="0.1524" layer="21"/>
<wire x1="0.635" y1="-1.27" x2="0" y2="-0.635" width="0.1524" layer="21"/>
<pad name="1" x="-1.27" y="0" drill="1.016" shape="square" rot="R90"/>
<pad name="2" x="1.27" y="0" drill="1.016" shape="long" rot="R90"/>
<text x="-2.6162" y="1.8288" size="1.27" layer="25" ratio="10">&gt;NAME</text>
<text x="-2.54" y="-3.175" size="1.27" layer="27">&gt;VALUE</text>
<rectangle x1="-1.524" y1="-0.254" x2="-1.016" y2="0.254" layer="51"/>
<rectangle x1="1.016" y1="-0.254" x2="1.524" y2="0.254" layer="51"/>
</package>
<package name="HRS_UFL">
<description>&lt;b&gt;Hirose U.FL SMT&lt;/b&gt;</description>
<smd name="SIG" x="0" y="-1.5025" dx="1" dy="1.05" layer="1"/>
<smd name="GND@2" x="1.4525" y="0" dx="1.05" dy="2.2" layer="1"/>
<smd name="GND@1" x="-1.4525" y="0" dx="1.05" dy="2.2" layer="1"/>
<circle x="0" y="0" radius="1" width="0.127" layer="51"/>
<circle x="0" y="0" radius="0.1" width="0.2" layer="51"/>
<wire x1="-1.3" y1="1.3" x2="1.3" y2="1.3" width="0.127" layer="51"/>
<wire x1="1.3" y1="1.3" x2="1.3" y2="-1.3" width="0.127" layer="51"/>
<wire x1="1.3" y1="-1.3" x2="-1.3" y2="-1.3" width="0.127" layer="51"/>
<wire x1="-1.3" y1="-1.3" x2="-1.3" y2="1.3" width="0.127" layer="51"/>
<rectangle x1="-1.6" y1="-1" x2="-1.3" y2="1" layer="51"/>
<rectangle x1="1.3" y1="-1" x2="1.6" y2="1" layer="51"/>
<rectangle x1="-0.4" y1="-1.6" x2="0.4" y2="-1.3" layer="51"/>
<wire x1="-1.5" y1="1.3" x2="-1.5" y2="1.5" width="0.127" layer="21"/>
<wire x1="-1.5" y1="1.5" x2="1.5" y2="1.5" width="0.127" layer="21"/>
<wire x1="1.5" y1="1.5" x2="1.5" y2="1.3" width="0.127" layer="21"/>
<wire x1="-1.5" y1="-1.3" x2="-1.5" y2="-1.5" width="0.127" layer="21"/>
<wire x1="-1.5" y1="-1.5" x2="-0.8" y2="-1.5" width="0.127" layer="21"/>
<wire x1="0.8" y1="-1.5" x2="1.5" y2="-1.5" width="0.127" layer="21"/>
<wire x1="1.5" y1="-1.5" x2="1.5" y2="-1.3" width="0.127" layer="21"/>
<text x="-3" y="0" size="1.27" layer="25" rot="R90" align="center">&gt;NAME</text>
<text x="3" y="0" size="1.27" layer="27" rot="R90" align="center">&gt;VALUE</text>
</package>
<package name="SMA-F-S-TH">
<wire x1="-3.81" y1="1.5875" x2="-3.81" y2="-1.27" width="0.1524" layer="21"/>
<wire x1="-1.5875" y1="3.81" x2="1.5875" y2="3.81" width="0.1524" layer="21"/>
<wire x1="3.81" y1="1.5875" x2="3.81" y2="-1.5875" width="0.1524" layer="21"/>
<wire x1="-1.5875" y1="-3.81" x2="1.5875" y2="-3.81" width="0.1524" layer="21"/>
<wire x1="-3.81" y1="3.81" x2="-3.81" y2="3.4925" width="0.1524" layer="21"/>
<wire x1="-3.4925" y1="3.81" x2="-3.81" y2="3.81" width="0.1524" layer="21"/>
<wire x1="3.4925" y1="3.81" x2="3.81" y2="3.81" width="0.1524" layer="21"/>
<wire x1="3.81" y1="3.81" x2="3.81" y2="3.4925" width="0.1524" layer="21"/>
<wire x1="3.81" y1="-3.4925" x2="3.81" y2="-3.81" width="0.1524" layer="21"/>
<wire x1="3.81" y1="-3.81" x2="3.4925" y2="-3.81" width="0.1524" layer="21"/>
<wire x1="-3.81" y1="-3.4925" x2="-3.81" y2="-3.81" width="0.1524" layer="21"/>
<wire x1="-3.81" y1="-3.81" x2="-3.4925" y2="-3.81" width="0.1524" layer="21"/>
<wire x1="-3.81" y1="3.4925" x2="-3.81" y2="1.5875" width="0.1524" layer="51"/>
<wire x1="-3.4925" y1="3.81" x2="-1.5875" y2="3.81" width="0.1524" layer="51"/>
<wire x1="1.5875" y1="3.81" x2="3.4925" y2="3.81" width="0.1524" layer="51"/>
<wire x1="3.81" y1="3.4925" x2="3.81" y2="1.5875" width="0.1524" layer="51"/>
<wire x1="3.81" y1="-1.5875" x2="3.81" y2="-3.4925" width="0.1524" layer="51"/>
<wire x1="3.4925" y1="-3.81" x2="1.5875" y2="-3.81" width="0.1524" layer="51"/>
<wire x1="-1.5875" y1="-3.81" x2="-3.4925" y2="-3.81" width="0.1524" layer="51"/>
<wire x1="-3.81" y1="-3.4925" x2="-3.81" y2="-1.27" width="0.1524" layer="51"/>
<pad name="C" x="0" y="0" drill="1.524"/>
<pad name="G1" x="-2.54" y="2.54" drill="1.651"/>
<pad name="G2" x="2.54" y="2.54" drill="1.651"/>
<pad name="G4" x="2.54" y="-2.54" drill="1.651"/>
<pad name="G3" x="-2.54" y="-2.54" drill="1.651"/>
<text x="-3.81" y="4.1275" size="1.27" layer="25" font="vector" ratio="10">&gt;NAME</text>
<text x="-3.81" y="-5.3975" size="1.27" layer="27" font="vector" ratio="10">&gt;VALUE</text>
</package>
</packages>
</library>
<library name="diodes-sysmocom">
<packages>
<package name="SMADIODE">
<description>&lt;b&gt;SMA Surface Mount Diode&lt;/b&gt;</description>
<wire x1="-2.15" y1="1.3" x2="2.15" y2="1.3" width="0.2032" layer="51"/>
<wire x1="2.15" y1="1.3" x2="2.15" y2="-1.3" width="0.2032" layer="51"/>
<wire x1="2.15" y1="-1.3" x2="-2.15" y2="-1.3" width="0.2032" layer="51"/>
<wire x1="-2.15" y1="-1.3" x2="-2.15" y2="1.3" width="0.2032" layer="51"/>
<wire x1="-3.63025" y1="-1.394" x2="-3.63025" y2="-1.146" width="0.127" layer="21"/>
<wire x1="-3.63025" y1="-1.146" x2="-3.63025" y2="1.6" width="0.2032" layer="21"/>
<wire x1="-3.63025" y1="1.6" x2="3.65725" y2="1.6" width="0.2032" layer="21"/>
<wire x1="3.65725" y1="1.6" x2="3.65725" y2="-1.6" width="0.2032" layer="21"/>
<wire x1="3.65725" y1="-1.6" x2="-3.63025" y2="-1.6" width="0.2032" layer="21"/>
<wire x1="-3.63025" y1="-1.6" x2="-3.63025" y2="-1.146" width="0.2032" layer="21"/>
<wire x1="0.254" y1="0.762" x2="0.254" y2="-0.762" width="0.2032" layer="21"/>
<wire x1="0.254" y1="-0.762" x2="-0.508" y2="0" width="0.2032" layer="21"/>
<wire x1="-0.508" y1="0" x2="0.254" y2="0.762" width="0.2032" layer="21"/>
<wire x1="-0.508" y1="0.762" x2="-0.508" y2="0" width="0.2032" layer="21"/>
<wire x1="-0.508" y1="0" x2="-0.508" y2="-0.762" width="0.2032" layer="21"/>
<text x="-2.54" y="1.905" size="1.016" layer="25" font="vector" ratio="17">&gt;NAME</text>
<text x="-2.54" y="-2.286" size="0.4064" layer="27" font="vector" ratio="10">&gt;VALUE</text>
<rectangle x1="-2.825" y1="-0.75" x2="-2.175" y2="0.75" layer="51"/>
<rectangle x1="2.175" y1="-0.75" x2="2.825" y2="0.75" layer="51"/>
<rectangle x1="-1.75" y1="-1.225" x2="-1.075" y2="1.225" layer="51"/>
<smd name="C" x="-2.2225" y="0" dx="2" dy="2" layer="1" roundness="30" cream="no"/>
<smd name="A" x="2.2225" y="0" dx="2" dy="2" layer="1" roundness="30" cream="no"/>
<polygon width="0.3048" layer="31">
<vertex x="-3.01625" y="0.79375"/>
<vertex x="-3.01625" y="-0.79375"/>
<vertex x="-1.905" y="-0.79375"/>
<vertex x="-1.42875" y="0"/>
<vertex x="-1.905" y="0.79375"/>
</polygon>
<polygon width="0.3048" layer="31">
<vertex x="3.01625" y="0.79375"/>
<vertex x="1.905" y="0.79375"/>
<vertex x="1.42875" y="0"/>
<vertex x="1.905" y="-0.79375"/>
<vertex x="3.01625" y="-0.79375"/>
</polygon>
</package>
</packages>
</library>
<library name="littlefuse">
<packages>
<package name="1206L">
<description>From Littelfuse POLY-FUSE 1206L data sheet</description>
<smd name="1" x="-1.4" y="0" dx="1" dy="1.8" layer="1" roundness="30"/>
<smd name="2" x="1.4" y="0" dx="1" dy="1.8" layer="1" roundness="30"/>
<wire x1="-1.6" y1="0.85" x2="1.6" y2="0.85" width="0.127" layer="51"/>
<wire x1="1.6" y1="0.85" x2="1.6" y2="0.2" width="0.127" layer="51"/>
<wire x1="1.6" y1="-0.2" x2="1.6" y2="-0.85" width="0.127" layer="51"/>
<wire x1="1.6" y1="-0.85" x2="-1.6" y2="-0.85" width="0.127" layer="51"/>
<wire x1="-1.6" y1="-0.85" x2="-1.6" y2="-0.2" width="0.127" layer="51"/>
<wire x1="-1.6" y1="0.2" x2="-1.6" y2="0.85" width="0.127" layer="51"/>
<wire x1="-1.6" y1="0.2" x2="-1.6" y2="-0.2" width="0.127" layer="51" curve="-180"/>
<wire x1="1.6" y1="-0.2" x2="1.6" y2="0.2" width="0.127" layer="51" curve="-180"/>
<text x="-1.5" y="1" size="0.8128" layer="25" font="vector">&gt;NAME</text>
<text x="1.6" y="-1" size="0.8128" layer="27" font="vector" rot="R180">&gt;VALUE</text>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="JP2">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
<wire x1="-3.81" y1="-1.016" x2="-3.81" y2="1.016" width="0.1524" layer="21"/>
<wire x1="3.556" y1="1.27" x2="1.524" y2="1.27" width="0.1524" layer="21"/>
<wire x1="1.27" y1="1.016" x2="1.524" y2="1.27" width="0.1524" layer="21"/>
<wire x1="3.556" y1="-1.27" x2="1.524" y2="-1.27" width="0.1524" layer="21"/>
<wire x1="1.27" y1="-1.016" x2="1.524" y2="-1.27" width="0.1524" layer="21"/>
<wire x1="3.556" y1="-1.27" x2="3.81" y2="-1.016" width="0.1524" layer="21"/>
<wire x1="3.556" y1="1.27" x2="3.81" y2="1.016" width="0.1524" layer="21"/>
<wire x1="3.81" y1="1.016" x2="3.81" y2="-1.016" width="0.1524" layer="21"/>
<wire x1="1.016" y1="1.27" x2="1.27" y2="1.016" width="0.1524" layer="21"/>
<wire x1="1.016" y1="1.27" x2="-1.016" y2="1.27" width="0.1524" layer="21"/>
<wire x1="-1.27" y1="1.016" x2="-1.016" y2="1.27" width="0.1524" layer="21"/>
<wire x1="-1.524" y1="1.27" x2="-1.27" y2="1.016" width="0.1524" layer="21"/>
<wire x1="-3.81" y1="1.016" x2="-3.556" y2="1.27" width="0.1524" layer="21"/>
<wire x1="-1.524" y1="1.27" x2="-3.556" y2="1.27" width="0.1524" layer="21"/>
<wire x1="1.016" y1="-1.27" x2="1.27" y2="-1.016" width="0.1524" layer="21"/>
<wire x1="-1.27" y1="-1.016" x2="-1.016" y2="-1.27" width="0.1524" layer="21"/>
<wire x1="-1.524" y1="-1.27" x2="-1.27" y2="-1.016" width="0.1524" layer="21"/>
<wire x1="-3.81" y1="-1.016" x2="-3.556" y2="-1.27" width="0.1524" layer="21"/>
<wire x1="1.016" y1="-1.27" x2="-1.016" y2="-1.27" width="0.1524" layer="21"/>
<wire x1="-1.524" y1="-1.27" x2="-3.556" y2="-1.27" width="0.1524" layer="21"/>
<pad name="1" x="-2.54" y="0" drill="0.9144" shape="long" rot="R90"/>
<pad name="2" x="0" y="0" drill="0.9144" shape="long" rot="R90"/>
<pad name="3" x="2.54" y="0" drill="0.9144" shape="long" rot="R90"/>
<text x="-3.556" y="1.651" size="1.27" layer="25" ratio="10">&gt;NAME</text>
<text x="-2.54" y="-2.667" size="0.9906" layer="21" ratio="12">1</text>
<text x="0" y="-2.667" size="0.9906" layer="21" ratio="12">2</text>
<text x="2.54" y="-2.667" size="0.9906" layer="21" ratio="12">3</text>
<text x="-3.556" y="-4.318" size="1.27" layer="27" ratio="10">&gt;VALUE</text>
<rectangle x1="-2.8448" y1="-0.3048" x2="-2.2352" y2="0.3048" layer="51"/>
<rectangle x1="-0.3048" y1="-0.3048" x2="0.3048" y2="0.3048" layer="51"/>
<rectangle x1="2.2352" y1="-0.3048" x2="2.8448" y2="0.3048" layer="51"/>
</package>
<package name="JP1">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
<wire x1="-1.016" y1="0" x2="-1.27" y2="0.254" width="0.1524" layer="21"/>
<wire x1="-1.016" y1="0" x2="-1.27" y2="-0.254" width="0.1524" layer="21"/>
<wire x1="1.016" y1="0" x2="1.27" y2="0.254" width="0.1524" layer="21"/>
<wire x1="1.016" y1="0" x2="1.27" y2="-0.254" width="0.1524" layer="21"/>
<wire x1="1.27" y1="-0.254" x2="1.27" y2="-2.286" width="0.1524" layer="21"/>
<wire x1="1.016" y1="-2.54" x2="1.27" y2="-2.286" width="0.1524" layer="21"/>
<wire x1="1.27" y1="2.286" x2="1.016" y2="2.54" width="0.1524" layer="21"/>
<wire x1="1.27" y1="2.286" x2="1.27" y2="0.254" width="0.1524" layer="21"/>
<wire x1="1.016" y1="2.54" x2="-1.016" y2="2.54" width="0.1524" layer="21"/>
<wire x1="-1.27" y1="2.286" x2="-1.016" y2="2.54" width="0.1524" layer="21"/>
<wire x1="-1.27" y1="2.286" x2="-1.27" y2="0.254" width="0.1524" layer="21"/>
<wire x1="-1.27" y1="-0.254" x2="-1.27" y2="-2.286" width="0.1524" layer="21"/>
<wire x1="-1.016" y1="-2.54" x2="-1.27" y2="-2.286" width="0.1524" layer="21"/>
<wire x1="-1.016" y1="-2.54" x2="1.016" y2="-2.54" width="0.1524" layer="21"/>
<pad name="1" x="0" y="-1.27" drill="0.9144" shape="long"/>
<pad name="2" x="0" y="1.27" drill="0.9144" shape="long"/>
<text x="-1.651" y="-2.54" size="1.27" layer="25" ratio="10" rot="R90">&gt;NAME</text>
<text x="2.921" y="-2.54" size="1.27" layer="27" ratio="10" rot="R90">&gt;VALUE</text>
<rectangle x1="-0.3048" y1="0.9652" x2="0.3048" y2="1.5748" layer="51"/>
<rectangle x1="-0.3048" y1="-1.5748" x2="0.3048" y2="-0.9652" layer="51"/>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<wire x1="0" y1="0.635" x2="0.635" y2="1.27" width="0.1524" layer="21"/>
<wire x1="0.635" y1="1.27" x2="1.905" y2="1.27" width="0.1524" layer="21"/>
<wire x1="1.905" y1="1.27" x2="2.54" y2="0.635" width="0.1524" layer="21"/>
<wire x1="2.54" y1="0.635" x2="2.54" y2="-0.635" width="0.1524" layer="21"/>
<wire x1="2.54" y1="-0.635" x2="1.905" y2="-1.27" width="0.1524" layer="21"/>
<wire x1="1.905" y1="-1.27" x2="0.635" y2="-1.27" width="0.1524" layer="21"/>
<wire x1="0.635" y1="-1.27" x2="0" y2="-0.635" width="0.1524" layer="21"/>
<wire x1="-4.445" y1="1.27" x2="-3.175" y2="1.27" width="0.1524" layer="21"/>
<wire x1="-3.175" y1="1.27" x2="-2.54" y2="0.635" width="0.1524" layer="21"/>
<wire x1="-2.54" y1="0.635" x2="-2.54" y2="-0.635" width="0.1524" layer="21"/>
<wire x1="-2.54" y1="-0.635" x2="-3.175" y2="-1.27" width="0.1524" layer="21"/>
<wire x1="-2.54" y1="0.635" x2="-1.905" y2="1.27" width="0.1524" layer="21"/>
<wire x1="-1.905" y1="1.27" x2="-0.635" y2="1.27" width="0.1524" layer="21"/>
<wire x1="-0.635" y1="1.27" x2="0" y2="0.635" width="0.1524" layer="21"/>
<wire x1="0" y1="0.635" x2="0" y2="-0.635" width="0.1524" layer="21"/>
<wire x1="0" y1="-0.635" x2="-0.635" y2="-1.27" width="0.1524" layer="21"/>
<wire x1="-0.635" y1="-1.27" x2="-1.905" y2="-1.27" width="0.1524" layer="21"/>
<wire x1="-1.905" y1="-1.27" x2="-2.54" y2="-0.635" width="0.1524" layer="21"/>
<wire x1="-5.08" y1="0.635" x2="-5.08" y2="-0.635" width="0.1524" layer="21"/>
<wire x1="-4.445" y1="1.27" x2="-5.08" y2="0.635" width="0.1524" layer="21"/>
<wire x1="-5.08" y1="-0.635" x2="-4.445" y2="-1.27" width="0.1524" layer="21"/>
<wire x1="-3.175" y1="-1.27" x2="-4.445" y2="-1.27" width="0.1524" layer="21"/>
<wire x1="3.175" y1="1.27" x2="4.445" y2="1.27" width="0.1524" layer="21"/>
<wire x1="4.445" y1="1.27" x2="5.08" y2="0.635" width="0.1524" layer="21"/>
<wire x1="5.08" y1="0.635" x2="5.08" y2="-0.635" width="0.1524" layer="21"/>
<wire x1="5.08" y1="-0.635" x2="4.445" y2="-1.27" width="0.1524" layer="21"/>
<wire x1="3.175" y1="1.27" x2="2.54" y2="0.635" width="0.1524" layer="21"/>
<wire x1="2.54" y1="-0.635" x2="3.175" y2="-1.27" width="0.1524" layer="21"/>
<wire x1="4.445" y1="-1.27" x2="3.175" y2="-1.27" width="0.1524" layer="21"/>
<pad name="1" x="-3.81" y="0" drill="1.016" shape="long" rot="R90"/>
<pad name="2" x="-1.27" y="0" drill="1.016" shape="long" rot="R90"/>
<pad name="3" x="1.27" y="0" drill="1.016" shape="long" rot="R90"/>
<pad name="4" x="3.81" y="0" drill="1.016" shape="long" rot="R90"/>
<text x="-5.1562" y="1.8288" size="1.27" layer="25" ratio="10">&gt;NAME</text>
<text x="-5.08" y="-3.175" size="1.27" layer="27">&gt;VALUE</text>
<rectangle x1="1.016" y1="-0.254" x2="1.524" y2="0.254" layer="51"/>
<rectangle x1="-1.524" y1="-0.254" x2="-1.016" y2="0.254" layer="51"/>
<rectangle x1="-4.064" y1="-0.254" x2="-3.556" y2="0.254" layer="51"/>
<rectangle x1="3.556" y1="-0.254" x2="4.064" y2="0.254" layer="51"/>
</package>
</packages>
</library>
<library name="Wurth_Elektronik_Electromechanic_DC_Power_Jack_Connectors_rev15c">
<description>&lt;BR&gt;Wurth Elektronik - DC Power Jack Connectors&lt;br&gt;&lt;Hr&gt;
&lt;BR&gt;&lt;BR&gt; 
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-405&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/eagle"&gt;http://www.we-online.com/eagle &lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither CadSoft nor WE-eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;&lt;BR&gt;&lt;br&gt;
&lt;hr&gt;
Eagle Version 6, Library Revision 2015c, 2015-06-02&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="694108106102">
<description>&lt;b&gt;694108106102&lt;/b&gt;&lt;p&gt;

WR-DC_DC Power Jack_Right Angled_SMT Center Pin Ø2.5_Plug ID Ø2.55_Plug OD Ø5.5_with 4 Soldering Pad &amp; Peg</description>
<wire x1="0.199859375" y1="4.50001875" x2="0.0000125" y2="4.299821875" width="0.2" layer="21" curve="97.0981"/>
<wire x1="-0.000009375" y1="-4.30015" x2="0.2001875" y2="-4.499996875" width="0.2" layer="21" curve="97.0981"/>
<wire x1="0" y1="-4.31" x2="0" y2="4.31" width="0.2" layer="21"/>
<wire x1="14.7" y1="-4.5" x2="14.7" y2="4.5" width="0.2" layer="21"/>
<smd name="1" x="11.15" y="5.5" dx="2.4" dy="2" layer="1" roundness="30"/>
<smd name="1-1" x="5" y="5.5" dx="2.4" dy="2" layer="1" roundness="30"/>
<smd name="2" x="5" y="-5.5" dx="2.4" dy="2" layer="1" roundness="30"/>
<smd name="3" x="11.15" y="-5.5" dx="2.4" dy="2" layer="1" roundness="30"/>
<text x="0.299640625" y="8.4306" size="2.032" layer="25" font="vector" ratio="13" rot="SR0">&gt;NAME</text>
<text x="0.699640625" y="-10.1134" size="2.032" layer="27" font="vector" ratio="13" rot="SR0">&gt;VALUE</text>
<hole x="5" y="0" drill="1.6"/>
<hole x="9.5" y="0" drill="1.8"/>
<wire x1="-0.25" y1="6.75" x2="14.95" y2="6.75" width="0.2" layer="39"/>
<wire x1="-0.25" y1="-6.75" x2="14.95" y2="-6.75" width="0.2" layer="39"/>
<wire x1="0.19" y1="4.5" x2="4" y2="4.5" width="0.2" layer="21"/>
<wire x1="4" y1="4.5" x2="6" y2="4.5" width="0.2" layer="51"/>
<wire x1="6" y1="4.5" x2="10.15" y2="4.5" width="0.2" layer="21"/>
<wire x1="10.15" y1="4.5" x2="12.15" y2="4.5" width="0.2" layer="51"/>
<wire x1="12.15" y1="4.5" x2="14.7" y2="4.5" width="0.2" layer="21"/>
<wire x1="0.19" y1="-4.5" x2="4" y2="-4.5" width="0.2" layer="21"/>
<wire x1="4" y1="-4.5" x2="6" y2="-4.5" width="0.2" layer="51"/>
<wire x1="6" y1="-4.5" x2="10.15" y2="-4.5" width="0.2" layer="21"/>
<wire x1="10.15" y1="-4.5" x2="12.15" y2="-4.5" width="0.2" layer="51"/>
<wire x1="12.15" y1="-4.5" x2="14.7" y2="-4.5" width="0.2" layer="21"/>
<wire x1="-0.25" y1="6.75" x2="-0.25" y2="-6.75" width="0.2" layer="39"/>
<wire x1="14.95" y1="6.75" x2="14.95" y2="-6.75" width="0.2" layer="39"/>
<text x="-1.01" y="-2.94" size="0.8128" layer="51" rot="R90">PCB Edge</text>
</package>
</packages>
</library>
<library name="cdclvc-clockbuf">
<packages>
<package name="MSOP12">
<description>12MSOP package according to LTC6957-3 data sheet (LTC DWG# 05-08-1668 Rvv A)</description>
<wire x1="-2.02" y1="1.5" x2="2.02" y2="1.5" width="0.127" layer="21"/>
<wire x1="2.02" y1="1.5" x2="2.02" y2="-1.5" width="0.127" layer="21"/>
<wire x1="2.02" y1="-1.5" x2="-2.02" y2="-1.5" width="0.127" layer="21"/>
<wire x1="-2.02" y1="-1.5" x2="-2.02" y2="1.5" width="0.127" layer="21"/>
<smd name="1" x="-1.625" y="-2.105" dx="0.42" dy="0.889" layer="1"/>
<smd name="2" x="-0.975" y="-2.105" dx="0.42" dy="0.889" layer="1"/>
<smd name="3" x="-0.325" y="-2.105" dx="0.42" dy="0.889" layer="1"/>
<smd name="4" x="0.325" y="-2.105" dx="0.42" dy="0.889" layer="1"/>
<smd name="5" x="0.975" y="-2.105" dx="0.42" dy="0.889" layer="1"/>
<smd name="6" x="1.625" y="-2.105" dx="0.42" dy="0.889" layer="1"/>
<smd name="7" x="1.625" y="2.105" dx="0.42" dy="0.889" layer="1" rot="R180"/>
<smd name="8" x="0.975" y="2.105" dx="0.42" dy="0.889" layer="1" rot="R180"/>
<smd name="9" x="0.325" y="2.105" dx="0.42" dy="0.889" layer="1" rot="R180"/>
<smd name="10" x="-0.325" y="2.105" dx="0.42" dy="0.889" layer="1" rot="R180"/>
<smd name="11" x="-0.975" y="2.105" dx="0.42" dy="0.889" layer="1" rot="R180"/>
<smd name="12" x="-1.625" y="2.105" dx="0.42" dy="0.889" layer="1" rot="R180"/>
<circle x="-1.625" y="-0.975" radius="0.1" width="0.127" layer="21"/>
<text x="-2.275" y="-1.3" size="1.27" layer="21" font="vector" ratio="14" rot="R90">&gt;NAME</text>
</package>
</packages>
</library>
<library name="ldo">
<description>&lt;b&gt;PCB Matrix Packages&lt;/b&gt;&lt;p&gt;</description>
<packages>
<package name="SOT23L">
<wire x1="1.422" y1="0.81" x2="1.422" y2="-0.81" width="0.1524" layer="21"/>
<wire x1="1.422" y1="-0.81" x2="-1.422" y2="-0.81" width="0.1524" layer="51"/>
<wire x1="-1.422" y1="-0.81" x2="-1.422" y2="0.81" width="0.1524" layer="21"/>
<wire x1="-1.422" y1="0.81" x2="1.422" y2="0.81" width="0.1524" layer="51"/>
<wire x1="-0.522" y1="0.81" x2="0.522" y2="0.81" width="0.1524" layer="21"/>
<wire x1="-0.428" y1="-0.81" x2="-0.522" y2="-0.81" width="0.1524" layer="21"/>
<wire x1="0.522" y1="-0.81" x2="0.428" y2="-0.81" width="0.1524" layer="21"/>
<wire x1="-1.328" y1="-0.81" x2="-1.422" y2="-0.81" width="0.1524" layer="21"/>
<wire x1="1.422" y1="-0.81" x2="1.328" y2="-0.81" width="0.1524" layer="21"/>
<wire x1="1.328" y1="0.81" x2="1.422" y2="0.81" width="0.1524" layer="21"/>
<wire x1="-1.422" y1="0.81" x2="-1.328" y2="0.81" width="0.1524" layer="21"/>
<smd name="1" x="-0.95" y="-1.3" dx="0.55" dy="1.2" layer="1" roundness="30"/>
<smd name="2" x="0" y="-1.3" dx="0.55" dy="1.2" layer="1" roundness="30"/>
<smd name="3" x="0.95" y="-1.3" dx="0.55" dy="1.2" layer="1" roundness="30"/>
<smd name="4" x="0.95" y="1.3" dx="0.55" dy="1.2" layer="1" roundness="30"/>
<smd name="5" x="-0.95" y="1.3" dx="0.55" dy="1.2" layer="1" roundness="30"/>
<text x="-1.905" y="-1.905" size="1.27" layer="25" ratio="17" rot="R90">&gt;NAME</text>
<text x="3.429" y="-1.905" size="1.27" layer="27" ratio="17" rot="R90">&gt;VALUE</text>
<rectangle x1="-1.2" y1="-1.5" x2="-0.7" y2="-0.85" layer="51"/>
<rectangle x1="-0.25" y1="-1.5" x2="0.25" y2="-0.85" layer="51"/>
<rectangle x1="0.7" y1="-1.5" x2="1.2" y2="-0.85" layer="51"/>
<rectangle x1="0.7" y1="0.85" x2="1.2" y2="1.5" layer="51"/>
<rectangle x1="-1.2" y1="0.85" x2="-0.7" y2="1.5" layer="51"/>
</package>
</packages>
</library>
<library name="LED-PLCC2">
<packages>
<package name="PLCC2-MIN">
<smd name="A" x="-1.524" y="0" dx="1.5" dy="2.3" layer="1" roundness="50" cream="no"/>
<smd name="K" x="1.524" y="0" dx="1.5" dy="2.3" layer="1" roundness="50" cream="no"/>
<wire x1="0.3175" y1="0" x2="-0.34925" y2="0.53975" width="0.1" layer="51"/>
<wire x1="-0.34925" y1="0.53975" x2="-0.34925" y2="-0.53975" width="0.1" layer="51"/>
<wire x1="-0.34925" y1="-0.53975" x2="0.3175" y2="0" width="0.1" layer="51"/>
<wire x1="0.3175" y1="0" x2="0.3175" y2="0.53975" width="0.1" layer="51"/>
<wire x1="0.3175" y1="0" x2="0.3175" y2="-0.53975" width="0.1" layer="51"/>
<text x="-2.54" y="1.905" size="1.27" layer="25" ratio="10">&gt;NAME</text>
<text x="-2.54" y="-3.175" size="1.27" layer="27" ratio="10">&gt;VALUE</text>
<polygon width="0.3048" layer="31">
<vertex x="-2.06375" y="0.79375"/>
<vertex x="-1.42875" y="0.79375"/>
<vertex x="-0.9525" y="0"/>
<vertex x="-1.42875" y="-0.79375"/>
<vertex x="-2.06375" y="-0.79375"/>
</polygon>
<polygon width="0.3048" layer="31">
<vertex x="2.06375" y="0.79375"/>
<vertex x="1.42875" y="0.79375"/>
<vertex x="0.9525" y="0"/>
<vertex x="1.42875" y="-0.79375"/>
<vertex x="2.06375" y="-0.79375"/>
</polygon>
<wire x1="-1.6" y1="1.5" x2="-1.6" y2="-1.5" width="0.127" layer="51"/>
<wire x1="-1.6" y1="-1.5" x2="1.01125" y2="-1.5" width="0.127" layer="51"/>
<wire x1="1.01125" y1="-1.5" x2="1.6" y2="-1.5" width="0.127" layer="51"/>
<wire x1="1.6" y1="-1.5" x2="1.6" y2="1.5" width="0.127" layer="51"/>
<wire x1="1.6" y1="1.5" x2="-1.6" y2="1.5" width="0.127" layer="51"/>
<circle x="0" y="0" radius="1.01649375" width="0.127" layer="51"/>
<wire x1="1.5875" y1="-0.9" x2="1.01125" y2="-1.5" width="0.127" layer="51"/>
<wire x1="-1.5875" y1="0.79375" x2="-1.905" y2="0.79375" width="0.127" layer="51"/>
<wire x1="-1.905" y1="0.79375" x2="-1.905" y2="-0.79375" width="0.127" layer="51"/>
<wire x1="-1.905" y1="-0.79375" x2="-1.5875" y2="-0.79375" width="0.127" layer="51"/>
<wire x1="1.5875" y1="0.79375" x2="1.905" y2="0.79375" width="0.127" layer="51"/>
<wire x1="1.905" y1="0.79375" x2="1.905" y2="-0.79375" width="0.127" layer="51"/>
<wire x1="1.905" y1="-0.79375" x2="1.5875" y2="-0.79375" width="0.127" layer="51"/>
<wire x1="-2.5" y1="1.4" x2="-2.5" y2="-1.4" width="0.127" layer="21"/>
<wire x1="-2.5" y1="-1.4" x2="-1.6" y2="-1.4" width="0.127" layer="21"/>
<wire x1="-1.6" y1="-1.4" x2="-1.6" y2="-1.5" width="0.127" layer="21"/>
<wire x1="-1.6" y1="-1.5" x2="1.6" y2="-1.5" width="0.127" layer="21"/>
<wire x1="1.6" y1="-1.5" x2="1.6" y2="-1.4" width="0.127" layer="21"/>
<wire x1="1.6" y1="-1.4" x2="2.5" y2="-1.4" width="0.127" layer="21"/>
<wire x1="2.5" y1="-1.4" x2="2.5" y2="1.4" width="0.127" layer="21"/>
<wire x1="2.5" y1="1.4" x2="1.6" y2="1.4" width="0.127" layer="21"/>
<wire x1="1.6" y1="1.4" x2="1.6" y2="1.5" width="0.127" layer="21"/>
<wire x1="1.6" y1="1.5" x2="-1.6" y2="1.5" width="0.127" layer="21"/>
<wire x1="-1.6" y1="1.5" x2="-1.6" y2="1.4" width="0.127" layer="21"/>
<wire x1="-1.6" y1="1.4" x2="-2.5" y2="1.4" width="0.127" layer="21"/>
</package>
</packages>
</library>
<library name="Mentor_lightpipe">
<packages>
<package name="1270.1001">
<description>MENTOR 1270.1001, PCB Mounted 2-Way Right Angle LED Light Pipe, Bi-Level Clear Round Lens</description>
<wire x1="-8.128" y1="-1.5" x2="-4.148" y2="-1.5" width="0.127" layer="21"/>
<wire x1="-4.148" y1="-1.5" x2="15.476" y2="-1.5" width="0.127" layer="21"/>
<wire x1="15.476" y1="-1.5" x2="15.476" y2="1.5" width="0.127" layer="21"/>
<hole x="13.5" y="0" drill="2.4"/>
<hole x="0" y="0" drill="2.4"/>
<wire x1="-8.128" y1="1.5" x2="-4.148" y2="1.5" width="0.127" layer="21"/>
<wire x1="-4.148" y1="1.5" x2="15.476" y2="1.5" width="0.127" layer="21"/>
<wire x1="-8.148" y1="-1.5" x2="-8.148" y2="1.5" width="0.127" layer="21"/>
<rectangle x1="6" y1="-1.5" x2="7.5" y2="1.5" layer="39"/>
<wire x1="-4.148" y1="-1.5" x2="-4.148" y2="1.5" width="0.127" layer="21"/>
</package>
</packages>
</library>
<library name="oshw">
<description>&lt;p&gt;&lt;strong&gt;Open Source Hardware PCB Logos&lt;/strong&gt;
&lt;p&gt;A simple polygon based version of the OSHWA logos for use on Eagle PCB's
&lt;p&gt;For use please refer to the OSHWA definition at &lt;a href="http://www.oshwa.org/definition/"&gt;http://www.oshwa.org/definition/&lt;/a&gt;
&lt;p&gt;Based on the NBitWonder version (&lt;a href="http://nbitwonder.com"&gt;http://nbitwonder.com&lt;/a&gt;)
&lt;p&gt;&lt;strong&gt;Andrew Cooper&lt;/strong&gt;&lt;br&gt;28Nov2016&lt;br&gt;&lt;a href="http://www.darkerview.com"&gt;www.DarkerView.com&lt;/a&gt;</description>
<packages>
<package name="OSHW_8MM">
<polygon width="0.0508" layer="25">
<vertex x="-0.381" y="-0.9906" curve="-160.613168"/>
<vertex x="0" y="1.0668" curve="-162.088112"/>
<vertex x="0.4572" y="-0.9906"/>
<vertex x="1.1176" y="-2.6924"/>
<vertex x="1.2954" y="-2.5908"/>
<vertex x="1.4732" y="-2.4892"/>
<vertex x="1.651" y="-2.3876"/>
<vertex x="2.4892" y="-2.9972"/>
<vertex x="2.667" y="-2.8194"/>
<vertex x="2.8194" y="-2.667"/>
<vertex x="2.9718" y="-2.4892"/>
<vertex x="3.1242" y="-2.3114"/>
<vertex x="2.5146" y="-1.397"/>
<vertex x="2.6416" y="-1.1938"/>
<vertex x="2.7178" y="-0.9652"/>
<vertex x="2.794" y="-0.7366"/>
<vertex x="2.8448" y="-0.5588"/>
<vertex x="3.8608" y="-0.381"/>
<vertex x="3.8862" y="-0.1016"/>
<vertex x="3.8862" y="0.127"/>
<vertex x="3.8608" y="0.3302"/>
<vertex x="3.8354" y="0.5842"/>
<vertex x="2.794" y="0.762"/>
<vertex x="2.6924" y="1.0414"/>
<vertex x="2.6416" y="1.1938"/>
<vertex x="2.54" y="1.3716"/>
<vertex x="2.413" y="1.5748"/>
<vertex x="3.048" y="2.3876"/>
<vertex x="2.8956" y="2.5654"/>
<vertex x="2.7178" y="2.7432"/>
<vertex x="2.5146" y="2.921"/>
<vertex x="2.3114" y="3.0988"/>
<vertex x="1.4478" y="2.4892"/>
<vertex x="1.2192" y="2.5908"/>
<vertex x="1.016" y="2.6924"/>
<vertex x="0.8382" y="2.7432"/>
<vertex x="0.6604" y="2.794"/>
<vertex x="0.508" y="3.8354"/>
<vertex x="0.2286" y="3.8354"/>
<vertex x="0" y="3.8354"/>
<vertex x="-0.2794" y="3.8354"/>
<vertex x="-0.4572" y="3.8354"/>
<vertex x="-0.6604" y="2.794"/>
<vertex x="-0.9398" y="2.7178"/>
<vertex x="-1.143" y="2.6162"/>
<vertex x="-1.4478" y="2.4638"/>
<vertex x="-2.3114" y="3.0734"/>
<vertex x="-2.4892" y="2.921"/>
<vertex x="-2.667" y="2.7432"/>
<vertex x="-2.8448" y="2.5654"/>
<vertex x="-2.9972" y="2.3876"/>
<vertex x="-2.413" y="1.524"/>
<vertex x="-2.54" y="1.2954"/>
<vertex x="-2.6416" y="1.0668"/>
<vertex x="-2.7178" y="0.8636"/>
<vertex x="-2.794" y="0.6604"/>
<vertex x="-3.81" y="0.508"/>
<vertex x="-3.8354" y="0.2032"/>
<vertex x="-3.8354" y="0"/>
<vertex x="-3.8354" y="-0.2286"/>
<vertex x="-3.8354" y="-0.4572"/>
<vertex x="-2.7686" y="-0.635"/>
<vertex x="-2.7178" y="-0.889"/>
<vertex x="-2.6162" y="-1.143"/>
<vertex x="-2.5146" y="-1.3716"/>
<vertex x="-2.413" y="-1.5748"/>
<vertex x="-3.0226" y="-2.3876"/>
<vertex x="-2.8702" y="-2.5654"/>
<vertex x="-2.6924" y="-2.7432"/>
<vertex x="-2.5146" y="-2.921"/>
<vertex x="-2.3622" y="-3.048"/>
<vertex x="-1.4986" y="-2.4638"/>
<vertex x="-1.3208" y="-2.5654"/>
<vertex x="-1.143" y="-2.6416"/>
<vertex x="-0.9906" y="-2.7178"/>
</polygon>
<text x="4.8006" y="-3.6576" size="1.27" layer="25" rot="R180">open source
  hardware</text>
</package>
</packages>
</library>
</libraries>
<attributes>
<attribute name="REVISION" value="v1"/>
</attributes>
<variantdefs>
</variantdefs>
<classes>
<class number="0" name="default" width="0" drill="0">
</class>
<class number="1" name="50ohms" width="1.1" drill="0">
<clearance class="1" value="0.2"/>
</class>
<class number="2" name="supply" width="0" drill="0">
</class>
<class number="3" name="usb" width="0.6" drill="0.2">
<clearance class="3" value="0.2"/>
</class>
<class number="4" name="gnd-poly" width="0.4" drill="0.2">
<clearance class="4" value="0.3"/>
</class>
</classes>
<designrules name="SeeedStudio_2layer_DRU_no_angle_20140221 *">
<description language="de">&lt;b&gt;EAGLE Design Rules&lt;/b&gt;
&lt;p&gt;
Die Standard-Design-Rules sind so gewählt, dass sie für 
die meisten Anwendungen passen. Sollte ihre Platine 
besondere Anforderungen haben, treffen Sie die erforderlichen
Einstellungen hier und speichern die Design Rules unter 
einem neuen Namen ab.</description>
<description language="en">&lt;b&gt;EAGLE Design Rules&lt;/b&gt;
&lt;p&gt;
The default Design Rules have been set to cover
a wide range of applications. Your particular design
may have different requirements, so please make the
necessary adjustments and save your customized
design rules under a new name.</description>
<description language="zh">&lt;b&gt;Seeed Studio EAGLE Design Rules&lt;/b&gt;
</description>
<param name="layerSetup" value="(1*16)"/>
<param name="mtCopper" value="0.035mm 0.0175mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.0175mm 0.035mm"/>
<param name="mtIsolate" value="1.5mm 1.1mm 0.2mm 0.15mm 0.2mm 0.15mm 0.2mm 0.15mm 0.2mm 0.15mm 0.2mm 0.15mm 0.2mm 0.15mm 0.2mm"/>
<param name="mdWireWire" value="6mil"/>
<param name="mdWirePad" value="6mil"/>
<param name="mdWireVia" value="6mil"/>
<param name="mdPadPad" value="6mil"/>
<param name="mdPadVia" value="6mil"/>
<param name="mdViaVia" value="6mil"/>
<param name="mdSmdPad" value="0mil"/>
<param name="mdSmdVia" value="0mil"/>
<param name="mdSmdSmd" value="0mil"/>
<param name="mdViaViaSameLayer" value="8mil"/>
<param name="mnLayersViaInSmd" value="2"/>
<param name="mdCopperDimension" value="10mil"/>
<param name="mdDrill" value="10mil"/>
<param name="mdSmdStop" value="0mil"/>
<param name="msWidth" value="6mil"/>
<param name="msDrill" value="0.3mm"/>
<param name="msMicroVia" value="12mil"/>
<param name="msBlindViaRatio" value="0.5"/>
<param name="rvPadTop" value="0.25"/>
<param name="rvPadInner" value="0.25"/>
<param name="rvPadBottom" value="0.25"/>
<param name="rvViaOuter" value="0.25"/>
<param name="rvViaInner" value="0.25"/>
<param name="rvMicroViaOuter" value="0.25"/>
<param name="rvMicroViaInner" value="0.25"/>
<param name="rlMinPadTop" value="10mil"/>
<param name="rlMaxPadTop" value="20mil"/>
<param name="rlMinPadInner" value="10mil"/>
<param name="rlMaxPadInner" value="20mil"/>
<param name="rlMinPadBottom" value="10mil"/>
<param name="rlMaxPadBottom" value="20mil"/>
<param name="rlMinViaOuter" value="6mil"/>
<param name="rlMaxViaOuter" value="20mil"/>
<param name="rlMinViaInner" value="6mil"/>
<param name="rlMaxViaInner" value="20mil"/>
<param name="rlMinMicroViaOuter" value="4mil"/>
<param name="rlMaxMicroViaOuter" value="20mil"/>
<param name="rlMinMicroViaInner" value="4mil"/>
<param name="rlMaxMicroViaInner" value="20mil"/>
<param name="psTop" value="-1"/>
<param name="psBottom" value="-1"/>
<param name="psFirst" value="0"/>
<param name="psElongationLong" value="100"/>
<param name="psElongationOffset" value="100"/>
<param name="mvStopFrame" value="1"/>
<param name="mvCreamFrame" value="0"/>
<param name="mlMinStopFrame" value="2mil"/>
<param name="mlMaxStopFrame" value="2mil"/>
<param name="mlMinCreamFrame" value="0mil"/>
<param name="mlMaxCreamFrame" value="0mil"/>
<param name="mlViaStopLimit" value="100mil"/>
<param name="srRoundness" value="0"/>
<param name="srMinRoundness" value="0mil"/>
<param name="srMaxRoundness" value="0mil"/>
<param name="slThermalIsolate" value="10mil"/>
<param name="slThermalsForVias" value="0"/>
<param name="dpMaxLengthDifference" value="10mm"/>
<param name="dpGapFactor" value="2.5"/>
<param name="checkGrid" value="0"/>
<param name="checkAngle" value="0"/>
<param name="checkFont" value="1"/>
<param name="checkRestrict" value="0"/>
<param name="useDiameter" value="13"/>
<param name="maxErrors" value="50"/>
</designrules>
<autorouter>
<pass name="Default">
<param name="RoutingGrid" value="50mil"/>
<param name="AutoGrid" value="1"/>
<param name="Efforts" value="0"/>
<param name="TopRouterVariant" value="1"/>
<param name="tpViaShape" value="round"/>
<param name="PrefDir.1" value="a"/>
<param name="PrefDir.2" value="0"/>
<param name="PrefDir.3" value="0"/>
<param name="PrefDir.4" value="0"/>
<param name="PrefDir.5" value="0"/>
<param name="PrefDir.6" value="0"/>
<param name="PrefDir.7" value="0"/>
<param name="PrefDir.8" value="0"/>
<param name="PrefDir.9" value="0"/>
<param name="PrefDir.10" value="0"/>
<param name="PrefDir.11" value="0"/>
<param name="PrefDir.12" value="0"/>
<param name="PrefDir.13" value="0"/>
<param name="PrefDir.14" value="0"/>
<param name="PrefDir.15" value="0"/>
<param name="PrefDir.16" value="a"/>
<param name="cfVia" value="8"/>
<param name="cfNonPref" value="5"/>
<param name="cfChangeDir" value="2"/>
<param name="cfOrthStep" value="2"/>
<param name="cfDiagStep" value="3"/>
<param name="cfExtdStep" value="0"/>
<param name="cfBonusStep" value="1"/>
<param name="cfMalusStep" value="1"/>
<param name="cfPadImpact" value="4"/>
<param name="cfSmdImpact" value="4"/>
<param name="cfBusImpact" value="0"/>
<param name="cfHugging" value="3"/>
<param name="cfAvoid" value="4"/>
<param name="cfPolygon" value="10"/>
<param name="cfBase.1" value="0"/>
<param name="cfBase.2" value="1"/>
<param name="cfBase.3" value="1"/>
<param name="cfBase.4" value="1"/>
<param name="cfBase.5" value="1"/>
<param name="cfBase.6" value="1"/>
<param name="cfBase.7" value="1"/>
<param name="cfBase.8" value="1"/>
<param name="cfBase.9" value="1"/>
<param name="cfBase.10" value="1"/>
<param name="cfBase.11" value="1"/>
<param name="cfBase.12" value="1"/>
<param name="cfBase.13" value="1"/>
<param name="cfBase.14" value="1"/>
<param name="cfBase.15" value="1"/>
<param name="cfBase.16" value="0"/>
<param name="mnVias" value="20"/>
<param name="mnSegments" value="9999"/>
<param name="mnExtdSteps" value="9999"/>
<param name="mnRipupLevel" value="10"/>
<param name="mnRipupSteps" value="100"/>
<param name="mnRipupTotal" value="100"/>
</pass>
<pass name="Follow-me" refer="Default" active="yes">
</pass>
<pass name="Busses" refer="Default" active="yes">
<param name="cfNonPref" value="4"/>
<param name="cfBusImpact" value="4"/>
<param name="cfHugging" value="0"/>
<param name="mnVias" value="0"/>
</pass>
<pass name="Route" refer="Default" active="yes">
</pass>
<pass name="Optimize1" refer="Default" active="yes">
<param name="cfVia" value="99"/>
<param name="cfExtdStep" value="10"/>
<param name="cfHugging" value="1"/>
<param name="mnExtdSteps" value="1"/>
<param name="mnRipupLevel" value="0"/>
</pass>
<pass name="Optimize2" refer="Optimize1" active="yes">
<param name="cfNonPref" value="0"/>
<param name="cfChangeDir" value="6"/>
<param name="cfExtdStep" value="0"/>
<param name="cfBonusStep" value="2"/>
<param name="cfMalusStep" value="2"/>
<param name="cfPadImpact" value="2"/>
<param name="cfSmdImpact" value="2"/>
<param name="cfHugging" value="0"/>
</pass>
<pass name="Optimize3" refer="Optimize2" active="yes">
<param name="cfChangeDir" value="8"/>
<param name="cfPadImpact" value="0"/>
<param name="cfSmdImpact" value="0"/>
</pass>
<pass name="Optimize4" refer="Optimize3" active="yes">
<param name="cfChangeDir" value="25"/>
</pass>
</autorouter>
<elements>
<element name="C1" library="rc-sysmocom" package="_0603" value="100n" x="28.956" y="33.528" smashed="yes" rot="R90">
<attribute name="NAME" x="29.5275" y="35.2425" size="1.016" layer="25" font="vector" ratio="14" rot="R90"/>
<attribute name="VALUE" x="30.4483" y="31.9405" size="0.508" layer="27" font="vector" ratio="10" rot="R90"/>
<attribute name="DESCRIPTION" value="CAP CER 0.1UF 16V X7R 0603" x="28.956" y="33.528" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics" x="28.956" y="33.528" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL10B104KO8NNNC" x="28.956" y="33.528" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="28.956" y="33.528" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1005-1-ND" x="28.956" y="33.528" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="28.956" y="33.528" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="POPULATED" value="TRUE" x="28.956" y="33.528" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="CLASS" value="CAPACITOR" x="28.956" y="33.528" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/samsung-electro-mechanics/CL10B104KO8NNNC/1276-1005-1-ND/3889091" x="28.956" y="33.528" size="1.778" layer="27" rot="R90" display="off"/>
</element>
<element name="C10" library="rc-sysmocom" package="_0805" value="4.7u" x="38.1" y="88.138" smashed="yes" rot="R270">
<attribute name="NAME" x="38.608" y="90.551" size="1.016" layer="25" font="vector" ratio="14" rot="R90"/>
<attribute name="VALUE" x="36.449" y="90.0429" size="0.508" layer="27" font="vector" ratio="10" rot="R270"/>
<attribute name="DESCRIPTION" value="CAP CER 4.7UF 16V X5R 0805" x="38.1" y="88.138" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics" x="38.1" y="88.138" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL21A475KOFNNNE" x="38.1" y="88.138" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="38.1" y="88.138" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1065-1-ND" x="38.1" y="88.138" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="38.1" y="88.138" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="POPULATED" value="TRUE" x="38.1" y="88.138" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="CLASS" value="CAPACITOR" x="38.1" y="88.138" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/samsung-electro-mechanics/CL21A475KOFNNNE/1276-1065-1-ND/3889151" x="38.1" y="88.138" size="1.778" layer="27" rot="R270" display="off"/>
</element>
<element name="C11" library="rc-sysmocom" package="_0603" value="10n" x="18.288" y="44.45" rot="R180">
<attribute name="DESCRIPTION" value="CAP CER 10000PF 50V X7R 0603" x="18.288" y="44.45" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="MANUFACTURER" value="KEMET" x="18.288" y="44.45" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="C0603C103M5RACTU" x="18.288" y="44.45" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="18.288" y="44.45" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="399-7842-1-ND" x="18.288" y="44.45" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="18.288" y="44.45" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="POPULATED" value="TRUE" x="18.288" y="44.45" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="CLASS" value="CAPACITOR" x="18.288" y="44.45" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/kemet/C0603C103M5RACTU/399-7842-1-ND/3471565" x="18.288" y="44.45" size="1.778" layer="27" rot="R180" display="off"/>
</element>
<element name="C2" library="rc-sysmocom" package="_0603" value="100n" x="28.956" y="29.718" smashed="yes" rot="R270">
<attribute name="NAME" x="28.6385" y="28.0035" size="1.016" layer="25" font="vector" ratio="14" rot="R270"/>
<attribute name="VALUE" x="27.4637" y="31.3055" size="0.508" layer="27" font="vector" ratio="10" rot="R270"/>
<attribute name="DESCRIPTION" value="CAP CER 0.1UF 16V X7R 0603" x="28.956" y="29.718" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics" x="28.956" y="29.718" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL10B104KO8NNNC" x="28.956" y="29.718" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="28.956" y="29.718" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1005-1-ND" x="28.956" y="29.718" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="28.956" y="29.718" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="POPULATED" value="TRUE" x="28.956" y="29.718" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="CLASS" value="CAPACITOR" x="28.956" y="29.718" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/samsung-electro-mechanics/CL10B104KO8NNNC/1276-1005-1-ND/3889091" x="28.956" y="29.718" size="1.778" layer="27" rot="R270" display="off"/>
</element>
<element name="C3" library="rc-sysmocom" package="_0603" value="10n" x="21.844" y="6.35" smashed="yes">
<attribute name="NAME" x="20.2565" y="7.3025" size="1.016" layer="25" font="vector" ratio="14"/>
<attribute name="VALUE" x="20.2565" y="4.8577" size="0.508" layer="27" font="vector" ratio="10"/>
<attribute name="DESCRIPTION" value="CAP CER 10000PF 50V X7R 0603" x="21.844" y="6.35" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURER" value="KEMET" x="21.844" y="6.35" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="C0603C103M5RACTU" x="21.844" y="6.35" size="1.778" layer="27" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="21.844" y="6.35" size="1.778" layer="27" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="399-7842-1-ND" x="21.844" y="6.35" size="1.778" layer="27" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="21.844" y="6.35" size="1.778" layer="27" display="off"/>
<attribute name="POPULATED" value="TRUE" x="21.844" y="6.35" size="1.778" layer="27" display="off"/>
<attribute name="CLASS" value="CAPACITOR" x="21.844" y="6.35" size="1.778" layer="27" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/kemet/C0603C103M5RACTU/399-7842-1-ND/3471565" x="21.844" y="6.35" size="1.778" layer="27" display="off"/>
</element>
<element name="C4" library="rc-sysmocom" package="_0603" value="10n" x="21.59" y="19.05" smashed="yes">
<attribute name="NAME" x="20.0025" y="20.0025" size="1.016" layer="25" font="vector" ratio="14"/>
<attribute name="VALUE" x="20.0025" y="17.5577" size="0.508" layer="27" font="vector" ratio="10"/>
<attribute name="DESCRIPTION" value="CAP CER 10000PF 50V X7R 0603" x="21.59" y="19.05" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURER" value="KEMET" x="21.59" y="19.05" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="C0603C103M5RACTU" x="21.59" y="19.05" size="1.778" layer="27" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="21.59" y="19.05" size="1.778" layer="27" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="399-7842-1-ND" x="21.59" y="19.05" size="1.778" layer="27" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="21.59" y="19.05" size="1.778" layer="27" display="off"/>
<attribute name="POPULATED" value="TRUE" x="21.59" y="19.05" size="1.778" layer="27" display="off"/>
<attribute name="CLASS" value="CAPACITOR" x="21.59" y="19.05" size="1.778" layer="27" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/kemet/C0603C103M5RACTU/399-7842-1-ND/3471565" x="21.59" y="19.05" size="1.778" layer="27" display="off"/>
</element>
<element name="C5" library="rc-sysmocom" package="_0603" value="10n" x="18.542" y="60.198" smashed="yes" rot="R180">
<attribute name="NAME" x="18.2245" y="61.1505" size="1.016" layer="25" font="vector" ratio="14"/>
<attribute name="VALUE" x="20.1295" y="61.6903" size="0.508" layer="27" font="vector" ratio="10" rot="R180"/>
<attribute name="DESCRIPTION" value="CAP CER 10000PF 50V X7R 0603" x="18.542" y="60.198" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="MANUFACTURER" value="KEMET" x="18.542" y="60.198" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="C0603C103M5RACTU" x="18.542" y="60.198" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="18.542" y="60.198" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="399-7842-1-ND" x="18.542" y="60.198" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="18.542" y="60.198" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="POPULATED" value="TRUE" x="18.542" y="60.198" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="CLASS" value="CAPACITOR" x="18.542" y="60.198" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/kemet/C0603C103M5RACTU/399-7842-1-ND/3471565" x="18.542" y="60.198" size="1.778" layer="27" rot="R180" display="off"/>
</element>
<element name="C6" library="rc-sysmocom" package="_0603" value="100n" x="30.988" y="88.9" smashed="yes" rot="R90">
<attribute name="NAME" x="31.5595" y="85.2805" size="1.016" layer="25" font="vector" ratio="14" rot="R90"/>
<attribute name="VALUE" x="32.4803" y="87.3125" size="0.508" layer="27" font="vector" ratio="10" rot="R90"/>
<attribute name="DESCRIPTION" value="CAP CER 0.1UF 16V X7R 0603" x="30.988" y="88.9" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics" x="30.988" y="88.9" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL10B104KO8NNNC" x="30.988" y="88.9" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="30.988" y="88.9" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1005-1-ND" x="30.988" y="88.9" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="30.988" y="88.9" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="POPULATED" value="TRUE" x="30.988" y="88.9" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="CLASS" value="CAPACITOR" x="30.988" y="88.9" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/samsung-electro-mechanics/CL10B104KO8NNNC/1276-1005-1-ND/3889091" x="30.988" y="88.9" size="1.778" layer="27" rot="R90" display="off"/>
</element>
<element name="C7" library="rc-sysmocom" package="_0603" value="100n" x="36.068" y="87.884" smashed="yes" rot="R270">
<attribute name="NAME" x="36.6395" y="89.8525" size="1.016" layer="25" font="vector" ratio="14" rot="R90"/>
<attribute name="VALUE" x="34.5757" y="89.4715" size="0.508" layer="27" font="vector" ratio="10" rot="R270"/>
<attribute name="DESCRIPTION" value="CAP CER 0.1UF 16V X7R 0603" x="36.068" y="87.884" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics" x="36.068" y="87.884" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL10B104KO8NNNC" x="36.068" y="87.884" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="36.068" y="87.884" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1005-1-ND" x="36.068" y="87.884" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="36.068" y="87.884" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="POPULATED" value="TRUE" x="36.068" y="87.884" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="CLASS" value="CAPACITOR" x="36.068" y="87.884" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/samsung-electro-mechanics/CL10B104KO8NNNC/1276-1005-1-ND/3889091" x="36.068" y="87.884" size="1.778" layer="27" rot="R270" display="off"/>
</element>
<element name="C8" library="rc-sysmocom" package="_0805" value="4.7u" x="28.956" y="88.646" smashed="yes" rot="R90">
<attribute name="NAME" x="29.464" y="84.709" size="1.016" layer="25" font="vector" ratio="14" rot="R90"/>
<attribute name="VALUE" x="30.607" y="86.7411" size="0.508" layer="27" font="vector" ratio="10" rot="R90"/>
<attribute name="DESCRIPTION" value="CAP CER 4.7UF 16V X5R 0805" x="28.956" y="88.646" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics" x="28.956" y="88.646" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL21A475KOFNNNE" x="28.956" y="88.646" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="28.956" y="88.646" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1065-1-ND" x="28.956" y="88.646" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="28.956" y="88.646" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="POPULATED" value="TRUE" x="28.956" y="88.646" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="CLASS" value="CAPACITOR" x="28.956" y="88.646" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/samsung-electro-mechanics/CL21A475KOFNNNE/1276-1065-1-ND/3889151" x="28.956" y="88.646" size="1.778" layer="27" rot="R90" display="off"/>
</element>
<element name="D1" library="laforge" package="0603" value="0603ESDA-TR" x="16.256" y="59.436" smashed="yes" rot="R90">
<attribute name="NAME" x="15.875" y="57.785" size="1.016" layer="25" font="vector" ratio="14" rot="R270"/>
<attribute name="VALUE" x="18.161" y="58.801" size="1.27" layer="27" rot="R90"/>
<attribute name="DESCRIPTION" value="SUPPRESSOR ESD 30VDC 0603 SMD" x="16.256" y="59.436" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MANUFACTURER" value="Eaton - Electronics Division" x="16.256" y="59.436" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="0603ESDA2-TR2" x="16.256" y="59.436" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="16.256" y="59.436" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="283-4156-1-ND" x="16.256" y="59.436" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="16.256" y="59.436" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="POPULATED" value="TRUE" x="16.256" y="59.436" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="CLASS" value="DIODE" x="16.256" y="59.436" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/eaton-electronics-division/0603ESDA2-TR2/283-4156-1-ND/3681415" x="16.256" y="59.436" size="1.778" layer="27" rot="R90" display="off"/>
</element>
<element name="D2" library="laforge" package="0603" value="0603ESDA-TR" x="16.002" y="43.688" smashed="yes" rot="R90">
<attribute name="NAME" x="15.621" y="42.037" size="1.016" layer="25" font="vector" ratio="14" rot="R270"/>
<attribute name="VALUE" x="17.907" y="43.053" size="1.27" layer="27" rot="R90"/>
<attribute name="DESCRIPTION" value="SUPPRESSOR ESD 30VDC 0603 SMD" x="16.002" y="43.688" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MANUFACTURER" value="Eaton - Electronics Division" x="16.002" y="43.688" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="0603ESDA2-TR2" x="16.002" y="43.688" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="16.002" y="43.688" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="283-4156-1-ND" x="16.002" y="43.688" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="16.002" y="43.688" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="POPULATED" value="TRUE" x="16.002" y="43.688" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="CLASS" value="DIODE" x="16.002" y="43.688" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/eaton-electronics-division/0603ESDA2-TR2/283-4156-1-ND/3681415" x="16.002" y="43.688" size="1.778" layer="27" rot="R90" display="off"/>
</element>
<element name="D3" library="laforge" package="0603" value="0603ESDA-TR" x="14.224" y="5.588" smashed="yes" rot="R90">
<attribute name="NAME" x="14.605" y="7.239" size="1.016" layer="25" font="vector" ratio="14" rot="R90"/>
<attribute name="VALUE" x="16.129" y="4.953" size="1.27" layer="27" rot="R90"/>
<attribute name="DESCRIPTION" value="SUPPRESSOR ESD 30VDC 0603 SMD" x="14.224" y="5.588" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MANUFACTURER" value="Eaton - Electronics Division" x="14.224" y="5.588" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="0603ESDA2-TR2" x="14.224" y="5.588" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="14.224" y="5.588" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="283-4156-1-ND" x="14.224" y="5.588" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="14.224" y="5.588" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="POPULATED" value="TRUE" x="14.224" y="5.588" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="CLASS" value="DIODE" x="14.224" y="5.588" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/eaton-electronics-division/0603ESDA2-TR2/283-4156-1-ND/3681415" x="14.224" y="5.588" size="1.778" layer="27" rot="R90" display="off"/>
</element>
<element name="D4" library="laforge" package="0603" value="0603ESDA-TR" x="14.224" y="18.288" smashed="yes" rot="R90">
<attribute name="NAME" x="13.589" y="16.637" size="1.016" layer="25" font="vector" ratio="14" rot="R270"/>
<attribute name="VALUE" x="16.129" y="17.653" size="1.27" layer="27" rot="R90"/>
<attribute name="DESCRIPTION" value="SUPPRESSOR ESD 30VDC 0603 SMD" x="14.224" y="18.288" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MANUFACTURER" value="Eaton - Electronics Division" x="14.224" y="18.288" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="0603ESDA2-TR2" x="14.224" y="18.288" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="14.224" y="18.288" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="283-4156-1-ND" x="14.224" y="18.288" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="14.224" y="18.288" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="POPULATED" value="TRUE" x="14.224" y="18.288" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="CLASS" value="DIODE" x="14.224" y="18.288" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/eaton-electronics-division/0603ESDA2-TR2/283-4156-1-ND/3681415" x="14.224" y="18.288" size="1.778" layer="27" rot="R90" display="off"/>
</element>
<element name="D5" library="diodes-sysmocom" package="SMADIODE" value="5.6V" x="25.4" y="93.98" smashed="yes" rot="R90">
<attribute name="NAME" x="28.321" y="93.472" size="1.016" layer="25" font="vector" ratio="17" rot="R90"/>
<attribute name="VALUE" x="27.686" y="91.44" size="0.4064" layer="27" font="vector" ratio="10" rot="R90"/>
<attribute name="DESCRIPTION" value="DIODE ZENER 5.6V 3W DO214AC" x="25.4" y="93.98" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MANUFACTURER" value="Micro Commercial Co" x="25.4" y="93.98" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="3SMAJ5919B-TP" x="25.4" y="93.98" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="25.4" y="93.98" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="3SMAJ5919B-TPMSCT-ND" x="25.4" y="93.98" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="25.4" y="93.98" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="POPULATED" value="TRUE" x="25.4" y="93.98" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="CLASS" value="DIODE" x="25.4" y="93.98" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/micro-commercial-co/3SMAJ5919B-TP/3SMAJ5919B-TPMSCT-ND/1793296" x="25.4" y="93.98" size="1.778" layer="27" rot="R90" display="off"/>
</element>
<element name="D6" library="diodes-sysmocom" package="SMADIODE" value="" x="21.59" y="93.98" smashed="yes" rot="R90">
<attribute name="NAME" x="20.701" y="88.138" size="1.016" layer="25" font="vector" ratio="17" rot="R90"/>
<attribute name="VALUE" x="23.876" y="91.44" size="0.4064" layer="27" font="vector" ratio="10" rot="R90"/>
<attribute name="DESCRIPTION" value="DIODE SCHOTTKY 30V 800MA USC" x="21.59" y="93.98" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MANUFACTURER" value="Toshiba Semiconductor and Storage" x="21.59" y="93.98" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CUS08F30,H3F" x="21.59" y="93.98" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="21.59" y="93.98" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="CUS08F30H3FCT-ND" x="21.59" y="93.98" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="21.59" y="93.98" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="POPULATED" value="TRUE" x="21.59" y="93.98" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="CLASS" value="DIODE" x="21.59" y="93.98" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/toshiba-semiconductor-and-storage/CUS08F30H3F/CUS08F30H3FCT-ND/5114376" x="21.59" y="93.98" size="1.778" layer="27" rot="R90" display="off"/>
</element>
<element name="F1" library="littlefuse" package="1206L" value="100mA" x="23.368" y="89.154" smashed="yes" rot="R180">
<attribute name="NAME" x="24.868" y="88.154" size="1.016" layer="25" font="vector" ratio="14" rot="R180"/>
<attribute name="VALUE" x="21.768" y="90.154" size="0.8128" layer="27" font="vector"/>
<attribute name="DESCRIPTION" value="PTC RESET FUSE 30V 200MA 1206" x="23.368" y="89.154" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="MANUFACTURER" value="Bel Fuse Inc." x="23.368" y="89.154" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="0ZCJ0020FF2E" x="23.368" y="89.154" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="23.368" y="89.154" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="507-1797-1-ND" x="23.368" y="89.154" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="23.368" y="89.154" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="POPULATED" value="TRUE" x="23.368" y="89.154" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="CLASS" value="UNKNOWN CLASS" x="23.368" y="89.154" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/0ZCJ0020FF2E/507-1797-1-ND/4156228/?itemSeq=282618602" x="23.368" y="89.154" size="1.778" layer="27" rot="R180" display="off"/>
</element>
<element name="JP1" library="jumper" package="JP2" value="FILTA" x="32.766" y="41.148" smashed="yes" rot="R90">
<attribute name="NAME" x="32.131" y="37.084" size="1.016" layer="25" font="vector" ratio="14" rot="R270"/>
<attribute name="VALUE" x="37.084" y="37.592" size="1.27" layer="27" ratio="10" rot="R90"/>
<attribute name="DESCRIPTION" value="CONN HEADER VERT 3POS 2.54MM" x="32.766" y="41.148" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MANUFACTURER" value="Wurth Electronics Inc." x="32.766" y="41.148" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="61300311121" x="32.766" y="41.148" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="32.766" y="41.148" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="732-5316-ND" x="32.766" y="41.148" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="32.766" y="41.148" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="POPULATED" value="TRUE" x="32.766" y="41.148" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="CLASS" value="CONNECTOR\JUMPER" x="32.766" y="41.148" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/wurth-electronics-inc/61300311121/732-5316-ND/4846825" x="32.766" y="41.148" size="1.778" layer="27" rot="R90" display="off"/>
</element>
<element name="JP2" library="jumper" package="JP2" value="FILTB" x="17.526" y="35.306" smashed="yes" rot="R180">
<attribute name="NAME" x="12.954" y="35.941" size="1.016" layer="25" font="vector" ratio="14" rot="R180"/>
<attribute name="VALUE" x="21.082" y="39.624" size="1.27" layer="27" ratio="10" rot="R180"/>
<attribute name="DESCRIPTION" value="CONN HEADER VERT 3POS 2.54MM" x="17.526" y="35.306" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="MANUFACTURER" value="Wurth Electronics Inc." x="17.526" y="35.306" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="61300311121" x="17.526" y="35.306" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="17.526" y="35.306" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="732-5316-ND" x="17.526" y="35.306" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="17.526" y="35.306" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="POPULATED" value="TRUE" x="17.526" y="35.306" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="CLASS" value="CONNECTOR\JUMPER" x="17.526" y="35.306" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/wurth-electronics-inc/61300311121/732-5316-ND/4846825" x="17.526" y="35.306" size="1.778" layer="27" rot="R180" display="off"/>
</element>
<element name="JP3" library="jumper" package="JP2" value="SD1" x="34.036" y="25.908" smashed="yes" rot="R90">
<attribute name="NAME" x="33.401" y="21.59" size="1.016" layer="25" font="vector" ratio="14" rot="R270"/>
<attribute name="VALUE" x="38.354" y="22.352" size="1.27" layer="27" ratio="10" rot="R90"/>
<attribute name="DESCRIPTION" value="CONN HEADER VERT 3POS 2.54MM" x="34.036" y="25.908" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MANUFACTURER" value="Wurth Electronics Inc." x="34.036" y="25.908" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="61300311121" x="34.036" y="25.908" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="34.036" y="25.908" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="732-5316-ND" x="34.036" y="25.908" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="34.036" y="25.908" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="POPULATED" value="TRUE" x="34.036" y="25.908" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="CLASS" value="CONNECTOR\JUMPER" x="34.036" y="25.908" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/wurth-electronics-inc/61300311121/732-5316-ND/4846825" x="34.036" y="25.908" size="1.778" layer="27" rot="R90" display="off"/>
</element>
<element name="JP4" library="jumper" package="JP2" value="SD2" x="17.526" y="28.194" smashed="yes" rot="R180">
<attribute name="NAME" x="13.208" y="28.829" size="1.016" layer="25" font="vector" ratio="14" rot="R180"/>
<attribute name="VALUE" x="21.082" y="32.512" size="1.27" layer="27" ratio="10" rot="R180"/>
<attribute name="DESCRIPTION" value="CONN HEADER VERT 3POS 2.54MM" x="17.526" y="28.194" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="MANUFACTURER" value="Wurth Electronics Inc." x="17.526" y="28.194" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="61300311121" x="17.526" y="28.194" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="17.526" y="28.194" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="732-5316-ND" x="17.526" y="28.194" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="17.526" y="28.194" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="POPULATED" value="TRUE" x="17.526" y="28.194" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="CLASS" value="CONNECTOR\JUMPER" x="17.526" y="28.194" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/wurth-electronics-inc/61300311121/732-5316-ND/4846825" x="17.526" y="28.194" size="1.778" layer="27" rot="R180" display="off"/>
</element>
<element name="JP5" library="laforge" package="1X02" value="DC IN" x="17.526" y="94.996" locked="yes" smashed="yes" rot="R270">
<attribute name="NAME" x="16.8148" y="91.5162" size="1.016" layer="25" font="vector" ratio="14" rot="R270"/>
<attribute name="VALUE" x="14.351" y="97.536" size="1.27" layer="27" rot="R270"/>
<attribute name="DESCRIPTION" value="CONN HEADER VERT 2POS 2.54MM" x="17.526" y="94.996" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="MANUFACTURER" value="Sullins Connector Solutions" x="17.526" y="94.996" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="PREC002SAAN-RC" x="17.526" y="94.996" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="17.526" y="94.996" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="S1012EC-02-ND" x="17.526" y="94.996" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="17.526" y="94.996" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="POPULATED" value="TRUE" x="17.526" y="94.996" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="CLASS" value="CONNECTOR\JUMPER" x="17.526" y="94.996" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/PREC002SAAN-RC/S1012EC-02-ND/2774852" x="17.526" y="94.996" size="1.778" layer="27" rot="R270" display="off"/>
</element>
<element name="JP6" library="pinhead" package="1X04" value="VDD_SEL" x="28.448" y="81.28" smashed="yes">
<attribute name="NAME" x="35.4838" y="80.8228" size="1.016" layer="25" font="vector" ratio="14"/>
<attribute name="VALUE" x="23.368" y="78.105" size="1.27" layer="27"/>
<attribute name="DESCRIPTION" value="CONN HEADER VERT 4POS 2.54MM" x="28.448" y="81.28" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURER" value="Sullins Connector Solutions" x="28.448" y="81.28" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="PRPC004SAAN-RC" x="28.448" y="81.28" size="1.778" layer="27" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="28.448" y="81.28" size="1.778" layer="27" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="S1011EC-04-ND" x="28.448" y="81.28" size="1.778" layer="27" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="28.448" y="81.28" size="1.778" layer="27" display="off"/>
<attribute name="POPULATED" value="TRUE" x="28.448" y="81.28" size="1.778" layer="27" display="off"/>
<attribute name="CLASS" value="CONNECTOR\JUMPER" x="28.448" y="81.28" size="1.778" layer="27" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/sullins-connector-solutions/PRPC004SAAN-RC/S1011EC-04-ND/2775250" x="28.448" y="81.28" size="1.778" layer="27" display="off"/>
</element>
<element name="K1" library="Wurth_Elektronik_Electromechanic_DC_Power_Jack_Connectors_rev15c" package="694108106102" value="DC IN" x="-1.275" y="90.931" locked="yes" smashed="yes">
<attribute name="NAME" x="-0.975359375" y="99.3616" size="2.032" layer="25" font="vector" ratio="13" rot="SR0"/>
<attribute name="VALUE" x="-0.575359375" y="80.8176" size="2.032" layer="27" font="vector" ratio="13" rot="SR0"/>
<attribute name="DESCRIPTION" value="CONN PWR JACK 2.5X5.5MM SOLDER" x="-1.275" y="90.931" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURER" value="Wurth Electronics Inc." x="-1.275" y="90.931" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="694108106102" x="-1.275" y="90.931" size="1.778" layer="27" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="-1.275" y="90.931" size="1.778" layer="27" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="732-5933-1-ND" x="-1.275" y="90.931" size="1.778" layer="27" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="-1.275" y="90.931" size="1.778" layer="27" display="off"/>
<attribute name="POPULATED" value="TRUE" x="-1.275" y="90.931" size="1.778" layer="27" display="off"/>
<attribute name="CLASS" value="RELAY" x="-1.275" y="90.931" size="1.778" layer="27" display="off"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/wurth-electronics-inc/694108106102/732-5933-1-ND/5047628" x="-1.275" y="90.931" size="1.778" layer="27" display="off"/>
</element>
<element name="R1" library="rc-sysmocom" package="_0603" value="330k" x="29.972" y="41.91" smashed="yes" rot="R90">
<attribute name="NAME" x="30.2895" y="43.8785" size="1.016" layer="25" font="vector" ratio="14" rot="R90"/>
<attribute name="VALUE" x="31.4643" y="40.3225" size="0.508" layer="27" font="vector" ratio="10" rot="R90"/>
<attribute name="DESCRIPTION" value="RES 330K OHM 5%% 1/10W 0603" x="29.972" y="41.91" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MANUFACTURER" value="Stackpole Electronics Inc" x="29.972" y="41.91" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RMCF0603JG330K" x="29.972" y="41.91" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="29.972" y="41.91" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="RMCF0603JG330KCT-ND" x="29.972" y="41.91" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="29.972" y="41.91" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="POPULATED" value="TRUE" x="29.972" y="41.91" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="CLASS" value="RESISTOR" x="29.972" y="41.91" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/stackpole-electronics-inc/RMCF0603JG330K/RMCF0603JG330KCT-ND/6053832" x="29.972" y="41.91" size="1.778" layer="27" rot="R90" display="off"/>
</element>
<element name="R10" library="rc-sysmocom" package="_0603" value="49.9" x="14.224" y="43.688" smashed="yes" rot="R270">
<attribute name="NAME" x="13.6525" y="41.9735" size="1.016" layer="25" font="vector" ratio="14" rot="R270"/>
<attribute name="VALUE" x="12.7317" y="45.2755" size="0.508" layer="27" font="vector" ratio="10" rot="R270"/>
<attribute name="DESCRIPTION" value="RES 49.9 OHM 1%% 1/10W 0603" x="14.224" y="43.688" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="MANUFACTURER" value="Stackpole Electronics Inc" x="14.224" y="43.688" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RMCF0603FT49R9" x="14.224" y="43.688" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="14.224" y="43.688" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="RMCF0603FT49R9CT-ND" x="14.224" y="43.688" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="14.224" y="43.688" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="POPULATED" value="TRUE" x="14.224" y="43.688" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="CLASS" value="RESISTOR" x="14.224" y="43.688" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/stackpole-electronics-inc/RMCF0603FT49R9/RMCF0603FT49R9CT-ND/1942956" x="14.224" y="43.688" size="1.778" layer="27" rot="R270" display="off"/>
</element>
<element name="R2" library="rc-sysmocom" package="_0603" value="330k" x="18.796" y="32.766" smashed="yes">
<attribute name="NAME" x="16.8275" y="33.3375" size="1.016" layer="25" font="vector" ratio="14" rot="R180"/>
<attribute name="VALUE" x="17.2085" y="31.2737" size="0.508" layer="27" font="vector" ratio="10"/>
<attribute name="DESCRIPTION" value="RES 330K OHM 5%% 1/10W 0603" x="18.796" y="32.766" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURER" value="Stackpole Electronics Inc" x="18.796" y="32.766" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RMCF0603JG330K" x="18.796" y="32.766" size="1.778" layer="27" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="18.796" y="32.766" size="1.778" layer="27" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="RMCF0603JG330KCT-ND" x="18.796" y="32.766" size="1.778" layer="27" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="18.796" y="32.766" size="1.778" layer="27" display="off"/>
<attribute name="POPULATED" value="TRUE" x="18.796" y="32.766" size="1.778" layer="27" display="off"/>
<attribute name="CLASS" value="RESISTOR" x="18.796" y="32.766" size="1.778" layer="27" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/stackpole-electronics-inc/RMCF0603JG330K/RMCF0603JG330KCT-ND/6053832" x="18.796" y="32.766" size="1.778" layer="27" display="off"/>
</element>
<element name="R3" library="rc-sysmocom" package="_0603" value="330k" x="31.496" y="24.638" smashed="yes" rot="R270">
<attribute name="NAME" x="31.8135" y="26.6065" size="1.016" layer="25" font="vector" ratio="14" rot="R90"/>
<attribute name="VALUE" x="30.0037" y="26.2255" size="0.508" layer="27" font="vector" ratio="10" rot="R270"/>
<attribute name="DESCRIPTION" value="RES 330K OHM 5%% 1/10W 0603" x="31.496" y="24.638" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="MANUFACTURER" value="Stackpole Electronics Inc" x="31.496" y="24.638" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RMCF0603JG330K" x="31.496" y="24.638" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="31.496" y="24.638" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="RMCF0603JG330KCT-ND" x="31.496" y="24.638" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="31.496" y="24.638" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="POPULATED" value="TRUE" x="31.496" y="24.638" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="CLASS" value="RESISTOR" x="31.496" y="24.638" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/stackpole-electronics-inc/RMCF0603JG330K/RMCF0603JG330KCT-ND/6053832" x="31.496" y="24.638" size="1.778" layer="27" rot="R270" display="off"/>
</element>
<element name="R4" library="rc-sysmocom" package="_0603" value="330k" x="18.796" y="25.654" smashed="yes">
<attribute name="NAME" x="16.8275" y="26.2255" size="1.016" layer="25" font="vector" ratio="14" rot="R180"/>
<attribute name="VALUE" x="17.2085" y="24.1617" size="0.508" layer="27" font="vector" ratio="10"/>
<attribute name="DESCRIPTION" value="RES 330K OHM 5%% 1/10W 0603" x="18.796" y="25.654" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURER" value="Stackpole Electronics Inc" x="18.796" y="25.654" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RMCF0603JG330K" x="18.796" y="25.654" size="1.778" layer="27" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="18.796" y="25.654" size="1.778" layer="27" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="RMCF0603JG330KCT-ND" x="18.796" y="25.654" size="1.778" layer="27" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="18.796" y="25.654" size="1.778" layer="27" display="off"/>
<attribute name="POPULATED" value="TRUE" x="18.796" y="25.654" size="1.778" layer="27" display="off"/>
<attribute name="CLASS" value="RESISTOR" x="18.796" y="25.654" size="1.778" layer="27" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/stackpole-electronics-inc/RMCF0603JG330K/RMCF0603JG330KCT-ND/6053832" x="18.796" y="25.654" size="1.778" layer="27" display="off"/>
</element>
<element name="R5" library="rc-sysmocom" package="_0603" value="100" x="18.542" y="6.35" smashed="yes">
<attribute name="NAME" x="16.9545" y="7.3025" size="1.016" layer="25" font="vector" ratio="14"/>
<attribute name="VALUE" x="16.9545" y="4.8577" size="0.508" layer="27" font="vector" ratio="10"/>
<attribute name="DESCRIPTION" value="RES 100 OHM 5%% 1/10W 0603" x="18.542" y="6.35" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURER" value="Stackpole Electronics Inc" x="18.542" y="6.35" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RMCF0603JT100R" x="18.542" y="6.35" size="1.778" layer="27" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="18.542" y="6.35" size="1.778" layer="27" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="RMCF0603JT100RCT-ND" x="18.542" y="6.35" size="1.778" layer="27" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="18.542" y="6.35" size="1.778" layer="27" display="off"/>
<attribute name="POPULATED" value="TRUE" x="18.542" y="6.35" size="1.778" layer="27" display="off"/>
<attribute name="CLASS" value="RESISTOR" x="18.542" y="6.35" size="1.778" layer="27" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/stackpole-electronics-inc/RMCF0603JT100R/RMCF0603JT100RCT-ND/1943156" x="18.542" y="6.35" size="1.778" layer="27" display="off"/>
</element>
<element name="R6" library="rc-sysmocom" package="_0603" value="100" x="16.002" y="5.588" smashed="yes" rot="R270">
<attribute name="NAME" x="16.5735" y="7.5565" size="1.016" layer="25" font="vector" ratio="14" rot="R90"/>
<attribute name="VALUE" x="14.5097" y="7.1755" size="0.508" layer="27" font="vector" ratio="10" rot="R270"/>
<attribute name="DESCRIPTION" value="RES 100 OHM 5%% 1/10W 0603" x="16.002" y="5.588" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="MANUFACTURER" value="Stackpole Electronics Inc" x="16.002" y="5.588" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RMCF0603JT100R" x="16.002" y="5.588" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="16.002" y="5.588" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="RMCF0603JT100RCT-ND" x="16.002" y="5.588" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="16.002" y="5.588" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="POPULATED" value="TRUE" x="16.002" y="5.588" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="CLASS" value="RESISTOR" x="16.002" y="5.588" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/stackpole-electronics-inc/RMCF0603JT100R/RMCF0603JT100RCT-ND/1943156" x="16.002" y="5.588" size="1.778" layer="27" rot="R270" display="off"/>
</element>
<element name="R7" library="rc-sysmocom" package="_0603" value="100" x="18.542" y="19.05" smashed="yes">
<attribute name="NAME" x="16.9545" y="20.0025" size="1.016" layer="25" font="vector" ratio="14"/>
<attribute name="VALUE" x="16.9545" y="17.5577" size="0.508" layer="27" font="vector" ratio="10"/>
<attribute name="DESCRIPTION" value="RES 100 OHM 5%% 1/10W 0603" x="18.542" y="19.05" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURER" value="Stackpole Electronics Inc" x="18.542" y="19.05" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RMCF0603JT100R" x="18.542" y="19.05" size="1.778" layer="27" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="18.542" y="19.05" size="1.778" layer="27" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="RMCF0603JT100RCT-ND" x="18.542" y="19.05" size="1.778" layer="27" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="18.542" y="19.05" size="1.778" layer="27" display="off"/>
<attribute name="POPULATED" value="TRUE" x="18.542" y="19.05" size="1.778" layer="27" display="off"/>
<attribute name="CLASS" value="RESISTOR" x="18.542" y="19.05" size="1.778" layer="27" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/stackpole-electronics-inc/RMCF0603JT100R/RMCF0603JT100RCT-ND/1943156" x="18.542" y="19.05" size="1.778" layer="27" display="off"/>
</element>
<element name="R8" library="rc-sysmocom" package="_0603" value="100" x="16.002" y="18.288" smashed="yes" rot="R270">
<attribute name="NAME" x="15.6845" y="16.5735" size="1.016" layer="25" font="vector" ratio="14" rot="R270"/>
<attribute name="VALUE" x="14.5097" y="19.8755" size="0.508" layer="27" font="vector" ratio="10" rot="R270"/>
<attribute name="DESCRIPTION" value="RES 100 OHM 5%% 1/10W 0603" x="16.002" y="18.288" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="MANUFACTURER" value="Stackpole Electronics Inc" x="16.002" y="18.288" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RMCF0603JT100R" x="16.002" y="18.288" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="16.002" y="18.288" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="RMCF0603JT100RCT-ND" x="16.002" y="18.288" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="16.002" y="18.288" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="POPULATED" value="TRUE" x="16.002" y="18.288" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="CLASS" value="RESISTOR" x="16.002" y="18.288" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/stackpole-electronics-inc/RMCF0603JT100R/RMCF0603JT100RCT-ND/1943156" x="16.002" y="18.288" size="1.778" layer="27" rot="R270" display="off"/>
</element>
<element name="R9" library="rc-sysmocom" package="_0603" value="49.9" x="14.478" y="59.436" smashed="yes" rot="R270">
<attribute name="NAME" x="14.1605" y="57.7215" size="1.016" layer="25" font="vector" ratio="14" rot="R270"/>
<attribute name="VALUE" x="12.9857" y="61.0235" size="0.508" layer="27" font="vector" ratio="10" rot="R270"/>
<attribute name="DESCRIPTION" value="RES 49.9 OHM 1%% 1/10W 0603" x="14.478" y="59.436" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="MANUFACTURER" value="Stackpole Electronics Inc" x="14.478" y="59.436" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RMCF0603FT49R9" x="14.478" y="59.436" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="14.478" y="59.436" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="RMCF0603FT49R9CT-ND" x="14.478" y="59.436" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="14.478" y="59.436" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="POPULATED" value="TRUE" x="14.478" y="59.436" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="CLASS" value="RESISTOR" x="14.478" y="59.436" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/stackpole-electronics-inc/RMCF0603FT49R9/RMCF0603FT49R9CT-ND/1942956" x="14.478" y="59.436" size="1.778" layer="27" rot="R270" display="off"/>
</element>
<element name="U1" library="cdclvc-clockbuf" package="MSOP12" value="LTC6957-4" x="25.146" y="30.988" smashed="yes" rot="R180">
<attribute name="NAME" x="24.608" y="27.929" size="1.27" layer="21" font="vector" ratio="14"/>
<attribute name="DESCRIPTION" value="IC CLK BUFFER DVR 1:2 12MSOP" x="25.146" y="30.988" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="MANUFACTURER" value="Linear Technology/Analog Devices" x="25.146" y="30.988" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="LTC6957IMS-3#PBF" x="25.146" y="30.988" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="25.146" y="30.988" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="LTC6957IMS-3#PBF-ND" x="25.146" y="30.988" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="25.146" y="30.988" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="POPULATED" value="TRUE" x="25.146" y="30.988" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="CLASS" value="IC" x="25.146" y="30.988" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/linear-technology-analog-devices/LTC6957IMS-3-PBF/LTC6957IMS-3-PBF-ND/3973487" x="25.146" y="30.988" size="1.778" layer="27" rot="R180" display="off"/>
</element>
<element name="U2" library="ldo" package="SOT23L" value="ADP151AUJZ" x="33.528" y="88.392" smashed="yes" rot="R180">
<attribute name="NAME" x="32.385" y="90.551" size="1.016" layer="25" font="vector" ratio="14"/>
<attribute name="VALUE" x="30.099" y="90.297" size="1.27" layer="27" ratio="17" rot="R270"/>
<attribute name="DESCRIPTION" value="IC REG LINEAR 3V 200MA TSOT5" x="33.528" y="88.392" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="MANUFACTURER" value="Analog Devices Inc." x="33.528" y="88.392" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="ADP151AUJZ-3.0-R7" x="33.528" y="88.392" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="33.528" y="88.392" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="ADP151AUJZ-3.0-R7CT-ND" x="33.528" y="88.392" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="33.528" y="88.392" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="POPULATED" value="TRUE" x="33.528" y="88.392" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="CLASS" value="IC" x="33.528" y="88.392" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/analog-devices-inc/ADP151AUJZ-3.0-R7/ADP151AUJZ-3.0-R7CT-ND/2334207" x="33.528" y="88.392" size="1.778" layer="27" rot="R180" display="off"/>
</element>
<element name="X1" library="laforge" package="HRS_UFL" value="IN+" x="11.176" y="60.198" smashed="yes" rot="R90">
<attribute name="OC_DIGIKEY" value="H9161CT-ND" x="11.176" y="60.198" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="NAME" x="11.176" y="57.198" size="1.016" layer="25" font="vector" ratio="14" rot="R180" align="center"/>
<attribute name="VALUE" x="11.176" y="63.198" size="1.27" layer="27" rot="R180" align="center"/>
<attribute name="DESCRIPTION" value="CONN U.FL RCPT STR 50 OHM SMD" x="11.176" y="60.198" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MANUFACTURER" value="Hirose Electric Co Ltd" x="11.176" y="60.198" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="U.FL-R-SMT(10)" x="11.176" y="60.198" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="11.176" y="60.198" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="H9161CT-ND" x="11.176" y="60.198" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="11.176" y="60.198" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="POPULATED" value="TRUE" x="11.176" y="60.198" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="CLASS" value="CONNECTOR" x="11.176" y="60.198" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/hirose-electric-co-ltd/U.FL-R-SMT-10/H9161CT-ND/2135256" x="11.176" y="60.198" size="1.778" layer="27" rot="R90" display="off"/>
</element>
<element name="X2" library="laforge" package="HRS_UFL" value="IN-" x="11.176" y="44.45" smashed="yes" rot="R90">
<attribute name="OC_DIGIKEY" value="H9161CT-ND" x="11.176" y="44.45" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="NAME" x="11.176" y="41.45" size="1.016" layer="25" font="vector" ratio="14" rot="R180" align="center"/>
<attribute name="VALUE" x="11.176" y="47.45" size="1.27" layer="27" rot="R180" align="center"/>
<attribute name="DESCRIPTION" value="CONN U.FL RCPT STR 50 OHM SMD" x="11.176" y="44.45" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MANUFACTURER" value="Hirose Electric Co Ltd" x="11.176" y="44.45" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="U.FL-R-SMT(10)" x="11.176" y="44.45" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="11.176" y="44.45" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="H9161CT-ND" x="11.176" y="44.45" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="11.176" y="44.45" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="POPULATED" value="TRUE" x="11.176" y="44.45" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="CLASS" value="CONNECTOR" x="11.176" y="44.45" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/hirose-electric-co-ltd/U.FL-R-SMT-10/H9161CT-ND/2135256" x="11.176" y="44.45" size="1.778" layer="27" rot="R90" display="off"/>
</element>
<element name="X3" library="laforge" package="HRS_UFL" value="OUT1" x="11.176" y="6.35" smashed="yes" rot="R90">
<attribute name="OC_DIGIKEY" value="H9161CT-ND" x="11.176" y="6.35" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="NAME" x="11.176" y="3.35" size="1.016" layer="25" font="vector" ratio="14" rot="R180" align="center"/>
<attribute name="VALUE" x="11.176" y="9.35" size="1.27" layer="27" rot="R180" align="center"/>
<attribute name="DESCRIPTION" value="CONN U.FL RCPT STR 50 OHM SMD" x="11.176" y="6.35" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MANUFACTURER" value="Hirose Electric Co Ltd" x="11.176" y="6.35" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="U.FL-R-SMT(10)" x="11.176" y="6.35" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="11.176" y="6.35" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="H9161CT-ND" x="11.176" y="6.35" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="11.176" y="6.35" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="POPULATED" value="TRUE" x="11.176" y="6.35" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="CLASS" value="CONNECTOR" x="11.176" y="6.35" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/hirose-electric-co-ltd/U.FL-R-SMT-10/H9161CT-ND/2135256" x="11.176" y="6.35" size="1.778" layer="27" rot="R90" display="off"/>
</element>
<element name="X4" library="laforge" package="HRS_UFL" value="OUT2" x="11.176" y="19.05" smashed="yes" rot="R90">
<attribute name="OC_DIGIKEY" value="H9161CT-ND" x="11.176" y="19.05" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="NAME" x="11.176" y="16.05" size="1.016" layer="25" font="vector" ratio="14" rot="R180" align="center"/>
<attribute name="VALUE" x="11.176" y="22.05" size="1.27" layer="27" rot="R180" align="center"/>
<attribute name="DESCRIPTION" value="CONN U.FL RCPT STR 50 OHM SMD" x="11.176" y="19.05" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MANUFACTURER" value="Hirose Electric Co Ltd" x="11.176" y="19.05" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="U.FL-R-SMT(10)" x="11.176" y="19.05" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="11.176" y="19.05" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="H9161CT-ND" x="11.176" y="19.05" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="11.176" y="19.05" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="POPULATED" value="TRUE" x="11.176" y="19.05" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="CLASS" value="CONNECTOR" x="11.176" y="19.05" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/hirose-electric-co-ltd/U.FL-R-SMT-10/H9161CT-ND/2135256" x="11.176" y="19.05" size="1.778" layer="27" rot="R90" display="off"/>
</element>
<element name="X5" library="laforge" package="SMA-F-S-TH" value="IN+" x="5.08" y="60.198" locked="yes" smashed="yes">
<attribute name="NAME" x="1.27" y="64.3255" size="1.016" layer="25" font="vector" ratio="14"/>
<attribute name="VALUE" x="1.27" y="54.8005" size="1.27" layer="27" font="vector" ratio="10"/>
<attribute name="DESCRIPTION" value="CONN SMA JACK R/A 50 OHM PCB" x="5.08" y="60.198" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURER" value="TE Connectivity AMP Connectors" x="5.08" y="60.198" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="619540-1" x="5.08" y="60.198" size="1.778" layer="27" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="5.08" y="60.198" size="1.778" layer="27" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="A120734-ND" x="5.08" y="60.198" size="1.778" layer="27" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="5.08" y="60.198" size="1.778" layer="27" display="off"/>
<attribute name="POPULATED" value="TRUE" x="5.08" y="60.198" size="1.778" layer="27" display="off"/>
<attribute name="CLASS" value="CONNECTOR" x="5.08" y="60.198" size="1.778" layer="27" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/te-connectivity-amp-connectors/619540-1/A120734-ND/5021655" x="5.08" y="60.198" size="1.778" layer="27" display="off"/>
</element>
<element name="X6" library="laforge" package="SMA-F-S-TH" value="IN-" x="5.08" y="44.45" locked="yes" smashed="yes">
<attribute name="NAME" x="1.27" y="48.5775" size="1.27" layer="25" font="vector" ratio="10"/>
<attribute name="VALUE" x="1.27" y="39.0525" size="1.27" layer="27" font="vector" ratio="10"/>
<attribute name="DESCRIPTION" value="CONN SMA JACK R/A 50 OHM PCB" x="5.08" y="44.45" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURER" value="TE Connectivity AMP Connectors" x="5.08" y="44.45" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="619540-1" x="5.08" y="44.45" size="1.778" layer="27" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="5.08" y="44.45" size="1.778" layer="27" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="A120734-ND" x="5.08" y="44.45" size="1.778" layer="27" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="5.08" y="44.45" size="1.778" layer="27" display="off"/>
<attribute name="POPULATED" value="TRUE" x="5.08" y="44.45" size="1.778" layer="27" display="off"/>
<attribute name="CLASS" value="CONNECTOR" x="5.08" y="44.45" size="1.778" layer="27" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/te-connectivity-amp-connectors/619540-1/A120734-ND/5021655" x="5.08" y="44.45" size="1.778" layer="27" display="off"/>
</element>
<element name="X7" library="laforge" package="SMA-F-S-TH" value="OUT1" x="5.08" y="6.35" locked="yes" smashed="yes" rot="R180">
<attribute name="NAME" x="8.89" y="2.2225" size="1.016" layer="25" font="vector" ratio="14" rot="R180"/>
<attribute name="VALUE" x="8.89" y="11.7475" size="1.27" layer="27" font="vector" ratio="10" rot="R180"/>
<attribute name="DESCRIPTION" value="CONN SMA JACK R/A 50 OHM PCB" x="5.08" y="6.35" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="MANUFACTURER" value="TE Connectivity AMP Connectors" x="5.08" y="6.35" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="619540-1" x="5.08" y="6.35" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="5.08" y="6.35" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="A120734-ND" x="5.08" y="6.35" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="5.08" y="6.35" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="POPULATED" value="TRUE" x="5.08" y="6.35" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="CLASS" value="CONNECTOR" x="5.08" y="6.35" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/te-connectivity-amp-connectors/619540-1/A120734-ND/5021655" x="5.08" y="6.35" size="1.778" layer="27" rot="R180" display="off"/>
</element>
<element name="X8" library="laforge" package="SMA-F-S-TH" value="OUT2" x="5.08" y="19.05" locked="yes" smashed="yes" rot="R180">
<attribute name="NAME" x="8.89" y="14.9225" size="1.016" layer="25" font="vector" ratio="14" rot="R180"/>
<attribute name="VALUE" x="8.89" y="24.4475" size="1.27" layer="27" font="vector" ratio="10" rot="R180"/>
<attribute name="DESCRIPTION" value="CONN SMA JACK R/A 50 OHM PCB" x="5.08" y="19.05" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="MANUFACTURER" value="TE Connectivity AMP Connectors" x="5.08" y="19.05" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="619540-1" x="5.08" y="19.05" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="5.08" y="19.05" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="A120734-ND" x="5.08" y="19.05" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="5.08" y="19.05" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="POPULATED" value="TRUE" x="5.08" y="19.05" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="CLASS" value="CONNECTOR" x="5.08" y="19.05" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/te-connectivity-amp-connectors/619540-1/A120734-ND/5021655" x="5.08" y="19.05" size="1.778" layer="27" rot="R180" display="off"/>
</element>
<element name="LED1" library="LED-PLCC2" package="PLCC2-MIN" value="green" x="9.652" y="68.834" locked="yes" smashed="yes">
<attribute name="NAME" x="7.874" y="65.659" size="1.016" layer="25" font="vector" ratio="14"/>
<attribute name="VALUE" x="7.112" y="65.659" size="1.27" layer="27" ratio="10"/>
<attribute name="DESCRIPTION" value="LED GREEN CLEAR 2PLCC SMD" x="9.652" y="68.834" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURER" value="OSRAM Opto Semiconductors Inc." x="9.652" y="68.834" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="LG T67F-R1T1-24" x="9.652" y="68.834" size="1.778" layer="27" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="9.652" y="68.834" size="1.778" layer="27" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="475-3413-1-ND" x="9.652" y="68.834" size="1.778" layer="27" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="9.652" y="68.834" size="1.778" layer="27" display="off"/>
<attribute name="POPULATED" value="TRUE" x="9.652" y="68.834" size="1.778" layer="27" display="off"/>
<attribute name="CLASS" value="LED" x="9.652" y="68.834" size="1.778" layer="27" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/osram-opto-semiconductors-inc/LG-T67F-R1T1-24/475-3413-1-ND/7908021" x="9.652" y="68.834" size="1.778" layer="27" display="off"/>
</element>
<element name="LED2" library="LED-PLCC2" package="PLCC2-MIN" value="yellow" x="15.494" y="68.834" locked="yes" smashed="yes">
<attribute name="NAME" x="12.954" y="65.659" size="1.016" layer="25" font="vector" ratio="14"/>
<attribute name="VALUE" x="12.954" y="65.659" size="1.27" layer="27" ratio="10"/>
<attribute name="DESCRIPTION" value="LED YELLOW CLEAR 2PLCC SMD" x="15.494" y="68.834" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURER" value="OSRAM Opto Semiconductors Inc." x="15.494" y="68.834" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="LY T676-S1T1-26-Z" x="15.494" y="68.834" size="1.778" layer="27" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="15.494" y="68.834" size="1.778" layer="27" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="475-2665-1-ND" x="15.494" y="68.834" size="1.778" layer="27" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="15.494" y="68.834" size="1.778" layer="27" display="off"/>
<attribute name="POPULATED" value="TRUE" x="15.494" y="68.834" size="1.778" layer="27" display="off"/>
<attribute name="CLASS" value="LED" x="15.494" y="68.834" size="1.778" layer="27" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/osram-opto-semiconductors-inc/LY-T676-S1T1-26-Z/475-2665-1-ND" x="15.494" y="68.834" size="1.778" layer="27" display="off"/>
</element>
<element name="M1" library="Mentor_lightpipe" package="1270.1001" value="MENTOR_12701001" x="5.842" y="68.834" locked="yes">
<attribute name="DESCRIPTION" value="NO DESCRIPTION" x="5.842" y="68.834" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER" x="5.842" y="68.834" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER" x="5.842" y="68.834" size="1.778" layer="27" display="off"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE" x="5.842" y="68.834" size="1.778" layer="27" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER" x="5.842" y="68.834" size="1.778" layer="27" display="off"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE" x="5.842" y="68.834" size="1.778" layer="27" display="off"/>
<attribute name="POPULATED" value="TRUE" x="5.842" y="68.834" size="1.778" layer="27" display="off"/>
<attribute name="CLASS" value="UNKNOWN CLASS" x="5.842" y="68.834" size="1.778" layer="27" display="off"/>
<attribute name="LINK" value="UNKNOWN LINK" x="5.842" y="68.834" size="1.778" layer="27" display="off"/>
</element>
<element name="R11" library="rc-sysmocom" package="_0603" value="330" x="8.89" y="71.882">
<attribute name="DESCRIPTION" value="RES 330 OHM 5%% 1/10W 0603" x="8.89" y="71.882" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURER" value="Stackpole Electronics Inc" x="8.89" y="71.882" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RMCF0603JT330R" x="8.89" y="71.882" size="1.778" layer="27" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="8.89" y="71.882" size="1.778" layer="27" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="RMCF0603JT330RCT-ND" x="8.89" y="71.882" size="1.778" layer="27" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="8.89" y="71.882" size="1.778" layer="27" display="off"/>
<attribute name="POPULATED" value="TRUE" x="8.89" y="71.882" size="1.778" layer="27" display="off"/>
<attribute name="CLASS" value="RESISTOR" x="8.89" y="71.882" size="1.778" layer="27" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/stackpole-electronics-inc/RMCF0603JT330R/RMCF0603JT330RCT-ND/1943164" x="8.89" y="71.882" size="1.778" layer="27" display="off"/>
</element>
<element name="R12" library="rc-sysmocom" package="_0603" value="330" x="14.732" y="71.628">
<attribute name="DESCRIPTION" value="RES 330 OHM 5%% 1/10W 0603" x="14.732" y="71.628" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURER" value="Stackpole Electronics Inc" x="14.732" y="71.628" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RMCF0603JT330R" x="14.732" y="71.628" size="1.778" layer="27" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="14.732" y="71.628" size="1.778" layer="27" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="RMCF0603JT330RCT-ND" x="14.732" y="71.628" size="1.778" layer="27" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="14.732" y="71.628" size="1.778" layer="27" display="off"/>
<attribute name="POPULATED" value="TRUE" x="14.732" y="71.628" size="1.778" layer="27" display="off"/>
<attribute name="CLASS" value="RESISTOR" x="14.732" y="71.628" size="1.778" layer="27" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/stackpole-electronics-inc/RMCF0603JT330R/RMCF0603JT330RCT-ND/1943164" x="14.732" y="71.628" size="1.778" layer="27" display="off"/>
</element>
<element name="C9" library="rc-sysmocom" package="_0603" value="10n" x="16.764" y="48.768" smashed="yes" rot="R270">
<attribute name="NAME" x="17.0815" y="51.4985" size="1.016" layer="25" font="vector" ratio="14" rot="R90"/>
<attribute name="VALUE" x="15.2717" y="50.3555" size="0.508" layer="27" font="vector" ratio="10" rot="R270"/>
<attribute name="DESCRIPTION" value="CAP CER 10000PF 50V X7R 0603" x="16.764" y="48.768" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="MANUFACTURER" value="KEMET" x="16.764" y="48.768" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="C0603C103M5RACTU" x="16.764" y="48.768" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="16.764" y="48.768" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="399-7842-1-ND" x="16.764" y="48.768" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="16.764" y="48.768" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="POPULATED" value="TRUE" x="16.764" y="48.768" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="CLASS" value="CAPACITOR" x="16.764" y="48.768" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/kemet/C0603C103M5RACTU/399-7842-1-ND/3471565" x="16.764" y="48.768" size="1.778" layer="27" rot="R270" display="off"/>
</element>
<element name="JP7" library="jumper" package="JP1" value="SE" x="19.558" y="48.26" smashed="yes">
<attribute name="NAME" x="20.193" y="51.308" size="1.016" layer="25" font="vector" ratio="14" rot="R90"/>
<attribute name="VALUE" x="22.479" y="45.72" size="1.27" layer="27" ratio="10" rot="R90"/>
<attribute name="DESCRIPTION" value="CONN HEADER VERT 2POS 2.54MM" x="19.558" y="48.26" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURER" value="Sullins Connector Solutions" x="19.558" y="48.26" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURERPARTNUMBER" value="PREC002SAAN-RC" x="19.558" y="48.26" size="1.778" layer="27" display="off"/>
<attribute name="SOURCE" value="DIGIKEY" x="19.558" y="48.26" size="1.778" layer="27" display="off"/>
<attribute name="SOURCEPARTNUMBER" value="S1012EC-02-ND" x="19.558" y="48.26" size="1.778" layer="27" display="off"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform" x="19.558" y="48.26" size="1.778" layer="27" display="off"/>
<attribute name="POPULATED" value="TRUE" x="19.558" y="48.26" size="1.778" layer="27" display="off"/>
<attribute name="CLASS" value="CONNECTOR\JUMPER" x="19.558" y="48.26" size="1.778" layer="27" display="off"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/PREC002SAAN-RC/S1012EC-02-ND/2774852" x="19.558" y="48.26" size="1.778" layer="27" display="off"/>
</element>
<element name="U$1" library="oshw" package="OSHW_8MM" value="" x="30.6075" y="9.0235"/>
</elements>
<signals>
<signal name="GND" class="2">
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="8"/>
<contactref element="U2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="C8" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="R10" pad="2"/>
<contactref element="X1" pad="GND@1"/>
<contactref element="X1" pad="GND@2"/>
<contactref element="X5" pad="G3"/>
<contactref element="X5" pad="G4"/>
<contactref element="X5" pad="G2"/>
<contactref element="X5" pad="G1"/>
<contactref element="X2" pad="GND@1"/>
<contactref element="X2" pad="GND@2"/>
<contactref element="X6" pad="G1"/>
<contactref element="X6" pad="G2"/>
<contactref element="X6" pad="G3"/>
<contactref element="X6" pad="G4"/>
<contactref element="D2" pad="1"/>
<contactref element="D3" pad="1"/>
<contactref element="X3" pad="GND@2"/>
<contactref element="X3" pad="GND@1"/>
<contactref element="X7" pad="G4"/>
<contactref element="X7" pad="G3"/>
<contactref element="X7" pad="G2"/>
<contactref element="X7" pad="G1"/>
<contactref element="X4" pad="GND@2"/>
<contactref element="X4" pad="GND@1"/>
<contactref element="X8" pad="G1"/>
<contactref element="X8" pad="G2"/>
<contactref element="X8" pad="G3"/>
<contactref element="X8" pad="G4"/>
<contactref element="D4" pad="1"/>
<contactref element="D1" pad="1"/>
<contactref element="D5" pad="A"/>
<contactref element="JP5" pad="2"/>
<contactref element="K1" pad="3"/>
<contactref element="K1" pad="2"/>
<contactref element="JP6" pad="4"/>
<contactref element="LED1" pad="K"/>
<contactref element="LED2" pad="K"/>
<polygon width="0.4064" layer="1" rank="6">
<vertex x="0" y="2"/>
<vertex x="50" y="2"/>
<vertex x="50" y="98"/>
<vertex x="0" y="98"/>
</polygon>
<via x="38.1" y="12.954" extent="1-16" drill="2.6" diameter="5"/>
<via x="11.176" y="12.7" extent="1-16" drill="2.6" diameter="5"/>
<via x="46.228" y="91.476" extent="1-16" drill="2.6" diameter="5"/>
<via x="15.24" y="82.55" extent="1-16" drill="2.6" diameter="5"/>
<contactref element="C9" pad="2"/>
</signal>
<signal name="VDD" class="2">
<contactref element="U1" pad="11"/>
<contactref element="C2" pad="1"/>
<contactref element="JP6" pad="3"/>
<contactref element="R12" pad="2"/>
<wire x1="26.121" y1="28.883" x2="26.121" y2="30.185" width="0.4064" layer="1"/>
<wire x1="26.121" y1="30.185" x2="26.416" y2="30.48" width="0.4064" layer="1"/>
<wire x1="26.416" y1="30.48" x2="28.956" y2="30.48" width="0.4064" layer="1"/>
<wire x1="29.718" y1="81.28" x2="29.718" y2="75.692" width="1.016" layer="1"/>
<wire x1="29.718" y1="75.692" x2="33.782" y2="71.628" width="1.016" layer="1"/>
<wire x1="33.782" y1="71.628" x2="33.782" y2="52.07" width="1.016" layer="1"/>
<wire x1="33.782" y1="52.07" x2="37.084" y2="48.768" width="1.016" layer="1"/>
<wire x1="37.084" y1="48.768" x2="37.084" y2="35.814" width="1.016" layer="1"/>
<wire x1="37.084" y1="35.814" x2="34.036" y2="32.766" width="1.016" layer="1"/>
<wire x1="34.036" y1="32.766" x2="32.258" y2="32.766" width="1.016" layer="1"/>
<wire x1="32.258" y1="32.766" x2="29.972" y2="30.48" width="1.016" layer="1"/>
<wire x1="29.972" y1="30.48" x2="28.956" y2="30.48" width="1.016" layer="1"/>
<wire x1="15.494" y1="71.628" x2="17.018" y2="71.628" width="0.4064" layer="1"/>
<via x="17.018" y="71.628" extent="1-16" drill="0.3" diameter="0.4064"/>
<wire x1="17.018" y1="71.628" x2="25.654" y2="71.628" width="0.4064" layer="16"/>
<wire x1="25.654" y1="71.628" x2="29.718" y2="75.692" width="0.4064" layer="16"/>
<via x="29.718" y="75.692" extent="1-16" drill="0.3" diameter="0.4064"/>
</signal>
<signal name="FILTA">
<contactref element="U1" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="JP1" pad="2"/>
<wire x1="26.771" y1="33.093" x2="26.771" y2="33.883" width="0.254" layer="1"/>
<wire x1="26.771" y1="33.883" x2="30.226" y2="37.338" width="0.254" layer="1"/>
<wire x1="30.226" y1="37.338" x2="30.226" y2="40.894" width="0.254" layer="1"/>
<wire x1="30.226" y1="40.894" x2="29.972" y2="41.148" width="0.254" layer="1"/>
<wire x1="29.972" y1="41.148" x2="32.766" y2="41.148" width="0.4064" layer="1"/>
</signal>
<signal name="FILTB">
<contactref element="U1" pad="6"/>
<contactref element="R2" pad="1"/>
<contactref element="JP2" pad="2"/>
<wire x1="17.526" y1="35.306" x2="17.526" y2="33.274" width="0.6096" layer="1"/>
<wire x1="17.526" y1="33.274" x2="18.034" y2="32.766" width="0.6096" layer="1"/>
<wire x1="18.034" y1="32.766" x2="18.034" y2="32.258" width="0.4064" layer="1"/>
<wire x1="18.034" y1="32.258" x2="18.542" y2="31.75" width="0.4064" layer="1"/>
<wire x1="18.542" y1="31.75" x2="22.86" y2="31.75" width="0.4064" layer="1"/>
<wire x1="22.86" y1="31.75" x2="23.521" y2="32.411" width="0.4064" layer="1"/>
<wire x1="23.521" y1="32.411" x2="23.521" y2="33.093" width="0.4064" layer="1"/>
</signal>
<signal name="SD1">
<contactref element="U1" pad="12"/>
<contactref element="R3" pad="1"/>
<contactref element="JP3" pad="2"/>
<wire x1="26.771" y1="28.883" x2="30.254" y2="25.4" width="0.4064" layer="1"/>
<wire x1="30.254" y1="25.4" x2="31.496" y2="25.4" width="0.4064" layer="1"/>
<wire x1="31.496" y1="25.4" x2="32.004" y2="25.908" width="0.4064" layer="1"/>
<wire x1="32.004" y1="25.908" x2="34.036" y2="25.908" width="0.4064" layer="1"/>
</signal>
<signal name="SD2">
<contactref element="U1" pad="7"/>
<contactref element="R4" pad="1"/>
<contactref element="JP4" pad="2"/>
<wire x1="18.034" y1="25.654" x2="17.526" y2="26.162" width="0.4064" layer="1"/>
<wire x1="17.526" y1="26.162" x2="17.526" y2="28.194" width="0.4064" layer="1"/>
<wire x1="17.526" y1="28.194" x2="17.526" y2="29.464" width="0.4064" layer="1"/>
<wire x1="17.526" y1="29.464" x2="18.288" y2="30.226" width="0.4064" layer="1"/>
<wire x1="18.288" y1="30.226" x2="22.86" y2="30.226" width="0.4064" layer="1"/>
<wire x1="22.86" y1="30.226" x2="23.521" y2="29.565" width="0.4064" layer="1"/>
<wire x1="23.521" y1="29.565" x2="23.521" y2="28.883" width="0.4064" layer="1"/>
</signal>
<signal name="V+" class="2">
<contactref element="JP1" pad="3"/>
<contactref element="JP4" pad="3"/>
<contactref element="JP3" pad="3"/>
<contactref element="JP2" pad="3"/>
<contactref element="U1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="U2" pad="5"/>
<contactref element="C7" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="JP6" pad="2"/>
<contactref element="R11" pad="2"/>
<polygon width="0.4064" layer="16" rank="6">
<vertex x="0" y="2"/>
<vertex x="50" y="2"/>
<vertex x="50" y="98"/>
<vertex x="0" y="98"/>
</polygon>
<wire x1="34.478" y1="87.092" x2="34.508" y2="87.122" width="0.8128" layer="1"/>
<wire x1="34.508" y1="87.122" x2="36.068" y2="87.122" width="0.8128" layer="1"/>
<wire x1="36.068" y1="87.122" x2="38.1" y2="87.122" width="1.016" layer="1"/>
<polygon width="0.254" layer="1">
<vertex x="34.29" y="87.63"/>
<vertex x="39.116" y="87.63"/>
<vertex x="39.116" y="85.09"/>
<vertex x="34.29" y="85.09"/>
</polygon>
<via x="34.798" y="85.598" extent="1-16" drill="0.3" diameter="0.254"/>
<via x="36.068" y="85.598" extent="1-16" drill="0.3" diameter="0.254"/>
<via x="37.338" y="85.598" extent="1-16" drill="0.3" diameter="0.254"/>
<via x="38.354" y="85.598" extent="1-16" drill="0.3" diameter="0.254"/>
<wire x1="9.652" y1="71.882" x2="11.176" y2="71.882" width="0.4064" layer="1"/>
<via x="11.176" y="71.882" extent="1-16" drill="0.3" diameter="0.254"/>
<wire x1="11.176" y1="71.882" x2="24.13" y2="78.994" width="0.4064" layer="16"/>
<wire x1="24.13" y1="78.994" x2="25.654" y2="77.47" width="0.4064" layer="16"/>
<wire x1="26.121" y1="33.093" x2="26.121" y2="32.299" width="0.4064" layer="1"/>
<wire x1="26.121" y1="32.299" x2="26.416" y2="32.004" width="0.4064" layer="1"/>
<wire x1="26.416" y1="32.004" x2="28.194" y2="32.004" width="0.4064" layer="1"/>
<wire x1="28.194" y1="32.004" x2="28.956" y2="32.766" width="0.4064" layer="1"/>
<wire x1="28.956" y1="32.766" x2="27.94" y2="32.766" width="0.6096" layer="1"/>
<via x="27.94" y="32.766" extent="1-16" drill="0.3" diameter="0.4064"/>
<wire x1="27.94" y1="32.766" x2="27.94" y2="31.242" width="0.6096" layer="16"/>
</signal>
<signal name="N$2" class="1">
<contactref element="U1" pad="10"/>
<contactref element="C3" pad="2"/>
<wire x1="22.606" y1="6.35" x2="25.654" y2="9.398" width="1.1" layer="1" curve="90"/>
<wire x1="25.654" y1="9.398" x2="25.654" y2="26.924" width="1.1" layer="1"/>
<wire x1="25.654" y1="26.924" x2="25.654" y2="27.178" width="1.1" layer="1"/>
<wire x1="25.471" y1="28.883" x2="25.471" y2="27.107" width="0.4064" layer="1"/>
<wire x1="25.471" y1="27.107" x2="25.654" y2="26.924" width="0.4064" layer="1"/>
</signal>
<signal name="N$6" class="1">
<contactref element="C3" pad="1"/>
<contactref element="R5" pad="2"/>
<wire x1="19.304" y1="6.35" x2="21.082" y2="6.35" width="1.1" layer="1"/>
</signal>
<signal name="OUT1" class="1">
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="X3" pad="SIG"/>
<contactref element="D3" pad="2"/>
<contactref element="X7" pad="C"/>
<wire x1="5.08" y1="6.35" x2="12.6785" y2="6.35" width="1.1" layer="1"/>
<wire x1="12.6785" y1="6.35" x2="14.224" y2="6.35" width="1.1" layer="1"/>
<wire x1="14.224" y1="6.35" x2="14.224" y2="6.438" width="1.1" layer="1"/>
<wire x1="14.224" y1="6.438" x2="16.002" y2="6.438" width="1.1" layer="1"/>
<wire x1="16.002" y1="6.438" x2="16.002" y2="6.35" width="1.1" layer="1"/>
<wire x1="16.002" y1="6.35" x2="17.78" y2="6.35" width="1.1" layer="1"/>
</signal>
<signal name="N$8" class="1">
<contactref element="U1" pad="9"/>
<contactref element="C4" pad="2"/>
<wire x1="22.352" y1="19.05" x2="23.876" y2="20.574" width="1.1" layer="1" curve="90"/>
<wire x1="23.876" y1="20.574" x2="23.876" y2="26.924" width="1.1" layer="1"/>
<wire x1="24.821" y1="28.883" x2="24.821" y2="27.869" width="0.4064" layer="1"/>
<wire x1="24.821" y1="27.869" x2="23.876" y2="26.924" width="0.4064" layer="1"/>
</signal>
<signal name="N$9" class="1">
<contactref element="C4" pad="1"/>
<contactref element="R7" pad="2"/>
<wire x1="19.304" y1="19.05" x2="20.828" y2="19.05" width="1.1" layer="1"/>
</signal>
<signal name="OUT2" class="1">
<contactref element="R7" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="X4" pad="SIG"/>
<contactref element="D4" pad="2"/>
<contactref element="X8" pad="C"/>
<wire x1="5.08" y1="19.05" x2="12.6785" y2="19.05" width="1.1" layer="1"/>
<wire x1="12.6785" y1="19.05" x2="14.224" y2="19.05" width="1.1" layer="1"/>
<wire x1="14.224" y1="19.05" x2="14.224" y2="19.138" width="1.1" layer="1"/>
<wire x1="14.224" y1="19.138" x2="16.002" y2="19.138" width="1.1" layer="1"/>
<wire x1="16.002" y1="19.138" x2="16.002" y2="19.05" width="1.1" layer="1"/>
<wire x1="16.002" y1="19.05" x2="17.78" y2="19.05" width="1.1" layer="1"/>
</signal>
<signal name="IN+" class="1">
<contactref element="U1" pad="3"/>
<contactref element="C5" pad="1"/>
<wire x1="19.304" y1="60.198" x2="25.908" y2="53.594" width="1.1" layer="1" curve="-90"/>
<wire x1="25.908" y1="53.594" x2="25.908" y2="35.306" width="1.1" layer="1"/>
<wire x1="25.908" y1="35.306" x2="25.908" y2="35.052" width="1.1" layer="1"/>
<wire x1="25.471" y1="33.093" x2="25.471" y2="34.869" width="0.4064" layer="1"/>
<wire x1="25.471" y1="34.869" x2="25.908" y2="35.306" width="0.4064" layer="1"/>
</signal>
<signal name="N$12" class="1">
<contactref element="C5" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="X1" pad="SIG"/>
<contactref element="D1" pad="2"/>
<contactref element="X5" pad="C"/>
<wire x1="5.08" y1="60.198" x2="12.6785" y2="60.198" width="1.1" layer="1"/>
<wire x1="12.6785" y1="60.198" x2="14.478" y2="60.198" width="1.1" layer="1"/>
<wire x1="14.478" y1="60.198" x2="14.566" y2="60.286" width="1.1" layer="1" curve="-90"/>
<wire x1="14.566" y1="60.286" x2="16.256" y2="60.286" width="1.1" layer="1"/>
<wire x1="16.256" y1="60.286" x2="16.344" y2="60.198" width="1.1" layer="1" curve="90"/>
<wire x1="16.344" y1="60.198" x2="17.78" y2="60.198" width="1.1" layer="1"/>
</signal>
<signal name="V_IN" class="2">
<contactref element="C8" pad="2"/>
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="C6" pad="2"/>
<contactref element="F1" pad="1"/>
<contactref element="D5" pad="C"/>
<contactref element="JP6" pad="1"/>
<wire x1="24.768" y1="89.154" x2="25.4" y2="89.786" width="1.6764" layer="1"/>
<wire x1="25.4" y1="89.786" x2="25.4" y2="91.7575" width="1.6764" layer="1"/>
<wire x1="25.4" y1="89.786" x2="25.524" y2="89.662" width="1.4224" layer="1"/>
<wire x1="25.524" y1="89.662" x2="28.956" y2="89.662" width="1.4224" layer="1"/>
<wire x1="28.956" y1="89.662" x2="30.988" y2="89.662" width="1.4224" layer="1"/>
<wire x1="30.988" y1="89.662" x2="31.018" y2="89.692" width="0.8128" layer="1"/>
<wire x1="31.018" y1="89.692" x2="32.578" y2="89.692" width="0.8128" layer="1"/>
<wire x1="32.578" y1="89.692" x2="32.512" y2="89.758" width="0.8128" layer="1"/>
<wire x1="32.512" y1="89.758" x2="32.512" y2="90.678" width="0.8128" layer="1"/>
<wire x1="32.512" y1="90.678" x2="32.766" y2="90.932" width="0.8128" layer="1"/>
<wire x1="32.766" y1="90.932" x2="34.036" y2="90.932" width="0.8128" layer="1"/>
<wire x1="34.036" y1="90.932" x2="34.478" y2="90.49" width="0.8128" layer="1"/>
<wire x1="34.478" y1="90.49" x2="34.478" y2="89.692" width="0.8128" layer="1"/>
<wire x1="24.638" y1="81.28" x2="24.768" y2="83.69" width="1.27" layer="1"/>
<wire x1="24.768" y1="83.69" x2="24.768" y2="89.154" width="1.27" layer="1"/>
</signal>
<signal name="N$7" class="1">
<contactref element="U1" pad="4"/>
<contactref element="C11" pad="1"/>
<wire x1="19.05" y1="44.45" x2="24.13" y2="39.37" width="1.1" layer="1" curve="-90"/>
<wire x1="24.13" y1="39.37" x2="24.13" y2="35.052" width="1.1" layer="1"/>
<wire x1="24.13" y1="35.052" x2="24.821" y2="34.361" width="0.4064" layer="1"/>
<wire x1="24.821" y1="34.361" x2="24.821" y2="33.093" width="0.4064" layer="1"/>
<contactref element="JP7" pad="1"/>
<wire x1="19.05" y1="44.45" x2="19.05" y2="46.482" width="1.1" layer="1"/>
<wire x1="19.05" y1="46.482" x2="19.558" y2="46.99" width="1.1" layer="1"/>
</signal>
<signal name="N$10" class="1">
<contactref element="C11" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="X2" pad="SIG"/>
<contactref element="D2" pad="2"/>
<contactref element="X6" pad="C"/>
<wire x1="5.08" y1="44.45" x2="12.6785" y2="44.45" width="1.1" layer="1"/>
<wire x1="12.6785" y1="44.45" x2="14.224" y2="44.45" width="1.1" layer="1"/>
<wire x1="14.224" y1="44.45" x2="16.002" y2="44.45" width="1.1" layer="1"/>
<wire x1="16.002" y1="44.45" x2="16.002" y2="44.538" width="1.1" layer="1"/>
<wire x1="16.002" y1="44.538" x2="16.09" y2="44.45" width="1.1" layer="1" curve="90"/>
<wire x1="16.09" y1="44.45" x2="17.526" y2="44.45" width="1.1" layer="1"/>
</signal>
<signal name="N$5" class="2">
<contactref element="D6" pad="C"/>
<contactref element="F1" pad="2"/>
<wire x1="21.59" y1="91.7575" x2="21.968" y2="91.3795" width="1.6764" layer="1"/>
<wire x1="21.968" y1="91.3795" x2="21.968" y2="89.154" width="1.6764" layer="1"/>
</signal>
<signal name="N$14" class="2">
<contactref element="JP5" pad="1"/>
<contactref element="D6" pad="A"/>
<contactref element="K1" pad="1"/>
<contactref element="K1" pad="1-1"/>
<wire x1="3.725" y1="96.431" x2="9.875" y2="96.431" width="1.6764" layer="1"/>
<wire x1="9.875" y1="96.431" x2="10.04" y2="96.266" width="1.6764" layer="1"/>
<wire x1="10.04" y1="96.266" x2="17.526" y2="96.266" width="1.6764" layer="1"/>
<wire x1="17.526" y1="96.266" x2="17.5895" y2="96.2025" width="1.6764" layer="1"/>
<wire x1="17.5895" y1="96.2025" x2="21.59" y2="96.2025" width="1.6764" layer="1"/>
</signal>
<signal name="N$1">
<contactref element="LED1" pad="A"/>
<contactref element="R11" pad="1"/>
<wire x1="8.128" y1="68.834" x2="8.128" y2="71.882" width="0.4064" layer="1"/>
</signal>
<signal name="N$3">
<contactref element="LED2" pad="A"/>
<contactref element="R12" pad="1"/>
<wire x1="13.97" y1="68.834" x2="13.97" y2="71.628" width="0.4064" layer="1"/>
</signal>
<signal name="N$4">
<contactref element="C9" pad="1"/>
<contactref element="JP7" pad="2"/>
<wire x1="16.764" y1="49.53" x2="19.558" y2="49.53" width="0.8128" layer="1"/>
</signal>
</signals>
</board>
</drawing>
<compatibility>
<note version="6.3" minversion="6.2.2" severity="warning">
Since Version 6.2.2 text objects can contain more than one line,
which will not be processed correctly with this version.
</note>
</compatibility>
</eagle>
