<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="43.876" y1="0" x2="-26.124" y2="0" width="0" layer="20"/>
<wire x1="-26.124" y1="0" x2="-26.124" y2="70" width="0" layer="20"/>
<wire x1="-26.124" y1="70" x2="43.876" y2="70" width="0" layer="20"/>
<wire x1="43.876" y1="70" x2="43.876" y2="0" width="0" layer="20"/>
<text>GTM900 breakout</text>
<text>(C) 2020 sysmocom GmbH
License: CC-BY-SA</text>
<text>&gt;VERSION</text>
<text>1</text>
<text>DC
IN</text>
<text>6.5V max!</text>
<text>GTM900 breakout</text>
<text>(C) 2020 sysmocom GmbH
License: CC-BY-SA</text>
<text>&gt;VERSION</text>
<text>!PWRON</text>
<text>PWR</text>
<text>MDM</text>
<text>PWON</text>
<text>RESET</text>
<text>1</text>
<text>1</text>
<text>USB</text>
</plain>
<libraries>
<library name="SF7W008S1A-SIM">
<packages>
<package name="SF7W008S1A-RESTR">
<description>JAE SF7W008S1A SIM card holder with lock and card detect switch - additional restrict areas for SIM contacts</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="JP1">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
<package name="JP2">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="rc-sysmocom">
<packages>
<package name="_0603">
<description>&lt;b&gt;0603&lt;/b&gt;</description>
</package>
<package name="_0805">
<description>&lt;b&gt;0805&lt;/b&gt;</description>
</package>
<package name="_0402">
<description>&lt;b&gt; 0402&lt;/b&gt;</description>
</package>
<package name="1206">
<description>&lt;b&gt;1206 (3216 Metric)&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="laforge">
<description>&lt;b&gt;PCB Matrix Packages&lt;/b&gt;&lt;p&gt;</description>
<packages>
<package name="SMA-F-S-TH">
</package>
<package name="HRS_UFL">
<description>&lt;b&gt;Hirose U.FL SMT&lt;/b&gt;</description>
</package>
<package name="SOT666">
<description>SOT666 package outline (NXP semiconductors, taken from PED5V0U5BV DS 04-11-08)</description>
</package>
<package name="WEEE_BIN">
</package>
<package name="TSOP-6">
<description>TSOP-6 CAS E318G-02 ISSUE V (ON Semiconductor)</description>
</package>
<package name="1X03">
</package>
<package name="JACK2.5_SJ-2523">
</package>
<package name="VQFN-N16">
</package>
</packages>
</library>
<library name="ldo">
<description>&lt;b&gt;PCB Matrix Packages&lt;/b&gt;&lt;p&gt;</description>
<packages>
<package name="TI_KTT_DPAK2">
<description>KTT (R-PSFM-G5) Plastic Flange Mount Package</description>
</package>
<package name="SC70-5">
</package>
</packages>
</library>
<library name="Wurth_Elektronik_Electromechanic_DC_Power_Jack_Connectors_rev15c">
<description>&lt;BR&gt;Wurth Elektronik - DC Power Jack Connectors&lt;br&gt;&lt;Hr&gt;
&lt;BR&gt;&lt;BR&gt; 
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-405&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/eagle"&gt;http://www.we-online.com/eagle &lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither CadSoft nor WE-eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;&lt;BR&gt;&lt;br&gt;
&lt;hr&gt;
Eagle Version 6, Library Revision 2015c, 2015-06-02&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="694108106102">
<description>&lt;b&gt;694108106102&lt;/b&gt;&lt;p&gt;

WR-DC_DC Power Jack_Right Angled_SMT Center Pin Ø2.5_Plug ID Ø2.55_Plug OD Ø5.5_with 4 Soldering Pad &amp; Peg</description>
</package>
</packages>
</library>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="UD-8X10_NICHICON">
<description>&lt;b&gt;ALUMINUM ELECTROLYTIC CAPACITORS&lt;/b&gt; UD Series 8 x 10 mm&lt;p&gt;
Source: http://products.nichicon.co.jp/en/pdf/XJA043/e-ud.pdf</description>
</package>
<package name="SMC_E">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
</packages>
</library>
<library name="FH12A-40S-0.5SH(55)">
<description>
</description>
<packages>
<package name="HIROSE_FH12A-40S-0.5SH(55)">
</package>
</packages>
</library>
<library name="GTM900">
<packages>
<package name="GTM900-WRTHSPACER">
</package>
</packages>
</library>
<library name="diodes-sysmocom">
<packages>
<package name="SMBDIODE">
<description>SMB(J)</description>
</package>
<package name="_0402">
<description>&lt;b&gt; 0402&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="microbuilder">
<description>&lt;h2&gt;&lt;b&gt;microBuilder.eu&lt;/b&gt; Eagle Footprint Library&lt;/h2&gt;

&lt;p&gt;Footprints for common components used in our projects and products.  This is the same library that we use internally, and it is regularly updated.  The newest version can always be found at &lt;b&gt;www.microBuilder.eu&lt;/b&gt;.  If you find this library useful, please feel free to purchase something from our online store. Please also note that all holes are optimised for metric drill bits!&lt;/p&gt;

&lt;h3&gt;Obligatory Warning&lt;/h3&gt;
&lt;p&gt;While it probably goes without saying, there are no guarantees that the footprints or schematic symbols in this library are flawless, and we make no promises of fitness for production, prototyping or any other purpose. These libraries are provided for information puposes only, and are used at your own discretion.  While we make every effort to produce accurate footprints, and many of the items found in this library have be proven in production, we can't make any promises of suitability for a specific purpose. If you do find any errors, though, please feel free to contact us at www.microbuilder.eu to let us know about it so that we can update the library accordingly!&lt;/p&gt;

&lt;h3&gt;License&lt;/h3&gt;
&lt;p&gt;This work is placed in the public domain, and may be freely used for commercial and non-commercial work with the following conditions:&lt;/p&gt;
&lt;p&gt;THIS SOFTWARE IS PROVIDED ''AS IS'' AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED.  IN NO EVENT SHALL THE INSTITUTE OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING,  BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
&lt;/p&gt;</description>
<packages>
<package name="EVQ-Q2">
</package>
<package name="1X04_ROUND_76">
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23-BEC">
<description>TO-236 ITT Intermetall</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<packages>
<package name="AUDIO-JACK-TRRS-SMD">
</package>
</packages>
</library>
<library name="con-hirose">
<description>&lt;b&gt;Hirose Connectors&lt;/b&gt;&lt;p&gt;
www.hirose.co.jp&lt;p&gt;
Include : &lt;br&gt;
con-hirose-df12d(3.0)60dp0.5v80.lbr from Bob Starr &amp;lt;rtzaudio@mindspring.com&amp;gt;&lt;br&gt;
con-hirose.lbr from Bob Starr &amp;lt;rtzaudio@mindspring.com&amp;gt;&lt;br&gt;</description>
<packages>
<package name="UX60-MB-5ST">
<description>&lt;b&gt;MINI USB Connector HI-SPEED Certified&lt;/b&gt; Metal Shield SMT Type With Positioning Post&lt;p&gt;
Source: http://www.hirose.co.jp/cataloge_hp/e24000019.pdf</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP10R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="oshw">
<description>&lt;p&gt;&lt;strong&gt;Open Source Hardware PCB Logos&lt;/strong&gt;
&lt;p&gt;A simple polygon based version of the OSHWA logos for use on Eagle PCB's
&lt;p&gt;For use please refer to the OSHWA definition at &lt;a href="http://www.oshwa.org/definition/"&gt;http://www.oshwa.org/definition/&lt;/a&gt;
&lt;p&gt;Based on the NBitWonder version (&lt;a href="http://nbitwonder.com"&gt;http://nbitwonder.com&lt;/a&gt;)
&lt;p&gt;&lt;strong&gt;Andrew Cooper&lt;/strong&gt;&lt;br&gt;28Nov2016&lt;br&gt;&lt;a href="http://www.darkerview.com"&gt;www.DarkerView.com&lt;/a&gt;</description>
<packages>
<package name="OSHW_8MM_COPPER">
</package>
</packages>
</library>
<library name="NCP303">
<description>
</description>
<packages>
<package name="SOT23-5">
<description>
</description>
</package>
</packages>
</library>
<library name="silabs_CP2102X">
<packages>
<package name="QFN28">
<description>&lt;b&gt;QFN28&lt;/b&gt;&lt;p&gt;
Source: www.silabs.com .. CP210X.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<packages>
<package name="OSHW-LOGO-S">
</package>
</packages>
</library>
</libraries>
<attributes>
<attribute name="VERSION" value="v2"/>
</attributes>
<variantdefs>
<variantdef name="default (no gps)"/>
</variantdefs>
<elements>
<element name="SIM1" library="SF7W008S1A-SIM" package="SF7W008S1A-RESTR" value="SF7W008S1A-R">
<attribute name="OC_DIGIKEY" value="670-2985-1-ND"/>
<attribute name="DESCRIPTION" value="CONN SIM CARD HINGED TYPE R/A"/>
<attribute name="MANUFACTURER" value="JAE Electronics"/>
<attribute name="MANUFACTURERPARTNUMBER" value="SF7W008S1AR900"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="670-2985-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="UNKNOWN CLASS"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/jae-electronics/SF7W008S1AR900/670-2985-1-ND"/>
</element>
<element name="LED2" library="led" package="CHIP-LED0603" value="YELLOW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="LED"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
</element>
<element name="R3" library="rc-sysmocom" package="_0603" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="RES SMD 47 OHM 5%% 1/10W 0603"/>
<attribute name="MANUFACTURER" value="Yageo"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RC0603JR-0747RL"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="311-47GRCT-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/yageo/RC0603JR-0747RL/311-47GRCT-ND/729740"/>
</element>
<element name="R2" library="rc-sysmocom" package="_0603" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="RES SMD 47 OHM 5%% 1/10W 0603"/>
<attribute name="MANUFACTURER" value="Yageo"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RC0603JR-0747RL"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="311-47GRCT-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/yageo/RC0603JR-0747RL/311-47GRCT-ND/729740"/>
</element>
<element name="U2" library="ldo" package="TI_KTT_DPAK2" value="MCP1827T-ADJE/ET">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="IC REG LIN POS ADJ 1.5A 5DDPAK"/>
<attribute name="MANUFACTURER" value="Microchip Technology"/>
<attribute name="MANUFACTURERPARTNUMBER" value="MCP1827T-ADJE/ET"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="MCP1827T-ADJE/ETCT-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="IC"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/microchip-technology/MCP1827T-ADJE-ET/MCP1827T-ADJE-ETCT-ND/8538072"/>
</element>
<element name="C12" library="rc-sysmocom" package="_0805" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="CAP CER 10UF 16V X5R 0805"/>
<attribute name="MANUFACTURER" value="Murata Electronics"/>
<attribute name="MANUFACTURERPARTNUMBER" value="GRM21BR61C106KE15K"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="490-6473-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/murata-electronics/GRM21BR61C106KE15K/490-6473-1-ND"/>
</element>
<element name="C16" library="rc-sysmocom" package="_0805" value="10u">
<attribute name="DESCRIPTION" value="CAP CER 10UF 16V X5R 0805"/>
<attribute name="MANUFACTURER" value="Murata Electronics"/>
<attribute name="MANUFACTURERPARTNUMBER" value="GRM21BR61C106KE15K"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="490-6473-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/murata-electronics/GRM21BR61C106KE15K/490-6473-1-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="K1" library="Wurth_Elektronik_Electromechanic_DC_Power_Jack_Connectors_rev15c" package="694108106102" value="PJ-002BH-SMT-TR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="CONN PWR JACK 2.5X5.5MM SOLDER"/>
<attribute name="MANUFACTURER" value="CUI Devices"/>
<attribute name="MANUFACTURERPARTNUMBER" value="PJ-002BH-SMT-TR"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="CP-002BHPJCT-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CONNECTOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/cui-inc/PJ-002BH-SMT-TR/CP-002BHPJCT-ND"/>
</element>
<element name="C11" library="rcl" package="UD-8X10_NICHICON" value="470u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="CAP ALUM 470UF 20%% 6.3V SMD"/>
<attribute name="MANUFACTURER" value="Nichicon"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UUR0J471MNL1GS"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="493-6207-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/nichicon/UUR0J471MNL1GS/493-6207-1-ND/3438720"/>
</element>
<element name="C17" library="rcl" package="SMC_E" value="DNP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="FALSE"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
</element>
<element name="C8" library="rc-sysmocom" package="_0402" value="33p">
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics America, Inc."/>
<attribute name="SOURCEPARTNUMBER" value="1276-1272-1-ND"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/CL05C330JB5NNNC/1276-1272-1-ND/3889358"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL05C330JB5NNNC"/>
<attribute name="DESCRIPTION" value="CAP CER 33PF 50V NP0 0402"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="rc-sysmocom" package="_0603" value="10p">
<attribute name="MANUFACTURER" value="Kemet"/>
<attribute name="SOURCEPARTNUMBER" value="399-1049-1-ND"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/C0603C100J5GACTU/399-1049-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="C0603C100J5GACTU"/>
<attribute name="DESCRIPTION" value="CAP CER 10PF 50V NP0 0603"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="rc-sysmocom" package="_0603" value="100n">
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics America, Inc"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1005-1-ND"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/foo/1276-1005-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL10B104KO8NNNC"/>
<attribute name="DESCRIPTION" value="CAP CER 0.1UF 16V 10% X7R 0603"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="rc-sysmocom" package="1206" value="100u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="CAP CER 100UF 6.3V X5R 1206"/>
<attribute name="MANUFACTURER" value="Murata Electronics"/>
<attribute name="MANUFACTURERPARTNUMBER" value="GRM31CR60J107ME39K"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="490-7217-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/murata-electronics-north-america/GRM31CR60J107ME39K/490-7217-1-ND/3991203"/>
</element>
<element name="C3" library="rc-sysmocom" package="_0402" value="33p">
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics America, Inc."/>
<attribute name="SOURCEPARTNUMBER" value="1276-1272-1-ND"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/CL05C330JB5NNNC/1276-1272-1-ND/3889358"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL05C330JB5NNNC"/>
<attribute name="DESCRIPTION" value="CAP CER 33PF 50V NP0 0402"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rc-sysmocom" package="_0402" value="33p">
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics America, Inc."/>
<attribute name="SOURCEPARTNUMBER" value="1276-1272-1-ND"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/CL05C330JB5NNNC/1276-1272-1-ND/3889358"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL05C330JB5NNNC"/>
<attribute name="DESCRIPTION" value="CAP CER 33PF 50V NP0 0402"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="rc-sysmocom" package="_0402" value="33p">
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics America, Inc."/>
<attribute name="SOURCEPARTNUMBER" value="1276-1272-1-ND"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/CL05C330JB5NNNC/1276-1272-1-ND/3889358"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL05C330JB5NNNC"/>
<attribute name="DESCRIPTION" value="CAP CER 33PF 50V NP0 0402"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="rc-sysmocom" package="_0603" value="100n">
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics America, Inc"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1005-1-ND"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/foo/1276-1005-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL10B104KO8NNNC"/>
<attribute name="DESCRIPTION" value="CAP CER 0.1UF 16V 10% X7R 0603"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led" package="CHIP-LED0603" value="GREEN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="LED"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
</element>
<element name="R6" library="rc-sysmocom" package="_0603" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="RES SMD 330 OHM 5%% 1/10W 0603"/>
<attribute name="MANUFACTURER" value="Yageo"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RC0603JR-07330RL"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="311-330GRCT-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/yageo/RC0603JR-07330RL/311-330GRCT-ND/729716"/>
</element>
<element name="C5" library="rc-sysmocom" package="1206" value="100u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="CAP CER 100UF 6.3V X5R 1206"/>
<attribute name="MANUFACTURER" value="Murata Electronics"/>
<attribute name="MANUFACTURERPARTNUMBER" value="GRM31CR60J107ME39K"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="490-7217-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/murata-electronics-north-america/GRM31CR60J107ME39K/490-7217-1-ND/3991203"/>
</element>
<element name="C10" library="rc-sysmocom" package="1206" value="100u">
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/murata-electronics-north-america/GRM31CR60J107ME39K/490-7217-1-ND/3991203"/>
<attribute name="DESCRIPTION" value="CAP CER 100UF 6.3V X5R 1206"/>
<attribute name="MANUFACTURER" value="Murata Electronics"/>
<attribute name="MANUFACTURERPARTNUMBER" value="GRM31CR60J107ME39K"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="490-7217-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X2" library="laforge" package="SMA-F-S-TH" value="">
<attribute name="DESCRIPTION" value="CONN SMA JACK STR 50 OHM PCB"/>
<attribute name="MANUFACTURER" value="TE Connectivity AMP Connectors"/>
<attribute name="MANUFACTURERPARTNUMBER" value="5-1814832-1"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="A97594-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CONNECTOR"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/te-connectivity-amp-connectors/5-1814832-1/A97594-ND/1755982"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X3" library="laforge" package="HRS_UFL" value="">
<attribute name="OC_DIGIKEY" value="H9161CT-ND"/>
<attribute name="DESCRIPTION" value="CONN U.FL RCPT STR 50 OHM SMD"/>
<attribute name="MANUFACTURER" value="Hirose Electric Co Ltd"/>
<attribute name="MANUFACTURERPARTNUMBER" value="U.FL-R-SMT(01)"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="H9161-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CONNECTOR"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/hirose-electric-co-ltd/U.FL-R-SMT(01)/H9161-ND/513010"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="rc-sysmocom" package="_0603" value="200k">
<attribute name="MANUFACTURER" value="TE Connectivity"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="DESCRIPTION" value="RES 200K OHM 1/16W 1% 0603"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="A102235CT-ND"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/8-1879338-5/A102235CT-ND/2728211"/>
<attribute name="MANUFACTURERPARTNUMBER" value="8-1879338-5"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="rc-sysmocom" package="_0603" value="22k">
<attribute name="MANUFACTURER" value="Yageo"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="DESCRIPTION" value="RES SMD 22K OHM 1%% 1/10W 0603"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="311-22.0KHRCT-ND"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/yageo/RC0603FR-0722KL/311-22-0KHRCT-ND/730003"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RC0603FR-0722KL"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="laforge" package="SOT666" value="PESD5V0UBV">
<attribute name="MANUFACTURER" value="Nexperia USA Inc."/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="DESCRIPTION" value="TVS DIODE 5V SOT666"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="1727-5806-1-ND"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/nexperia-usa-inc/PESD5V0U5BV,115/1727-5806-1-ND"/>
<attribute name="OC_DIGIKEY" value="568-7356-1-ND"/>
<attribute name="MANUFACTURERPARTNUMBER" value="PESD5V0U5BV,115"/>
<attribute name="CLASS" value="DIODE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="rc-sysmocom" package="_0603" value="15k">
<attribute name="MANUFACTURER" value="Yageo"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="DESCRIPTION" value="RES SMD 15K OHM 1%% 1/10W 0603"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="311-15.0KHRCT-ND"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/yageo/RC0603FR-0715KL/311-15.0KHRCT-ND"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RC0603FR-0715KL"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MDM1" library="GTM900" package="GTM900-WRTHSPACER" value="GTM900-BM2-SPACER">
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="UNKNOWN CLASS"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
</element>
<element name="D3" library="diodes-sysmocom" package="SMBDIODE" value="SMBJP6KE6.8A-TP">
<attribute name="MANUFACTURER" value="Micro Commercial Co"/>
<attribute name="DESCRIPTION" value="TVS DIODE 5.8V 10.5V DO214AA"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/micro-commercial-co/SMBJP6KE6.8A-TP/SMBJP6KE6.8A-TPMSCT-ND"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="CLASS" value="DIODE"/>
<attribute name="MANUFACTURERPARTNUMBER" value="SMBJP6KE6.8A-TP"/>
<attribute name="SOURCEPARTNUMBER" value="SMBJP6KE6.8A-TPMSCT-ND"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="diodes-sysmocom" package="SMBDIODE" value="ACDBB540-HF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="DIODE SCHOTTKY 40V 5A DO214AA"/>
<attribute name="MANUFACTURER" value="Comchip Technology"/>
<attribute name="MANUFACTURERPARTNUMBER" value="ACDBB540-HF"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="641-1898-2-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="DIODE"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/comchip-technology/ACDBB540-HF/641-1898-2-ND"/>
</element>
<element name="U1" library="FH12A-40S-0.5SH(55)" package="HIROSE_FH12A-40S-0.5SH(55)" value="FH12A-40S-0.5SH(55)">
<attribute name="PACKAGE" value="SOCKET FFC/FPC, ZIF, 0.5MM, 40WAY"/>
<attribute name="SUPPLIER" value="Hirose"/>
<attribute name="OC_FARNELL" value="1324569"/>
<attribute name="MPN" value="FH12A-40S-0.5SH(55)"/>
<attribute name="OC_NEWARK" value="34M6194"/>
<attribute name="DESCRIPTION" value="CONN FFC TOP 40POS 0.50MM R/A"/>
<attribute name="MANUFACTURER" value="Hirose Electric Co Ltd"/>
<attribute name="MANUFACTURERPARTNUMBER" value="FH12A-40S-0.5SH(55)"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="HFK140CT-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CONNECTOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/hirose-electric-co-ltd/FH12A-40S-0-5SH-55/HFK140CT-ND/"/>
</element>
<element name="D4" library="diodes-sysmocom" package="_0402" value="GG040205170N2P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="TVS DIODE 5V 15.5V 0402"/>
<attribute name="MANUFACTURER" value="AVX Corporation"/>
<attribute name="MANUFACTURERPARTNUMBER" value="GG0402050R3C2P"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="478-10591-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="DIODE"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/avx-corporation/GG0402050R3C2P/478-10591-1-ND"/>
</element>
<element name="B1" library="microbuilder" package="EVQ-Q2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="SWITCH TACTILE SPST-NO 0.02A 15V"/>
<attribute name="MANUFACTURER" value="Panasonic Electronic Components"/>
<attribute name="MANUFACTURERPARTNUMBER" value="EVQ-Q2M03W"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="P12946SCT-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="TACT SWITCH"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/panasonic-electronic-components/EVQ-Q2M03W/P12946SCT-ND"/>
</element>
<element name="R12" library="rc-sysmocom" package="_0603" value="DNP">
<attribute name="MANUFACTURER" value="Yageo"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RC0603FR-0715KL"/>
<attribute name="POPULATED" value="FALSE"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="DESCRIPTION" value="RES SMD 15K OHM 1%% 1/10W 0603"/>
<attribute name="SOURCEPARTNUMBER" value="311-15.0KHRCT-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/yageo/RC0603FR-0715KL/311-15.0KHRCT-ND"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T3" library="transistor" package="SOT23-BEC" value="BC847">
<attribute name="CLASS" value="TRANSISTOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="BC847C,215"/>
<attribute name="DESCRIPTION" value="TRANS NPN 45V 0.1A SOT23"/>
<attribute name="SOURCEPARTNUMBER" value="1727-2924-1-ND"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/nexperia-usa-inc/BC847C,215/1727-2924-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Nexperia USA Inc."/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="rc-sysmocom" package="_0603" value="330">
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RC0603JR-07330RL"/>
<attribute name="DESCRIPTION" value="RES SMD 330 OHM 5%% 1/10W 0603"/>
<attribute name="SOURCEPARTNUMBER" value="311-330GRCT-ND"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/yageo/RC0603JR-07330RL/311-330GRCT-ND/729716"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Yageo"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="rc-sysmocom" package="_0603" value="22k">
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RC0603FR-0722KL"/>
<attribute name="DESCRIPTION" value="RES SMD 22K OHM 1%% 1/10W 0603"/>
<attribute name="SOURCEPARTNUMBER" value="311-22.0KHRCT-ND"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/yageo/RC0603FR-0722KL/311-22-0KHRCT-ND/730003"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Yageo"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="rc-sysmocom" package="_0603" value="22k">
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RC0603FR-0722KL"/>
<attribute name="DESCRIPTION" value="RES SMD 22K OHM 1%% 1/10W 0603"/>
<attribute name="SOURCEPARTNUMBER" value="311-22.0KHRCT-ND"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/yageo/RC0603FR-0722KL/311-22-0KHRCT-ND/730003"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Yageo"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="laforge" package="WEEE_BIN" value=""/>
<element name="X4" library="con-hirose" package="UX60-MB-5ST" value="MINI-USB-SHIELD-UX60-MB-5ST">
<attribute name="CLASS" value="CONNECTOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UX60-MB-5ST"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="DESCRIPTION" value="CONN RCPT USB2.0 MINI B SMD R/A"/>
<attribute name="SOURCEPARTNUMBER" value="H2959CT-ND"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/hirose-electric-co-ltd/UX60-MB-5ST/H2959CT-ND/597538"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Hirose Electric Co Ltd"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U5" library="laforge" package="TSOP-6" value="IP4234CZ6">
<attribute name="OC_DIGIKEY" value="568-5869-1-ND"/>
<attribute name="CLASS" value="IC"/>
<attribute name="MANUFACTURERPARTNUMBER" value="IP4234CZ6,125"/>
<attribute name="DESCRIPTION" value="TVS DIODE 5.5V 6TSOP"/>
<attribute name="SOURCEPARTNUMBER" value="1727-4717-1-ND"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/nxp-semiconductors/IP4234CZ6,125/568-5869-1-ND/2531156"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Nexperia USA Inc."/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="rc-sysmocom" package="_0603" value="100n">
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="GRM033R61C104KE84D"/>
<attribute name="DESCRIPTION" value="CAP CER 0.1UF 16V X5R 0201"/>
<attribute name="SOURCEPARTNUMBER" value="490-9985-1-ND"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/murata-electronics-north-america/GRM033R61C104KE84D/490-9985-1-ND/5026290"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Murata Electronics"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="rc-sysmocom" package="_0603" value="100n">
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="GRM033R61C104KE84D"/>
<attribute name="DESCRIPTION" value="CAP CER 0.1UF 16V X5R 0201"/>
<attribute name="SOURCEPARTNUMBER" value="490-9985-1-ND"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/murata-electronics-north-america/GRM033R61C104KE84D/490-9985-1-ND/5026290"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Murata Electronics"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="rc-sysmocom" package="_0603" value="4.7u">
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL10A475MP8NNNC"/>
<attribute name="DESCRIPTION" value="CAP CER 4.7UF 10V X5R 0603"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1905-1-ND"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/samsung-electro-mechanics/CL10A475MP8NNNC/1276-1905-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="rc-sysmocom" package="_0603" value="1u">
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL10A105KO8NNNC"/>
<attribute name="DESCRIPTION" value="CAP CER 1UF 16V X5R 0603"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1034-1-ND"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/samsung-electro-mechanics/CL10A105KO8NNNC/1276-1034-1-ND/"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="rc-sysmocom" package="_0603" value="100n">
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="GRM033R61C104KE84D"/>
<attribute name="DESCRIPTION" value="CAP CER 0.1UF 16V X5R 0201"/>
<attribute name="SOURCEPARTNUMBER" value="490-9985-1-ND"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/murata-electronics-north-america/GRM033R61C104KE84D/490-9985-1-ND/5026290"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Murata Electronics"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="rc-sysmocom" package="_0603" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="RES SMD 1M OHM 1%% 1/10W 0603"/>
<attribute name="MANUFACTURER" value="Yageo"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RC0603FR-071ML"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="311-1.00MHRCT-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/yageo/RC0603FR-071ML/311-1-00MHRCT-ND/729791"/>
</element>
<element name="C28" library="rc-sysmocom" package="_0402" value="33p">
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL05C330JB5NNNC"/>
<attribute name="DESCRIPTION" value="CAP CER 33PF 50V NP0 0402"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1272-1-ND"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/CL05C330JB5NNNC/1276-1272-1-ND/3889358"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics America, Inc."/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C33" library="rc-sysmocom" package="_0402" value="33p">
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL05C330JB5NNNC"/>
<attribute name="DESCRIPTION" value="CAP CER 33PF 50V NP0 0402"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1272-1-ND"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/CL05C330JB5NNNC/1276-1272-1-ND/3889358"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics America, Inc."/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C34" library="rc-sysmocom" package="_0402" value="33p">
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL05C330JB5NNNC"/>
<attribute name="DESCRIPTION" value="CAP CER 33PF 50V NP0 0402"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1272-1-ND"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/CL05C330JB5NNNC/1276-1272-1-ND/3889358"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics America, Inc."/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="laforge" package="SOT666" value="PESD5V0UBV">
<attribute name="OC_DIGIKEY" value="568-7356-1-ND"/>
<attribute name="CLASS" value="DIODE"/>
<attribute name="MANUFACTURERPARTNUMBER" value="PESD5V0U5BV,115"/>
<attribute name="DESCRIPTION" value="TVS DIODE 5V SOT666"/>
<attribute name="SOURCEPARTNUMBER" value="1727-5806-1-ND"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/nexperia-usa-inc/PESD5V0U5BV,115/1727-5806-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Nexperia USA Inc."/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="B2" library="microbuilder" package="EVQ-Q2" value="">
<attribute name="CLASS" value="TACT SWITCH"/>
<attribute name="MANUFACTURERPARTNUMBER" value="EVQ-Q2M03W"/>
<attribute name="DESCRIPTION" value="SWITCH TACTILE SPST-NO 0.02A 15V"/>
<attribute name="SOURCEPARTNUMBER" value="P12946SCT-ND"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/panasonic-electronic-components/EVQ-Q2M03W/P12946SCT-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Panasonic Electronic Components"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="rc-sysmocom" package="_0402" value="33p">
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL05C330JB5NNNC"/>
<attribute name="DESCRIPTION" value="CAP CER 33PF 50V NP0 0402"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1272-1-ND"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/CL05C330JB5NNNC/1276-1272-1-ND/3889358"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics America, Inc."/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C32" library="rc-sysmocom" package="_0805" value="10u">
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="GRM21BR61C106KE15K"/>
<attribute name="DESCRIPTION" value="CAP CER 10UF 16V X5R 0805"/>
<attribute name="SOURCEPARTNUMBER" value="490-6473-1-ND"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/murata-electronics/GRM21BR61C106KE15K/490-6473-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Murata Electronics"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C29" library="rc-sysmocom" package="_0402" value="33p">
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL05C330JB5NNNC"/>
<attribute name="DESCRIPTION" value="CAP CER 33PF 50V NP0 0402"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1272-1-ND"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/CL05C330JB5NNNC/1276-1272-1-ND/3889358"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics America, Inc."/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C31" library="rc-sysmocom" package="_0805" value="10u">
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="GRM21BR61C106KE15K"/>
<attribute name="DESCRIPTION" value="CAP CER 10UF 16V X5R 0805"/>
<attribute name="SOURCEPARTNUMBER" value="490-6473-1-ND"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/murata-electronics/GRM21BR61C106KE15K/490-6473-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Murata Electronics"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C30" library="rc-sysmocom" package="_0402" value="33p">
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL05C330JB5NNNC"/>
<attribute name="DESCRIPTION" value="CAP CER 33PF 50V NP0 0402"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1272-1-ND"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/CL05C330JB5NNNC/1276-1272-1-ND/3889358"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics America, Inc."/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="ldo" package="SC70-5" value="MIC5366">
<attribute name="DESCRIPTION" value="IC REG LINEAR 2.8V 150MA SC70-5"/>
<attribute name="MANUFACTURER" value="Microchip Technology"/>
<attribute name="MANUFACTURERPARTNUMBER" value="MIC5366-2.8YC5-TR"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="576-3209-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="IC"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/microchip-technology/MIC5366-2-8YC5-TR/576-3209-1-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rc-sysmocom" package="_0603" value="4.7k">
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RC0603JR-074K7L"/>
<attribute name="DESCRIPTION" value="RES SMD 4.7K OHM 5%% 1/10W 0603"/>
<attribute name="SOURCEPARTNUMBER" value="311-4.7KGRCT-ND"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/yageo/RC0603JR-074K7L/311-4.7KGRCT-ND/729732"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Yageo"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rc-sysmocom" package="_0603" value="47k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="RES SMD 47K OHM 1%% 1/10W 0603"/>
<attribute name="MANUFACTURER" value="Yageo"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RC0603FR-0747KL"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="311-47.0KHRCT-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/yageo/RC0603FR-0747KL/311-47-0KHRCT-ND/730200"/>
</element>
<element name="C14" library="rc-sysmocom" package="_0603" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="CAP CER 1UF 16V X5R 0603"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL10A105KO8NNNC"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1034-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/samsung-electro-mechanics/CL10A105KO8NNNC/1276-1034-1-ND/"/>
</element>
<element name="C15" library="rc-sysmocom" package="_0603" value="1u">
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL10A105KO8NNNC"/>
<attribute name="DESCRIPTION" value="CAP CER 1UF 16V X5R 0603"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1034-1-ND"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/samsung-electro-mechanics/CL10A105KO8NNNC/1276-1034-1-ND/"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP1" library="testpad" package="TP10R" value="TPTP10R">
<attribute name="CLASS" value="UNKNOWN CLASS"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="POPULATED" value="FALSE"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="rc-sysmocom" package="_0603" value="100n">
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL10B104KO8NNNC"/>
<attribute name="DESCRIPTION" value="CAP CER 0.1UF 16V 10% X7R 0603"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1005-1-ND"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/foo/1276-1005-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics America, Inc"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="rc-sysmocom" package="_0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="RES SMD 1K OHM 0.5%% 1/16W 0603"/>
<attribute name="MANUFACTURER" value="Susumu"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RR0816P-102-D"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="RR08P1.0KDCT-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/susumu/RR0816P-102-D/RR08P1-0KDCT-ND/432724"/>
</element>
<element name="R13" library="rc-sysmocom" package="_0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="RES SMD 1K OHM 0.5%% 1/16W 0603"/>
<attribute name="MANUFACTURER" value="Susumu"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RR0816P-102-D"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="RR08P1.0KDCT-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/susumu/RR0816P-102-D/RR08P1-0KDCT-ND/432724"/>
</element>
<element name="C13" library="rc-sysmocom" package="_0603" value="100n">
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL10B104KO8NNNC"/>
<attribute name="DESCRIPTION" value="CAP CER 0.1UF 16V 10% X7R 0603"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1005-1-ND"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/foo/1276-1005-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics America, Inc"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="microbuilder" package="1X04_ROUND_76" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CONNECTOR\JUMPER"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
</element>
<element name="R27" library="rc-sysmocom" package="_0603" value="0">
<attribute name="DESCRIPTION" value="RES 0 OHM JUMPER 1/16W 0402"/>
<attribute name="MANUFACTURER" value="Stackpole Electronics Inc"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RMCF0402ZT0R00"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="RMCF0402ZT0R00CT-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/stackpole-electronics-inc/RMCF0402ZT0R00/RMCF0402ZT0R00CT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="rc-sysmocom" package="_0402" value="33p">
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL05C330JB5NNNC"/>
<attribute name="DESCRIPTION" value="CAP CER 33PF 50V NP0 0402"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1272-1-ND"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/CL05C330JB5NNNC/1276-1272-1-ND/3889358"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics America, Inc."/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="rc-sysmocom" package="_0402" value="33p">
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL05C330JB5NNNC"/>
<attribute name="DESCRIPTION" value="CAP CER 33PF 50V NP0 0402"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1272-1-ND"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/CL05C330JB5NNNC/1276-1272-1-ND/3889358"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics America, Inc."/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="laforge" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CONNECTOR"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
</element>
<element name="TP2" library="testpad" package="TP10R" value="TPTP10R">
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="FALSE"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="CLASS" value="UNKNOWN CLASS"/>
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP3" library="testpad" package="TP10R" value="TPTP10R">
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="FALSE"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="CLASS" value="UNKNOWN CLASS"/>
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP4" library="testpad" package="TP10R" value="TPTP10R">
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="FALSE"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="CLASS" value="UNKNOWN CLASS"/>
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP5" library="testpad" package="TP10R" value="TPTP10R">
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="FALSE"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="CLASS" value="UNKNOWN CLASS"/>
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="AUDIO-JACK-TRRS-SMD" value="AUDIO-JACK3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="AUDIO JACK, 3.5 MM, RT, 4 CONDUC"/>
<attribute name="MANUFACTURER" value="CUI Devices"/>
<attribute name="MANUFACTURERPARTNUMBER" value="SJ2-3574A-SMT-TR"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="CP-SJ2-3574A-SMT-CT-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CONNECTOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/cui-devices/SJ2-3574A-SMT-TR/CP-SJ2-3574A-SMT-CT-ND"/>
</element>
<element name="U$3" library="oshw" package="OSHW_8MM_COPPER" value=""/>
<element name="T2" library="transistor" package="SOT23-BEC" value="BC847">
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="SOURCEPARTNUMBER" value="1727-2924-1-ND"/>
<attribute name="MANUFACTURER" value="Nexperia USA Inc."/>
<attribute name="MANUFACTURERPARTNUMBER" value="BC847C,215"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="CLASS" value="TRANSISTOR"/>
<attribute name="DESCRIPTION" value="TRANS NPN 45V 0.1A SOT23"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/nexperia-usa-inc/BC847C,215/1727-2924-1-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="rc-sysmocom" package="_0603" value="22k">
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="SOURCEPARTNUMBER" value="311-22.0KHRCT-ND"/>
<attribute name="MANUFACTURER" value="Yageo"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RC0603FR-0722KL"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="DESCRIPTION" value="RES SMD 22K OHM 1%% 1/10W 0603"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/yageo/RC0603FR-0722KL/311-22-0KHRCT-ND/730003"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="rc-sysmocom" package="_0603" value="22k">
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="SOURCEPARTNUMBER" value="311-22.0KHRCT-ND"/>
<attribute name="MANUFACTURER" value="Yageo"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RC0603FR-0722KL"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="DESCRIPTION" value="RES SMD 22K OHM 1%% 1/10W 0603"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/yageo/RC0603FR-0722KL/311-22-0KHRCT-ND/730003"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="rc-sysmocom" package="_0603" value="4.7k">
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="SOURCEPARTNUMBER" value="311-4.7KGRCT-ND"/>
<attribute name="MANUFACTURER" value="Yageo"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RC0603JR-074K7L"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="DESCRIPTION" value="RES SMD 4.7K OHM 5%% 1/10W 0603"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/yageo/RC0603JR-074K7L/311-4.7KGRCT-ND/729732"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="jumper" package="JP2" value="">
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="CLASS" value="CONNECTOR\JUMPER"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="jumper" package="JP1" value="">
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CONNECTOR\JUMPER"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X5" library="laforge" package="JACK2.5_SJ-2523" value="OsmoSer">
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CONNECTOR"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U6" library="laforge" package="VQFN-N16" value="SN74AVC4T245-VQFN">
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="IC"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
</element>
<element name="R29" library="rc-sysmocom" package="_0603" value="4K7">
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="rc-sysmocom" package="_0603" value="10k">
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C36" library="rc-sysmocom" package="_0603" value="100n">
<attribute name="DESCRIPTION" value="CAP CER 0.1UF 16V X5R 0201"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Murata Electronics"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/murata-electronics-north-america/GRM033R61C104KE84D/490-9985-1-ND/5026290"/>
<attribute name="MANUFACTURERPARTNUMBER" value="GRM033R61C104KE84D"/>
<attribute name="SOURCEPARTNUMBER" value="490-9985-1-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C35" library="rc-sysmocom" package="_0603" value="100n">
<attribute name="DESCRIPTION" value="CAP CER 0.1UF 16V X5R 0201"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Murata Electronics"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/murata-electronics-north-america/GRM033R61C104KE84D/490-9985-1-ND/5026290"/>
<attribute name="MANUFACTURERPARTNUMBER" value="GRM033R61C104KE84D"/>
<attribute name="SOURCEPARTNUMBER" value="490-9985-1-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="NCP303" package="SOT23-5" value="NCP303">
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="UNKNOWN CLASS"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="rc-sysmocom" package="_0603" value="1u">
<attribute name="DESCRIPTION" value="CAP CER 1UF 16V X5R 0603"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/samsung-electro-mechanics/CL10A105KO8NNNC/1276-1034-1-ND/"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL10A105KO8NNNC"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1034-1-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="rc-sysmocom" package="_0603" value="0">
<attribute name="DESCRIPTION" value="RES 0 OHM JUMPER 1/16W 0402"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Stackpole Electronics Inc"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/stackpole-electronics-inc/RMCF0402ZT0R00/RMCF0402ZT0R00CT-ND"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RMCF0402ZT0R00"/>
<attribute name="SOURCEPARTNUMBER" value="RMCF0402ZT0R00CT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP7" library="testpad" package="TP10R" value="TPTP10R">
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="CLASS" value="UNKNOWN CLASS"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="POPULATED" value="FALSE"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP8" library="testpad" package="TP10R" value="TPTP10R">
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="CLASS" value="UNKNOWN CLASS"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="POPULATED" value="FALSE"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP9" library="testpad" package="TP10R" value="TPTP10R">
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="CLASS" value="UNKNOWN CLASS"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="POPULATED" value="FALSE"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP10" library="testpad" package="TP10R" value="TPTP10R">
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="CLASS" value="UNKNOWN CLASS"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="POPULATED" value="FALSE"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP6" library="testpad" package="TP10R" value="TPTP10R">
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="CLASS" value="UNKNOWN CLASS"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="POPULATED" value="FALSE"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP11" library="testpad" package="TP10R" value="TPTP10R">
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="CLASS" value="UNKNOWN CLASS"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="POPULATED" value="FALSE"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP12" library="testpad" package="TP10R" value="TPTP10R">
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="CLASS" value="UNKNOWN CLASS"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="POPULATED" value="FALSE"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP13" library="testpad" package="TP10R" value="TPTP10R">
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="CLASS" value="UNKNOWN CLASS"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="POPULATED" value="FALSE"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP14" library="testpad" package="TP10R" value="TPTP10R">
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="CLASS" value="UNKNOWN CLASS"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="POPULATED" value="FALSE"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP15" library="testpad" package="TP10R" value="TPTP10R">
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="CLASS" value="UNKNOWN CLASS"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="POPULATED" value="FALSE"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP16" library="testpad" package="TP10R" value="TPTP10R">
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="CLASS" value="UNKNOWN CLASS"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="POPULATED" value="FALSE"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="rc-sysmocom" package="_0603" value="0">
<attribute name="DESCRIPTION" value="RES 0 OHM JUMPER 1/16W 0402"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Stackpole Electronics Inc"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/stackpole-electronics-inc/RMCF0402ZT0R00/RMCF0402ZT0R00CT-ND"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RMCF0402ZT0R00"/>
<attribute name="SOURCEPARTNUMBER" value="RMCF0402ZT0R00CT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="silabs_CP2102X" package="QFN28" value="CP2102N_28">
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="UNKNOWN CLASS"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="rc-sysmocom" package="_0603" value="22k">
<attribute name="DESCRIPTION" value="RES SMD 22K OHM 1%% 1/10W 0603"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Yageo"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/yageo/RC0603FR-0722KL/311-22-0KHRCT-ND/730003"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RC0603FR-0722KL"/>
<attribute name="SOURCEPARTNUMBER" value="311-22.0KHRCT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="rc-sysmocom" package="_0603" value="47k">
<attribute name="DESCRIPTION" value="RES SMD 47K OHM 1%% 1/10W 0603"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Yageo"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/yageo/RC0603FR-0747KL/311-47-0KHRCT-ND/730200"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RC0603FR-0747KL"/>
<attribute name="SOURCEPARTNUMBER" value="311-47.0KHRCT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="U2" pad="3"/>
<contactref element="C12" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="C11" pad="-"/>
<contactref element="C17" pad="-"/>
<contactref element="C8" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="C9" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="X2" pad="G1"/>
<contactref element="X3" pad="GND@1"/>
<contactref element="X2" pad="G2"/>
<contactref element="X2" pad="G3"/>
<contactref element="X2" pad="G4"/>
<contactref element="D1" pad="2"/>
<contactref element="MDM1" pad="1"/>
<contactref element="MDM1" pad="2"/>
<contactref element="MDM1" pad="3"/>
<contactref element="MDM1" pad="4"/>
<contactref element="SIM1" pad="5"/>
<contactref element="D3" pad="A"/>
<contactref element="K1" pad="3"/>
<contactref element="K1" pad="2"/>
<contactref element="U2" pad="PAD"/>
<contactref element="R16" pad="2"/>
<contactref element="U1" pad="32"/>
<contactref element="U1" pad="34"/>
<contactref element="U1" pad="31"/>
<contactref element="U1" pad="33"/>
<contactref element="U1" pad="35"/>
<contactref element="D4" pad="1"/>
<contactref element="X3" pad="GND@2"/>
<contactref element="B1" pad="B"/>
<contactref element="B1" pad="B'"/>
<contactref element="T3" pad="E"/>
<contactref element="R18" pad="2"/>
<contactref element="X4" pad="5"/>
<contactref element="U5" pad="2"/>
<contactref element="R26" pad="1"/>
<contactref element="C24" pad="1"/>
<contactref element="D5" pad="2"/>
<contactref element="B2" pad="B'"/>
<contactref element="B2" pad="B"/>
<contactref element="C34" pad="1"/>
<contactref element="C33" pad="2"/>
<contactref element="C28" pad="2"/>
<contactref element="C29" pad="2"/>
<contactref element="C31" pad="2"/>
<contactref element="U3" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="C18" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="R27" pad="1"/>
<contactref element="C26" pad="2"/>
<contactref element="C27" pad="1"/>
<contactref element="X1" pad="3"/>
<contactref element="J1" pad="4"/>
<contactref element="R10" pad="2"/>
<contactref element="T2" pad="E"/>
<contactref element="U1" pad="12"/>
<contactref element="U6" pad="9"/>
<contactref element="U6" pad="3"/>
<contactref element="U6" pad="8"/>
<contactref element="C36" pad="1"/>
<contactref element="X5" pad="1"/>
<contactref element="C35" pad="2"/>
<contactref element="C20" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="C23" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="C19" pad="1"/>
<contactref element="R14" pad="2"/>
<contactref element="JP4" pad="2"/>
<contactref element="IC2" pad="EXP"/>
<contactref element="IC2" pad="3"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="USIM_CLK">
<contactref element="R3" pad="2"/>
<contactref element="SIM1" pad="3"/>
<contactref element="C3" pad="1"/>
<contactref element="D1" pad="4"/>
</signal>
<signal name="USIM_RESET">
<contactref element="R2" pad="2"/>
<contactref element="SIM1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="D1" pad="6"/>
</signal>
<signal name="USIM_VPP">
<contactref element="SIM1" pad="6"/>
</signal>
<signal name="VCC_4V1">
<contactref element="U2" pad="4"/>
<contactref element="C16" pad="2"/>
<contactref element="C17" pad="+"/>
<contactref element="C8" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="C9" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="LED1" pad="A"/>
<contactref element="C5" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="R15" pad="2"/>
<contactref element="U1" pad="36"/>
<contactref element="U1" pad="38"/>
<contactref element="U1" pad="40"/>
<contactref element="U1" pad="37"/>
<contactref element="U1" pad="39"/>
<contactref element="R19" pad="1"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="_USIM_CLK">
<contactref element="U1" pad="14"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="_USIM_RESET">
<contactref element="U1" pad="16"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="LDO_IN">
<contactref element="U2" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C11" pad="+"/>
<contactref element="D3" pad="C"/>
<contactref element="D2" pad="C"/>
<contactref element="U3" pad="1"/>
<contactref element="C14" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="R25" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="LED1" pad="C"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="X2" pad="C"/>
<contactref element="X3" pad="SIG"/>
<contactref element="D4" pad="2"/>
</signal>
<signal name="USIM_VCC">
<contactref element="R1" pad="2"/>
<contactref element="SIM1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="13"/>
<contactref element="D1" pad="1"/>
</signal>
<signal name="USIM_IO">
<contactref element="R1" pad="1"/>
<contactref element="SIM1" pad="7"/>
<contactref element="C4" pad="1"/>
<contactref element="D1" pad="5"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="RXD2">
<contactref element="U1" pad="30"/>
<contactref element="U6" pad="13"/>
</signal>
<signal name="VDD">
<contactref element="U1" pad="28"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="!PWON">
<contactref element="U1" pad="26"/>
<contactref element="R23" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="UART_RI">
<contactref element="U1" pad="24"/>
<contactref element="TP7" pad="TP"/>
</signal>
<signal name="UART_TXD">
<contactref element="U1" pad="22"/>
<contactref element="U6" pad="10"/>
</signal>
<signal name="UART_RTS">
<contactref element="U1" pad="20"/>
<contactref element="TP8" pad="TP"/>
</signal>
<signal name="UART_DCD">
<contactref element="U1" pad="18"/>
<contactref element="TP6" pad="TP"/>
</signal>
<signal name="!RST">
<contactref element="U1" pad="10"/>
<contactref element="R12" pad="2"/>
<contactref element="R13" pad="1"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="AUXO+">
<contactref element="U1" pad="8"/>
<contactref element="TP2" pad="TP"/>
</signal>
<signal name="EAR+">
<contactref element="U1" pad="6"/>
<contactref element="D5" pad="3"/>
<contactref element="C25" pad="2"/>
<contactref element="C32" pad="2"/>
<contactref element="JP3" pad="3"/>
<contactref element="C26" pad="1"/>
</signal>
<signal name="MIC+">
<contactref element="U1" pad="4"/>
<contactref element="C28" pad="1"/>
<contactref element="D5" pad="4"/>
<contactref element="C30" pad="1"/>
<contactref element="C33" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="AUXI+">
<contactref element="U1" pad="2"/>
<contactref element="TP3" pad="TP"/>
</signal>
<signal name="TXD2">
<contactref element="U1" pad="29"/>
<contactref element="U6" pad="11"/>
</signal>
<signal name="ADC">
<contactref element="U1" pad="27"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="UART_DSR">
<contactref element="U1" pad="25"/>
<contactref element="TP9" pad="TP"/>
</signal>
<signal name="UART_RXD">
<contactref element="U1" pad="23"/>
<contactref element="U6" pad="12"/>
</signal>
<signal name="UART_CTS">
<contactref element="U1" pad="21"/>
<contactref element="TP10" pad="TP"/>
</signal>
<signal name="UART_DTR">
<contactref element="U1" pad="19"/>
<contactref element="TP16" pad="TP"/>
</signal>
<signal name="USIM_CD">
<contactref element="U1" pad="17"/>
<contactref element="SIM1" pad="81"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="VBACKUP">
<contactref element="U1" pad="11"/>
<contactref element="X1" pad="2"/>
</signal>
<signal name="LPG">
<contactref element="U1" pad="9"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="AUXO-">
<contactref element="U1" pad="7"/>
<contactref element="TP4" pad="TP"/>
</signal>
<signal name="EAR-">
<contactref element="U1" pad="5"/>
<contactref element="R27" pad="2"/>
<contactref element="C25" pad="1"/>
<contactref element="D5" pad="1"/>
<contactref element="C27" pad="2"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="MIC-">
<contactref element="U1" pad="3"/>
<contactref element="C29" pad="1"/>
<contactref element="C31" pad="1"/>
<contactref element="C30" pad="2"/>
<contactref element="JP3" pad="2"/>
<contactref element="D5" pad="5"/>
</signal>
<signal name="AUXI-">
<contactref element="U1" pad="1"/>
<contactref element="TP5" pad="TP"/>
</signal>
<signal name="N$4">
<contactref element="K1" pad="1"/>
<contactref element="K1" pad="1-1"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="R16" pad="1"/>
<contactref element="R15" pad="1"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="R19" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="T3" pad="C"/>
<contactref element="LED2" pad="C"/>
</signal>
<signal name="N$5">
<contactref element="T3" pad="B"/>
<contactref element="R17" pad="2"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="_USB_DN">
<contactref element="U5" pad="6"/>
<contactref element="X4" pad="2"/>
</signal>
<signal name="_USB_DP">
<contactref element="U5" pad="1"/>
<contactref element="X4" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="X4" pad="M1"/>
<contactref element="X4" pad="M4"/>
<contactref element="X4" pad="M3"/>
<contactref element="X4" pad="M2"/>
<contactref element="R26" pad="2"/>
<contactref element="C24" pad="2"/>
</signal>
<signal name="USB_VBUS">
<contactref element="U5" pad="5"/>
<contactref element="X4" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="USB_D_N">
<contactref element="U5" pad="4"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="USB_D_P">
<contactref element="U5" pad="3"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="N$8">
<contactref element="C34" pad="2"/>
<contactref element="C32" pad="1"/>
<contactref element="J1" pad="3"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="VIO_2V8">
<contactref element="U3" pad="5"/>
<contactref element="C15" pad="2"/>
<contactref element="R12" pad="1"/>
<contactref element="U6" pad="16"/>
<contactref element="C35" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="SIM1" pad="82"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="B2" pad="A'"/>
<contactref element="B2" pad="A"/>
<contactref element="R23" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="B1" pad="A"/>
<contactref element="B1" pad="A'"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="R8" pad="2"/>
<contactref element="JP4" pad="1"/>
<contactref element="T2" pad="B"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="D2" pad="A"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="EN_VCC">
<contactref element="R11" pad="1"/>
<contactref element="T2" pad="C"/>
<contactref element="U2" pad="1"/>
<contactref element="U3" pad="3"/>
</signal>
<signal name="N$18">
<contactref element="X5" pad="3"/>
<contactref element="U6" pad="6"/>
</signal>
<signal name="N$20">
<contactref element="X5" pad="2"/>
<contactref element="R32" pad="1"/>
<contactref element="U6" pad="4"/>
</signal>
<signal name="_UART_TXD">
<contactref element="U6" pad="7"/>
<contactref element="IC2" pad="26"/>
</signal>
<signal name="_UART_RXD">
<contactref element="U6" pad="5"/>
<contactref element="IC2" pad="25"/>
</signal>
<signal name="CP_VDD">
<contactref element="C21" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="TP1" pad="TP"/>
<contactref element="R29" pad="1"/>
<contactref element="R32" pad="2"/>
<contactref element="C36" pad="2"/>
<contactref element="U6" pad="1"/>
<contactref element="U6" pad="2"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="CP_DTR">
<contactref element="R8" pad="1"/>
<contactref element="IC2" pad="28"/>
</signal>
<signal name="N$23">
<contactref element="C19" pad="2"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="N$22">
<contactref element="U6" pad="14"/>
<contactref element="U6" pad="15"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="IC2" pad="8"/>
<contactref element="R7" pad="2"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="IC2" pad="7"/>
<contactref element="R25" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="IC2" pad="9"/>
<contactref element="R29" pad="2"/>
</signal>
<signal name="GPIO6">
<contactref element="IC2" pad="20"/>
</signal>
<signal name="GPIO5">
<contactref element="IC2" pad="21"/>
</signal>
<signal name="GPIO4">
<contactref element="IC2" pad="22"/>
</signal>
<signal name="GPIO3/WAKEUP">
<contactref element="IC2" pad="16"/>
</signal>
<signal name="GPIO2/RS485">
<contactref element="IC2" pad="17"/>
</signal>
<signal name="GPIO1/RXT">
<contactref element="IC2" pad="18"/>
</signal>
<signal name="GPIO0/TXT">
<contactref element="IC2" pad="19"/>
</signal>
<signal name="N$15">
<contactref element="IC2" pad="23"/>
<contactref element="TP12" pad="TP"/>
</signal>
<signal name="N$16">
<contactref element="IC2" pad="24"/>
<contactref element="TP11" pad="TP"/>
</signal>
<signal name="N$30">
<contactref element="IC2" pad="27"/>
<contactref element="TP15" pad="TP"/>
</signal>
<signal name="N$32">
<contactref element="IC2" pad="1"/>
<contactref element="TP14" pad="TP"/>
</signal>
<signal name="N$14">
<contactref element="IC2" pad="2"/>
<contactref element="TP13" pad="TP"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
