<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="50" y2="0" width="0" layer="20"/>
<wire x1="50" y1="0" x2="50" y2="50" width="0" layer="20"/>
<wire x1="50" y1="50" x2="0" y2="50" width="0" layer="20"/>
<wire x1="0" y1="50" x2="0" y2="0" width="0" layer="20"/>
<text>DUS LMT splitter
by LaF0rge</text>
<text>DUS</text>
<text>ETH</text>
<text>RS232</text>
</plain>
<libraries>
<library name="stewart-rj45">
<packages>
<package name="SS-7188S-A-NF">
<description>Bel Stewart SS-7188S-A-NF</description>
</package>
</packages>
</library>
<library name="Wuerth_Elektronik_eiCan_Communication_Connectors_v6_20150113">
<description>&lt;BR&gt;Würth Elektronik -- Electronic Interconnect &amp; Electromechanical Solutions&lt;br&gt;&lt;Hr&gt;
&lt;BR&gt;&lt;BR&gt; 
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-405&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/eagle"&gt;http://www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither CadSoft nor WE-eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;&lt;BR&gt;&lt;br&gt;
&lt;hr&gt;
Version 6,  January 13th 2015
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="618009211821">
<description>WR-DSUB 8.08mm Female Angled PCB Connector without Hex Screw, 9 Pins</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="X1" library="stewart-rj45" package="SS-7188S-A-NF" value="SS-7188S-A-NF">
<attribute name="MANUFACTURER" value="Bel Stewart"/>
<attribute name="OC_DIGIKEY" value="380-1047-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X2" library="stewart-rj45" package="SS-7188S-A-NF" value="SS-7188S-A-NF">
<attribute name="MANUFACTURER" value="Bel Stewart"/>
<attribute name="OC_DIGIKEY" value="380-1047-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="K1" library="Wuerth_Elektronik_eiCan_Communication_Connectors_v6_20150113" package="618009211821" value="618009211821">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="PAIR12_P">
<contactref element="X1" pad="1"/>
<contactref element="X2" pad="1"/>
</signal>
<signal name="PAIR12_N">
<contactref element="X1" pad="2"/>
<contactref element="X2" pad="2"/>
</signal>
<signal name="PAIR36_P">
<contactref element="X1" pad="3"/>
<contactref element="X2" pad="3"/>
</signal>
<signal name="PAIR36_N">
<contactref element="X1" pad="6"/>
<contactref element="X2" pad="6"/>
</signal>
<signal name="RS232_COMPUTER_RXD">
<contactref element="X1" pad="4"/>
<contactref element="K1" pad="3"/>
</signal>
<signal name="RS232_COMPUTER_TXD">
<contactref element="X1" pad="7"/>
<contactref element="K1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="K1" pad="7"/>
<contactref element="K1" pad="8"/>
</signal>
<signal name="SHIIELD">
<contactref element="X1" pad="S2"/>
<contactref element="X2" pad="S2"/>
<contactref element="X1" pad="S1"/>
<contactref element="X2" pad="S1"/>
</signal>
<signal name="GND">
<contactref element="X1" pad="5"/>
<contactref element="K1" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
