-- Pretty-printed by Asnp, the pretty-printer of France Telecom R&D (http://asn1.elibel.tm.fr/asnp/)
MAP-MobileServiceOperations {itu-t identified-organization(4) etsi(0)
  mobileDomain(0) gsm-Network(1) modules(3) map-MobileServiceOperations(5)
  version8(8)} DEFINITIONS ::=
BEGIN

EXPORTS
  -- location registration operations
  updateLocation, cancelLocation, purgeMS,
    sendIdentification,
    -- gprs location registration operations
    updateGprsLocation,
    -- subscriber information enquiry operations
    provideSubscriberInfo,
    -- any time information enquiry operations
    anyTimeInterrogation,
    -- any time information handling operations
    anyTimeSubscriptionInterrogation,
    anyTimeModification,
    -- subscriber data modification notification operations
    noteSubscriberDataModified,
    -- handover operations
    prepareHandover, sendEndSignal, processAccessSignalling,
    forwardAccessSignalling,
    prepareSubsequentHandover,
    -- authentication management operations
    sendAuthenticationInfo,
    authenticationFailureReport,
    -- IMEI management operations
    checkIMEI,
    -- subscriber management operations
    insertSubscriberData,
    deleteSubscriberData,
    -- fault recovery operations
    reset, forwardCheckSS-Indication,
    restoreData,
    -- gprs location information retrieval operations
    sendRoutingInfoForGprs,
    -- failure reporting operations
    failureReport,
    -- gprs notification operations
    noteMsPresentForGprs,
    -- Mobility Management operations
    noteMM-Event;

IMPORTS
  OPERATION
    FROM Remote-Operations-Information-Objects {joint-iso-itu-t
      remote-operations(4) informationObjects(5) version1(0)}
  systemFailure, dataMissing, unexpectedDataValue, unknownSubscriber,
    unknownMSC, unidentifiedSubscriber, unknownEquipment, roamingNotAllowed,
    ati-NotAllowed, noHandoverNumberAvailable, subsequentHandoverFailure,
    absentSubscriber, mm-EventNotSupported, atsi-NotAllowed, atm-NotAllowed,
    bearerServiceNotProvisioned, teleserviceNotProvisioned, callBarred,
    illegalSS-Operation, ss-ErrorStatus, ss-NotAvailable, ss-Incompatibility,
    ss-SubscriptionViolation, informationNotAvailable,
    targetCellOutsideGroupCallArea
    FROM MAP-Errors {itu-t identified-organization(4) etsi(0) mobileDomain(0)
      gsm-Network(1) modules(3) map-Errors(10) version8(8)}
  UpdateLocationArg, UpdateLocationRes, CancelLocationArg, CancelLocationRes,
    PurgeMS-Arg, PurgeMS-Res, SendIdentificationArg, SendIdentificationRes,
    UpdateGprsLocationArg, UpdateGprsLocationRes, PrepareHO-Arg, PrepareHO-Res,
    ForwardAccessSignalling-Arg, ProcessAccessSignalling-Arg,
    SendEndSignal-Arg, SendEndSignal-Res, PrepareSubsequentHO-Res,
    PrepareSubsequentHO-Arg, SendAuthenticationInfoArg,
    SendAuthenticationInfoRes, AuthenticationFailureReportArg,
    AuthenticationFailureReportRes, CheckIMEI-Arg, CheckIMEI-Res,
    InsertSubscriberDataArg, InsertSubscriberDataRes, DeleteSubscriberDataArg,
    DeleteSubscriberDataRes, ResetArg, RestoreDataArg, RestoreDataRes,
    ProvideSubscriberInfoArg, ProvideSubscriberInfoRes,
    AnyTimeSubscriptionInterrogationArg, AnyTimeSubscriptionInterrogationRes,
    AnyTimeModificationArg, AnyTimeModificationRes,
    NoteSubscriberDataModifiedArg, NoteSubscriberDataModifiedRes,
    AnyTimeInterrogationArg, AnyTimeInterrogationRes,
    SendRoutingInfoForGprsArg, SendRoutingInfoForGprsRes, FailureReportArg,
    FailureReportRes, NoteMsPresentForGprsArg, NoteMsPresentForGprsRes,
    NoteMM-EventArg, NoteMM-EventRes
    FROM MAP-MS-DataTypes {itu-t identified-organization(4) etsi(0)
      mobileDomain(0) gsm-Network(1) modules(3) map-MS-DataTypes(11)
      version8(8)};

-- location registration operations
updateLocation OPERATION ::= { --Timer m
  ARGUMENT  UpdateLocationArg
  RESULT    UpdateLocationRes
  ERRORS
    {systemFailure | dataMissing | unexpectedDataValue | unknownSubscriber |
      roamingNotAllowed}
  CODE      local:2}

cancelLocation OPERATION ::= { --Timer m
  ARGUMENT  CancelLocationArg
  RESULT    CancelLocationRes
  -- optional
  ERRORS    {dataMissing | unexpectedDataValue}
  CODE      local:3}

purgeMS OPERATION ::= { --Timer m
  ARGUMENT  PurgeMS-Arg
  RESULT    PurgeMS-Res
  -- optional
  ERRORS    {dataMissing | unexpectedDataValue | unknownSubscriber}
  CODE      local:67}

sendIdentification OPERATION ::= { --Timer s
  ARGUMENT  SendIdentificationArg
  RESULT    SendIdentificationRes
  ERRORS    {dataMissing | unidentifiedSubscriber}
  CODE      local:55}

-- gprs location registration operations
updateGprsLocation OPERATION ::= { --Timer m
  ARGUMENT  UpdateGprsLocationArg
  RESULT    UpdateGprsLocationRes
  ERRORS
    {systemFailure | unexpectedDataValue | unknownSubscriber |
      roamingNotAllowed}
  CODE      local:23}

-- subscriber information enquiry operations
provideSubscriberInfo OPERATION ::= { --Timer m
  ARGUMENT  ProvideSubscriberInfoArg
  RESULT    ProvideSubscriberInfoRes
  ERRORS    {dataMissing | unexpectedDataValue}
  CODE      local:70}

-- any time information enquiry operations
anyTimeInterrogation OPERATION ::= { --Timer m
  ARGUMENT  AnyTimeInterrogationArg
  RESULT    AnyTimeInterrogationRes
  ERRORS
    {systemFailure | ati-NotAllowed | dataMissing | unexpectedDataValue |
      unknownSubscriber}
  CODE      local:71}

-- any time information handling operations
anyTimeSubscriptionInterrogation OPERATION ::= { --Timer m
  ARGUMENT  AnyTimeSubscriptionInterrogationArg
  RESULT    AnyTimeSubscriptionInterrogationRes
  ERRORS
    {atsi-NotAllowed | dataMissing | unexpectedDataValue | unknownSubscriber |
      bearerServiceNotProvisioned | teleserviceNotProvisioned | callBarred |
      illegalSS-Operation | ss-NotAvailable | informationNotAvailable}
  CODE      local:62}

anyTimeModification OPERATION ::= { --Timer m
  ARGUMENT  AnyTimeModificationArg
  RESULT    AnyTimeModificationRes
  ERRORS
    {atm-NotAllowed | dataMissing | unexpectedDataValue | unknownSubscriber |
      bearerServiceNotProvisioned | teleserviceNotProvisioned | callBarred |
      illegalSS-Operation | ss-SubscriptionViolation | ss-ErrorStatus |
      ss-Incompatibility | informationNotAvailable}
  CODE      local:65}

-- subscriber data modification notification operations
noteSubscriberDataModified OPERATION ::= { --Timer m
  ARGUMENT  NoteSubscriberDataModifiedArg
  RESULT    NoteSubscriberDataModifiedRes
  -- optional
  ERRORS    {dataMissing | unexpectedDataValue | unknownSubscriber}
  CODE      local:5}

-- handover operations
prepareHandover OPERATION ::= { --Timer m
  ARGUMENT  PrepareHO-Arg
  RESULT    PrepareHO-Res
  ERRORS
    {systemFailure | dataMissing | unexpectedDataValue |
      noHandoverNumberAvailable | targetCellOutsideGroupCallArea}
  CODE      local:68}

sendEndSignal OPERATION ::= { --Timer l
  ARGUMENT  SendEndSignal-Arg
  RESULT    SendEndSignal-Res
  CODE      local:29}

processAccessSignalling OPERATION ::= { --Timer s
  ARGUMENT  ProcessAccessSignalling-Arg
  CODE      local:33}

forwardAccessSignalling OPERATION ::= { --Timer s
  ARGUMENT  ForwardAccessSignalling-Arg
  CODE      local:34}

prepareSubsequentHandover OPERATION ::= { --Timer m
  ARGUMENT  PrepareSubsequentHO-Arg
  RESULT    PrepareSubsequentHO-Res
  ERRORS
    {unexpectedDataValue | dataMissing | unknownMSC |
      subsequentHandoverFailure}
  CODE      local:69}

-- authentication management operations
sendAuthenticationInfo OPERATION ::= { --Timer m
  ARGUMENT  SendAuthenticationInfoArg
  -- optional
  -- within a dialogue sendAuthenticationInfoArg shall not be present in
  -- subsequent invoke components. If received in a subsequent invoke component
  -- it shall be discarded.
  RESULT    SendAuthenticationInfoRes
  -- optional
  ERRORS
    {systemFailure | dataMissing | unexpectedDataValue | unknownSubscriber}
  CODE      local:56}

authenticationFailureReport OPERATION ::= { --Timer m
  ARGUMENT  AuthenticationFailureReportArg
  RESULT    AuthenticationFailureReportRes
  -- optional
  ERRORS    {systemFailure | unexpectedDataValue | unknownSubscriber}
  CODE      local:15}

-- IMEI management operations
checkIMEI OPERATION ::= { --Timer m
  ARGUMENT  CheckIMEI-Arg
  RESULT    CheckIMEI-Res
  ERRORS    {systemFailure | dataMissing | unknownEquipment}
  CODE      local:43}

-- subscriber management operations
insertSubscriberData OPERATION ::= { --Timer m
  ARGUMENT  InsertSubscriberDataArg
  RESULT    InsertSubscriberDataRes
  -- optional
  ERRORS    {dataMissing | unexpectedDataValue | unidentifiedSubscriber}
  CODE      local:7}

deleteSubscriberData OPERATION ::= { --Timer m
  ARGUMENT  DeleteSubscriberDataArg
  RESULT    DeleteSubscriberDataRes
  -- optional
  ERRORS    {dataMissing | unexpectedDataValue | unidentifiedSubscriber}
  CODE      local:8}

-- fault recovery operations
reset OPERATION ::= { --Timer m
	ARGUMENT  ResetArg
   CODE      local:37}

forwardCheckSS-Indication OPERATION ::= { --Timer s
   CODE  local:38}

restoreData OPERATION ::= { --Timer m
  ARGUMENT  RestoreDataArg
  RESULT    RestoreDataRes
  ERRORS
    {systemFailure | dataMissing | unexpectedDataValue | unknownSubscriber}
  CODE      local:57}

-- gprs location information retrieval operations
sendRoutingInfoForGprs OPERATION ::= { --Timer m
  ARGUMENT  SendRoutingInfoForGprsArg
  RESULT    SendRoutingInfoForGprsRes
  ERRORS
    {absentSubscriber | systemFailure | dataMissing | unexpectedDataValue |
      unknownSubscriber | callBarred}
  CODE      local:24}

-- failure reporting operations
failureReport OPERATION ::= { --Timer m
  ARGUMENT  FailureReportArg
  RESULT    FailureReportRes
  -- optional
  ERRORS
    {systemFailure | dataMissing | unexpectedDataValue | unknownSubscriber}
  CODE      local:25}

-- gprs notification operations
noteMsPresentForGprs OPERATION ::= { --Timer m
  ARGUMENT  NoteMsPresentForGprsArg
  RESULT    NoteMsPresentForGprsRes
  -- optional
  ERRORS
    {systemFailure | dataMissing | unexpectedDataValue | unknownSubscriber}
  CODE      local:26}

noteMM-Event OPERATION ::= { --Timer m
  ARGUMENT  NoteMM-EventArg
  RESULT    NoteMM-EventRes
  ERRORS
    {dataMissing | unexpectedDataValue | unknownSubscriber |
      mm-EventNotSupported}
  CODE      local:89}

END

