-- Pretty-printed by Asnp, the pretty-printer of France Telecom R&D (http://asn1.elibel.tm.fr/asnp/)
MAP-TS-Code {itu-t identified-organization(4) etsi(0) mobileDomain(0)
  gsm-Network(1) modules(3) map-TS-Code(19) version8(8)} DEFINITIONS ::=
BEGIN

TeleserviceCode ::= OCTET STRING(SIZE (1))

-- This type is used to represent the code identifying a single
-- teleservice, a group of teleservices, or all teleservices. The
-- services are defined in TS GSM 22.003 [4].
-- The internal structure is defined as follows:
-- bits 87654321: group (bits 8765) and specific service
-- (bits 4321)
Ext-TeleserviceCode ::= OCTET STRING(SIZE (1..5))

-- This type is used to represent the code identifying a single
-- teleservice, a group of teleservices, or all teleservices. The
-- services are defined in TS GSM 22.003 [4].
-- The internal structure is defined as follows:
-- OCTET 1:
-- bits 87654321: group (bits 8765) and specific service
-- (bits 4321)
-- OCTETS 2-5: reserved for future use. If received the
-- Ext-TeleserviceCode shall be
-- treated according to the exception handling defined for the
-- operation that uses this type.
-- Ext-TeleserviceCode includes all values defined for TeleserviceCode.
allTeleservices TeleserviceCode ::=
  '00000000'B

allSpeechTransmissionServices TeleserviceCode ::= '00010000'B

telephony TeleserviceCode ::= '00010001'B

emergencyCalls TeleserviceCode ::= '00010010'B

allShortMessageServices TeleserviceCode ::= '00100000'B

shortMessageMT-PP TeleserviceCode ::= '00100001'B

shortMessageMO-PP TeleserviceCode ::= '00100010'B

allFacsimileTransmissionServices TeleserviceCode ::= '01100000'B

facsimileGroup3AndAlterSpeech TeleserviceCode ::= '01100001'B

automaticFacsimileGroup3 TeleserviceCode ::= '01100010'B

facsimileGroup4 TeleserviceCode ::= '01100011'B

-- The following non-hierarchical Compound Teleservice Groups
-- are defined in TS 3GPP TS 22.030:
allDataTeleservices TeleserviceCode ::=
  '01110000'B

-- covers Teleservice Groups 'allFacsimileTransmissionServices'
-- and 'allShortMessageServices'
allTeleservices-ExeptSMS TeleserviceCode ::=
  '10000000'B

-- covers Teleservice Groups 'allSpeechTransmissionServices' and
-- 'allFacsimileTransmissionServices'
--
-- Compound Teleservice Group Codes are only used in call
-- independent supplementary service operations, i.e. they
-- are not used in InsertSubscriberData or in
-- DeleteSubscriberData messages.
allVoiceGroupCallServices TeleserviceCode ::=
  '10010000'B

voiceGroupCall TeleserviceCode ::= '10010001'B

voiceBroadcastCall TeleserviceCode ::= '10010010'B

allPLMN-specificTS TeleserviceCode ::= '11010000'B

plmn-specificTS-1 TeleserviceCode ::= '11010001'B

plmn-specificTS-2 TeleserviceCode ::= '11010010'B

plmn-specificTS-3 TeleserviceCode ::= '11010011'B

plmn-specificTS-4 TeleserviceCode ::= '11010100'B

plmn-specificTS-5 TeleserviceCode ::= '11010101'B

plmn-specificTS-6 TeleserviceCode ::= '11010110'B

plmn-specificTS-7 TeleserviceCode ::= '11010111'B

plmn-specificTS-8 TeleserviceCode ::= '11011000'B

plmn-specificTS-9 TeleserviceCode ::= '11011001'B

plmn-specificTS-A TeleserviceCode ::= '11011010'B

plmn-specificTS-B TeleserviceCode ::= '11011011'B

plmn-specificTS-C TeleserviceCode ::= '11011100'B

plmn-specificTS-D TeleserviceCode ::= '11011101'B

plmn-specificTS-E TeleserviceCode ::= '11011110'B

plmn-specificTS-F TeleserviceCode ::= '11011111'B

END

