GENTONES(1)

NAME
lcradmin - view and modify the state of a running lcr

SYNOPSIS
lcradmin state
lcradmin route
lcradmin interface
lcradmin block <port number>
lcradmin unload <port number>
lcradmin unload <port number>
lcradmin release <endpoint id>

DESCRIPTION

  lcradmin state
starts lcradmin in interactive mode. You will see a screen with the current calls and a list of keys for possible options.

  lcradmin route
makes lcr reload the routing.conf

  lcradmin interface
makes lcr reload the interface.conf

  lcradmin block
makes lcr block the specified port for further incoming and outgoing calls.

  lcradmin unblock
unblocks the port again

  lcradmin unload
makes lcr cease using the specified port. The port the be used by a different application, or to unload the mISDN driver. To load the port again, use lcradmin unblock as described above, or use lcradmin interface to reload all interfaces.

  lcradmin release
makes lcr release a pending call. The endpoint ID is shown in the status screen, as well as in the log, starting with "EP(<ID>)". This can be useful, if two members are joined in a conference, but they don't or even can't hang up for some reason. Also lost parked calls can be released.

SEE ALSO
http://www.linux-call-router.de/doc.html

AUTHOR
This minimal man page was written by Joerg Dorchain <joerg@dorchain.net>
from documentation created by Andreas Eversberg <jolly@eversberg.eu>