#
# .csv to store UE's information in HSS
# Kept in the following format: "Name,IMSI,Key,OP_Type,OP,AMF,SQN,QCI"
#
# Name:    Human readable name to help distinguish UE's. Ignored by the HSS
# IMSI:    UE's IMSI value
# Key:     UE's key, where other keys are derived from. Stored in hexadecimal
# OP_Type: Operator's code type, either OP or OPc
# OP/OPc:  Operator Code/Cyphered Operator Code, stored in hexadecimal
# AMF:     Authentication management field, stored in hexadecimal
# SQN:     UE's Sequence number for freshness of the authentication
# QCI:     QoS Class Identifier for the UE's default bearer.
#
# Note: Lines starting by '#' are ignored and will be overwritten
ue1,001010123456789,00112233445566778899aabbccddeeff,opc,63bfa50ee6523365ff14c1f45f88737d,9001,000000001234,7
ue2,001010123456780,00112233445566778899aabbccddeeff,opc,63bfa50ee6523365ff14c1f45f88737d,8000,000000001234,7
