(export (version D)
  (design
    (source /home/kevredon/simtrace/hardware/kicad/SIMtrace.sch)
    (date "So 17 Mai 2015 14:31:22 CEST")
    (tool "eeschema (2013-may-18)-stable"))
  (components
    (comp (ref R26)
      (value 100K)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53A3E46E))
    (comp (ref R25)
      (value 100K)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53A3E45D))
    (comp (ref R23)
      (value 100K)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4FB50700))
    (comp (ref IC4)
      (value CB3Q3244)
      (footprint SSOP20_BDQ)
      (libsource (lib SIMtrace) (part CB3Q3244))
      (sheetpath (names /) (tstamps /))
      (tstamp 4EB57076))
    (comp (ref C24)
      (value 100nF)
      (footprint SM0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DFF9964))
    (comp (ref R22)
      (value 100K)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DFF9902))
    (comp (ref IC2)
      (value AP7332)
      (footprint SOT26)
      (libsource (lib SIMtrace) (part AP7332))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DFF8B97))
    (comp (ref R21)
      (value 10k1%)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DFF746C))
    (comp (ref R20)
      (value 10k1%)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DFF7469))
    (comp (ref R19)
      (value 100K)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DFF73B0))
    (comp (ref J2)
      (value JACK_2.5)
      (footprint JACK_2.5)
      (libsource (lib SIMtrace) (part JACK_2.5))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DCBE233))
    (comp (ref P4)
      (value SIM)
      (footprint SIM_AMPHENOL)
      (libsource (lib smartcard) (part ISO7816_NO))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DC8FA06))
    (comp (ref C12)
      (value 2.2uF)
      (footprint SM0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DC8F97A))
    (comp (ref C1)
      (value 2.2uF)
      (footprint SM0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DC8F975))
    (comp (ref BT1)
      (value 4.5-6V)
      (footprint PIN_ARRAY_2X1)
      (libsource (lib device) (part BATTERY))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DC804A6))
    (comp (ref R16)
      (value 10K)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DC7A441))
    (comp (ref Q2)
      (value BC847)
      (footprint SOT23_BC847)
      (libsource (lib SIMtrace) (part BC847))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DC7A43A))
    (comp (ref Q1)
      (value BC847)
      (footprint SOT23_BC847)
      (libsource (lib SIMtrace) (part BC847))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DC7A1CA))
    (comp (ref C5)
      (value 33pF)
      (footprint SM0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DC79EDF))
    (comp (ref C13)
      (value 15pF)
      (footprint SM0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DC79EDC))
    (comp (ref C11)
      (value 15pF)
      (footprint SM0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DC79ED8))
    (comp (ref R1)
      (value 100K)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DC79ED1))
    (comp (ref R3)
      (value 1K5)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DC79ECE))
    (comp (ref R9)
      (value 27R)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DC79EAD))
    (comp (ref R10)
      (value 27R)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DC79EA7))
    (comp (ref R2)
      (value 10K)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DC79E9A))
    (comp (ref J1)
      (value USB-B_MINI)
      (footprint USB-MINI-B_UX60)
      (libsource (lib SIMtrace) (part USB-B_MINI))
      (sheetpath (names /) (tstamps /))
      (tstamp 4CFAC6EA))
    (comp (ref FB1)
      (value FILTER)
      (footprint SM0805)
      (libsource (lib device) (part FILTER))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DC79E48))
    (comp (ref R17)
      (value 10K)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DC799F2))
    (comp (ref C14)
      (value 4.7uF)
      (footprint SM0805)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DC6A5DE))
    (comp (ref C22)
      (value 1uF)
      (footprint SM0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DC6A5D9))
    (comp (ref C21)
      (value 1uF)
      (footprint SM0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DC6A5CB))
    (comp (ref C23)
      (value 100nF)
      (footprint SM0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DC68E45))
    (comp (ref FB2)
      (value FILTER)
      (footprint SM0805)
      (libsource (lib device) (part FILTER))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DC68E1D))
    (comp (ref SW2)
      (value BOOTLOADER)
      (footprint PUSH_BUTTON)
      (libsource (lib device) (part SW_PUSH))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DC6852C))
    (comp (ref JP2)
      (value ERASE)
      (footprint PIN_ARRAY_2X1)
      (libsource (lib device) (part JUMPER))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DC683ED))
    (comp (ref JP1)
      (value TEST)
      (footprint PIN_ARRAY_2X1)
      (libsource (lib device) (part JUMPER))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DC68259))
    (comp (ref C19)
      (value 100nF)
      (footprint SM0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DC664E0))
    (comp (ref C16)
      (value 100nF)
      (footprint SM0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DC664DD))
    (comp (ref C4)
      (value 100nF)
      (footprint SM0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DC66392))
    (comp (ref R18)
      (value 10K)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DC5A30D))
    (comp (ref U1)
      (value FLASH)
      (footprint SOC008_WIDE)
      (libsource (lib SIMtrace) (part FLASH_SPI))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DC5A250))
    (comp (ref R14)
      (value 150R)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DC555D0))
    (comp (ref R13)
      (value 150R)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4CF7BAEE))
    (comp (ref P3)
      (value REBELSIM)
      (footprint FFC_REBELSIM)
      (libsource (lib smartcard) (part REBELSIM))
      (sheetpath (names /) (tstamps /))
      (tstamp 4DC51F05))
    (comp (ref C3)
      (value 100nF)
      (footprint SM0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 4D037E30))
    (comp (ref C20)
      (value 100nF)
      (footprint SM0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 4D020EDF))
    (comp (ref C15)
      (value 100nF)
      (footprint SM0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 4D020ED8))
    (comp (ref C6)
      (value 10nF)
      (footprint SM0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 4D020DD3))
    (comp (ref C10)
      (value 1nF)
      (footprint SM0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 4D020DCD))
    (comp (ref R11)
      (value 1K5)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4D020DC6))
    (comp (ref C9)
      (value 100nF)
      (footprint SM0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 4D020BEB))
    (comp (ref C7)
      (value 100nF)
      (footprint SM0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 4D020BDE))
    (comp (ref SW1)
      (value RESET)
      (footprint PUSH_BUTTON)
      (libsource (lib device) (part SW_PUSH))
      (sheetpath (names /) (tstamps /))
      (tstamp 4D020733))
    (comp (ref R12)
      (value 100K)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4D0206C7))
    (comp (ref P1)
      (value JTAG)
      (footprint PIN_ARRAY_10X2)
      (libsource (lib SIMtrace) (part JTAG))
      (sheetpath (names /) (tstamps /))
      (tstamp 4CFCD6C9))
    (comp (ref D5)
      (value GREEN)
      (footprint LED-0805)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 4CF5471F))
    (comp (ref D4)
      (value RED)
      (footprint LED-0805)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 4CF54717))
    (comp (ref IC3)
      (value ATSAM3S2B)
      (footprint TQFP_64)
      (libsource (lib at91sam7sxxx-au) (part AT91SAM7S512/256/128/64/321-AU))
      (sheetpath (names /) (tstamps /))
      (tstamp 4CE84486))
    (comp (ref P2)
      (value DEBUG)
      (footprint PIN_ARRAY-6X1)
      (libsource (lib SIMtrace) (part DEBUG))
      (sheetpath (names /) (tstamps /))
      (tstamp 4CE9ADCF))
    (comp (ref R8)
      (value 100K)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4CE9A6AE))
    (comp (ref R7)
      (value 100K)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4CE9A6A9))
    (comp (ref R6)
      (value 100K)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4CE9A6A5))
    (comp (ref R5)
      (value 100K)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4CE9A69A))
    (comp (ref R4)
      (value 100K)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4CE9A68C))
    (comp (ref C18)
      (value 10pF)
      (footprint SM0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 4CE91633))
    (comp (ref C17)
      (value 10pF)
      (footprint SM0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 4CE9162F))
    (comp (ref X1)
      (value 18.432MHz)
      (footprint Q_49U3HMS)
      (libsource (lib device) (part CRYSTAL))
      (sheetpath (names /) (tstamps /))
      (tstamp 4CE915DE))
    (comp (ref IC1)
      (value FPF2109)
      (footprint SOT23-5)
      (datasheet https://www.fairchildsemi.com/ds/FP/FPF2110.pdf)
      (libsource (lib SIMtrace) (part FPF210X))
      (sheetpath (names /) (tstamps /))
      (tstamp 526C41E4))
    (comp (ref D1)
      (value MBR0530)
      (footprint SOD123)
      (libsource (lib SIMtrace) (part SCHOTTKY))
      (sheetpath (names /) (tstamps /))
      (tstamp 526C4CBB))
    (comp (ref D2)
      (value MBR0530)
      (footprint SOD123)
      (libsource (lib SIMtrace) (part SCHOTTKY))
      (sheetpath (names /) (tstamps /))
      (tstamp 526C4CDD))
    (comp (ref D3)
      (value MBR0530)
      (footprint SOD123)
      (libsource (lib SIMtrace) (part SCHOTTKY))
      (sheetpath (names /) (tstamps /))
      (tstamp 526C4CEC))
    (comp (ref D6)
      (value MBR0530)
      (footprint SOD123)
      (libsource (lib SIMtrace) (part SCHOTTKY))
      (sheetpath (names /) (tstamps /))
      (tstamp 526C4D13))
    (comp (ref R24)
      (value 100K)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 526C5026))
    (comp (ref R15)
      (value 100K)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 526C5035)))
  (libparts
    (libpart (lib device) (part BATTERY)
      (fields
        (field (name Reference) BT)
        (field (name Value) BATTERY)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name +) (type passive))
        (pin (num 2) (name -) (type passive))))
    (libpart (lib device) (part C)
      (description "Condensateur non polarise")
      (footprints
        (fp SM*)
        (fp C?)
        (fp C1-1))
      (fields
        (field (name Reference) C)
        (field (name Value) C)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part CRYSTAL)
      (fields
        (field (name Reference) X)
        (field (name Value) CRYSTAL)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib device) (part FILTER)
      (description "Filtre EMI")
      (fields
        (field (name Reference) FB)
        (field (name Value) FILTER)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib device) (part JUMPER)
      (fields
        (field (name Reference) JP)
        (field (name Value) JUMPER)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib device) (part LED)
      (footprints
        (fp LED-3MM)
        (fp LED-5MM)
        (fp LED-10MM)
        (fp LED-0603)
        (fp LED-0805)
        (fp LED-1206)
        (fp LEDV))
      (fields
        (field (name Reference) D)
        (field (name Value) LED)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib device) (part R)
      (description Resistance)
      (footprints
        (fp R?)
        (fp SM0603)
        (fp SM0805)
        (fp R?-*)
        (fp SM1206))
      (fields
        (field (name Reference) R)
        (field (name Value) R)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part SW_PUSH)
      (description "Push Button")
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_PUSH)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib at91sam7sxxx-au) (part AT91SAM7S512/256/128/64/321-AU)
      (fields
        (field (name Reference) IC)
        (field (name Value) AT91SAM7S512/256/128/64/321-AU)
        (field (name Footprint) at91sam7sxxx-au-LQFP64))
      (pins
        (pin (num 1) (name ADVREF) (type passive))
        (pin (num 2) (name GND@0) (type power_in))
        (pin (num 3) (name AD4) (type passive))
        (pin (num 4) (name AD5) (type passive))
        (pin (num 5) (name AD6) (type passive))
        (pin (num 6) (name AD7) (type passive))
        (pin (num 7) (name VDDIN) (type power_in))
        (pin (num 8) (name VDDOUT) (type power_out))
        (pin (num 9) (name PA17/TD/PCK1/AD0) (type BiDi))
        (pin (num 10) (name PA18/RD/PCK2/AD1) (type BiDi))
        (pin (num 11) (name PA21/RXD1/PCK1) (type BiDi))
        (pin (num 12) (name VDDCORE@0) (type power_in))
        (pin (num 13) (name PA19/RK/FIQ) (type BiDi))
        (pin (num 14) (name PA22/TXD1/NPCS3) (type BiDi))
        (pin (num 15) (name PA23/SCK1/PWM0) (type BiDi))
        (pin (num 16) (name PA20/RF/IRQ0/AD3) (type BiDi))
        (pin (num 17) (name GND@1) (type power_in))
        (pin (num 18) (name VDDIO@0) (type power_in))
        (pin (num 19) (name PA16/TK/TIOB1) (type BiDi))
        (pin (num 20) (name PA15/TF/TIOA1) (type BiDi))
        (pin (num 21) (name PA14/SPCK/PWM3) (type BiDi))
        (pin (num 22) (name PA13/MOSI/PWM2) (type BiDi))
        (pin (num 23) (name PA24/RTS1/PWM1) (type BiDi))
        (pin (num 24) (name VDDCORE@1) (type power_in))
        (pin (num 25) (name PA25/CTS1/PWM2) (type BiDi))
        (pin (num 26) (name PA26/DCD1/TIOA2) (type BiDi))
        (pin (num 27) (name PA12/MISO/PWM1) (type BiDi))
        (pin (num 28) (name PA11/NPCS0/PWM0) (type BiDi))
        (pin (num 29) (name PA10/DTXD/NPCS2) (type BiDi))
        (pin (num 30) (name PA9/DRXD/NPCS1) (type BiDi))
        (pin (num 31) (name PA8/CTS0/ADTRG) (type BiDi))
        (pin (num 32) (name PA7/RTS0/PWM3) (type BiDi))
        (pin (num 33) (name TDI) (type input))
        (pin (num 34) (name PA6/TXD0/PCK0) (type BiDi))
        (pin (num 35) (name PA5/RXD0/NPCS3) (type BiDi))
        (pin (num 36) (name PA4/TWCK/TLCK0) (type BiDi))
        (pin (num 37) (name PA27/DTR1/TIOB2) (type BiDi))
        (pin (num 38) (name PA28/DSR1/TCLK1) (type BiDi))
        (pin (num 39) (name /NRST) (type BiDi))
        (pin (num 40) (name TST) (type input))
        (pin (num 41) (name PA29/RI1/TCLK2) (type BiDi))
        (pin (num 42) (name PA30/IRQ1/NPCS2) (type BiDi))
        (pin (num 43) (name PA3/TWD/NPCS3) (type BiDi))
        (pin (num 44) (name PA2/PWM2/SCK0) (type BiDi))
        (pin (num 45) (name VDDIO@1) (type power_in))
        (pin (num 46) (name GND@2) (type power_in))
        (pin (num 47) (name PA1/PWM1/TIOB0) (type BiDi))
        (pin (num 48) (name PA0/PWM0/TIOA0) (type BiDi))
        (pin (num 49) (name TDO) (type output))
        (pin (num 50) (name JTAGSEL) (type input))
        (pin (num 51) (name TMS) (type input))
        (pin (num 52) (name PA31/NPCS1/PCK2) (type BiDi))
        (pin (num 53) (name TCK) (type input))
        (pin (num 54) (name VDDCORE@2) (type power_in))
        (pin (num 55) (name ERASE) (type input))
        (pin (num 56) (name DDM) (type passive))
        (pin (num 57) (name DDP) (type passive))
        (pin (num 58) (name VDDIO@2) (type power_in))
        (pin (num 59) (name VDDFLASH) (type power_in))
        (pin (num 60) (name GND@3) (type power_in))
        (pin (num 61) (name XOUT) (type passive))
        (pin (num 62) (name XIN) (type passive))
        (pin (num 63) (name PLLRC) (type passive))
        (pin (num 64) (name VDDPLL) (type power_in))))
    (libpart (lib SIMtrace) (part AP7332)
      (fields
        (field (name Reference) IC)
        (field (name Value) AP7332)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name VOUT2) (type power_out))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name EN2) (type input))
        (pin (num 4) (name EN1) (type input))
        (pin (num 5) (name VIN) (type power_in))
        (pin (num 6) (name VOUT1) (type power_out))))
    (libpart (lib SIMtrace) (part BC847)
      (docs transistors/bipolar/*.*)
      (fields
        (field (name Reference) Q)
        (field (name Value) BC847)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name B) (type input))
        (pin (num 2) (name E) (type passive))
        (pin (num 3) (name C) (type passive))))
    (libpart (lib SIMtrace) (part CB3Q3244)
      (description SN74CB3Q3244)
      (fields
        (field (name Reference) IC)
        (field (name Value) CB3Q3244)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name /1OE) (type input))
        (pin (num 2) (name 1A1) (type BiDi))
        (pin (num 3) (name 2B4) (type BiDi))
        (pin (num 4) (name 1A2) (type BiDi))
        (pin (num 5) (name 2B3) (type BiDi))
        (pin (num 6) (name 1A3) (type BiDi))
        (pin (num 7) (name 2B2) (type BiDi))
        (pin (num 8) (name 1A4) (type BiDi))
        (pin (num 9) (name 2B1) (type BiDi))
        (pin (num 10) (name GND) (type power_in))
        (pin (num 11) (name 2A1) (type BiDi))
        (pin (num 12) (name 1B4) (type BiDi))
        (pin (num 13) (name 2A2) (type BiDi))
        (pin (num 14) (name 1B3) (type BiDi))
        (pin (num 15) (name 2A3) (type BiDi))
        (pin (num 16) (name 1B2) (type BiDi))
        (pin (num 17) (name 2A4) (type BiDi))
        (pin (num 18) (name 1B1) (type BiDi))
        (pin (num 19) (name /2OE) (type input))
        (pin (num 20) (name VCC) (type power_in))))
    (libpart (lib SIMtrace) (part DEBUG)
      (fields
        (field (name Reference) P)
        (field (name Value) DEBUG)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name CTS) (type output))
        (pin (num 3) (name VCC) (type power_in))
        (pin (num 4) (name TXD) (type output))
        (pin (num 5) (name RXD) (type input))
        (pin (num 6) (name RTS) (type input))))
    (libpart (lib SIMtrace) (part FLASH_SPI)
      (fields
        (field (name Reference) U)
        (field (name Value) FLASH_SPI)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name /CS) (type input))
        (pin (num 2) (name SO) (type output))
        (pin (num 3) (name /WP) (type output))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name SI) (type input))
        (pin (num 6) (name SCK) (type input))
        (pin (num 7) (name /HOLD) (type input))
        (pin (num 8) (name VCC) (type power_in))))
    (libpart (lib SIMtrace) (part FPF210X)
      (description "Fairchild Semiconductors FPF2108-FPF2110 IC-switch")
      (fields
        (field (name Reference) IC)
        (field (name Value) FPF210X)
        (field (name Footprint) SOT23-5)
        (field (name Datasheet) https://www.fairchildsemi.com/ds/FP/FPF2110.pdf))
      (pins
        (pin (num 1) (name VIN) (type power_in))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name ON) (type input))
        (pin (num 4) (name FLAGB) (type input))
        (pin (num 5) (name VOUT) (type power_out))))
    (libpart (lib SIMtrace) (part JACK_2.5)
      (fields
        (field (name Reference) J)
        (field (name Value) JACK_2.5)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name SLEEVE) (type passive))
        (pin (num 2) (name TIP) (type passive))
        (pin (num 3) (name RING) (type passive))))
    (libpart (lib SIMtrace) (part JTAG)
      (description "symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) JTAG)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name VREF) (type passive))
        (pin (num 2) (name VCC) (type passive))
        (pin (num 3) (name nTRST) (type passive))
        (pin (num 4) (name GND) (type passive))
        (pin (num 5) (name TDI) (type passive))
        (pin (num 6) (name GND) (type passive))
        (pin (num 7) (name TMS) (type passive))
        (pin (num 8) (name GND) (type passive))
        (pin (num 9) (name TCK) (type passive))
        (pin (num 10) (name GND) (type passive))
        (pin (num 11) (name RTCK) (type passive))
        (pin (num 12) (name GND) (type passive))
        (pin (num 13) (name TDO) (type passive))
        (pin (num 14) (name GND) (type passive))
        (pin (num 15) (name nSRST) (type passive))
        (pin (num 16) (name GND) (type passive))
        (pin (num 17) (name DBGRQ) (type passive))
        (pin (num 18) (name GND) (type passive))
        (pin (num 19) (name DGBACK) (type passive))
        (pin (num 20) (name GND) (type passive))))
    (libpart (lib SIMtrace) (part SCHOTTKY)
      (description "Diode schottky")
      (footprints
        (fp D?)
        (fp S*))
      (fields
        (field (name Reference) D)
        (field (name Value) SCHOTTKY)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib SIMtrace) (part USB-B_MINI)
      (fields
        (field (name Reference) J)
        (field (name Value) USB-B_MINI)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name VCC) (type power_out))
        (pin (num 2) (name D-) (type BiDi))
        (pin (num 3) (name D+) (type BiDi))
        (pin (num 4) (name ID) (type passive))
        (pin (num 5) (name GND) (type power_in))))
    (libpart (lib smartcard) (part ISO7816_NO)
      (description "smart card with normally closed presence switch")
      (fields
        (field (name Reference) P)
        (field (name Value) ISO7816_NO))
      (pins
        (pin (num C1) (name VCC) (type power_in))
        (pin (num C2) (name RST) (type input))
        (pin (num C3) (name CLK) (type input))
        (pin (num C4) (name RFU) (type unspc))
        (pin (num C5) (name GND) (type power_in))
        (pin (num C6) (name VPP) (type power_in))
        (pin (num C7) (name I/O) (type BiDi))
        (pin (num C8) (name RFU) (type unspc))
        (pin (num SW1) (name ~) (type passive))
        (pin (num SW2) (name ~) (type passive))))
    (libpart (lib smartcard) (part REBELSIM)
      (description "ymbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) REBELSIM))
      (pins
        (pin (num 1) (name VCC) (type power_out))
        (pin (num 2) (name RST) (type output))
        (pin (num 3) (name CLK) (type output))
        (pin (num 4) (name I/O) (type BiDi))
        (pin (num 5) (name VPP) (type power_out))
        (pin (num 6) (name GND) (type power_out)))))
  (libraries
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical at91sam7sxxx-au)
      (uri lib/at91sam7sxxx-au.lib))
    (library (logical SIMtrace)
      (uri lib/SIMtrace.lib))
    (library (logical smartcard)
      (uri lib/smartcard.lib)))
  (nets
    (net (code 1) (name /TEST)
      (node (ref JP1) (pin 1))
      (node (ref IC3) (pin 40)))
    (net (code 2) (name /SC_SW)
      (node (ref IC3) (pin 16))
      (node (ref IC4) (pin 1)))
    (net (code 3) (name GND)
      (node (ref C18) (pin 2))
      (node (ref IC1) (pin 2))
      (node (ref R15) (pin 2))
      (node (ref R24) (pin 2))
      (node (ref C17) (pin 2))
      (node (ref P4) (pin C5))
      (node (ref J1) (pin 5))
      (node (ref R17) (pin 2))
      (node (ref IC3) (pin 46))
      (node (ref C13) (pin 2))
      (node (ref C11) (pin 2))
      (node (ref P2) (pin 1))
      (node (ref IC3) (pin 17))
      (node (ref IC3) (pin 4))
      (node (ref IC3) (pin 3))
      (node (ref IC3) (pin 2))
      (node (ref IC3) (pin 5))
      (node (ref IC3) (pin 60))
      (node (ref P1) (pin 12))
      (node (ref P1) (pin 18))
      (node (ref P1) (pin 4))
      (node (ref P1) (pin 16))
      (node (ref P1) (pin 14))
      (node (ref P1) (pin 20))
      (node (ref P1) (pin 10))
      (node (ref P1) (pin 8))
      (node (ref P1) (pin 6))
      (node (ref C9) (pin 2))
      (node (ref SW1) (pin 2))
      (node (ref C7) (pin 2))
      (node (ref C10) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref C15) (pin 2))
      (node (ref C20) (pin 2))
      (node (ref C24) (pin 2))
      (node (ref U1) (pin 4))
      (node (ref R23) (pin 1))
      (node (ref C21) (pin 2))
      (node (ref C22) (pin 2))
      (node (ref P4) (pin SW2))
      (node (ref C14) (pin 2))
      (node (ref C12) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref C19) (pin 2))
      (node (ref BT1) (pin 2))
      (node (ref C23) (pin 2))
      (node (ref P3) (pin 6))
      (node (ref C3) (pin 2))
      (node (ref IC2) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref C16) (pin 2))
      (node (ref IC4) (pin 10))
      (node (ref Q2) (pin 2))
      (node (ref J2) (pin 1))
      (node (ref SW2) (pin 2))
      (node (ref R19) (pin 1))
      (node (ref R21) (pin 1)))
    (net (code 4) (name /I/O_SIM)
      (node (ref IC3) (pin 34))
      (node (ref IC4) (pin 9))
      (node (ref P4) (pin C7))
      (node (ref IC3) (pin 47))
      (node (ref R26) (pin 2)))
    (net (code 5) (name /CLK_SIM)
      (node (ref IC3) (pin 44))
      (node (ref P4) (pin C3))
      (node (ref R25) (pin 2))
      (node (ref IC3) (pin 36))
      (node (ref IC4) (pin 14)))
    (net (code 6) (name /RST_SIM)
      (node (ref IC4) (pin 16))
      (node (ref IC3) (pin 32))
      (node (ref P4) (pin C2)))
    (net (code 7) (name /SCK)
      (node (ref U1) (pin 6))
      (node (ref IC3) (pin 21)))
    (net (code 8) (name "")
      (node (ref R18) (pin 1))
      (node (ref U1) (pin 7)))
    (net (code 9) (name /CS)
      (node (ref IC3) (pin 28))
      (node (ref U1) (pin 1)))
    (net (code 10) (name /MISO)
      (node (ref U1) (pin 2))
      (node (ref IC3) (pin 27)))
    (net (code 11) (name "")
      (node (ref P4) (pin C8)))
    (net (code 12) (name "")
      (node (ref R16) (pin 1))
      (node (ref Q2) (pin 1)))
    (net (code 13) (name "")
      (node (ref D3) (pin 1))
      (node (ref C14) (pin 1))
      (node (ref IC2) (pin 4))
      (node (ref IC2) (pin 5))
      (node (ref D2) (pin 1)))
    (net (code 14) (name "")
      (node (ref IC3) (pin 6))
      (node (ref R20) (pin 2))
      (node (ref R21) (pin 2)))
    (net (code 15) (name /UDP_PUP)
      (node (ref R1) (pin 2))
      (node (ref Q1) (pin 1))
      (node (ref D1) (pin 2))
      (node (ref Q2) (pin 3)))
    (net (code 16) (name "")
      (node (ref P4) (pin C4)))
    (net (code 17) (name /A-B-DETECT)
      (node (ref IC3) (pin 41))
      (node (ref J1) (pin 4))
      (node (ref R2) (pin 1)))
    (net (code 18) (name "")
      (node (ref R3) (pin 2))
      (node (ref Q1) (pin 2)))
    (net (code 19) (name /DDP)
      (node (ref C13) (pin 1))
      (node (ref IC3) (pin 57))
      (node (ref R10) (pin 1)))
    (net (code 20) (name "")
      (node (ref J1) (pin 3))
      (node (ref C5) (pin 2))
      (node (ref R10) (pin 2))
      (node (ref R3) (pin 1)))
    (net (code 21) (name "")
      (node (ref P2) (pin 2))
      (node (ref P2) (pin 6)))
    (net (code 22) (name "")
      (node (ref P2) (pin 3)))
    (net (code 23) (name /TDO)
      (node (ref IC3) (pin 49))
      (node (ref R8) (pin 1))
      (node (ref P1) (pin 13)))
    (net (code 24) (name "")
      (node (ref IC3) (pin 50)))
    (net (code 25) (name "")
      (node (ref JP2) (pin 2))
      (node (ref IC3) (pin 55)))
    (net (code 26) (name "")
      (node (ref IC3) (pin 37)))
    (net (code 27) (name "")
      (node (ref IC3) (pin 19))
      (node (ref R16) (pin 2)))
    (net (code 28) (name /DTXD)
      (node (ref P2) (pin 5))
      (node (ref J2) (pin 3))
      (node (ref IC3) (pin 29)))
    (net (code 29) (name "")
      (node (ref C18) (pin 1))
      (node (ref IC3) (pin 62))
      (node (ref X1) (pin 2)))
    (net (code 30) (name "")
      (node (ref R22) (pin 2))
      (node (ref IC1) (pin 4)))
    (net (code 31) (name //RESET)
      (node (ref P1) (pin 15))
      (node (ref R12) (pin 2))
      (node (ref SW1) (pin 1))
      (node (ref D1) (pin 1))
      (node (ref IC3) (pin 39)))
    (net (code 32) (name /USBVCC)
      (node (ref D2) (pin 2))
      (node (ref FB1) (pin 2)))
    (net (code 33) (name "")
      (node (ref D3) (pin 2))
      (node (ref BT1) (pin 1)))
    (net (code 34) (name "")
      (node (ref D6) (pin 2))
      (node (ref R24) (pin 1))
      (node (ref IC2) (pin 1))
      (node (ref C21) (pin 1)))
    (net (code 35) (name "")
      (node (ref IC3) (pin 42)))
    (net (code 36) (name "")
      (node (ref P1) (pin 19)))
    (net (code 37) (name "")
      (node (ref P1) (pin 17)))
    (net (code 38) (name "")
      (node (ref IC3) (pin 43)))
    (net (code 39) (name /I/O_PHONE)
      (node (ref IC4) (pin 11))
      (node (ref IC3) (pin 14))
      (node (ref P3) (pin 4))
      (node (ref IC3) (pin 11)))
    (net (code 40) (name /CLK_PHONE)
      (node (ref P3) (pin 3))
      (node (ref IC4) (pin 6))
      (node (ref IC3) (pin 15))
      (node (ref IC3) (pin 38)))
    (net (code 41) (name /VCC_SIM)
      (node (ref IC1) (pin 5))
      (node (ref D6) (pin 1))
      (node (ref R15) (pin 1))
      (node (ref C24) (pin 1))
      (node (ref P4) (pin C1)))
    (net (code 42) (name "")
      (node (ref C6) (pin 2))
      (node (ref R11) (pin 2)))
    (net (code 43) (name "")
      (node (ref P1) (pin 3))
      (node (ref R4) (pin 1)))
    (net (code 44) (name /MOSI)
      (node (ref IC3) (pin 22))
      (node (ref U1) (pin 5)))
    (net (code 45) (name /WP)
      (node (ref R17) (pin 1))
      (node (ref U1) (pin 3))
      (node (ref IC3) (pin 20)))
    (net (code 46) (name /TMS)
      (node (ref R6) (pin 1))
      (node (ref IC3) (pin 51))
      (node (ref P1) (pin 7)))
    (net (code 47) (name "")
      (node (ref IC3) (pin 61))
      (node (ref X1) (pin 1))
      (node (ref C17) (pin 1)))
    (net (code 48) (name /BOOTLOADER)
      (node (ref IC3) (pin 52))
      (node (ref SW2) (pin 1)))
    (net (code 49) (name /I/O_SW)
      (node (ref IC4) (pin 19))
      (node (ref IC3) (pin 13)))
    (net (code 50) (name "")
      (node (ref IC3) (pin 63))
      (node (ref C10) (pin 2))
      (node (ref R11) (pin 1)))
    (net (code 51) (name /SW_SIM)
      (node (ref IC3) (pin 31))
      (node (ref P4) (pin SW1)))
    (net (code 52) (name /SIM_PWEN)
      (node (ref IC2) (pin 3))
      (node (ref IC3) (pin 35)))
    (net (code 53) (name "")
      (node (ref R14) (pin 2))
      (node (ref D5) (pin 1)))
    (net (code 54) (name /LED_G)
      (node (ref IC3) (pin 10))
      (node (ref D5) (pin 2)))
    (net (code 55) (name "")
      (node (ref D4) (pin 1))
      (node (ref R13) (pin 2)))
    (net (code 56) (name /LED_R)
      (node (ref D4) (pin 2))
      (node (ref IC3) (pin 9)))
    (net (code 57) (name 3V3)
      (node (ref IC4) (pin 20))
      (node (ref R2) (pin 2))
      (node (ref JP1) (pin 2))
      (node (ref IC2) (pin 6))
      (node (ref IC3) (pin 59))
      (node (ref FB2) (pin 2))
      (node (ref R1) (pin 1))
      (node (ref Q1) (pin 3))
      (node (ref R18) (pin 2))
      (node (ref R26) (pin 1))
      (node (ref JP2) (pin 1))
      (node (ref R13) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref U1) (pin 8))
      (node (ref C22) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref R25) (pin 1))
      (node (ref R14) (pin 1))
      (node (ref R4) (pin 2))
      (node (ref R5) (pin 2))
      (node (ref IC3) (pin 7))
      (node (ref C7) (pin 1))
      (node (ref P1) (pin 2))
      (node (ref P1) (pin 1))
      (node (ref R12) (pin 1))
      (node (ref C9) (pin 1))
      (node (ref IC3) (pin 45))
      (node (ref R6) (pin 2))
      (node (ref R7) (pin 2))
      (node (ref R8) (pin 2))
      (node (ref IC3) (pin 58))
      (node (ref IC3) (pin 48))
      (node (ref IC3) (pin 18)))
    (net (code 58) (name /TDI)
      (node (ref IC3) (pin 33))
      (node (ref R5) (pin 1))
      (node (ref P1) (pin 5)))
    (net (code 59) (name /TCK)
      (node (ref IC3) (pin 53))
      (node (ref P1) (pin 9))
      (node (ref P1) (pin 11))
      (node (ref R7) (pin 1)))
    (net (code 60) (name /VCC_PHONE)
      (node (ref IC3) (pin 25))
      (node (ref R19) (pin 2))
      (node (ref IC1) (pin 1))
      (node (ref R20) (pin 1))
      (node (ref P3) (pin 1))
      (node (ref R22) (pin 1)))
    (net (code 61) (name "")
      (node (ref R9) (pin 2))
      (node (ref J1) (pin 2))
      (node (ref C5) (pin 1)))
    (net (code 62) (name "")
      (node (ref J1) (pin 1))
      (node (ref FB1) (pin 1)))
    (net (code 63) (name /DDM)
      (node (ref C11) (pin 1))
      (node (ref IC3) (pin 56))
      (node (ref R9) (pin 1)))
    (net (code 64) (name "")
      (node (ref FB2) (pin 1))
      (node (ref C23) (pin 1))
      (node (ref IC3) (pin 1)))
    (net (code 65) (name /DRXD)
      (node (ref P2) (pin 4))
      (node (ref J2) (pin 2))
      (node (ref IC3) (pin 30)))
    (net (code 66) (name /RST_PHONE)
      (node (ref R23) (pin 2))
      (node (ref IC3) (pin 23))
      (node (ref P3) (pin 2))
      (node (ref IC4) (pin 4)))
    (net (code 67) (name /VPP_SIM)
      (node (ref P4) (pin C6))
      (node (ref IC4) (pin 12)))
    (net (code 68) (name /VPP_PHONE)
      (node (ref P3) (pin 5))
      (node (ref IC4) (pin 8)))
    (net (code 69) (name /VCC_FWD)
      (node (ref IC1) (pin 3))
      (node (ref IC3) (pin 26)))
    (net (code 70) (name +1.8V)
      (node (ref C12) (pin 1))
      (node (ref C16) (pin 1))
      (node (ref C19) (pin 1))
      (node (ref IC3) (pin 8))
      (node (ref C20) (pin 1))
      (node (ref IC3) (pin 24))
      (node (ref IC3) (pin 12))
      (node (ref C15) (pin 1))
      (node (ref IC3) (pin 64))
      (node (ref IC3) (pin 54)))))